(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.5748)
    (drawings 35)
    (tracks 108)
    (zones 0)
    (modules 31)
    (nets 34)
  )
  (page A3)
  (title_block
    (date "15 nov 2012")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.6096 0.3048)
    (user_via 0.762 0.381)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.1)
    (segment_width 0.1)
    (pcb_text_width 0.15)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 200 150)
    (grid_origin 200 150)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 +5V)
  (net 3 GND)
  (net 4 /I2C1_SDA_5V0)
  (net 5 /I2C1_SCL_5V0)
  (net 6 /I2C1_SDA_3V3)
  (net 7 /I2C1_SCL_3V3)
  (net 8 "Net-(P1-Pad7)")
  (net 9 "Net-(P1-Pad8)")
  (net 10 "Net-(P1-Pad10)")
  (net 11 "Net-(P1-Pad11)")
  (net 12 "Net-(P1-Pad12)")
  (net 13 "Net-(P1-Pad13)")
  (net 14 "Net-(P1-Pad15)")
  (net 15 "Net-(P1-Pad16)")
  (net 16 "Net-(P1-Pad18)")
  (net 17 "Net-(P1-Pad19)")
  (net 18 "Net-(P1-Pad21)")
  (net 19 "Net-(P1-Pad22)")
  (net 20 "Net-(P1-Pad23)")
  (net 21 "Net-(P1-Pad24)")
  (net 22 "Net-(P1-Pad26)")
  (net 23 "Net-(P1-Pad27)")
  (net 24 "Net-(P1-Pad28)")
  (net 25 "Net-(P1-Pad29)")
  (net 26 "Net-(P1-Pad31)")
  (net 27 "Net-(P1-Pad32)")
  (net 28 "Net-(P1-Pad33)")
  (net 29 "Net-(P1-Pad35)")
  (net 30 "Net-(P1-Pad36)")
  (net 31 "Net-(P1-Pad37)")
  (net 32 "Net-(P1-Pad38)")
  (net 33 "Net-(P1-Pad40)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /I2C1_SCL_3V3)
    (add_net /I2C1_SCL_5V0)
    (add_net /I2C1_SDA_3V3)
    (add_net /I2C1_SDA_5V0)
    (add_net GND)
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad18)")
    (add_net "Net-(P1-Pad19)")
    (add_net "Net-(P1-Pad21)")
    (add_net "Net-(P1-Pad22)")
    (add_net "Net-(P1-Pad23)")
    (add_net "Net-(P1-Pad24)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad27)")
    (add_net "Net-(P1-Pad28)")
    (add_net "Net-(P1-Pad29)")
    (add_net "Net-(P1-Pad31)")
    (add_net "Net-(P1-Pad32)")
    (add_net "Net-(P1-Pad33)")
    (add_net "Net-(P1-Pad35)")
    (add_net "Net-(P1-Pad36)")
    (add_net "Net-(P1-Pad37)")
    (add_net "Net-(P1-Pad38)")
    (add_net "Net-(P1-Pad40)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.635)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net +3V3)
    (add_net +5V)
  )
  (module sqwr:sqwr_dark (layer B.Cu) (tedit 5D1BF471)
    (at 232.49168 122.36734 180)
    (descr "Imported from /Users/spacehog/Downloads/logo2 (1).svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference svg2mod (at 0 24.838943) (layer B.SilkS) hide)
    (fp_text value G*** (at 0 -24.838943) (layer B.SilkS) hide)
  )
  (module sqwr:sqwr_dark (layer F.Cu) (tedit 5D1B122C)
    (at 220.27682 117.28988)
    (descr "Imported from /Users/spacehog/Downloads/sqwr_solid.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 3.048) (layer F.SilkS) hide)
  )
  (module sqwr:sqwr_dark (layer F.Cu) (tedit 5D1B122C)
    (at 245.7962 117.7293)
    (descr "Imported from /Users/spacehog/Downloads/sqwr_solid.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 3.048) (layer F.SilkS) hide)
  )
  (module sqwr:sqwr_dark (layer F.Cu) (tedit 5D1B122C)
    (at 224.8666 118.16618)
    (descr "Imported from /Users/spacehog/Downloads/sqwr_solid.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 3.048) (layer F.SilkS) hide)
  )
  (module sqwr:sqwr_dark (layer F.Cu) (tedit 5D1B122C)
    (at 214.8844 118.31096)
    (descr "Imported from /Users/spacehog/Downloads/sqwr_solid.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 3.048) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 261.5 146.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK4 (at 0 -3.7) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 203.5 146.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK3 (at 0 -3.7) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 261.5 97.5 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK2 (at 0 -3.7) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 203.5 97.5 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK1 (at 0 -3.7) (layer F.SilkS))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 209.37514 130.85602)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP7 (at -2.57556 0) (layer F.SilkS))
    (fp_text value TP_GND (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 3 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 205.93598 108.5218)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP6 (at -2.51968 0) (layer F.SilkS))
    (fp_text value TP_P5V0 (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 2 +5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 205.93598 105.62112)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP5 (at -2.59842 -0.09652) (layer F.SilkS))
    (fp_text value TP_P3V3 (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 1 +3V3))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 210.87882 128.8164)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP4 (at -2.57302 0) (layer F.SilkS))
    (fp_text value TP_I2C1_SCL_5V0 (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 5 /I2C1_SCL_5V0))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 209.26846 126.66756)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP3 (at -3.12166 0.05334) (layer F.SilkS))
    (fp_text value TP_I2C1_SDA_5V0 (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 4 /I2C1_SDA_5V0))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 235.814 106.10626)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP2 (at 2.65176 0.05334) (layer F.SilkS))
    (fp_text value TP_I2C1_SCL_3V3 (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 7 /I2C1_SCL_3V3))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 218.3769 106.13166)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP1 (at 2.58064 0.05334) (layer F.SilkS))
    (fp_text value TP_I2C1_SDA_3V3 (at 2.52984 2.80924) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 6 /I2C1_SDA_3V3))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering_RevA_Date25Jun2010 (layer F.Cu) (tedit 0)
    (at 230.80004 111.46566 180)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering, Rev A, Date 25 Jun 2010,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering, Rev A, Date 25 Jun 2010,")
    (fp_text reference R4 (at 0.09906 -3.0988) (layer F.SilkS))
    (fp_text value 4K7 (at -0.39878 4.20116) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.99898 0 180) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 2 smd trapezoid (at 1.99898 0) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 +5V))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering_RevA_Date25Jun2010 (layer F.Cu) (tedit 0)
    (at 213.37564 111.46566 180)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering, Rev A, Date 25 Jun 2010,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering, Rev A, Date 25 Jun 2010,")
    (fp_text reference R3 (at 0.09906 -3.0988) (layer F.SilkS))
    (fp_text value 4K7 (at -0.39878 4.20116) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.99898 0 180) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 2 smd trapezoid (at 1.99898 0) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 +5V))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering_RevA_Date25Jun2010 (layer F.Cu) (tedit 0)
    (at 230.80004 103.15478 180)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering, Rev A, Date 25 Jun 2010,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering, Rev A, Date 25 Jun 2010,")
    (fp_text reference R2 (at 7.48284 -0.10922) (layer F.SilkS))
    (fp_text value DNP (at -0.39878 4.20116) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.99898 0 180) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 7 /I2C1_SCL_3V3))
    (pad 2 smd trapezoid (at 1.99898 0) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 7 /I2C1_SCL_3V3))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 +3V3))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering_RevA_Date25Jun2010 (layer F.Cu) (tedit 0)
    (at 213.37564 103.28686 180)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering, Rev A, Date 25 Jun 2010,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering, Rev A, Date 25 Jun 2010,")
    (fp_text reference R1 (at 7.5438 0) (layer F.SilkS))
    (fp_text value DNP (at -0.39878 4.20116) (layer F.Fab))
    (pad 1 smd trapezoid (at -1.99898 0 180) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 6 /I2C1_SDA_3V3))
    (pad 2 smd trapezoid (at 1.99898 0) (size 2.79908 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 /I2C1_SDA_3V3))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 +3V3))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 229.80106 107.328)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 1.921 1.3462) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /I2C1_SCL_3V3))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /I2C1_SCL_5V0))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 212.37666 107.328)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.94894 1.4224) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 /I2C1_SDA_3V3))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 /I2C1_SDA_5V0))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 260.30976 124.74732 270)
    (descr "JST PH series connector, B4B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J8 (at -4.09194 0.6175 90) (layer F.SilkS))
    (fp_text value CONN_JST_01x04 (at 3 3.8 90) (layer F.Fab))
    (fp_text user %R (at 3 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B4B-PH-K_04x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 254.0385 124.74732 270)
    (descr "JST PH series connector, B4B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J7 (at -4.09194 0.6175 90) (layer F.SilkS))
    (fp_text value CONN_JST_01x04 (at 3 3.8 90) (layer F.Fab))
    (fp_text user %R (at 3 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B4B-PH-K_04x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 247.76724 124.74732 270)
    (descr "JST PH series connector, B4B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J6 (at -4.09194 0.6175 90) (layer F.SilkS))
    (fp_text value CONN_JST_01x04 (at 3 3.8 90) (layer F.Fab))
    (fp_text user %R (at 3 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B4B-PH-K_04x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 241.49598 124.74732 270)
    (descr "JST PH series connector, B4B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J5 (at -4.09194 0.6175 90) (layer F.SilkS))
    (fp_text value CONN_JST_01x04 (at 3 3.8 90) (layer F.Fab))
    (fp_text user %R (at 3 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B4B-PH-K_04x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 235.22472 124.76002 270)
    (descr "JST PH series connector, B4B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J4 (at -4.09194 0.6175 90) (layer F.SilkS))
    (fp_text value CONN_JST_01x04 (at 3 3.8 90) (layer F.Fab))
    (fp_text user %R (at 3 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B4B-PH-K_04x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 228.95346 124.76002 270)
    (descr "JST PH series connector, B4B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J3 (at -4.09194 0.6175 90) (layer F.SilkS))
    (fp_text value CONN_JST_01x04 (at 3 3.8 90) (layer F.Fab))
    (fp_text user %R (at 3 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B4B-PH-K_04x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 222.6822 124.76002 270)
    (descr "JST PH series connector, B4B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J2 (at -4.09194 0.6175 90) (layer F.SilkS))
    (fp_text value CONN_JST_01x04 (at 3 3.8 90) (layer F.Fab))
    (fp_text user %R (at 3 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B4B-PH-K_04x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_B4B-PH-K_04x2.00mm_Straight (layer F.Cu) (tedit 58D3FE4F)
    (at 216.41094 124.76002 270)
    (descr "JST PH series connector, B4B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J1 (at -4.09194 0.6175 90) (layer F.SilkS))
    (fp_text value CONN_JST_01x04 (at 3 3.8 90) (layer F.Fab))
    (fp_text user %R (at 3 1.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /I2C1_SDA_5V0))
    (pad 3 thru_hole oval (at 4 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /I2C1_SCL_5V0))
    (pad 4 thru_hole oval (at 6 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B4B-PH-K_04x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433)
    (at 208.37 98.77 270)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference P1 (at 2.208 1.512) (layer B.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at -1.27 -51.03 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -24.13 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /I2C1_SDA_3V3))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /I2C1_SCL_3V3))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad16)"))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad18)"))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(P1-Pad19)"))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(P1-Pad21)"))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P1-Pad22)"))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(P1-Pad23)"))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P1-Pad24)"))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P1-Pad26)"))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(P1-Pad27)"))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P1-Pad28)"))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P1-Pad29)"))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P1-Pad31)"))
    (pad 32 thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P1-Pad32)"))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P1-Pad33)"))
    (pad 34 thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P1-Pad35)"))
    (pad 36 thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P1-Pad36)"))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad37)"))
    (pad 38 thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P1-Pad38)"))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 40 thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(P1-Pad40)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Raspberry Pi I2C Breakout x8 5V0 Rev1" (at 222.01672 146.63704) (layer F.SilkS))
  (gr_arc (start 200.5 131) (end 200 131) (angle 89.9) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 204.5 130) (end 205 130) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 200.5 113) (end 200.5 113.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 204.5 114) (end 204.5 113.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200 97) (end 200 113) (layer Edge.Cuts) (width 0.1))
  (gr_text DISPLAY (at 202.5 122 90) (layer Dwgs.User))
  (gr_text RJ45 (at 276.2 139.84) (layer Dwgs.User))
  (gr_text USB (at 277.724 121.552) (layer Dwgs.User))
  (gr_text USB (at 278.232 102.248) (layer Dwgs.User))
  (gr_arc (start 262 97) (end 262 94) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 262 147) (end 265 147) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 203 147) (end 203 150) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 203 97) (end 200 97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 262 94) (end 203 94) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 204.5 130.5) (end 200.5 130.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 205 114) (end 205 130) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200.5 113.5) (end 204.5 113.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 265 147) (end 265 97) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 203 150) (end 262 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200 131) (end 200 147) (layer Edge.Cuts) (width 0.1))
  (gr_text "RASPBERRY-PI 40-PIN ADDON BOARD\nVIEW FROM TOP\nNOTE: P1 SHOULD BE FITTED ON THE REVERSE OF THE BOARD\n\nADD EDGE CUTS FROM CAMERA AND DISPLAY PORTS AS REQUIRED" (at 200 160.16) (layer Dwgs.User))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 265.15608 149.99238) (xy 264.8462 94.18096) (xy 199.43104 94.18096) (xy 199.7968 150.11684) (xy 224.27732 149.99238)
        (xy 265.15608 149.99238) (xy 264.91224 150.11684)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 265.28054 150.23876) (xy 199.93904 150.36068) (xy 199.8349 94.4248) (xy 265.07226 93.93712)
      )
    )
  )
)
