<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22" y2="0" width="0" layer="20"/>
<wire x1="35.5" y1="4.5" x2="35.5" y2="20.5" width="0" layer="20"/>
<wire x1="22" y1="25" x2="0" y2="25" width="0" layer="20"/>
<wire x1="0" y1="25" x2="0" y2="0" width="0" layer="20"/>
<hole x="19.5" y="22" drill="3.2"/>
<hole x="19.5" y="3" drill="3.2"/>
<wire x1="22" y1="25" x2="35.5" y2="20.5" width="0" layer="20"/>
<wire x1="22" y1="0" x2="35.5" y2="4.5" width="0" layer="20"/>
<text>Mo
Power</text>
<text>britt@shapetable.com</text>
<text>2020</text>
</plain>
<libraries>
<library name="diskpower">
<packages>
<package name="AMP-RT-DISK-POWER">
</package>
</packages>
</library>
<library name="con-usb (1)">
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J5" library="diskpower" package="AMP-RT-DISK-POWER" value="AMP-DISK-POWER"/>
<element name="J7" library="con-usb (1)" package="USB-A-H" value="USB-A-H"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="3"/>
<contactref element="J7" pad="GND"/>
</signal>
<signal name="VCC">
<contactref element="J5" pad="1"/>
<contactref element="J7" pad="VBUS"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
