<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="29.1338" width="0" layer="20"/>
<wire x1="0" y1="29.1338" x2="21.082" y2="29.1338" width="0" layer="20"/>
<wire x1="21.082" y1="29.1338" x2="21.082" y2="0" width="0" layer="20"/>
<wire x1="21.082" y1="0" x2="0" y2="0" width="0" layer="20"/>
<text>A</text>
<text>R1</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>VR</text>
<text>C3</text>
<text>C2</text>
<text>C1</text>
<text>5V</text>
<text>GND</text>
<text>IRQ</text>
<text>SEL</text>
<text>SDI</text>
<text>SDO</text>
<text>SCK</text>
<text>D10\</text>
<text>D2</text>
<text>D11</text>
<text>D12</text>
<text>D13</text>
<text>R2</text>
<text>R3</text>
<text>3V3</text>
<text>G</text>
<text>Ant.</text>
<text>VCC</text>
<text>GND</text>
</plain>
<libraries>
<library name="JeeLabs">
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="lh-library">
<packages>
<package name="SJ_2S-NO-NOSILK">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="MA08-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="RFM12B">
<description>RFM12B radio module by HopeRF</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="ChipsParts">
<packages>
<package name="0805-POL">
</package>
<package name="SOT-89">
<description>SOT-89 Package from www.microchip.com/packaging</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1µ"/>
<element name="ANT" library="JeeLabs" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="10k"/>
<element name="R2" library="SparkFun-Resistors" package="0805" value="4k7"/>
<element name="R5" library="SparkFun-Resistors" package="0805" value="10k"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="4k7"/>
<element name="R6" library="SparkFun-Resistors" package="0805" value="10k"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="4k7"/>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.1µ"/>
<element name="C3" library="ChipsParts" package="0805-POL" value="10µ"/>
<element name="U$2" library="lh-library" package="RFM12B" value="RFM12B">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="lh-library" package="SJ_2S-NO-NOSILK" value="SOLDERJUMPERNO-NOSILK"/>
<element name="SJ2" library="lh-library" package="SJ_2S-NO-NOSILK" value="SOLDERJUMPERNO-NOSILK"/>
<element name="SJ3" library="lh-library" package="SJ_2S-NO-NOSILK" value="SOLDERJUMPERNO-NOSILK"/>
<element name="GND" library="JeeLabs" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="lh-library" package="MA08-1" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="ChipsParts" package="SOT-89" value="MCP1701"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U$2" pad="GND"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="GND" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="VDD"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="8"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="ANT" pad="1"/>
<contactref element="U$2" pad="ANT"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="U$2" pad="SCK"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U$2" pad="SDI"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="SJ3" pad="1"/>
<contactref element="U$2" pad="SEL"/>
</signal>
<signal name="IRQ">
<contactref element="U$2" pad="IRQ"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="SDI">
<contactref element="R2" pad="2"/>
<contactref element="SJ2" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="SDO">
<contactref element="U$2" pad="SDO"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="SEL">
<contactref element="R3" pad="2"/>
<contactref element="SJ3" pad="2"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="SCK">
<contactref element="SJ1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
