(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 15)
    (no_connects 0)
    (area 83.919287 84.93 145.01 123.985001)
    (thickness 1.6)
    (drawings 49)
    (tracks 25)
    (zones 0)
    (modules 14)
    (nets 11)
  )
  (page A4)
  (title_block
    (title "ZX Spectrum +2A/3 Composite Video PCB")
    (date 2016-12-20)
    (rev 0.99)
    (comment 4 "PCB footprint scaled down to fit within the RF modulator casing")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4572)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 142.24 83.185)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C301-Pad1)")
  (net 2 "Net-(C301-Pad2)")
  (net 3 "Net-(D301-Pad2)")
  (net 4 "Net-(D301-Pad1)")
  (net 5 "Net-(D302-Pad1)")
  (net 6 "Net-(D303-Pad1)")
  (net 7 "Net-(L301-Pad1)")
  (net 8 "Net-(P301-Pad4)")
  (net 9 "Net-(P302-Pad1)")
  (net 10 "Net-(Q301-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.4572)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C301-Pad2)")
    (add_net "Net-(D301-Pad1)")
    (add_net "Net-(D301-Pad2)")
    (add_net "Net-(D302-Pad1)")
    (add_net "Net-(D303-Pad1)")
    (add_net "Net-(L301-Pad1)")
  )
  (net_class +12 ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P301-Pad4)")
  )
  (net_class COVO ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P302-Pad1)")
    (add_net "Net-(Q301-Pad1)")
  )
  (net_class GND ""
    (clearance 0.1524)
    (trace_width 0.762)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C301-Pad1)")
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 5858EEAF)
    (at 118.11 100.965 270)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D301 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.41452 -3.55854 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D301-Pad2)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D301-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5858EE58)
    (at 129.54 112.395 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C301 (at 1.27 -2.54 450) (layer F.SilkS))
    (fp_text value 39p (at 1.25 2.5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C301-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C301-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585913C1)
    (at 129.54 109.855 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C302 (at 1.27 2.54 90) (layer F.SilkS))
    (fp_text value 47p (at 1.25 2.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C301-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C301-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 5858ED97)
    (at 120.65 100.965 270)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D302 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.41452 -3.55854 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D301-Pad1)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D302-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-35_SOD27_Horizontal_RM10 (layer F.Cu) (tedit 58591426)
    (at 123.19 100.965 270)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference D303 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.41452 -3.55854 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 10.16052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D302-Pad1)"))
    (pad 1 thru_hole rect (at 0.00052 -0.00254 90) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D303-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5858E7D1)
    (at 116.205 113.665)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference L301 (at 5.08 0) (layer F.SilkS))
    (fp_text value 15m (at 5.08 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(L301-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C301-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58593315)
    (at 113.03 113.665 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P301 (at -2.54 3.81 450) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(L301-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C301-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D301-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P301-Pad4)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 58591552)
    (at 113.03 98.425)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P302 (at 0 5.08 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P302-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C301-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 5859259F)
    (at 129.54 98.425 270)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q301 (at 6.985 -0.635 540) (layer F.SilkS))
    (fp_text value 2N3904 (at 0 3 270) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D303-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P301-Pad4)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(Q301-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 5858E653)
    (at 126.365 100.965 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R301 (at 5.08 0 270) (layer F.SilkS))
    (fp_text value 1.5k (at 5.08 3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(D303-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 "Net-(C301-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 585914E6)
    (at 116.205 98.425)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R302 (at 5.08 0) (layer F.SilkS))
    (fp_text value 75 (at 5.08 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(P302-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(Q301-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 585917C6)
    (at 112.395 116.84)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 2) (layer B.SilkS) hide)
    (fp_text value Measurement_Point_Square-SMD-Pad_Small (at 0 -2) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 585917D3)
    (at 123.19 95.885)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 2) (layer B.SilkS) hide)
    (fp_text value Measurement_Point_Square-SMD-Pad_Small (at 0 -2) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask))
  )
  (module "ZXSpecc+2 video mods:logo-speccypl" (layer F.Cu) (tedit 0)
    (at 121.92 116.84)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (dimension 35.56 (width 0.3) (layer Margin)
    (gr_text "1.4000 in" (at 116.205 123.27) (layer Margin))
    (feature1 (pts (xy 133.985 118.11) (xy 133.985 124.62)))
    (feature2 (pts (xy 98.425 118.11) (xy 98.425 124.62)))
    (crossbar (pts (xy 98.425 121.92) (xy 133.985 121.92)))
    (arrow1a (pts (xy 133.985 121.92) (xy 132.858496 122.506421)))
    (arrow1b (pts (xy 133.985 121.92) (xy 132.858496 121.333579)))
    (arrow2a (pts (xy 98.425 121.92) (xy 99.551504 122.506421)))
    (arrow2b (pts (xy 98.425 121.92) (xy 99.551504 121.333579)))
  )
  (gr_text "PCB v0.95 footprint" (at 92.075 107.315 90) (layer Cmts.User))
  (dimension 25.4 (width 0.3) (layer Cmts.User)
    (gr_text "1.0000 in" (at 86.28 107.315 90) (layer Cmts.User))
    (feature1 (pts (xy 90.805 94.615) (xy 84.93 94.615)))
    (feature2 (pts (xy 90.805 120.015) (xy 84.93 120.015)))
    (crossbar (pts (xy 87.63 120.015) (xy 87.63 94.615)))
    (arrow1a (pts (xy 87.63 94.615) (xy 88.216421 95.741504)))
    (arrow1b (pts (xy 87.63 94.615) (xy 87.043579 95.741504)))
    (arrow2a (pts (xy 87.63 120.015) (xy 88.216421 118.888496)))
    (arrow2b (pts (xy 87.63 120.015) (xy 87.043579 118.888496)))
  )
  (dimension 23.495 (width 0.3) (layer Margin)
    (gr_text "0.9250 in" (at 93.9 106.3625 90) (layer Margin))
    (feature1 (pts (xy 98.425 94.615) (xy 92.55 94.615)))
    (feature2 (pts (xy 98.425 118.11) (xy 92.55 118.11)))
    (crossbar (pts (xy 95.25 118.11) (xy 95.25 94.615)))
    (arrow1a (pts (xy 95.25 94.615) (xy 95.836421 95.741504)))
    (arrow1b (pts (xy 95.25 94.615) (xy 94.663579 95.741504)))
    (arrow2a (pts (xy 95.25 118.11) (xy 95.836421 116.983496)))
    (arrow2b (pts (xy 95.25 118.11) (xy 94.663579 116.983496)))
  )
  (dimension 43.18 (width 0.3) (layer Cmts.User)
    (gr_text "1.7000 in" (at 112.395 126.445) (layer Cmts.User))
    (feature1 (pts (xy 90.805 120.015) (xy 90.805 127.795)))
    (feature2 (pts (xy 133.985 120.015) (xy 133.985 127.795)))
    (crossbar (pts (xy 133.985 125.095) (xy 90.805 125.095)))
    (arrow1a (pts (xy 90.805 125.095) (xy 91.931504 124.508579)))
    (arrow1b (pts (xy 90.805 125.095) (xy 91.931504 125.681421)))
    (arrow2a (pts (xy 133.985 125.095) (xy 132.858496 124.508579)))
    (arrow2b (pts (xy 133.985 125.095) (xy 132.858496 125.681421)))
  )
  (gr_line (start 111.76 94.615) (end 110.49 95.885) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.715 94.615) (end 111.76 94.615) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.985 95.885) (end 132.715 94.615) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.985 116.84) (end 133.985 95.885) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.715 118.11) (end 133.985 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.76 118.11) (end 132.715 118.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 116.84) (end 111.76 118.11) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.49 95.885) (end 110.49 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 23.495 (width 0.3) (layer Dwgs.User)
    (gr_text "0.9250 in" (at 106.6 106.3625 90) (layer Dwgs.User))
    (feature1 (pts (xy 110.49 94.615) (xy 105.25 94.615)))
    (feature2 (pts (xy 110.49 118.11) (xy 105.25 118.11)))
    (crossbar (pts (xy 107.95 118.11) (xy 107.95 94.615)))
    (arrow1a (pts (xy 107.95 94.615) (xy 108.536421 95.741504)))
    (arrow1b (pts (xy 107.95 94.615) (xy 107.363579 95.741504)))
    (arrow2a (pts (xy 107.95 118.11) (xy 108.536421 116.983496)))
    (arrow2b (pts (xy 107.95 118.11) (xy 107.363579 116.983496)))
  )
  (gr_text "RF converter PCB footprint" (at 99.695 106.045 90) (layer Margin))
  (dimension 35.56 (width 0.3) (layer Margin)
    (gr_text "35.560 mm" (at 116.205 86.28) (layer Margin))
    (feature1 (pts (xy 133.985 94.615) (xy 133.985 84.93)))
    (feature2 (pts (xy 98.425 94.615) (xy 98.425 84.93)))
    (crossbar (pts (xy 98.425 87.63) (xy 133.985 87.63)))
    (arrow1a (pts (xy 133.985 87.63) (xy 132.858496 88.216421)))
    (arrow1b (pts (xy 133.985 87.63) (xy 132.858496 87.043579)))
    (arrow2a (pts (xy 98.425 87.63) (xy 99.551504 88.216421)))
    (arrow2b (pts (xy 98.425 87.63) (xy 99.551504 87.043579)))
  )
  (dimension 23.495 (width 0.3) (layer Margin)
    (gr_text "23.495 mm" (at 138.51 106.3625 270) (layer Margin))
    (feature1 (pts (xy 133.985 118.11) (xy 139.86 118.11)))
    (feature2 (pts (xy 133.985 94.615) (xy 139.86 94.615)))
    (crossbar (pts (xy 137.16 94.615) (xy 137.16 118.11)))
    (arrow1a (pts (xy 137.16 118.11) (xy 136.573579 116.983496)))
    (arrow1b (pts (xy 137.16 118.11) (xy 137.746421 116.983496)))
    (arrow2a (pts (xy 137.16 94.615) (xy 136.573579 95.741504)))
    (arrow2b (pts (xy 137.16 94.615) (xy 137.746421 95.741504)))
  )
  (gr_text 4 (at 111.125 106.045) (layer B.SilkS))
  (gr_text P301 (at 113.03 104.14) (layer B.SilkS))
  (gr_text 1 (at 111.125 113.665) (layer B.SilkS))
  (dimension 23.495 (width 0.3) (layer Dwgs.User)
    (gr_text "0.9250 in" (at 122.2375 90.725) (layer Dwgs.User))
    (feature1 (pts (xy 133.985 94.615) (xy 133.985 89.375)))
    (feature2 (pts (xy 110.49 94.615) (xy 110.49 89.375)))
    (crossbar (pts (xy 110.49 92.075) (xy 133.985 92.075)))
    (arrow1a (pts (xy 133.985 92.075) (xy 132.858496 92.661421)))
    (arrow1b (pts (xy 133.985 92.075) (xy 132.858496 91.488579)))
    (arrow2a (pts (xy 110.49 92.075) (xy 111.616504 92.661421)))
    (arrow2b (pts (xy 110.49 92.075) (xy 111.616504 91.488579)))
  )
  (gr_text "1. Video\n2. GND" (at 116.205 104.14 90) (layer F.SilkS))
  (gr_text "v. 0.99" (at 132.715 111.125 90) (layer B.Cu))
  (gr_text "P301:\n1. LUMI\n2. GND\n3. COVO\n4. +12V" (at 119.38 106.045) (layer B.SilkS))
  (gr_text "ZX Spectrum +2/3 Comp.Video" (at 121.92 95.885) (layer F.SilkS))
  (zone (net 1) (net_name "Net-(C301-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.985 95.885) (xy 133.985 116.84) (xy 132.715 118.11) (xy 111.76 118.11) (xy 110.49 116.84)
        (xy 110.49 95.885) (xy 111.76 94.615) (xy 132.715 94.615)
      )
    )
  )
)
