(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 40)
    (zones 0)
    (modules 8)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.8 6.8)
    (pad_drill 6.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory "DXF Files/"))
  )
  (net 0 "")
  (net 1 M1A)
  (net 2 M1B)
  (net 3 M2A)
  (net 4 M2B)
  (net 5 3_3V)
  (net 6 GND)
  (net 7 ROT_POT)
  (net 8 LIN_POT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3_3V)
    (add_net GND)
    (add_net LIN_POT)
    (add_net M1A)
    (add_net M1B)
    (add_net M2A)
    (add_net M2B)
    (add_net ROT_POT)
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 91.25 126.5)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference m3 (at 2.31 0.06) (layer F.SilkS))
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 4.77 -1.12) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_5.3mm_M5 (layer F.Cu) (tedit 6027E731)
    (at 94.06 119.6)
    (descr "Mounting Hole 5.3mm, no annular, M5")
    (tags "mounting hole 5.3mm no annular m5")
    (attr virtual)
    (fp_text reference Lm (at 3.78 -3.64) (layer F.SilkS))
    (fp_text value MountingHole_5.3mm_M5 (at 0 6.3) (layer F.Fab))
    (fp_text user %R (at -2.62 1.98) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 6.8 6.8) (drill 6.8) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_5.3mm_M5 (layer F.Cu) (tedit 6027E698)
    (at 82.5 128.8)
    (descr "Mounting Hole 5.3mm, no annular, M5")
    (tags "mounting hole 5.3mm no annular m5")
    (attr virtual)
    (fp_text reference wires (at -2.77 -1.94 70) (layer F.SilkS))
    (fp_text value MountingHole_5.3mm_M5 (at 0 6.3) (layer F.Fab))
    (fp_text user %R (at -2.62 1.98) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 5 5) (drill 5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 97.3 124.6)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference m2 (at 1.24 -1.78) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 3.51 -1.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 79.6 116.3)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference m1 (at 2.45 0.63) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 3.57 -2.83) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 77.260399 130.183806 165)
    (descr "Through hole angled pin header, 2x05, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x05 2.54mm double row")
    (fp_text reference J1 (at 0.968992 -2.605777 165) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 5.655 12.43 165) (layer F.Fab))
    (fp_text user %R (at 5.31 5.08 75) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 3_3V))
    (pad 4 thru_hole oval (at 2.54 2.54 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 5 thru_hole oval (at 0 5.08 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 ROT_POT))
    (pad 6 thru_hole oval (at 2.54 5.08 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 LIN_POT))
    (pad 7 thru_hole oval (at 0 7.62 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 M2A))
    (pad 8 thru_hole oval (at 2.54 7.62 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 M2B))
    (pad 9 thru_hole oval (at 0 10.16 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 M1A))
    (pad 10 thru_hole oval (at 2.54 10.16 165) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 M1B))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F98)
    (at 83.39 121.65)
    (descr "Terminal Block Phoenix MPT-0,5-2-2.54, 2 pins, pitch 2.54mm, size 5.54x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-2-2.54 pitch 2.54mm size 5.54x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J2 (at 4.95 0.13) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 1.27 4.16) (layer F.Fab))
    (fp_text user %R (at 5.11 2.66) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 M1A))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 M1B))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 5B294F99)
    (at 88.019409 132.6 210)
    (descr "Terminal Block Phoenix MPT-0,5-6-2.54, 6 pins, pitch 2.54mm, size 15.7x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MPT-0,5-6-2.54 pitch 2.54mm size 15.7x6.2mm^2 drill 1.1mm pad 2.2mm")
    (fp_text reference J3 (at 15.204735 -2.156556 30) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x06 (at 6.35 4.16 30) (layer F.Fab))
    (fp_text user %R (at 6.35 2 30) (layer F.Fab))
    (pad 6 thru_hole circle (at 12.7 0 210) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 5 thru_hole circle (at 10.16 0 210) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 3_3V))
    (pad 4 thru_hole circle (at 7.62 0 210) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 LIN_POT))
    (pad 3 thru_hole circle (at 5.08 0 210) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 ROT_POT))
    (pad 2 thru_hole circle (at 2.54 0 210) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 M2B))
    (pad 1 thru_hole rect (at 0 0 210) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 M2A))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MSRAL\n2021\nBVJ" (at 91.85 130.78 30) (layer F.SilkS))
  (gr_text V (at 76.93 133.94 -150) (layer F.SilkS))
  (gr_text L (at 79.09 132.67 -150) (layer F.SilkS))
  (gr_text R (at 81.06 131.62 -150) (layer F.SilkS))
  (gr_text M2A (at 86.82 128.19 -150) (layer F.SilkS))
  (gr_text M1B (at 85.86 126.17) (layer F.SilkS))
  (gr_text "GND\n" (at 74.76 135.14 -150) (layer F.SilkS))
  (gr_line (start 94 129.58) (end 94 133.45) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.3 126.28) (end 100 126.28) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 97.3 129.58) (end 97.3 126.28) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 81 113.73) (end 78.780001 113.730001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 84.18 117.88) (end 81 113.73) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 102.5 131.44) (end 78.780001 113.730001) (angle -61.85647624) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 94 133.45) (end 75.695582 144.002071) (layer Edge.Cuts) (width 0.05))
  (target plus (at 94.06 119.6) (size 5) (width 0.05) (layer Edge.Cuts))
  (gr_line (start 100 115.21) (end 100 126.28) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 91.75 115.21) (end 100 115.21) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87.56 117.88) (end 91.75 115.21) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 84.18 117.88) (end 87.56 117.88) (layer Edge.Cuts) (width 0.05))
)
