(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "olmBoard")
    (date "2019-11-03")
    (rev "0.1")
    (comment 1 "by azerimaker")
  )
  (layers
    (0 "F.Cu" mixed)
    (31 "B.Cu" power)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "C:/Users/RWB/Dropbox/PCB Design Files/PowerBank_5Ah_Design Files/Gerbers/3vNanoBuck/")
    )
  )
  (net 0 "")
  (net 1 "/Vin")
  (net 2 "GND")
  (net 3 "/Vout")
  (net 4 "Net-(JP4-Pad1)")
  (net 5 "Net-(L1-Pad1)")
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 153.983 100.27 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "MPN" "CL10A106MO8NQNC")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 1.303 -0.193 180) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "CAP, CERM, 10 µF, 4 V, ±20%, X5R, 0402" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text user "CL05A106MR5NRNC" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/Vin") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 155.38 100.27 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "MPN" "GRM188B31A475KE15D")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 1.353 -0.04 180) (layer "F.SilkS") hide)
    (fp_text value "4.7uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "0402 10 V 4.7 uF ±20% Tolerance X5R" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text user "GRM155R61A475MEAAD" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/Vin") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 157.47 99.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "MPN" "CL10A106MO8NQNC")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -6.49 -0.01) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "CAP, CERM, 10 µF, 4 V, ±20%, X5R, 0402" (at 0 0 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "CL05A106MR5NRNC" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/Vout") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 157.47 98.203 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "MPN" "CL10A106MO8NQNC")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -6.39 -0.107) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "CAP, CERM, 10 µF, 4 V, ±20%, X5R, 0402" (at 0 0 180 unlocked) (layer "F.SilkS") hide)
    (fp_text user "CL05A106MR5NRNC" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/Vout") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBE)
    (at 154.5 98.18)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "MPN" "GRM188B31A475KE15D")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 2.395 0.0195) (layer "F.SilkS") hide)
    (fp_text value "4.7uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "0402 10 V 4.7 uF ±20% Tolerance X5R" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text user "GRM155R61A475MEAAD" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/Vout") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "my_passives_footprints:L_0806" (layer "F.Cu")
    (tedit 5DBF3424)
    (at 160.04 100.13 90)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "MPN" "TFM201610GHM-2R2MTAA")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at 0 1.7145 180) (layer "F.SilkS") hide)
    (fp_text value "2.2uH" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "2.2uH 20% 1MHz Metal 1.8A 0.116Ohm DCR 0806 " (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text user "DFE201612E-2R2M=P2" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9375 0 90) (size 0.62 1.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(L1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9375 0 90) (size 0.62 1.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "/Vout") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TPS62840YBGR:BGA6N40P3X2_146X96X50N" (layer "F.Cu")
    (tedit 62AE8BC3)
    (at 157.53 101.33)
    (property "ALPHA_ROWS" "True")
    (property "A_MAX" "0.5")
    (property "A_MIN" "0.5")
    (property "A_NOM" "0.5")
    (property "BALL_COLUMNS" "")
    (property "BALL_ROWS" "")
    (property "BODY_DIAMETER" "")
    (property "B_NOM" "0.25")
    (property "COLLAPSING_BALL" "False")
    (property "COURTYARD_EXCESS" "1.0")
    (property "DMAX" "")
    (property "DMIN" "")
    (property "DNOM" "0.4")
    (property "D_MAX" "1.468")
    (property "D_MIN" "1.468")
    (property "D_NOM" "1.468")
    (property "EMAX" "")
    (property "EMIN" "")
    (property "ENOM" "0.4")
    (property "E_MAX" "0.968")
    (property "E_MIN" "0.968")
    (property "E_NOM" "0.968")
    (property "IPC" "")
    (property "JEDEC" "")
    (property "MANUFACTURER" "Texas Instruments")
    (property "PACKAGE_TYPE" "")
    (property "PARTREV" "D")
    (property "PINS" "")
    (property "PIN_COLUMNS" "")
    (property "PIN_COUNT_D" "3.0")
    (property "PIN_COUNT_E" "2.0")
    (property "SNAPEDA_PACKAGE_ID" "")
    (property "STANDARD" "IPC 7351B")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (property "THERMAL_PAD" "")
    (property "VACANCIES" "")
    (attr through_hole)
    (fp_text reference "U1" (at 1.691 -2.369) (layer "F.SilkS"))
    (fp_text value "TPS62840YBGR" (at 12.486 2.369) (layer "F.Fab"))
    (pad "A1" smd circle locked (at -0.2 -0.4) (size 0.25 0.25) (layers "F.Cu" "F.Paste")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (clearance 0.05))
    (pad "A2" smd circle locked (at 0.2 -0.4) (size 0.25 0.25) (layers "F.Cu" "F.Paste")
      (net 3 "/Vout") (pinfunction "VOS") (pintype "input") (clearance 0.05))
    (pad "B1" smd circle locked (at -0.2 0) (size 0.25 0.25) (layers "F.Cu" "F.Paste")
      (net 1 "/Vin") (pinfunction "VIN") (pintype "input") (clearance 0.05))
    (pad "B2" smd circle locked (at 0.2 0) (size 0.25 0.25) (layers "F.Cu" "F.Paste")
      (net 5 "Net-(L1-Pad1)") (pinfunction "SW") (pintype "passive") (clearance 0.05))
    (pad "C1" smd circle locked (at -0.2 0.4) (size 0.25 0.25) (layers "F.Cu" "F.Paste")
      (net 1 "/Vin") (pinfunction "EN") (pintype "input") (clearance 0.05))
    (pad "C2" smd circle locked (at 0.2 0.4) (size 0.25 0.25) (layers "F.Cu" "F.Paste")
      (net 4 "Net-(JP4-Pad1)") (pinfunction "VSET") (pintype "input") (clearance 0.05))
    (model "/Users/macbookpro/Downloads/TPS62840YBGR/TPS62840YBGR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 606A6359)
    (at 158.69 90.21)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_A" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab") hide)
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 -7.5 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 0))
    )
  )
  (footprint "adafruit:R0402" (layer "F.Cu")
    (tedit 606A599B)
    (at 157.53 103.58 180)
    (descr "RESISTOR")
    (tags "RESISTOR")
    (attr smd)
    (fp_text reference "R4" (at -0.02 -1.38) (layer "F.SilkS"))
    (fp_text value "RMCF0402ZT0R00" (at 3.175 1.397) (layer "F.SilkS") hide)
    (fp_text user "0402 Chip Resistor 0 Ohm - 3.4v Fixed Output" (at 0 0 180 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect (at -0.6477 0 180) (size 0.6985 0.89916) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND"))
    (pad "2" smd rect (at 0.6477 0 180) (size 0.6985 0.89916) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(JP4-Pad1)"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 606A1543)
    (at 164.84 104.24 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 -270) (layer "F.SilkS") hide)
    (fp_text value "Conn_A" (at 0 9.95 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab") hide)
    (pad "3" thru_hole rect (at -0.01 4.71 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 -7.5 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 606A1543)
    (at 166.24 102.85 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 -270) (layer "F.SilkS") hide)
    (fp_text value "Conn_A" (at 0 9.95 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab") hide)
    (pad "3" thru_hole rect (at -0.01 6.11 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 -7.5 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 606A639F)
    (at 160.08 92.45)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_A" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab") hide)
    (pad "3" thru_hole rect (at 0 5.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/Vout") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 -7.5 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 606A560F)
    (at 162.78 102.84 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_A" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab") hide)
    (pad "4" thru_hole rect (at -0.01 8.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/Vin") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 -7.5 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 606A639F)
    (at 160.08 91.67)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_A" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab") hide)
    (pad "3" thru_hole rect (at 0 4.82) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/Vout") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 -7.5 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 606A55FA)
    (at 162.78 104.23 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "olmBoard-v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_A" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab") hide)
    (pad "4" thru_hole rect (at -0.01 8.66 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "/Vin") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 -7.5 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -180 0 0))
    )
  )
  (gr_line (start 161.21 104.26) (end 161.1975 96.46) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 153.02 104.26) (end 161.21 104.26) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 161.1975 96.46) (end 153.0225 96.46) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 153.0225 96.46) (end 153.02 104.26) (layer "Edge.Cuts") (width 0.05))
  (gr_text "TPS62840\n\n6.5V MAX IN\n3.3V-.75A OUT MAX\n60nA Quiescent\n" (at 157.22 99.85) (layer "B.SilkS"))
  (gr_text "G\nN\nD" (at 158.99 103.25) (layer "B.SilkS"))
  (gr_text "OUT=3.3V" (at 156.22 97.14) (layer "B.SilkS"))
  (gr_text "INPUT\n4-6.5V" (at 156.14 103.14) (layer "B.SilkS"))
  (gr_text "IN" (at 155.42 103.19) (layer "F.SilkS"))
  (gr_text "OUT" (at 158.5 97.04) (layer "F.SilkS"))
  (gr_text "TPS62840 3.3v" (at 155.4 96.98) (layer "F.SilkS"))
  (gr_text "G\nN\nD" (at 159 103.21) (layer "F.SilkS"))
  (zone (net 5) (net_name "Net-(L1-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.125))
    (min_thickness 0.125) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 157.58 101.18)
        (xy 159.01 101.18)
        (xy 159.01 100.53)
        (xy 160.96 100.53)
        (xy 160.96 101.53)
        (xy 157.58 101.53)
      )
    )
  )
  (zone (net 3) (net_name "/Vout") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 157.591513 96.370377)
        (xy 157.601513 101.100377)
        (xy 158.68 101.1)
        (xy 158.68 100.1)
        (xy 159.09 99.76)
        (xy 160.94 99.76)
        (xy 160.93 96.36)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 157.491647 97.469298)
        (xy 157.510077 101.109306)
        (xy 156.500031 101.110072)
        (xy 156.32 100.4)
        (xy 156.08 100.2)
        (xy 153.27 100.2)
        (xy 153.251601 97.470064)
      )
    )
  )
  (zone (net 1) (net_name "/Vin") (layer "F.Cu") (hatch full 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.3))
    (polygon
      (pts
        (xy 153.27573 104.252507)
        (xy 153.26 100.6)
        (xy 156.08 100.6)
        (xy 156.08 101)
        (xy 156.28 101.18)
        (xy 157.530128 101.179934)
        (xy 157.530457 102.618067)
        (xy 156.320329 102.618136)
        (xy 156.321842 104.259699)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.15))
    (min_thickness 0.15) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 161.17 104.12)
        (xy 157.74 104.12)
        (xy 157.74 102.9)
        (xy 158 102.9)
        (xy 158 101.72)
        (xy 161.17 101.72)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 0.5))
    (polygon
      (pts
        (xy 161.12 96.43)
        (xy 161.12 104.26)
        (xy 153.15 104.26)
        (xy 153.15 96.43)
      )
    )
  )
)
