(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 17)
    (no_connects 0)
    (area 135.4 93.998809 176.745501 113.305001)
    (thickness 1.6)
    (drawings 20)
    (tracks 27)
    (zones 0)
    (modules 12)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C2-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(Q1-Pad1)")
  (net 4 "Net-(R1-Pad2)")
  (net 5 +5V)
  (net 6 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.762)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(P1-Pad2)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5BA70292)
    (at 173.355 99.695)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference BT1 (at -3.175 -4.445) (layer F.SilkS))
    (fp_text value "Solar Cell" (at -4.445 -4.445) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D16_L25_P7.5 (layer F.Cu) (tedit 5BA7028C)
    (at 162.56 100.965 270)
    (descr "Radial Electrolytic Capacitor Diameter 16mm x Length 25mm, Pitch 7.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at -5.715 -0.635 270) (layer F.SilkS))
    (fp_text value 4700uF (at 0 25.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D16_L25_P7.5.wrl
      (at (xyz 0.1476378 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Libraries:C_1206_MTS (layer F.Cu) (tedit 5BA6FFED)
    (at 147.955 105.41 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -2.54 -10.795 90) (layer F.Fab))
    (fp_text value .47uF (at 0 -1.905 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D10_L20_P5 (layer F.Cu) (tedit 5BA6FFDD)
    (at 162.56 100.965 270)
    (descr "Radial Electrolytic Capacitor Diameter 10mm x Length 20mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at -5.715 -0.635 270) (layer F.SilkS))
    (fp_text value . (at 2.54 26.035 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L20_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D7.5_L11.2_P2.5 (layer F.Cu) (tedit 5BA6FFE0)
    (at 162.56 100.965 270)
    (descr "Radial Electrolytic Capacitor Diameter 7.5mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at -5.715 -1.27 270) (layer F.SilkS))
    (fp_text value . (at 1.27 25.4 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D7.5_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5BA6FFAC)
    (at 142.24 109.855 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 4.445 0 180) (layer F.SilkS))
    (fp_text value Output (at 0 14.605 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Libraries:R_1206_MTS (layer F.Cu) (tedit 5BA7028F)
    (at 151.765 99.695 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 4.445 13.97 270) (layer F.Fab))
    (fp_text value 220 (at 0 -1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 5BA6FFDA)
    (at 152.4 110.49 90)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV1 (at 8.89 -15.24 90) (layer F.SilkS))
    (fp_text value 10k (at 10.16 -15.24 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C2-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5BA6FFB2)
    (at 147.955 99.695 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 10.795 -4.445 180) (layer F.SilkS))
    (fp_text value MMBT3904 (at 0 4.445 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5BA6FFB0)
    (at 151.765 105.41 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U1 (at 13.97 -0.635 180) (layer F.SilkS))
    (fp_text value MCP112-SOT23 (at 0.635 10.16 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5BA70291)
    (at 173.355 109.855)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at -1.905 -14.605) (layer F.SilkS))
    (fp_text value MountingHole_3mm (at -6.35 -14.605) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5BA6FFBB)
    (at 142.24 99.695)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 27.94 -4.445) (layer F.SilkS))
    (fp_text value MountingHole_3mm (at 1.27 -4.445) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (gr_text "Lots uF" (at 168.91 112.395) (layer F.SilkS))
  (gr_text 10k (at 155.575 111.125 90) (layer F.SilkS))
  (gr_text O (at 164.465 104.14) (layer B.Mask))
  (gr_text o (at 160.655 107.315) (layer B.Mask))
  (gr_text ><> (at 165.735 109.855) (layer B.Mask))
  (gr_text <>< (at 159.385 111.125) (layer B.Mask))
  (gr_text "Solar Chimes /\nMiller Solar Engine\nCC-BY-NC-SA 2018\nby @SmittyHalibut" (at 161.29 102.87) (layer B.SilkS))
  (gr_text "Solar Chimes/Miller Solar Engine" (at 171.45 94.615) (layer B.SilkS))
  (gr_text - (at 175.895 102.235) (layer F.SilkS))
  (gr_text + (at 175.895 99.695) (layer F.SilkS))
  (gr_text + (at 139.7 109.855) (layer F.SilkS))
  (gr_text - (at 139.7 107.315) (layer F.SilkS))
  (gr_text Out (at 142.24 104.775) (layer F.SilkS))
  (gr_text "Solar Cell" (at 171.45 97.155) (layer F.SilkS))
  (gr_line (start 139.065 113.03) (end 176.53 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.065 96.52) (end 176.53 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text MCP (at 153.67 106.68 90) (layer F.SilkS))
  (gr_text 3904 (at 145.415 99.06 90) (layer F.SilkS))
  (gr_line (start 176.53 96.52) (end 176.53 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.065 113.03) (end 139.065 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.065 96.52) (xy 176.53 96.52) (xy 176.53 113.03) (xy 139.065 113.03)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.065 96.52) (xy 143.51 96.52) (xy 145.415 98.425) (xy 145.415 100.965) (xy 143.51 102.87)
        (xy 140.97 102.87) (xy 139.065 100.965)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 108.585) (xy 176.53 113.03) (xy 172.085 113.03) (xy 170.18 111.125) (xy 170.18 108.585)
        (xy 172.085 106.68) (xy 174.625 106.68) (xy 176.53 108.585)
      )
    )
  )
  (zone (net 5) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.065 96.52) (xy 176.53 96.52) (xy 176.53 113.03) (xy 139.065 113.03)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.065 96.52) (xy 143.51 96.52) (xy 145.415 98.425) (xy 145.415 100.965) (xy 143.51 102.87)
        (xy 140.97 102.87) (xy 139.065 100.965)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 113.03) (xy 176.53 108.585) (xy 174.625 106.68) (xy 172.085 106.68) (xy 170.18 108.585)
        (xy 170.18 111.125) (xy 172.085 113.03)
      )
    )
  )
)
