<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="71.1075" y2="0" width="0" layer="20"/>
<wire x1="71.1075" y1="0" x2="71.1075" y2="27.295" width="0" layer="20"/>
<wire x1="71.1075" y1="27.295" x2="0" y2="27.295" width="0" layer="20"/>
<wire x1="0" y1="27.295" x2="0" y2="0" width="0" layer="20"/>
<text>Fitho 2014</text>
<text>GND</text>
<text>GND</text>
<text>~</text>
<text>~</text>
<text>~</text>
<text>5V</text>
<text>~</text>
<text>~</text>
<text>~</text>
</plain>
<libraries>
<library name="RBBB">
<description>Generated from &lt;b&gt;ByteseekerMini.sch&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="ELECTROLYTIC_CAP">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
<package name="ATMEGA328">
</package>
<package name="1X04_HEADER">
</package>
<package name="1X09_HEADER">
</package>
<package name="1X16_HEADER">
</package>
<package name="1X02_HEADER">
</package>
</packages>
</library>
<library name="ftdichip-5">
<description>&lt;b&gt;USB-Controller from Future Technology Devices International Ltd.&lt;/b&gt; 
&lt;br&gt;&lt;br&gt;
Based on the source of the libraries ftdichip-4.lbr and ftdichip-2.lbr.&lt;br&gt;
With new Vinculum-II Chips.&lt;br&gt;

Includes the following controller:&lt;br&gt;
&lt;ul&gt;
&lt;li&gt;FT232BL , FT245BL (2nd generation)
&lt;li&gt;FT2232L (3rd generation)
&lt;li&gt;FT232RL , FT245RL (4th generation)
&lt;li&gt;FT4232HL (5th generation)
&lt;li&gt;VNC1L
&lt;li&gt;VNC2-32
&lt;li&gt;VNC2-48 (symbol compatible&lt;sup&gt;*&lt;/sup&gt; with VNC1L)
&lt;li&gt;VNC2-64
&lt;/ul&gt;
http://www.ftdichip.com

&lt;br&gt;&lt;br&gt;

Originally by:
&lt;ul&gt;
&lt;li&gt;B.Redemann, 4232 by R.Pearce (ftdichip-4.lbr)
&lt;li&gt;Paul Carpenter, PC Services www.pcserviceselectronics.co.uk (ftdichip-2.lbr)
&lt;/ul&gt;
Updated with Vinculum-II by Marcin Zakaszewski.</description>
<packages>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOD-123">
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-hirose-(with-micro)">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="ZX62R-B-5P">
<description>&lt;b&gt;MINI USB Connector HI-SPEED Certified&lt;/b&gt; Metal Shield SMT Type Without Positioning Post&lt;p&gt;
Source: http://www.hirose.co.jp/cataloge_hp/e24000019.pdf</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="RBBB" package="ELECTROLYTIC_CAP" value="47uF"/>
<element name="C2" library="RBBB" package="ELECTROLYTIC_CAP" value="47uF"/>
<element name="IC2" library="RBBB" package="ATMEGA328" value="ATmega328P">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="RBBB" package="1X04_HEADER" value="">
<attribute name="VALUE"/>
<attribute name="D5"/>
<attribute name="D6"/>
<attribute name="D7"/>
<attribute name="D8"/>
</element>
<element name="JP3" library="RBBB" package="1X09_HEADER" value="1X09_HEADER&quot;">
<attribute name="5V"/>
<attribute name="D2"/>
<attribute name="D3"/>
<attribute name="D4"/>
<attribute name="GND"/>
<attribute name="RESET"/>
<attribute name="RX"/>
<attribute name="TX"/>
</element>
<element name="JP4" library="RBBB" package="1X16_HEADER" value="1X16_HEADER&quot;">
<attribute name="5V"/>
<attribute name="GND"/>
<attribute name="A5"/>
<attribute name="A0"/>
<attribute name="A1"/>
<attribute name="A2"/>
<attribute name="A3"/>
<attribute name="A4"/>
<attribute name="AREF"/>
<attribute name="D10"/>
<attribute name="D11"/>
<attribute name="D12"/>
<attribute name="D13"/>
<attribute name="D9"/>
</element>
<element name="FT232RL" library="ftdichip-5" package="SSOP28DB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="R4" library="adafruit" package="R0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="C5" library="eagle-ltspice" package="C0603" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="C3" library="eagle-ltspice" package="C0603" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="C6" library="eagle-ltspice" package="C0603" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="eagle-ltspice" package="C0603" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="HC49US" value="">
<attribute name="VALUE"/>
<attribute name="16MHZ"/>
</element>
<element name="C8" library="eagle-ltspice" package="C0603" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="adafruit" package="R0603" value="100">
<attribute name="NAME"/>
</element>
<element name="C9" library="eagle-ltspice" package="C0603" value="22pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="C10" library="eagle-ltspice" package="C0603" value="22pF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="adafruit" package="R0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="R7" library="adafruit" package="R0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="IC1" library="linear" package="TO220V" value="7805TV"/>
<element name="C11" library="eagle-ltspice" package="C0603" value="100nF">
<attribute name="SPICEMODEL" value="NONE"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="PWR" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="con-hirose-(with-micro)" package="ZX62R-B-5P" value="MICRO-USB-ZX62R-B-5P"/>
<element name="U$1" library="RBBB" package="1X02_HEADER" value="1X02_HEADER">
<attribute name="GND"/>
<attribute name="VIN"/>
</element>
<element name="D1" library="adafruit" package="SOD-123" value="">
<attribute name="VALUE"/>
</element>
<element name="RESET" library="switch-omron" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VIN">
<contactref element="C1" pad="+"/>
<contactref element="IC1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="+5V">
<contactref element="JP4" pad="1"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="9"/>
<contactref element="IC2" pad="20"/>
<contactref element="IC2" pad="7"/>
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="+"/>
<contactref element="R2" pad="2"/>
<contactref element="FT232RL" pad="4"/>
<contactref element="FT232RL" pad="20"/>
<contactref element="FT232RL" pad="19"/>
<contactref element="C6" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="JP4" pad="2"/>
<contactref element="JP4" pad="9"/>
<contactref element="JP4" pad="11"/>
<contactref element="JP3" pad="2"/>
<contactref element="IC2" pad="22"/>
<contactref element="IC2" pad="8"/>
<contactref element="C3" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="FT232RL" pad="21"/>
<contactref element="FT232RL" pad="18"/>
<contactref element="FT232RL" pad="7"/>
<contactref element="FT232RL" pad="25"/>
<contactref element="C5" pad="2"/>
<contactref element="FT232RL" pad="26"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="PWR" pad="C"/>
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="RESET" pad="3"/>
<contactref element="RESET" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="IC2" pad="9"/>
<contactref element="Y1" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="AREF">
<contactref element="IC2" pad="21"/>
<contactref element="JP4" pad="10"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="A0">
<contactref element="IC2" pad="23"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="A1">
<contactref element="IC2" pad="24"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="A2">
<contactref element="IC2" pad="25"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="A3">
<contactref element="IC2" pad="26"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="A4">
<contactref element="IC2" pad="27"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="A5">
<contactref element="IC2" pad="28"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="D0/RX">
<contactref element="IC2" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="D1/TX">
<contactref element="IC2" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="D2">
<contactref element="IC2" pad="4"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="D3">
<contactref element="IC2" pad="5"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="D4">
<contactref element="IC2" pad="6"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="D5">
<contactref element="IC2" pad="11"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="D6">
<contactref element="IC2" pad="12"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="D7">
<contactref element="IC2" pad="13"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="D8">
<contactref element="IC2" pad="14"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="D9">
<contactref element="IC2" pad="15"/>
<contactref element="JP4" pad="16"/>
</signal>
<signal name="D10">
<contactref element="IC2" pad="16"/>
<contactref element="JP4" pad="15"/>
</signal>
<signal name="D11">
<contactref element="IC2" pad="17"/>
<contactref element="JP4" pad="14"/>
</signal>
<signal name="D12">
<contactref element="IC2" pad="18"/>
<contactref element="JP4" pad="13"/>
</signal>
<signal name="D13">
<contactref element="IC2" pad="19"/>
<contactref element="JP4" pad="12"/>
</signal>
<signal name="RESET">
<contactref element="JP3" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="RESET" pad="1"/>
<contactref element="RESET" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="1"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="D+">
<contactref element="FT232RL" pad="15"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="D-">
<contactref element="FT232RL" pad="16"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="FT232RL" pad="23"/>
<contactref element="RX" pad="C"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="1"/>
<contactref element="RX" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="FT232RL" pad="22"/>
<contactref element="TX" pad="C"/>
</signal>
<signal name="N$15">
<contactref element="R4" pad="1"/>
<contactref element="TX" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="FT232RL" pad="17"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="FT232RL" pad="2"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="FT232RL" pad="3"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="IC2" pad="10"/>
<contactref element="Y1" pad="2"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="USBVCC">
<contactref element="C7" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="2"/>
<contactref element="FT232RL" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R7" pad="2"/>
<contactref element="FT232RL" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
