(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 40)
    (tracks 130)
    (zones 0)
    (modules 76)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.5)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "mfg/"))
  )
  (net 0 "")
  (net 1 /InterfaceGround)
  (net 2 /-15V)
  (net 3 /LineIn)
  (net 4 /+15V)
  (net 5 /OutNegative)
  (net 6 /OutPositive)
  (net 7 "Net-(D1-Pad2)")
  (net 8 /Vac_s)
  (net 9 /Is_s)
  (net 10 /Vdc_s)
  (net 11 "Net-(R1-Pad1)")
  (net 12 "Net-(R1-Pad2)")
  (net 13 "Net-(R2-Pad2)")
  (net 14 "Net-(R10-Pad2)")
  (net 15 /Mid2)
  (net 16 /Mid1)
  (net 17 "Net-(J18-Pad1)")
  (net 18 /12V)
  (net 19 "Net-(R7-Pad2)")
  (net 20 "Net-(R19-Pad1)")
  (net 21 "Net-(R19-Pad2)")
  (net 22 "Net-(R20-Pad2)")
  (net 23 "Net-(R21-Pad2)")
  (net 24 "Net-(R22-Pad2)")
  (net 25 "Net-(R23-Pad2)")
  (net 26 "Net-(C22-Pad2)")
  (net 27 /Line-PreFuse)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /12V)
    (add_net /Line-PreFuse)
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(J18-Pad1)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R7-Pad2)")
  )
  (net_class AC ""
    (clearance 2)
    (trace_width 15)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /LineIn)
    (add_net /Mid1)
    (add_net /Mid2)
  )
  (net_class "Ac copy" ""
    (clearance 0.8)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class "HV output" ""
    (clearance 2)
    (trace_width 15)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /OutNegative)
    (add_net /OutPositive)
    (add_net "Net-(R1-Pad2)")
  )
  (net_class "LV components" ""
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+15V)
    (add_net /-15V)
    (add_net /InterfaceGround)
    (add_net /Is_s)
    (add_net /Vac_s)
    (add_net /Vdc_s)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R2-Pad2)")
  )
  (net_class Outnegative ""
    (clearance 0.5)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 52 158)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference J29 (at 0 -4.5) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 158.7 41.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference J17 (at -5.5 -0.5) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 158.7 158)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference J16 (at 0 -4.5) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 52 41.5)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference J15 (at 0 -4.5) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module lineCapnew:R46KN422000P0M (layer F.Cu) (tedit 0)
    (at 6.5 192.5)
    (fp_text reference C1 (at 11.4554 0) (layer F.SilkS))
    (fp_text value R46KN422000P0M (at 11.4554 -2) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 thru_hole circle (at 22.9108 0) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 1 thru_hole rect (at 0 0) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 3 /LineIn))
  )
  (module lineCapnew:R46KN422000P0M (layer F.Cu) (tedit 0)
    (at 41 201 270)
    (fp_text reference C2 (at 11.4554 0 90) (layer F.SilkS))
    (fp_text value R46KN422000P0M (at 11.4554 2 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 3 /LineIn))
    (pad 2 thru_hole circle (at 22.9108 0 270) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 15 /Mid2))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 33.5 56.5375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value Cbypass (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 /InterfaceGround))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 2 /-15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lineCapnew:R46KN422000P0M (layer F.Cu) (tedit 0)
    (at 29.5 173.5 180)
    (fp_text reference C4 (at 11.4554 0) (layer F.SilkS))
    (fp_text value R46KN422000P0M (at 11.4554 2) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 2 thru_hole circle (at 22.9108 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 3 /LineIn))
  )
  (module lineCapnew:R46KN422000P0M (layer F.Cu) (tedit 0)
    (at 41 194 90)
    (fp_text reference C5 (at 11.4554 0 90) (layer F.SilkS))
    (fp_text value R46KN422000P0M (at 11.4554 -2 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 3 /LineIn))
    (pad 2 thru_hole circle (at 22.9108 0 90) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 15 /Mid2))
  )
  (module lineCapnew:R46KN422000P0M (layer F.Cu) (tedit 0)
    (at 6.763301 154.5)
    (fp_text reference C6 (at 11.4554 0) (layer F.SilkS))
    (fp_text value R46KN422000P0M (at 11.4554 -2) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 3 /LineIn))
    (pad 2 thru_hole circle (at 22.9108 0) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 15 /Mid2))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 76 70.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.68) (layer F.SilkS))
    (fp_text value Cbypass (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 /InterfaceGround))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 /+15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 38.5 56.4625 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value Cbypass (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 /InterfaceGround))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 /+15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 76.0375 78.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 0 -1.68) (layer F.SilkS))
    (fp_text value Cbypass (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 2 /-15V))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 /InterfaceGround))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 49 66.5375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value Cbypass (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 2 /-15V))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 /InterfaceGround))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 56 66.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value Cbypass (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 /+15V))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 /InterfaceGround))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEF0)
    (at 83.5 189.5 270)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value LEDbleed (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 5 /OutNegative))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 131 21 180)
    (fp_text reference J4 (at 5.399999 5.21) (layer F.SilkS))
    (fp_text value 7807-High1 (at -3.5 5 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 2 thru_hole circle (at 0 5.21 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 3 thru_hole circle (at 0 10.42 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 4 thru_hole circle (at 10.799999 0 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 5 thru_hole circle (at 10.799999 5.21 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 6 thru_hole circle (at 10.799999 10.42 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 10.5 116.5 90)
    (fp_text reference J8 (at 5.399999 5.21 90) (layer F.SilkS))
    (fp_text value 7807-L1 (at 15 5 180) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 3 /LineIn))
    (pad 2 thru_hole circle (at 0 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 3 /LineIn))
    (pad 3 thru_hole circle (at 0 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 3 /LineIn))
    (pad 4 thru_hole circle (at 10.799999 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 3 /LineIn))
    (pad 5 thru_hole circle (at 10.799999 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 3 /LineIn))
    (pad 6 thru_hole circle (at 10.799999 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 3 /LineIn))
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 10.5 138.5 90)
    (fp_text reference J9 (at 5.399999 5.21 90) (layer F.SilkS))
    (fp_text value 7807-LineIn (at 15 5 180) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 27 /Line-PreFuse))
    (pad 2 thru_hole circle (at 0 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 27 /Line-PreFuse))
    (pad 3 thru_hole circle (at 0 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 27 /Line-PreFuse))
    (pad 4 thru_hole circle (at 10.799999 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 27 /Line-PreFuse))
    (pad 5 thru_hole circle (at 10.799999 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 27 /Line-PreFuse))
    (pad 6 thru_hole circle (at 10.799999 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 27 /Line-PreFuse))
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 12.5 218 90)
    (fp_text reference J10 (at 5.399999 5.21 90) (layer F.SilkS))
    (fp_text value 7807-NeutralIn (at 15 5 180) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 6 thru_hole circle (at 10.799999 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 5 thru_hole circle (at 10.799999 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 4 thru_hole circle (at 10.799999 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 3 thru_hole circle (at 0 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 2 thru_hole circle (at 0 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 10 49.5 90)
    (fp_text reference J14 (at 5.399999 5.21 90) (layer F.SilkS))
    (fp_text value 7807-Mid1 (at 15 5) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 6 thru_hole circle (at 10.799999 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 16 /Mid1))
    (pad 5 thru_hole circle (at 10.799999 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 16 /Mid1))
    (pad 4 thru_hole circle (at 10.799999 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 16 /Mid1))
    (pad 3 thru_hole circle (at 0 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 16 /Mid1))
    (pad 2 thru_hole circle (at 0 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 16 /Mid1))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 16 /Mid1))
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 10.5 95.5 90)
    (fp_text reference J18 (at 5.399999 5.21 90) (layer F.SilkS))
    (fp_text value 7807-L2 (at 14 5 180) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 6 thru_hole circle (at 10.799999 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 17 "Net-(J18-Pad1)"))
    (pad 5 thru_hole circle (at 10.799999 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 17 "Net-(J18-Pad1)"))
    (pad 4 thru_hole circle (at 10.799999 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 17 "Net-(J18-Pad1)"))
    (pad 3 thru_hole circle (at 0 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 17 "Net-(J18-Pad1)"))
    (pad 2 thru_hole circle (at 0 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 17 "Net-(J18-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 17 "Net-(J18-Pad1)"))
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 164 21 180)
    (fp_text reference J19 (at 5.399999 5.21) (layer F.SilkS))
    (fp_text value 7807-Low1 (at -3.5 5 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 2 thru_hole circle (at 0 5.21 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 3 thru_hole circle (at 0 10.42 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 4 thru_hole circle (at 10.799999 0 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 5 thru_hole circle (at 10.799999 5.21 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 6 thru_hole circle (at 10.799999 10.42 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
  )
  (module Connector_BarrelJack:BarrelJack_CUI_PJ-036AH-SMT_Horizontal (layer F.Cu) (tedit 5A1DBF38)
    (at 65.5 19 180)
    (descr "Surface-mount DC Barrel Jack, http://www.cui.com/product/resource/pj-036ah-smt.pdf")
    (tags "Power Jack SMT")
    (attr smd)
    (fp_text reference J20 (at -4.5 -5.75) (layer F.SilkS))
    (fp_text value Barrel_Jack (at 0 11.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0.7 -5.8 180) (size 3.3 4.4) (layers F.Cu F.Paste F.Mask)
      (net 18 /12V))
    (pad 2 smd rect (at -6.45 3.2 180) (size 3.9 6.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C22-Pad2)"))
    (pad 3 smd rect (at 6.45 3.2 180) (size 3.9 6.2) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at 0 7 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-036AH-SMT_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 192.5 10.5)
    (fp_text reference J21 (at 5.399999 5.21) (layer F.SilkS))
    (fp_text value 7807-High2 (at 15 4 90) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 6 thru_hole circle (at 10.799999 10.42) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 5 thru_hole circle (at 10.799999 5.21) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 4 thru_hole circle (at 10.799999 0) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 3 thru_hole circle (at 0 10.42) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 2 thru_hole circle (at 0 5.21) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 1 thru_hole circle (at 0 0) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 66.5 54.5 90)
    (descr "Through hole straight pin header, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.54mm double row")
    (fp_text reference J22 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x07_Odd_Even (at 1.27 17.57 90) (layer F.Fab))
    (fp_text user %R (at 1.27 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /InterfaceGround))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Vac_s))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /InterfaceGround))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Is_s))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /InterfaceGround))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Vdc_s))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /InterfaceGround))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /InterfaceGround))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /InterfaceGround))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /+15V))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /InterfaceGround))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /-15V))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /InterfaceGround))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /InterfaceGround))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 52 5)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J24 (at 1.27 9) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(C22-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /12V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(C22-Pad2)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /12V))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 21 20.5 180)
    (fp_text reference J25 (at 5.399999 5.21) (layer F.SilkS))
    (fp_text value 7807-Mid2 (at 5.399999 7.277799) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 2 thru_hole circle (at 0 5.21 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 3 thru_hole circle (at 0 10.42 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 4 thru_hole circle (at 10.799999 0 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 5 thru_hole circle (at 10.799999 5.21 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (pad 6 thru_hole circle (at 10.799999 10.42 180) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 15 /Mid2))
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 224 11)
    (fp_text reference J26 (at 5.399999 5.21) (layer F.SilkS))
    (fp_text value 7807-Low2 (at 15 5 90) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 6 thru_hole circle (at 10.799999 10.42) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 5 thru_hole circle (at 10.799999 5.21) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 4 thru_hole circle (at 10.799999 0) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 3 thru_hole circle (at 0 10.42) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 2 thru_hole circle (at 0 5.21) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 1 thru_hole circle (at 0 0) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 228.5 74 90)
    (fp_text reference J27 (at 5.399999 5.21 90) (layer F.SilkS))
    (fp_text value 7807-OutPositive (at 5.399999 -4 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 2 thru_hole circle (at 0 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 3 thru_hole circle (at 0 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 4 thru_hole circle (at 10.799999 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 5 thru_hole circle (at 10.799999 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 6 thru_hole circle (at 10.799999 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
  )
  (module CONN_7807_KEY:7807 (layer F.Cu) (tedit 0)
    (at 228 134 90)
    (fp_text reference J28 (at 5.399999 5.21 90) (layer F.SilkS))
    (fp_text value 7807-OutNegative (at 5.399999 -4 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 6 thru_hole circle (at 10.799999 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 5 thru_hole circle (at 10.799999 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 4 thru_hole circle (at 10.799999 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 3 thru_hole circle (at 0 10.42 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 2 thru_hole circle (at 0 5.21 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.1496 3.1496) (drill 2.6416) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 54 95 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 2.62 270) (layer B.SilkS))
    (fp_text value R10kohm (at 0 -2.62 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -3.05 0 90) (size 1.4 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.1785707142857143)
      (net 11 "Net-(R1-Pad1)"))
    (pad 2 smd roundrect (at 3.05 0 90) (size 1.4 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.1785707142857143)
      (net 12 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 60.5 115 45)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -2.62 45) (layer F.SilkS))
    (fp_text value R10kohm (at 0 2.62 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 2 smd roundrect (at 3.05 0 45) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 13 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -3.05 0 45) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 3 /LineIn))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 64.5 105.5 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value R10kohm (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 13 "Net-(R2-Pad2)"))
    (pad 2 smd roundrect (at 3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 11 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder locked (layer B.Cu) (tedit 5F68FEEE)
    (at 59 95 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 2.62 270) (layer B.SilkS))
    (fp_text value R10kohm (at 0 -2.62 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 3.05 0 90) (size 1.4 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.1785707142857143)
      (net 12 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -3.05 0 90) (size 1.4 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.1785707142857143)
      (net 11 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 66.95 45.5 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 4.95 0) (layer F.SilkS))
    (fp_text value R390ohm (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 1 /InterfaceGround))
    (pad 1 smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 9 /Is_s))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 67 48.5 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R390ohm (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 1 /InterfaceGround))
    (pad 1 smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 9 /Is_s))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 58.364999 57.524999 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R150ohm (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 19 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 8 /Vac_s))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 52 55 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R120ohm (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 19 "Net-(R7-Pad2)"))
    (pad 2 smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 1 /InterfaceGround))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 58 52 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R150ohm (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 8 /Vac_s))
    (pad 2 smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 19 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 75.405001 41.585001)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R150ohm (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 14 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 10 /Vdc_s))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 80.95 44.5)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R120ohm (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 14 "Net-(R10-Pad2)"))
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 1 /InterfaceGround))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 74.95 46.5)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R150ohm (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 10 /Vdc_s))
    (pad 2 smd roundrect (at 1.55 0) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923069230769231)
      (net 14 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 71.5 197.5 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value R1Mohm (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 6 /OutPositive))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 79.5 197.5 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value R1Mohm (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 6 /OutPositive))
    (pad 2 smd roundrect (at 3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 103.5 197.5 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value R1Mohm (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 6 /OutPositive))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 95.5 197.5 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value R1Mohm (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 6 /OutPositive))
    (pad 2 smd roundrect (at 3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 87.5 197.5 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value R1Mohm (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 7 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 6 /OutPositive))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 63.5 197.5 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at 0 -2.62 90) (layer F.SilkS))
    (fp_text value R1Mohm (at 0 2.62 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 6 /OutPositive))
    (pad 2 smd roundrect (at 3.05 0 90) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 5 /OutNegative))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 119.624999 61.214999 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at 0 -2.62) (layer F.SilkS))
    (fp_text value R10kohm (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 20 "Net-(R19-Pad1)"))
    (pad 2 smd roundrect (at 3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 21 "Net-(R19-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 170 64 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at 0 -2.62) (layer F.SilkS))
    (fp_text value R10kohm (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 6 /OutPositive))
    (pad 2 smd roundrect (at 3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 22 "Net-(R20-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 160 64 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at 0 -2.62) (layer F.SilkS))
    (fp_text value R10kohm (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 22 "Net-(R20-Pad2)"))
    (pad 2 smd roundrect (at 3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 23 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 150 64 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at 0 -2.62) (layer F.SilkS))
    (fp_text value R10kohm (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 24 "Net-(R22-Pad2)"))
    (pad 1 smd roundrect (at -3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 23 "Net-(R21-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 140 64 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R23 (at 0 -2.62) (layer F.SilkS))
    (fp_text value R10kohm (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 24 "Net-(R22-Pad2)"))
    (pad 2 smd roundrect (at 3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 25 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 130 64 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R24 (at 0 -2.62) (layer F.SilkS))
    (fp_text value R10kohm (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 20 "Net-(R19-Pad1)"))
    (pad 1 smd roundrect (at -3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 25 "Net-(R23-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 119.95 68 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R25 (at 0 -2.62) (layer F.SilkS))
    (fp_text value R10kohm (at 0 2.62) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 21 "Net-(R19-Pad2)"))
    (pad 1 smd roundrect (at -3.05 0 180) (size 1.4 3.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1785707142857143)
      (net 20 "Net-(R19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sensor_Voltage:LEM_LV25-P (layer F.Cu) (tedit 5B2C0184)
    (at 49 96.5 90)
    (descr "LEM LV25-P Voltage transducer, https://www.lem.com/sites/default/files/products_datasheets/lv_25-p.pdf")
    (tags "LEM Hall Effect Voltage transducer")
    (fp_text reference U1 (at -1.524 -6.731 270) (layer F.SilkS))
    (fp_text value LV25-P (at 11.16 8.62 270) (layer F.Fab))
    (fp_text user %R (at 11.16 6.62 270) (layer F.Fab))
    (pad 5 thru_hole circle (at 20.32 7.62 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 /+15V))
    (pad 6 thru_hole circle (at 20.32 0 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /-15V))
    (pad 4 thru_hole circle (at 20.32 15.24 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 /Vac_s))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at 0 15.24 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 /Mid2))
    (model ${KISYS3DMOD}/Sensor_Voltage.3dshapes/LEM_LV25-P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "LAH_100-P:LAH 100-P" (layer F.Cu) (tedit 0)
    (at 15.5 74.5 90)
    (fp_text reference U2 (at 5.715 2.54 90) (layer F.SilkS))
    (fp_text value LAH_100-P (at 6 -9 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.159 2.159) (drill 1.651) (layers *.Cu *.Mask)
      (net 17 "Net-(J18-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 2.159 2.159) (drill 1.651) (layers *.Cu *.Mask)
      (net 17 "Net-(J18-Pad1)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 2.159 2.159) (drill 1.651) (layers *.Cu *.Mask)
      (net 17 "Net-(J18-Pad1)"))
    (pad 9 thru_hole circle (at 11.43 0 90) (size 2.159 2.159) (drill 1.651) (layers *.Cu *.Mask)
      (net 16 /Mid1))
    (pad 8 thru_hole circle (at 11.43 2.54 90) (size 2.159 2.159) (drill 1.651) (layers *.Cu *.Mask)
      (net 16 /Mid1))
    (pad 7 thru_hole circle (at 11.43 5.08 90) (size 2.159 2.159) (drill 1.651) (layers *.Cu *.Mask)
      (net 16 /Mid1))
    (pad 6 thru_hole circle (at 9.525 17.78 90) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 2 /-15V))
    (pad 5 thru_hole circle (at 9.525 20.32 90) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 4 /+15V))
    (pad 4 thru_hole circle (at 9.525 22.86 90) (size 1.4732 1.4732) (drill 0.9652) (layers *.Cu *.Mask)
      (net 9 /Is_s))
  )
  (module Sensor_Voltage:LEM_LV25-P (layer F.Cu) (tedit 5B2C0184)
    (at 106 78.5 180)
    (descr "LEM LV25-P Voltage transducer, https://www.lem.com/sites/default/files/products_datasheets/lv_25-p.pdf")
    (tags "LEM Hall Effect Voltage transducer")
    (fp_text reference U3 (at -1.524 -6.731 180) (layer F.SilkS))
    (fp_text value LV25-P (at 11.16 8.62 180) (layer F.Fab))
    (fp_text user %R (at 11.16 6.62 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 15.24 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(R19-Pad2)"))
    (pad 4 thru_hole circle (at 20.32 15.24 180) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 /Vdc_s))
    (pad 6 thru_hole circle (at 20.32 0 180) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /-15V))
    (pad 5 thru_hole circle (at 20.32 7.62 180) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 /+15V))
    (model ${KISYS3DMOD}/Sensor_Voltage.3dshapes/LEM_LV25-P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC:PhoenixContact_MCV_1,5_8-G-3.5_1x08_P3.50mm_Vertical (layer F.Cu) (tedit 5B784ED0)
    (at 80 12.5)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/8-G-3.5; number of pins: 08; pin pitch: 3.50mm; Vertical || order number: 1843664 8A 160V")
    (tags "phoenix_contact connector MCV_01x08_G_3.5mm")
    (fp_text reference J23 (at 6 4.5) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 12.25 4.2) (layer F.Fab))
    (fp_text user %R (at 12.25 -3.55) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.1388888888888889)
      (net 18 /12V))
    (pad 2 thru_hole oval (at 3.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(C22-Pad2)"))
    (pad 3 thru_hole oval (at 7 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 /12V))
    (pad 4 thru_hole oval (at 10.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(C22-Pad2)"))
    (pad 5 thru_hole oval (at 14 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 /12V))
    (pad 6 thru_hole oval (at 17.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(C22-Pad2)"))
    (pad 7 thru_hole oval (at 21 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 /12V))
    (pad 8 thru_hole oval (at 24.5 0) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_8-G-3.5_1x08_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 12V-cap:R60DN5100AA30K (layer F.Cu) (tedit 0)
    (at 81 25.5)
    (fp_text reference C22 (at 11.4554 0) (layer F.SilkS))
    (fp_text value R60DN5100AA30K (at 11.4554 0) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 18 /12V))
    (pad 2 thru_hole circle (at 22.9108 0) (size 1.6256 1.6256) (drill 1.1176) (layers *.Cu *.Mask)
      (net 26 "Net-(C22-Pad2)"))
  )
  (module Connector_BarrelJack:BarrelJack_CUI_PJ-036AH-SMT_Horizontal (layer F.Cu) (tedit 5A1DBF38)
    (at 41 19 180)
    (descr "Surface-mount DC Barrel Jack, http://www.cui.com/product/resource/pj-036ah-smt.pdf")
    (tags "Power Jack SMT")
    (attr smd)
    (fp_text reference J33 (at -4.5 -5.75) (layer F.SilkS))
    (fp_text value Barrel_Jack (at 0 11.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0.7 -5.8 180) (size 3.3 4.4) (layers F.Cu F.Paste F.Mask)
      (net 18 /12V))
    (pad 2 smd rect (at -6.45 3.2 180) (size 3.9 6.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C22-Pad2)"))
    (pad 3 smd rect (at 6.45 3.2 180) (size 3.9 6.2) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at 0 7 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-036AH-SMT_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 6.35 6.35)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference J1 (at 2 -2.5) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 247.65 6.35)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference J2 (at -3 0) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 6.35 222.25)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference J3 (at 3.35 0.75) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 247.65 222.25)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (attr virtual)
    (fp_text reference J5 (at 0 -4.5) (layer F.SilkS))
    (fp_text value Conn_01x01_Male (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module 3557-2:3557-2 (layer F.Cu) (tedit 0)
    (at 30 136.5)
    (fp_text reference J6 (at 8 6.5) (layer F.SilkS))
    (fp_text value 3557-2 (at 6.5 0.5) (layer F.SilkS))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2352 2.2352) (drill 1.7272) (layers *.Cu *.Mask)
      (net 27 /Line-PreFuse))
    (pad 2 thru_hole circle (at 0 3.302) (size 2.2352 2.2352) (drill 1.7272) (layers *.Cu *.Mask)
      (net 27 /Line-PreFuse))
    (pad 3 thru_hole circle (at 13.462 0) (size 2.2352 2.2352) (drill 1.7272) (layers *.Cu *.Mask)
      (net 3 /LineIn))
    (pad 4 thru_hole circle (at 13.462 3.302) (size 2.2352 2.2352) (drill 1.7272) (layers *.Cu *.Mask)
      (net 3 /LineIn))
  )
  (module CAP_48C65010JY5_VIS:DCP4N055009FD4KSSD (layer B.Cu) (tedit 6165A599)
    (at 164 169 270)
    (fp_text reference C12 (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text value cap4pin (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer B.SilkS))
    (fp_text user * (at 0 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 2 thru_hole circle (at 0 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 3 thru_hole circle (at 52.499995 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 4 thru_hole circle (at 52.499995 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
  )
  (module CAP_48C65010JY5_VIS:DCP4N055009FD4KSSD (layer B.Cu) (tedit 6165A599)
    (at 83.5 108 270)
    (fp_text reference C13 (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text value cap4pin (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text user * (at 0 0 90) (layer B.Fab))
    (fp_text user * (at 0 0 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 4 thru_hole circle (at 52.499995 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 3 thru_hole circle (at 52.499995 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 2 thru_hole circle (at 0 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 1 thru_hole circle (at 0 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
  )
  (module CAP_48C65010JY5_VIS:DCP4N055009FD4KSSD (layer B.Cu) (tedit 6165A599)
    (at 232 221.5 90)
    (fp_text reference C14 (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text value cap4pin (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer B.SilkS))
    (fp_text user * (at 0 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 2 thru_hole circle (at 0 -20.2946 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 3 thru_hole circle (at 52.499995 -20.2946 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 4 thru_hole circle (at 52.499995 0 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
  )
  (module CAP_48C65010JY5_VIS:DCP4N055009FD4KSSD (layer B.Cu) (tedit 6165A599)
    (at 151.5 160.5 90)
    (fp_text reference C15 (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text value cap4pin (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer B.SilkS))
    (fp_text user * (at 0 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 2 thru_hole circle (at 0 -20.2946 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 3 thru_hole circle (at 52.499995 -20.2946 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 4 thru_hole circle (at 52.499995 0 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
  )
  (module CAP_48C65010JY5_VIS:DCP4N055009FD4KSSD (layer B.Cu) (tedit 6165A599)
    (at 122.5 48.5 270)
    (fp_text reference C16 (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text value cap4pin (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text user * (at 0 0 90) (layer B.Fab))
    (fp_text user * (at 0 0 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 4 thru_hole circle (at 52.499995 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 3 thru_hole circle (at 52.499995 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 2 thru_hole circle (at 0 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 1 thru_hole circle (at 0 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
  )
  (module CAP_48C65010JY5_VIS:DCP4N055009FD4KSSD (layer B.Cu) (tedit 6165A599)
    (at 137 221.5 90)
    (fp_text reference C17 (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text value cap4pin (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text user * (at 0 0 90) (layer B.Fab))
    (fp_text user * (at 0 0 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 4 thru_hole circle (at 52.499995 0 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 3 thru_hole circle (at 52.499995 -20.2946 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 2 thru_hole circle (at 0 -20.2946 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
  )
  (module CAP_48C65010JY5_VIS:DCP4N055009FD4KSSD (layer B.Cu) (tedit 6165A599)
    (at 170 48.5 270)
    (fp_text reference C18 (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text value cap4pin (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer B.SilkS))
    (fp_text user * (at 0 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 2 thru_hole circle (at 0 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 3 thru_hole circle (at 52.499995 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 4 thru_hole circle (at 52.499995 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
  )
  (module CAP_48C65010JY5_VIS:DCP4N055009FD4KSSD (layer B.Cu) (tedit 6165A599)
    (at 69.5 169 270)
    (fp_text reference C19 (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text value cap4pin (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer B.SilkS))
    (fp_text user * (at 0 0 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 2 thru_hole circle (at 0 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 3 thru_hole circle (at 52.499995 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 4 thru_hole circle (at 52.499995 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
  )
  (module CAP_48C65010JY5_VIS:DCP4N055009FD4KSSD (layer B.Cu) (tedit 6165A599)
    (at 178.5 108 270)
    (fp_text reference C21 (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text value cap4pin (at 26.249998 -10.1473 90) (layer B.SilkS))
    (fp_text user * (at 0 0 90) (layer B.Fab))
    (fp_text user * (at 0 0 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 4 thru_hole circle (at 52.499995 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 3 thru_hole circle (at 52.499995 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 5 /OutNegative))
    (pad 2 thru_hole circle (at 0 -20.2946 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
    (pad 1 thru_hole circle (at 0 0 270) (size 3.4 3.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 6 /OutPositive))
  )
  (gr_text "Power Board V1\nOct 2021" (at 141.5 125.5) (layer F.SilkS))
  (gr_text "GND\n" (at 54.5 2 90) (layer F.SilkS))
  (gr_text "12V\n" (at 52 2 90) (layer F.SilkS))
  (gr_text GND (at 104.5 4.5 90) (layer F.SilkS))
  (gr_text GND (at 97.5 4.5 90) (layer F.SilkS))
  (gr_text GND (at 90.5 4.5 90) (layer F.SilkS))
  (gr_text GND (at 83.5 4.5 90) (layer F.SilkS))
  (gr_text "12V\n" (at 101 4.5 90) (layer F.SilkS))
  (gr_text "12V\n" (at 94 4.5 90) (layer F.SilkS))
  (gr_text "12V\n" (at 87 4.5 90) (layer F.SilkS))
  (gr_text "12V\n" (at 80 4.5 90) (layer F.SilkS))
  (gr_text "MID 2" (at 16 5.5) (layer F.SilkS))
  (gr_text MID2 (at 16 25.5) (layer F.SilkS))
  (gr_text NEUTRAL (at 27.5 213 -90) (layer F.SilkS))
  (gr_text NEUTRAL (at 7.5 213 -90) (layer F.SilkS))
  (gr_text "LINE IN" (at 5.5 133.5 -90) (layer F.SilkS))
  (gr_text "LINE IN" (at 25.5 133.5 -90) (layer F.SilkS))
  (gr_text L1 (at 5.5 110.5 -90) (layer F.SilkS))
  (gr_text L1 (at 25.5 110.5 -90) (layer F.SilkS))
  (gr_text L2 (at 5.5 90.5 -90) (layer F.SilkS))
  (gr_text L2 (at 25.5 90.5 -90) (layer F.SilkS))
  (gr_text "MID 1" (at 5 44.5 270) (layer F.SilkS))
  (gr_text "MID 1" (at 25 44.5 270) (layer F.SilkS))
  (gr_text "HIGH 1" (at 125.5 6.5) (layer F.SilkS))
  (gr_text "HIGH 1" (at 125.5 26.5) (layer F.SilkS))
  (gr_text "LOW 1" (at 158.5 6.5) (layer F.SilkS))
  (gr_text "LOW 1" (at 158.5 26.5) (layer F.SilkS))
  (gr_text "LOW 2" (at 230 7) (layer F.SilkS))
  (gr_text "HIGH 2" (at 197.5 6.5) (layer F.SilkS))
  (gr_text "LOW 2" (at 230 27) (layer F.SilkS))
  (gr_text "HIGH 2" (at 197.5 26.5) (layer F.SilkS))
  (gr_text "OUTPUT -" (at 234 140) (layer F.SilkS))
  (gr_text "OUTPUT -" (at 234 118) (layer F.SilkS))
  (gr_text "OUTPUT +" (at 234.5 58) (layer F.SilkS))
  (gr_text "OUTPUT +" (at 234.5 80) (layer F.SilkS))
  (gr_text "HV BLEED" (at 79.5 188.5 90) (layer F.SilkS))
  (gr_line (start 254 0) (end 254 228.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0 0) (end 254 0) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 0 228.6) (end 0 0) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 254 228.6) (end 0 228.6) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name /InterfaceGround) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.5 35.5) (xy 89.5 79) (xy 87 81.5) (xy 36 81.5) (xy 30.5 76)
        (xy 30.5 35.5) (xy 31.5 34.5) (xy 88.5 34.5)
      )
    )
  )
  (zone (net 4) (net_name /+15V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.5 35.5) (xy 89.5 79) (xy 87 81.5) (xy 36 81.5) (xy 30.5 76)
        (xy 30.5 35.5) (xy 31.5 34.5) (xy 88.5 34.5)
      )
    )
  )
  (zone (net 3) (net_name /LineIn) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 27.5 101.5) (xy 38.5 87) (xy 42.5 87) (xy 43.5 88) (xy 43.5 98.5)
        (xy 43.5 100.5) (xy 44.5 101.5) (xy 58.5 101.5) (xy 59.5 102.5) (xy 59.5 108.5)
        (xy 57.5 110.5) (xy 57.5 115) (xy 61 118) (xy 52 128) (xy 52 223.5)
        (xy 51 224.5) (xy 3.5 224.5) (xy 3.5 191.5) (xy 3.5 147) (xy 4.5 146)
        (xy 35 146) (xy 36 145) (xy 36 122) (xy 35 121) (xy 4.5 121)
        (xy 3.5 120) (xy 3.5 102.5) (xy 4.5 101.5)
      )
    )
  )
  (zone (net 15) (net_name /Mid2) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 24.5 3.5) (xy 25.5 4.5) (xy 25.5 78.5) (xy 34 87) (xy 66 87)
        (xy 67 88) (xy 67 98.5) (xy 67 99) (xy 67 111.5) (xy 52 128)
        (xy 52 223.5) (xy 51 224.5) (xy 3.5 224.5) (xy 3.5 191.5) (xy 3.5 3.5)
        (xy 7.5 3.5) (xy 21.5 3.5)
      )
    )
  )
  (zone (net 18) (net_name /12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 106.5 4.5) (xy 106.5 27.5) (xy 105.5 28.5) (xy 87 28.5) (xy 31.5 28.5)
        (xy 30.5 27.5) (xy 30.5 4.5) (xy 31.5 3.5) (xy 105.5 3.5)
      )
    )
  )
  (zone (net 17) (net_name "Net-(J18-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 25.5 73.5) (xy 25.5 78.5) (xy 33.5 86.5) (xy 25.5 96.5) (xy 24.5 97.5)
        (xy 4.5 97.5) (xy 3.5 96.5) (xy 3.5 73.5) (xy 4.5 72.5) (xy 24.5 72.5)
      )
    )
  )
  (zone (net 16) (net_name /Mid1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 25.5 35.5) (xy 25.5 64.5) (xy 24.5 65.5) (xy 4.5 65.5) (xy 3.5 64.5)
        (xy 3.5 35.5) (xy 4.5 34.5) (xy 24.5 34.5)
      )
    )
  )
  (zone (net 26) (net_name "Net-(C22-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 106.5 4.5) (xy 106.5 27.5) (xy 105.5 28.5) (xy 87 28.5) (xy 31.5 28.5)
        (xy 30.5 27.5) (xy 30.5 4.5) (xy 31.5 3.5) (xy 105.5 3.5)
      )
    )
  )
  (zone (net 6) (net_name /OutPositive) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 113 3.5) (xy 134.5 3.5) (xy 138.5 3.5) (xy 143 3.5) (xy 149 3.5)
        (xy 224 3.5) (xy 231.5 3.5) (xy 236 3.5) (xy 239.5 3.5) (xy 250 3.5)
        (xy 250 224.5) (xy 176 224.5) (xy 128 224.5) (xy 58 224.5) (xy 57 223.5)
        (xy 57 200.5) (xy 58 199.5) (xy 107.5 199.5) (xy 108.5 198.5) (xy 108.5 182)
        (xy 107.5 181) (xy 58 181) (xy 57 180) (xy 57 132) (xy 74 113)
        (xy 74 87.5) (xy 75 86.5) (xy 89.5 86.5) (xy 91 85) (xy 115 85)
        (xy 125 75) (xy 171 75) (xy 172 74) (xy 172 55.5) (xy 171 54.5)
        (xy 95.5 54.5) (xy 94.5 53.5) (xy 94.5 35.5) (xy 95.5 34.5) (xy 107.5 34.5)
        (xy 111.5 30.5) (xy 111.5 5)
      )
    )
  )
  (zone (net 15) (net_name /Mid2) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 25.5 4.5) (xy 25.5 27) (xy 24.5 28) (xy 4.5 28) (xy 3.5 27)
        (xy 3.5 3.5) (xy 24.5 3.5)
      )
    )
  )
  (zone (net 27) (net_name /Line-PreFuse) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 32.5 126) (xy 32.5 141) (xy 31.5 142) (xy 4.5 142) (xy 3.5 141)
        (xy 3.5 126) (xy 4.5 125) (xy 31.5 125)
      )
    )
  )
  (zone (net 5) (net_name /OutNegative) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 113 3.5) (xy 134.5 3.5) (xy 138.5 3.5) (xy 143 3.5) (xy 149 3.5)
        (xy 224 3.5) (xy 231.5 3.5) (xy 236 3.5) (xy 239.5 3.5) (xy 250 3.5)
        (xy 250 224.5) (xy 58 224.5) (xy 57 223.5) (xy 57 132) (xy 74 113)
        (xy 74 87.5) (xy 75 86.5) (xy 89.5 86.5) (xy 94.5 81.5) (xy 94.5 58)
        (xy 94.5 35.5) (xy 95.5 34.5) (xy 107.5 34.5) (xy 111.5 30.5) (xy 111.5 5)
      )
    )
  )
)
