(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 14)
    (no_connects 0)
    (area 99.899999 99.899999 116.150001 111.500001)
    (thickness 1.6)
    (drawings 21)
    (tracks 28)
    (zones 0)
    (modules 5)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J2-Pad3)")
  (net 8 "Net-(J3-Pad1)")
  (net 9 "Net-(J3-Pad2)")
  (net 10 "Net-(J3-Pad3)")
  (net 11 "Net-(J3-Pad4)")
  (net 12 "Net-(J4-Pad1)")
  (net 13 "Net-(J4-Pad2)")
  (net 14 "Net-(J4-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5A35B9CE)
    (at 101.9048 101.9048)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 9.95) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A35B9C9)
    (at 105.5116 109.4994 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 2.4892 -1.016 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5A35B9D2)
    (at 114.1476 109.4994 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 9.95 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5A35B9DB)
    (at 110.5916 101.9048 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 7.41 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_LGA:LGA-14L-2.5x3x0.86mm (layer F.Cu) (tedit 5A35BAF3)
    (at 108.0262 105.7656)
    (fp_text reference U1 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value ISM330DLC (at 0 2) (layer F.Fab) hide)
    (fp_text user REF** (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1625 -0.75 90) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -1.1625 -0.25 90) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -1.1625 0.25 90) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -1.1625 0.75 90) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -0.5 0.9125) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 6 smd rect (at 0 0.9125) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 7 smd rect (at 0.5 0.9125) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 8 smd rect (at 1.1625 0.75 90) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad1)"))
    (pad 9 smd rect (at 1.1625 0.25 90) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad2)"))
    (pad 11 smd rect (at 1.1625 -0.75 90) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad4)"))
    (pad 10 smd rect (at 1.1625 -0.25 90) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (pad 12 smd rect (at 0.5 -0.9125) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J4-Pad1)"))
    (pad 13 smd rect (at 0 -0.9125) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J4-Pad2)"))
    (pad 14 smd rect (at -0.5 -0.9125) (size 0.25 0.475) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J4-Pad3)"))
  )
  (gr_text "LGA-14L Breakout\nRyan Bahneman\n" (at 108.0262 106.299) (layer B.SilkS))
  (gr_text Breakout (at 111.7346 105.6132 270) (layer F.SilkS))
  (gr_text "LGA-14L\n" (at 104.3178 105.6386 90) (layer F.SilkS))
  (gr_text 12 (at 109.0422 103.9368) (layer F.SilkS))
  (gr_text 13 (at 108.0262 103.9368) (layer F.SilkS))
  (gr_text 14 (at 106.9594 103.9622) (layer F.SilkS))
  (gr_text 11 (at 110.2106 104.6226) (layer F.SilkS))
  (gr_text 10 (at 110.2106 105.3846) (layer F.SilkS))
  (gr_text 9 (at 110.2106 106.172) (layer F.SilkS))
  (gr_text 8 (at 110.2106 106.9594) (layer F.SilkS))
  (gr_text 7 (at 109.1184 107.569) (layer F.SilkS))
  (gr_text 6 (at 108.0516 107.569) (layer F.SilkS))
  (gr_text 5 (at 107.0102 107.569) (layer F.SilkS))
  (gr_text 4 (at 105.8418 106.9594) (layer F.SilkS))
  (gr_text 3 (at 105.8418 106.172) (layer F.SilkS))
  (gr_text 2 (at 105.8418 105.3846) (layer F.SilkS))
  (gr_text 1 (at 105.8164 104.6226) (layer F.SilkS))
  (gr_line (start 116.05 100) (end 116.05 111.4) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100 111.4) (end 116.05 111.4) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100 100) (end 116.05 100) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 100 100) (end 100 111.4) (angle 90) (layer Edge.Cuts) (width 0.2))
)
