<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="52.578" y2="0" width="0" layer="20"/>
<wire x1="52.578" y1="0" x2="52.578" y2="55.88" width="0" layer="20"/>
<wire x1="0" y1="55.88" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="55.88" x2="52.578" y2="55.88" width="0" layer="20"/>
<text>CAN module</text>
<text>CAN
Term-
ination</text>
<text>STATE</text>
<text>#Cyl</text>
<text>0 0 0
0 0 1
0 1 0
0 1 1
1 0 0
1 0 1
1 1 0
1 1 1</text>
<text>2
3
4
5
6
8
10
12</text>
<text>CAN-bus to Analog
Tachometer Driver</text>
<text>© EV West 2020</text>
</plain>
<libraries>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-04">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="TeslaParkingBrakeParts">
<packages>
<package name="MP1584EN_DCDC">
</package>
<package name="SPI_CAN_MODULE">
</package>
</packages>
</library>
<library name="Arduino-clone">
<description>Arduino Clone pinheaders
By cl@xganon.com
http://www.xganon.com</description>
<packages>
<package name="NANO">
</package>
</packages>
</library>
<library name="TachDriverParts">
<packages>
<package name="SCREW_HARNESS_OUT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LM358N" library="linear" package="DIL08" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="VALUE"/>
</element>
<element name="DIP4" library="special" package="EDG-04" value="">
<attribute name="POPULARITY" value="8"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="TeslaParkingBrakeParts" package="MP1584EN_DCDC" value="MP1584EN_DCDC"/>
<element name="U$1" library="Arduino-clone" package="NANO" value="NANO"/>
<element name="U$4" library="TachDriverParts" package="SCREW_HARNESS_OUT" value="SCREW_HARNESS_OUT"/>
<element name="U$2" library="TeslaParkingBrakeParts" package="SPI_CAN_MODULE" value="SPI_CAN_MODULE"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$3" pad="5VOUT1"/>
<contactref element="U$3" pad="5VOUT2"/>
<contactref element="U$1" pad="RAW"/>
</signal>
<signal name="3V3">
<contactref element="LM358N" pad="2"/>
<contactref element="U$1" pad="3.3V"/>
</signal>
<signal name="D9">
<contactref element="LM358N" pad="3"/>
<contactref element="U$1" pad="D9"/>
</signal>
<signal name="12V+">
<contactref element="LM358N" pad="8"/>
<contactref element="U$3" pad="12VIN1"/>
<contactref element="U$3" pad="12VIN2"/>
<contactref element="U$4" pad="12V+"/>
</signal>
<signal name="GND">
<contactref element="LM358N" pad="4"/>
<contactref element="U$3" pad="GNDIN1"/>
<contactref element="U$3" pad="GNDIN2"/>
<contactref element="U$3" pad="GNDOUT1"/>
<contactref element="U$3" pad="GNDOUT2"/>
<contactref element="DIP4" pad="2"/>
<contactref element="DIP4" pad="3"/>
<contactref element="DIP4" pad="4"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$4" pad="12V-"/>
<contactref element="U$2" pad="GND"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="5V"/>
<contactref element="U$2" pad="VCC"/>
</signal>
<signal name="A0">
<contactref element="DIP4" pad="7"/>
<contactref element="U$1" pad="A0"/>
</signal>
<signal name="A1">
<contactref element="DIP4" pad="6"/>
<contactref element="U$1" pad="A1"/>
</signal>
<signal name="A2">
<contactref element="DIP4" pad="5"/>
<contactref element="U$1" pad="A2"/>
</signal>
<signal name="TERM_2">
<contactref element="DIP4" pad="1"/>
<contactref element="U$2" pad="T_2"/>
</signal>
<signal name="TERM_1">
<contactref element="DIP4" pad="8"/>
<contactref element="U$2" pad="T_1"/>
</signal>
<signal name="SO">
<contactref element="U$1" pad="D12"/>
<contactref element="U$2" pad="SO"/>
</signal>
<signal name="SI">
<contactref element="U$1" pad="D11"/>
<contactref element="U$2" pad="SI"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="D13"/>
<contactref element="U$2" pad="SCK"/>
</signal>
<signal name="D7">
<contactref element="U$1" pad="D7"/>
<contactref element="U$2" pad="CS"/>
</signal>
<signal name="CAN_H">
<contactref element="U$4" pad="CAN_H"/>
<contactref element="U$2" pad="CAN_H"/>
</signal>
<signal name="CAN_L">
<contactref element="U$4" pad="CAN_L"/>
<contactref element="U$2" pad="CAN_L"/>
</signal>
<signal name="TACH">
<contactref element="LM358N" pad="1"/>
<contactref element="U$4" pad="TACH"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
