(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6002)
    (drawings 14)
    (tracks 203)
    (zones 0)
    (modules 30)
    (nets 1)
  )
  (page A4)
  (title_block
    (date "18 jul 2013")
  )
  (layers
    (0 Front signal)
    (31 Back signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.8001)
    (user_trace_width 1.00076)
    (user_trace_width 1.19888)
    (user_trace_width 1.50114)
    (user_trace_width 1.80086)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.09906)
    (segment_width 0.381)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.381)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 2.54 2.54)
    (pad_drill 0.8001)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.2032)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Pad1 (layer Front) (tedit 51E797AC)
    (at 107.95 82.55)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad -LED thru_hole circle (at 0 0) (size 2.54 2.54) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pad1 (layer Front) (tedit 51E797A3)
    (at 104.14 85.09)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad +LED thru_hole circle (at 0 0) (size 2.54 2.54) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
  )
  (module switch (layer Front) (tedit 51B75FBB)
    (at 170.815 78.105 270)
    (tags DIL)
    (fp_text reference " " (at 0.635 2.54 270) (layer F.SilkS))
    (fp_text value ON/OFF (at 0 -2.54 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 0 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 2.54 -5.08 270) (size 2.99974 2.99974) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -2.54 -5.08 270) (size 2.99974 2.99974) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module morsetto_2pin (layer Front) (tedit 51E797CC)
    (at 146.685 101.6 180)
    (descr "Morsetto Elcart verde 2 pins drills 1,5mm")
    (fp_text reference " " (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value "AUDIO OUT" (at 0 -3.81 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
  )
  (module morsetto_2pin (layer Front) (tedit 51E64ABF)
    (at 160.02 101.6 180)
    (descr "Morsetto Elcart verde 2 pins drills 1,5mm")
    (fp_text reference " " (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value "GND  + 18V" (at 0 -3.81 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
  )
  (module Cap_NP (layer Front) (tedit 51B75EEB)
    (at 125.095 71.12)
    (descr "capacitor np")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27) (layer F.SilkS))
    (fp_text value 100nF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_NP (layer Front) (tedit 51B75E27)
    (at 104.14 100.33 90)
    (descr "capacitor np")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module morsetto_2pin (layer Front) (tedit 51B75233)
    (at 95.885 101.6 180)
    (descr "Morsetto Elcart verde 2 pins drills 1,5mm")
    (fp_text reference " " (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value ANT (at 0 -3.81 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
  )
  (module morsetto_2pin (layer Front) (tedit 51B7524E)
    (at 112.395 101.6 180)
    (descr "Morsetto Elcart verde 2 pins drills 1,5mm")
    (fp_text reference " " (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value "CAP VAR" (at 0 -3.81 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
  )
  (module jack_3_5mm (layer Front) (tedit 51B75FAC)
    (at 173.355 90.805 270)
    (descr "capacitor np")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference "HEADPHONE " (at 0 -10.16 270) (layer F.SilkS))
    (fp_text value " " (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 3.81 5.715 270) (size 2.49936 2.49936) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -4.445 6.35 270) (size 2.49936 2.49936) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad SW thru_hole circle (at -2.54 3.81 270) (size 2.49936 2.49936) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad GND thru_hole circle (at -2.54 -3.175 270) (size 2.99974 2.99974) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_NP (layer Front) (tedit 51B75F1C)
    (at 106.045 63.5 180)
    (descr "capacitor np")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_standard (layer Front) (tedit 51B75E9F)
    (at 124.46 78.105 90)
    (descr "Resistor 7.5 mm")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 100K (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module morsetto_3pin (layer Front) (tedit 51B7528C)
    (at 121.285 63.5)
    (descr "Morsetto Elcart verde 3 pins drills 1,5mm")
    (fp_text reference " " (at 0.635 -2.54) (layer F.SilkS))
    (fp_text value "POT 47K" (at 0 -3.81) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 0) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 5.08 0) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
  )
  (module ECC82V3 (layer Front) (tedit 51B75DD5)
    (at 103.505 80.01)
    (fp_text reference ECC82 (at 0 -11.43) (layer F.SilkS))
    (fp_text value "" (at 0 11.43) (layer F.SilkS))
    (pad 1 thru_hole circle (at 5.08 6.985 306) (size 3.59918 3.59918) (drill oval 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 8.255 2.54 306) (size 3.59918 3.59918) (drill oval 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 8.255 -2.54 306) (size 3.59918 3.59918) (drill oval 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 5.08 -6.35 306) (size 3.59918 3.59918) (drill oval 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at 0 -8.255 306) (size 3.59918 3.59918) (drill oval 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -5.08 -6.985 306) (size 3.59918 3.59918) (drill oval 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -7.62 -2.54 306) (size 3.59918 3.59918) (drill oval 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at -7.62 2.54 306) (size 3.59918 3.59918) (drill oval 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at -5.08 6.985 306) (size 3.59918 3.59918) (drill oval 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 0 0) (size 5.99948 5.99948) (drill 4.0005) (layers *.Cu *.Mask F.SilkS))
    (model valves/ecc83.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module screw (layer Front) (tedit 4C70E85B)
    (at 84.455 103.505)
    (descr "screw pcb")
    (tags DEV)
    (fp_text reference " " (at 0.381 3.302) (layer F.SilkS))
    (fp_text value " " (at 0.635 -3.175) (layer F.SilkS))
    (pad "" thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module Cap_NP (layer Front) (tedit 51B75DEF)
    (at 95.885 63.5)
    (descr "capacitor np")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27) (layer F.SilkS))
    (fp_text value 330pF (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_NP (layer Front) (tedit 51B75E07)
    (at 88.9 90.17 270)
    (descr "capacitor np")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 330pF (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module screw (layer Front) (tedit 4C70E85B)
    (at 84.455 61.595)
    (descr "screw pcb")
    (tags DEV)
    (fp_text reference " " (at 0.381 3.302) (layer F.SilkS))
    (fp_text value " " (at 0.635 -3.175) (layer F.SilkS))
    (pad "" thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module morsetto_3pin (layer Front) (tedit 51B7525F)
    (at 128.27 101.6 180)
    (descr "Morsetto Elcart verde 3 pins drills 1,5mm")
    (fp_text reference " " (at 0.635 -2.54 180) (layer F.SilkS))
    (fp_text value COIL (at 0 -3.81 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 3.048 4.064) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
  )
  (module Res_standard (layer Front) (tedit 51B75E0F)
    (at 85.725 78.74 270)
    (descr "Resistor 7.5 mm")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 2M2 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Res_standard (layer Front) (tedit 51B75E6D)
    (at 119.38 74.295 90)
    (descr "Resistor 7.5 mm")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 1M (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Cap_NP (layer Front) (tedit 51B75E57)
    (at 119.38 83.82 90)
    (descr "capacitor np")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 22nF (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module electrolitic47uF (layer Front) (tedit 51B82B9F)
    (at 170.18 67.945 180)
    (descr "electrolitic cap 47uF 16V/25V 3.5mm pins")
    (tags DIL)
    (fp_text reference " " (at 0.635 3.175 180) (layer F.SilkS))
    (fp_text value + (at 2.54 1.905 180) (layer F.SilkS))
    (fp_text user 22uF (at 0 0.635 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 1.5748 2.286) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.5748 2.286) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module screw (layer Front) (tedit 4C70E85B)
    (at 176.53 103.505)
    (descr "screw pcb")
    (tags DEV)
    (fp_text reference " " (at 0.381 3.302) (layer F.SilkS))
    (fp_text value " " (at 0.635 -3.175) (layer F.SilkS))
    (pad "" thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module screw (layer Front) (tedit 4C70E85B)
    (at 176.53 61.595)
    (descr "screw pcb")
    (tags DEV)
    (fp_text reference " " (at 0.381 3.302) (layer F.SilkS))
    (fp_text value " " (at 0.635 -3.175) (layer F.SilkS))
    (pad "" thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
  )
  (module Res_standard (layer Front) (tedit 51E79741)
    (at 121.92 90.17)
    (descr "Resistor 7.5 mm")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27) (layer F.SilkS))
    (fp_text value 330 (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module led3mm (layer Front) (tedit 51E797BC)
    (at 130.175 88.265)
    (descr "led 3mm")
    (tags DIL)
    (fp_text reference " " (at 0.635 3.175) (layer F.SilkS))
    (fp_text value LED (at 0 -2.794) (layer F.SilkS))
    (fp_text user + (at 2.921 -0.127) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.5748 2.286) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.5748 2.286) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module trafo-05VA (layer Front) (tedit 51E667F9)
    (at 149.225 76.2 90)
    (fp_text reference Transformador (at -0.635 4.445 90) (layer F.SilkS))
    (fp_text value " Pri: 220V Sec: 9V + 9V   " (at 0 6.985 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -10.16 10.795 90) (size 2.99974 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -5.08 10.795 90) (size 2.99974 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at 5.08 10.795 90) (size 2.99974 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 10.16 10.795 90) (size 2.99974 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -10.16 -9.525 90) (size 2.99974 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at 10.16 -9.525 90) (size 2.99974 2.99974) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
  )
  (module TO220 (layer Front) (tedit 51E64A8A)
    (at 130.81 74.295 270)
    (descr "TO220, BD137,B138, 7805 drill 1mm")
    (tags TO220)
    (fp_text reference " " (at 0.635 2.54 270) (layer F.SilkS))
    (fp_text value 7812 (at 0 -3.175 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 1.67386 2.286) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 0 270) (size 1.67386 2.286) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.67386 2.286) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (model dil/dil_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bridge10mm (layer Front) (tedit 4C78E7F6)
    (at 124.46 67.945)
    (descr "capacitor np")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference " " (at 0 1.27) (layer F.SilkS))
    (fp_text value " " (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 180.34 57.785) (end 180.34 63.5) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 80.645 57.785) (end 180.34 57.785) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 80.645 63.5) (end 80.645 57.785) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_text WWW.INVENTABLE.EU (at 150.495 76.835 90) (layer Back))
  (gr_line (start 80.645 63.5) (end 80.645 64.77) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 180.34 64.77) (end 180.34 63.5) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 80.645 64.77) (end 80.645 93.345) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 80.645 94.615) (end 80.645 106.045) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 180.34 106.045) (end 180.34 66.04) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 80.645 107.315) (end 180.34 107.315) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 180.34 107.315) (end 180.34 106.045) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 80.645 107.315) (end 80.645 106.045) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 80.645 93.345) (end 80.645 94.615) (angle 90) (layer Edge.Cuts) (width 0.09906))
  (gr_line (start 180.34 66.04) (end 180.34 64.77) (angle 90) (layer Edge.Cuts) (width 0.09906))
)
