(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 346)
    (zones 0)
    (modules 15)
    (nets 62)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.1524)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 100 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D1-Pad3)")
  (net 6 "Net-(D1-Pad4)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(J2-Pad2)")
  (net 10 "Net-(J2-Pad3)")
  (net 11 +3V3)
  (net 12 "Net-(J2-Pad5)")
  (net 13 "Net-(J2-Pad6)")
  (net 14 /DALIRX)
  (net 15 "Net-(J2-Pad8)")
  (net 16 /DALITX)
  (net 17 "Net-(J2-Pad10)")
  (net 18 "Net-(J2-Pad11)")
  (net 19 "Net-(J2-Pad12)")
  (net 20 /RX)
  (net 21 /TX)
  (net 22 /SCL)
  (net 23 /SDA)
  (net 24 "Net-(J3-Pad4)")
  (net 25 "Net-(J3-Pad3)")
  (net 26 "Net-(J3-Pad2)")
  (net 27 "Net-(J3-Pad1)")
  (net 28 /IO1)
  (net 29 /IO2)
  (net 30 /IO3)
  (net 31 /IO4)
  (net 32 /IO5)
  (net 33 /IO6)
  (net 34 /IO7)
  (net 35 /IO8)
  (net 36 "Net-(TR1-Pad2)")
  (net 37 "Net-(TR1-Pad7)")
  (net 38 "Net-(U1-Pad4)")
  (net 39 "Net-(U2-Pad39)")
  (net 40 "Net-(U2-Pad38)")
  (net 41 "Net-(U2-Pad3)")
  (net 42 "Net-(U2-Pad37)")
  (net 43 "Net-(U2-Pad4)")
  (net 44 "Net-(U2-Pad32)")
  (net 45 "Net-(U2-Pad31)")
  (net 46 "Net-(U2-Pad11)")
  (net 47 "Net-(U2-Pad12)")
  (net 48 "Net-(U2-Pad15)")
  (net 49 "Net-(U2-Pad16)")
  (net 50 "Net-(U2-Pad17)")
  (net 51 "Net-(U2-Pad18)")
  (net 52 "Net-(U2-Pad19)")
  (net 53 "Net-(U2-Pad20)")
  (net 54 /TX-)
  (net 55 /TX+)
  (net 56 /RX-)
  (net 57 /RX+)
  (net 58 /TD+)
  (net 59 /TD-)
  (net 60 /RD+)
  (net 61 /RD-)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /DALIRX)
    (add_net /DALITX)
    (add_net /IO1)
    (add_net /IO2)
    (add_net /IO3)
    (add_net /IO4)
    (add_net /IO5)
    (add_net /IO6)
    (add_net /IO7)
    (add_net /IO8)
    (add_net /RD+)
    (add_net /RD-)
    (add_net /RX)
    (add_net /RX+)
    (add_net /RX-)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TD+)
    (add_net /TD-)
    (add_net /TX)
    (add_net /TX+)
    (add_net /TX-)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(TR1-Pad2)")
    (add_net "Net-(TR1-Pad7)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad4)")
  )
  (module Connector_RJ:RJ45_Wuerth_615008148521_Horizontal (layer F.Cu) (tedit 5DAB2B7B)
    (at 158.5 64.1 270)
    (fp_text reference J1 (at 13.45 -8.3 270) (layer F.SilkS))
    (fp_text value RJ45_ModeB (at 8.45 3.45 270) (layer F.Fab))
    (pad 8 thru_hole circle (at 3.93 -4.84 270) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 7 thru_hole circle (at 4.95 -2.3 270) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 6 thru_hole circle (at 5.97 -4.84 270) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 /TX-))
    (pad 5 thru_hole circle (at 6.99 -2.3 270) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 4 thru_hole circle (at 8.01 -4.84 270) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 3 thru_hole circle (at 9.03 -2.3 270) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 /TX+))
    (pad 2 thru_hole circle (at 10.05 -4.84 270) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 /RX-))
    (pad 1 thru_hole circle (at 11.07 -2.3 270) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 57 /RX+))
    (pad "" np_thru_hole circle (at 15 0 270) (size 2.36 2.36) (drill 2.36) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 270) (size 2.36 2.36) (drill 2.36) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 185.7 51.1)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value "10uF 25V" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_6.3x5.8 (layer F.Cu) (tedit 5BCA39D0)
    (at 185.5 44.4)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x5.8mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at 0 -4.35) (layer F.SilkS))
    (fp_text value "100uF 25V" (at 0 4.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.7 0) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_6.3x5.8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-269AA (layer F.Cu) (tedit 5A4F6848)
    (at 170.4 57.6 180)
    (descr "SMD package TO-269AA (e.g. diode bridge), see http://www.vishay.com/docs/88854/padlayouts.pdf")
    (tags "TO-269AA MBS diode bridge")
    (attr smd)
    (fp_text reference D1 (at -2.9 -3.6) (layer F.SilkS))
    (fp_text value MB4S (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 -0.065) (layer F.Fab))
    (pad 4 smd rect (at 3.075 -1.27 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at 3.075 1.27 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at -3.075 1.27 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -3.075 -1.27 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-269AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-269AA (layer F.Cu) (tedit 5A4F6848)
    (at 159.6 57.6 180)
    (descr "SMD package TO-269AA (e.g. diode bridge), see http://www.vishay.com/docs/88854/padlayouts.pdf")
    (tags "TO-269AA MBS diode bridge")
    (attr smd)
    (fp_text reference D2 (at -2.5 -3.6) (layer F.SilkS))
    (fp_text value MB4S (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 -0.065) (layer F.Fab))
    (pad 4 smd rect (at 3.075 -1.27 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad4)"))
    (pad 3 smd rect (at 3.075 1.27 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (pad 2 smd rect (at -3.075 1.27 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -3.075 -1.27 180) (size 1 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TO-269AA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA_Handsoldering (layer F.Cu) (tedit 58643398)
    (at 159.1 45.2)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D3 (at -2.6 2.7) (layer F.SilkS))
    (fp_text value D_Zener (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 2 smd rect (at 2.5 0) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad4)"))
    (pad 1 smd rect (at -2.5 0) (size 3.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad3)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 237.4 37.4)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (fp_text reference J2 (at 5.655 -2.27) (layer F.SilkS))
    (fp_text value Conn_02x06_Odd_Even (at 5.655 14.97) (layer F.Fab))
    (fp_text user %R (at 5.31 6.35 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /DALITX))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /DALIRX))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 185.6 40.6)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 2.62) (layer B.SilkS))
    (fp_text value R (at 0 -2.62) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_2512_6332Metric_Pad1.52x3.35mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 185.5 32.6)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 2.62) (layer B.SilkS))
    (fp_text value R (at 0 -2.62) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.163934)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Transformer_SMD:Transformer_Ethernet_Bourns_PT61017PEL (layer F.Cu) (tedit 5C422741)
    (at 178 71.1 180)
    (descr https://www.bourns.com/docs/Product-Datasheets/PT61017PEL.pdf)
    (tags "Transformer Ethernet Single Center-Tap")
    (attr smd)
    (fp_text reference TR1 (at -0.1 -7.9) (layer F.SilkS))
    (fp_text value 749013011 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 12 smd rect (at 4.4 0.635 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 4.4 -4.445 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 57 /RX+))
    (pad 13 smd rect (at 4.4 -0.635 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 4.4 3.175 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 15 smd rect (at 4.4 -3.175 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 9 smd rect (at 4.4 4.445 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 54 /TX-))
    (pad 11 smd rect (at 4.4 1.905 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 55 /TX+))
    (pad 14 smd rect (at 4.4 -1.905 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 56 /RX-))
    (pad 8 smd rect (at -4.4 4.445 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 58 /TD+))
    (pad 6 smd rect (at -4.4 1.905 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 59 /TD-))
    (pad 5 smd rect (at -4.4 0.635 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -4.4 3.175 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(TR1-Pad7)"))
    (pad 4 smd rect (at -4.4 -0.635 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.4 -1.905 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 60 /RD+))
    (pad 2 smd rect (at -4.4 -3.175 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(TR1-Pad2)"))
    (pad 1 smd rect (at -4.4 -4.445 180) (size 1.7 0.76) (layers F.Cu F.Paste F.Mask)
      (net 61 /RD-))
    (model ${KISYS3DMOD}/Transformer_SMD.3dshapes/Transformer_Ethernet_Bourns_PT61017PEL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:Infomart_PEM1400 (layer F.Cu) (tedit 5DAB27D5)
    (at 157.2 36.9)
    (fp_text reference U1 (at 1.8 3.7) (layer F.SilkS))
    (fp_text value PEM1400 (at 15 -0.5) (layer F.Fab))
    (pad 5 thru_hole circle (at 30.87 0) (size 1.6 1.6) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 28.33 0) (size 1.6 1.6) (drill 1.02) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad4)"))
    (pad 3 thru_hole circle (at 25.79 0) (size 1.6 1.6) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad4)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad3)"))
  )
  (module Module:mbed_LPC1768 (layer F.Cu) (tedit 5DA341B5)
    (at 217.6 55.1 90)
    (fp_text reference U2 (at -26.23 0) (layer F.SilkS))
    (fp_text value mbed_LPC1768 (at 0 0 90) (layer F.Fab))
    (pad 20 thru_hole oval (at 24.13 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 "Net-(U2-Pad20)"))
    (pad 21 thru_hole oval (at 24.13 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 /DALIRX))
    (pad 19 thru_hole oval (at 21.59 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 "Net-(U2-Pad19)"))
    (pad 22 thru_hole oval (at 21.59 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 /DALITX))
    (pad 18 thru_hole oval (at 19.05 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "Net-(U2-Pad18)"))
    (pad 23 thru_hole oval (at 19.05 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 /IO8))
    (pad 17 thru_hole oval (at 16.51 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(U2-Pad17)"))
    (pad 24 thru_hole oval (at 16.51 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 /IO7))
    (pad 16 thru_hole oval (at 13.97 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 "Net-(U2-Pad16)"))
    (pad 25 thru_hole oval (at 13.97 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 /IO6))
    (pad 15 thru_hole oval (at 11.43 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 "Net-(U2-Pad15)"))
    (pad 26 thru_hole oval (at 11.43 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 /IO5))
    (pad 14 thru_hole oval (at 8.89 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 /RX))
    (pad 27 thru_hole oval (at 8.89 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 /IO3))
    (pad 13 thru_hole oval (at 6.35 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 /TX))
    (pad 28 thru_hole oval (at 6.35 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 /IO4))
    (pad 12 thru_hole oval (at 3.81 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "Net-(U2-Pad12)"))
    (pad 29 thru_hole oval (at 3.81 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 /IO2))
    (pad 11 thru_hole oval (at 1.27 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(U2-Pad11)"))
    (pad 30 thru_hole oval (at 1.27 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 /IO1))
    (pad 10 thru_hole oval (at -1.27 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 /SCL))
    (pad 31 thru_hole oval (at -1.27 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Net-(U2-Pad31)"))
    (pad 9 thru_hole oval (at -3.81 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 /SDA))
    (pad 32 thru_hole oval (at -3.81 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(U2-Pad32)"))
    (pad 8 thru_hole oval (at -6.35 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad1)"))
    (pad 33 thru_hole oval (at -6.35 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 /TD+))
    (pad 7 thru_hole oval (at -8.89 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad4)"))
    (pad 34 thru_hole oval (at -8.89 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 59 /TD-))
    (pad 6 thru_hole oval (at -11.43 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad3)"))
    (pad 35 thru_hole oval (at -11.43 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 60 /RD+))
    (pad 5 thru_hole oval (at -13.97 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad2)"))
    (pad 36 thru_hole oval (at -13.97 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 61 /RD-))
    (pad 4 thru_hole oval (at -16.51 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Net-(U2-Pad4)"))
    (pad 37 thru_hole oval (at -16.51 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(U2-Pad37)"))
    (pad 3 thru_hole oval (at -19.05 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(U2-Pad3)"))
    (pad 38 thru_hole oval (at -19.05 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(U2-Pad38)"))
    (pad 2 thru_hole oval (at -21.59 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 39 thru_hole oval (at -21.59 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(U2-Pad39)"))
    (pad 1 thru_hole oval (at -24.13 11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at -24.13 -11.43 90) (size 1.2 2) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 +3V3))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Horizontal_pmod (layer F.Cu) (tedit 5DAB3238)
    (at 237.4 60.26)
    (descr "Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x06 2.54mm double row")
    (fp_text reference J3 (at 5.655 -2.27) (layer F.SilkS))
    (fp_text value Conn_02x06_Top_Bottom (at 5.655 14.97) (layer F.Fab))
    (fp_text user %R (at 5.31 6.35 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3V3))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3V3))
    (pad 11 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /RX))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad4)"))
    (pad 9 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /TX))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad3)"))
    (pad 8 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad2)"))
    (pad 7 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /SDA))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 201.1 61.5 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 2.7 -2.8) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /IO1))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /IO2))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /IO3))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /IO4))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 201 43.9 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J5 (at 2.9 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3V3))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /IO8))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /IO7))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /IO6))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /IO5))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 97.8 (width 0.12) (layer Dwgs.User)
    (gr_text "97.800 mm" (at 201.2 93.07) (layer Dwgs.User))
    (feature1 (pts (xy 152.3 82.9) (xy 152.3 92.386421)))
    (feature2 (pts (xy 250.1 82.9) (xy 250.1 92.386421)))
    (crossbar (pts (xy 250.1 91.8) (xy 152.3 91.8)))
    (arrow1a (pts (xy 152.3 91.8) (xy 153.426504 91.213579)))
    (arrow1b (pts (xy 152.3 91.8) (xy 153.426504 92.386421)))
    (arrow2a (pts (xy 250.1 91.8) (xy 248.973496 91.213579)))
    (arrow2b (pts (xy 250.1 91.8) (xy 248.973496 92.386421)))
  )
  (dimension 55 (width 0.12) (layer Dwgs.User)
    (gr_text "55.000 mm" (at 262.77 55.4 270) (layer Dwgs.User))
    (feature1 (pts (xy 250.3 82.9) (xy 262.086421 82.9)))
    (feature2 (pts (xy 250.3 27.9) (xy 262.086421 27.9)))
    (crossbar (pts (xy 261.5 27.9) (xy 261.5 82.9)))
    (arrow1a (pts (xy 261.5 82.9) (xy 260.913579 81.773496)))
    (arrow1b (pts (xy 261.5 82.9) (xy 262.086421 81.773496)))
    (arrow2a (pts (xy 261.5 27.9) (xy 260.913579 29.026504)))
    (arrow2b (pts (xy 261.5 27.9) (xy 262.086421 29.026504)))
  )
  (gr_line (start 152.3 82.9) (end 152.3 27.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 250.1 82.9) (end 152.3 82.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 250.1 27.9) (end 250.1 82.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 152.3 27.9) (end 250.1 27.9) (layer Edge.Cuts) (width 0.05))
  (gr_text "UART\n" (at 195.3 55.1 90) (layer F.SilkS))
  (gr_text "CAN\n" (at 195.2 60.1 90) (layer F.SilkS))
  (gr_text TD (at 197.5 59) (layer F.SilkS))
  (gr_text "RD\n" (at 197.4 61.4) (layer F.SilkS))
  (gr_text RX (at 197.4 56.3) (layer F.SilkS))
  (gr_text "TX\n" (at 197.4 53.8) (layer F.SilkS))
  (gr_text GND (at 196.9 51.3) (layer F.SilkS))
  (gr_text "3V3\n" (at 196.9 48.8) (layer F.SilkS))
  (gr_text "p23\n" (at 197 36.3) (layer F.SilkS))
  (gr_text "p24\n" (at 197 38.8) (layer F.SilkS))
  (gr_text "p25\n" (at 197 41.3) (layer F.SilkS))
  (gr_text p26 (at 197 43.8) (layer F.SilkS))
  (gr_text "3V3\n" (at 196.9 31.1) (layer F.SilkS))
  (gr_text GND (at 196.9 33.8) (layer F.SilkS))
  (gr_text "PMOD Type 3 UART" (at 193 55 90) (layer F.SilkS))
  (gr_text "PMOD Type 1 GPIO" (at 193.1 37.4 90) (layer F.SilkS))
  (gr_text "PMOD Type 2 A SPI\n" (at 241.8 77.8) (layer F.SilkS))
  (gr_text "NXP IOH DALI" (at 241.8 33.4) (layer F.SilkS))
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.3 53) (xy 185.3 29.2) (xy 177 29.2) (xy 177 53)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177 29.2) (xy 185.3 29.2) (xy 185.3 53) (xy 177 53)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 249.6 29.2) (xy 186.1 29.2) (xy 186.1 53.5) (xy 181.3 53.5) (xy 181.3 81.8)
        (xy 249.6 81.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.1 53) (xy 194.4 53) (xy 194.4 29.2) (xy 186.1 29.2)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.1 29.2) (xy 194.4 29.2) (xy 194.4 53) (xy 186.1 53)
      )
    )
  )
)
