<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="13.95" y1="20.32" x2="1.27" y2="20.32" width="0" layer="20"/>
<wire x1="1.27" y1="20.32" x2="0" y2="19.05" width="0" layer="20" curve="90"/>
<wire x1="0" y1="19.05" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="13.95" y2="0" width="0" layer="20"/>
<wire x1="13.95" y1="0" x2="15.22" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="15.22" y1="1.27" x2="15.22" y2="19.05" width="0" layer="20"/>
<wire x1="15.22" y1="19.05" x2="13.95" y2="20.32" width="0" layer="20" curve="90"/>
<text>Capable Robot</text>
<text>[CR7CSZ]</text>
<text>capablerobot.com</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>G</text>
<text>V</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>G</text>
<text>V</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>G</text>
<text>V</text>
</plain>
<libraries>
<library name="CapableRobot">
<packages>
<package name="HDRRAR12W64P254_2X6_1524X736X556B">
<description>Double-row, 12-pin Receptacle Header (Female) Right Angle, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 7.36 mm insulator length, 15.24 X 7.36 X 5.56 mm body
&lt;p&gt;Double-row (2X6), 12-pin Receptacle Header (Female) Right Angle package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 7.36 mm insulator length with body size 15.24 X 7.36 X 5.56 mm, pin pattern - Follow Digilend PMOD&lt;/p&gt;</description>
</package>
<package name="HDRRA12W64P254_2X6_1524X254X556B">
<description>Double-row, 12-pin Pin Header (Male) Right Angle, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 15.24 X 2.54 X 5.56 mm body
&lt;p&gt;Double-row (2X6), 12-pin Pin Header (Male) Right Angle package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.00 mm tail length and 5.84 mm mating length with body size 15.24 X 2.54 X 5.56 mm, pin pattern - Follow Digilent PMOD
&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PMOD" library="CapableRobot" package="HDRRAR12W64P254_2X6_1524X736X556B" value="PMOD-HOST">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BEAGLE" library="CapableRobot" package="HDRRA12W64P254_2X6_1524X254X556B" value="PMOD-BEAGLEWIRE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+3V3">
<contactref element="PMOD" pad="12"/>
<contactref element="PMOD" pad="6"/>
<contactref element="BEAGLE" pad="7"/>
<contactref element="BEAGLE" pad="1"/>
</signal>
<signal name="GND">
<contactref element="PMOD" pad="11"/>
<contactref element="PMOD" pad="5"/>
<contactref element="BEAGLE" pad="2"/>
<contactref element="BEAGLE" pad="8"/>
</signal>
<signal name="IO4">
<contactref element="PMOD" pad="4"/>
<contactref element="BEAGLE" pad="6"/>
</signal>
<signal name="IO3">
<contactref element="PMOD" pad="3"/>
<contactref element="BEAGLE" pad="5"/>
</signal>
<signal name="IO2">
<contactref element="PMOD" pad="2"/>
<contactref element="BEAGLE" pad="4"/>
</signal>
<signal name="IO1">
<contactref element="PMOD" pad="1"/>
<contactref element="BEAGLE" pad="3"/>
</signal>
<signal name="IO5">
<contactref element="PMOD" pad="7"/>
<contactref element="BEAGLE" pad="9"/>
</signal>
<signal name="IO6">
<contactref element="PMOD" pad="8"/>
<contactref element="BEAGLE" pad="10"/>
</signal>
<signal name="IO7">
<contactref element="PMOD" pad="9"/>
<contactref element="BEAGLE" pad="11"/>
</signal>
<signal name="IO8">
<contactref element="PMOD" pad="10"/>
<contactref element="BEAGLE" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
