(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 52)
    (no_connects 0)
    (area 153.975 79.705 172.185001 110.175)
    (thickness 1.6)
    (drawings 6)
    (tracks 339)
    (zones 0)
    (modules 18)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.16)
    (zone_clearance 0.16)
    (zone_45_only no)
    (trace_min 0.14)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.45)
    (via_drill 0.3302)
    (via_min_size 0.4)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(R1-Pad1)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 +2V8)
  (net 8 /CA_D1)
  (net 9 /CA_D3)
  (net 10 "Net-(P1-Pad7)")
  (net 11 /CA_D0)
  (net 12 /CA_D2)
  (net 13 "Net-(P1-Pad12)")
  (net 14 /CAB_SDA)
  (net 15 /CA_HREF)
  (net 16 /CAB_XCLK)
  (net 17 /CA_PWDN)
  (net 18 /CAB_SCL)
  (net 19 /CA_VSYNC)
  (net 20 "Net-(P1-Pad19)")
  (net 21 /CA_RST)
  (net 22 "Net-(R2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.2)
    (via_dia 0.45)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class BGA ""
    (clearance 0.05)
    (trace_width 0.14)
    (via_dia 0.4)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V8)
    (add_net /CAB_SCL)
    (add_net /CAB_SDA)
    (add_net /CAB_XCLK)
    (add_net /CA_D0)
    (add_net /CA_D1)
    (add_net /CA_D2)
    (add_net /CA_D3)
    (add_net /CA_HREF)
    (add_net /CA_PWDN)
    (add_net /CA_RST)
    (add_net /CA_VSYNC)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad19)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad2)")
  )
  (module gj_feet:BGA_29_x500_y520 (layer F.Cu) (tedit 58929D7A)
    (at 159.482 93.734 90)
    (fp_text reference U1 (at -0.016 2.898 90) (layer F.SilkS))
    (fp_text value OVM6211 (at 0.6 3.3 90) (layer F.Fab) hide)
    (pad A2 smd circle (at -0.5 -1.3 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)") (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad A3 smd circle (at 0 -1.3 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)") (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad A4 smd circle (at 0.5 -1.3 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad A5 smd circle (at 1 -1.3 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad B1 smd circle (at -1 -0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)") (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad B2 smd circle (at -0.5 -0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /CA_D0) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad B3 smd circle (at 0 -0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)") (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad B4 smd circle (at 0.5 -0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad B5 smd circle (at 1 -0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 /CAB_SDA) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad C1 smd circle (at -1 -0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad C2 smd circle (at -0.5 -0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /CA_D2) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad C3 smd circle (at 0 -0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /CAB_SCL) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad C4 smd circle (at 0.5 -0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 /CA_VSYNC) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad C5 smd circle (at 1 -0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R2-Pad2)") (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad D1 smd circle (at -1 0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad D2 smd circle (at -0.5 0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /CA_D1) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad D3 smd circle (at 0 0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad D4 smd circle (at 0.5 0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 /CA_HREF) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad D5 smd circle (at 1 0.26 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /CA_PWDN) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad E1 smd circle (at -1 0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R1-Pad1)") (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad E2 smd circle (at -0.5 0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /CA_D3) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad E3 smd circle (at 0 0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad E4 smd circle (at 0.5 0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAB_XCLK) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad E5 smd circle (at 1 0.78 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad F1 smd circle (at -1 1.3 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /CA_D3) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad F2 smd circle (at -0.5 1.3 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad F3 smd circle (at 0 1.3 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 /CA_RST) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad F4 smd circle (at 0.5 1.3 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
    (pad F5 smd circle (at 1 1.3 90) (size 0.25 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAB_XCLK) (solder_mask_margin 0.0375) (thermal_width 0.15) (thermal_gap 0.4))
  )
  (module gj_feet:HOLE-2.5 locked (layer F.Cu) (tedit 5894FF19)
    (at 158.5 83)
    (descr "Hole 2.5 mm")
    (tags hole)
    (fp_text reference H** (at 0.3 -2.5) (layer F.SilkS) hide)
    (fp_text value 2.5mm (at 0 2.3) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.6) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 160.32 97.98 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.85 -1.42 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 156.65 95.47 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.54 0.04 90) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 156.67 91.94 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -3.03 -0.05 270) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 159.74 93.73)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.76 0.08) (layer B.SilkS))
    (fp_text value "1 uF" (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 158.05 97.63 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.92 -1.21 450) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 160.56 100.56 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -0.06 -1.62 270) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 158.03 101.29 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.05 -1.3 90) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 161.8 87.6)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 2.6 -0.1 90) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 161.8 89.3)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 2.6 0.2 90) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 161.8 85.9)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.63 -0.27 270) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:WurthFFC_1mm_20 (layer F.Cu) (tedit 0)
    (at 166.742 94.955 90)
    (fp_text reference P1 (at -0.045 2.458 90) (layer F.SilkS))
    (fp_text value CONN_01X20 (at 0 3.5 90) (layer F.Fab))
    (pad 1 smd rect (at -9.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -8.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8))
    (pad 3 smd rect (at -7.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -6.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 8 /CA_D1))
    (pad 5 smd rect (at -5.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 9 /CA_D3))
    (pad 6 smd rect (at -4.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 7 smd rect (at -3.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P1-Pad7)"))
    (pad 8 smd rect (at -2.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 9 smd rect (at -1.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /CA_D0))
    (pad 10 smd rect (at -0.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 12 /CA_D2))
    (pad 11 smd rect (at 0.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 12 smd rect (at 1.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P1-Pad12)"))
    (pad 13 smd rect (at 2.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 14 /CAB_SDA))
    (pad 14 smd rect (at 3.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 15 /CA_HREF))
    (pad 15 smd rect (at 4.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 16 /CAB_XCLK))
    (pad 16 smd rect (at 5.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 17 /CA_PWDN))
    (pad 17 smd rect (at 6.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 18 /CAB_SCL))
    (pad 18 smd rect (at 7.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 19 /CA_VSYNC))
    (pad 19 smd rect (at 8.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad19)"))
    (pad 20 smd rect (at 9.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 21 /CA_RST))
    (pad 0 smd rect (at -12.5 2.9 90) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 12.5 2.9 90) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 158.9 88.1 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.48 1.34 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +2V8))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 164 107.5 90)
    (fp_text reference W1 (at -0.74 -2.69 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3 90) (layer F.Fab))
    (pad 1 smd oval (at 0 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P1-Pad12)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 163.3 82.8 90)
    (fp_text reference W2 (at 1.47 -2.4 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3 90) (layer F.Fab))
    (pad 1 smd oval (at 0 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P1-Pad19)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 162.2 104.6 90)
    (fp_text reference W3 (at 1.86 0.83 180) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3 90) (layer F.Fab))
    (pad 1 smd oval (at 0 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P1-Pad7)"))
  )
  (module gj_feet:HOLE-2.5 locked (layer F.Cu) (tedit 5894FF19)
    (at 158.5 107)
    (descr "Hole 2.5 mm")
    (tags hole)
    (fp_text reference H** (at 0.3 -2.5) (layer F.SilkS) hide)
    (fp_text value 2.5mm (at 0 2.3) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 2.6) (layers *.Cu *.Mask))
  )
  (gr_text "OVM6211 v1.1" (at 170.41 89.36 90) (layer B.SilkS))
  (gr_line (start 155.79 80.43) (end 172.11 80.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.79 109.37) (end 155.79 80.43) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.89 109.37) (end 155.79 109.37) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.11 109.37) (end 155.89 109.37) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.11 80.419999) (end 172.11 109.37) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.16)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 172.1 109.4) (xy 155.8 109.4) (xy 155.8 80.4) (xy 172.1 80.4)
      )
    )
  )
)
