<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="-25.4" y1="-40.386" x2="25.4" y2="-40.386" width="0" layer="20"/>
<wire x1="25.4" y1="-40.386" x2="27.94" y2="-37.846" width="0" layer="20" curve="90"/>
<wire x1="27.94" y1="-37.846" x2="27.94" y2="37.846" width="0" layer="20"/>
<wire x1="25.4" y1="40.386" x2="-25.4" y2="40.386" width="0" layer="20"/>
<wire x1="-27.94" y1="37.846" x2="-27.94" y2="-37.846" width="0" layer="20"/>
<wire x1="-27.94" y1="-37.846" x2="-25.4" y2="-40.386" width="0" layer="20" curve="90"/>
<text>
by Joey Castillo / @josecastillo.
Includes elements of @Adafruit's
Sharp Memory Display Breakout.
Looks best in @OSHPark After Dark.
Crafted with   in Brooklyn, NY.
Lazer bear by @DoctorDevens.
plz don't steal the bear =)</text>
<wire x1="-25.4" y1="40.386" x2="-27.94" y2="37.846" width="0" layer="20" curve="90"/>
<wire x1="27.94" y1="37.846" x2="25.4" y2="40.386" width="0" layer="20" curve="90"/>
<text>RST</text>
<text>SWCLK</text>
<text>3V3</text>
<text>GND</text>
<text>SWDIO</text>
<text>OSO-PYCO-A1-02</text>
<wire x1="-22.86" y1="9.144" x2="-24.13" y2="10.414" width="0" layer="20" curve="90"/>
<wire x1="-24.13" y1="10.414" x2="-25.4" y2="9.144" width="0" layer="20" curve="90"/>
<wire x1="-25.4" y1="9.144" x2="-25.4" y2="-2.286" width="0" layer="20"/>
<wire x1="-25.4" y1="-2.286" x2="-24.13" y2="-3.556" width="0" layer="20" curve="90"/>
<wire x1="-24.13" y1="-3.556" x2="-22.86" y2="-2.286" width="0" layer="20" curve="90"/>
<wire x1="-22.86" y1="-2.286" x2="-22.86" y2="9.144" width="0" layer="20"/>
<text>THE PYCORDER</text>
<text>The PyCorder</text>
<text>+  -</text>
<text>CC-BY-SA 4.0</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="MOUNTINGHOLE_2.5_PLATED">
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="_0603MP">
<description>&lt;b&gt;0603 MicroPitch&lt;/b&gt;</description>
</package>
<package name="0805-NO">
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
<package name="JST_SH9">
</package>
<package name="SOD-123">
<description>&lt;b&gt;SOD-123&lt;/b&gt;
&lt;p&gt;Source: http://www.diodes.com/datasheets/ds30139.pdf&lt;/p&gt;</description>
</package>
<package name="SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
<package name="JSTPH2">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="JSTPH3">
</package>
<package name="TESTPOINT_ROUND_2MM_NO">
</package>
<package name="SOIC8_150MIL">
<description>&lt;b&gt;Small Outline IC - 150mil Wide&lt;/b&gt;</description>
</package>
<package name="6MMX6MM_TACTILE_SMT">
</package>
</packages>
</library>
<library name="adafruit_display">
<packages>
<package name="SHARP_2.7IN">
<description>&lt;b&gt;Source: &lt;/b&gt;http://www.molex.com/pdm_docs/sd/528921095_sd.pdf</description>
</package>
</packages>
</library>
<library name="My Stuff">
<description>Generated from &lt;b&gt;Hiking Log FeatherWing.brd&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="OSO_WORDMARK_THREELINE_450MIL_1000DPI">
</package>
<package name="SOT23-6">
<description>&lt;h3&gt;SOT23-6&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;MCP4725&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OSO_BEAR_525X750MIL_1000DPI">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="JS102011SAQN">
<packages>
<package name="SW_JS102011SAQN">
</package>
</packages>
</library>
<library name="SM04B-SRSS-TB_LF__SN_">
<packages>
<package name="JST_SM04B-SRSS-TB(LF)(SN)">
</package>
</packages>
</library>
<library name="ATSAMD51G18AMUT">
<packages>
<package name="QFN48_7X7MC">
</package>
</packages>
</library>
<library name="REG710NA-5_3K">
<packages>
<package name="SOT95P280X145-6N">
</package>
</packages>
</library>
<library name="USB4105-GF-A">
<packages>
<package name="GCT_USB4105-GF-A">
</package>
</packages>
</library>
<library name="oddlyspecific">
<packages>
<package name="TL3330A">
</package>
</packages>
</library>
<library name="K1-5202UA">
<packages>
<package name="K1-5202UA">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="REV" value="A"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FFC" library="adafruit_display" package="SHARP_2.7IN" value="LS027B7DH01">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FID1" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL_1MM">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="FID2" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL_1MM">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="C18" library="microbuilder" package="_0603MP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="microbuilder" package="_0603MP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="microbuilder" package="_0603MP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="microbuilder" package="_0805" value="FERRITE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB2" library="microbuilder" package="_0805" value="FERRITE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="CHECKED" value="KTOWN"/>
<attribute name="COMPANY" value="ADAFRUIT INDUSTRIES"/>
<attribute name="DRAWN" value="KTOWN"/>
<attribute name="NAME"/>
<attribute name="REV" value="A"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="CHECKED" value="KTOWN"/>
<attribute name="COMPANY" value="ADAFRUIT INDUSTRIES"/>
<attribute name="DRAWN" value="KTOWN"/>
<attribute name="NAME"/>
<attribute name="REV" value="A"/>
<attribute name="VALUE"/>
</element>
<element name="U$27" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="CHECKED" value="KTOWN"/>
<attribute name="COMPANY" value="ADAFRUIT INDUSTRIES"/>
<attribute name="DRAWN" value="KTOWN"/>
<attribute name="REV" value="A"/>
</element>
<element name="U$28" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="CHECKED" value="KTOWN"/>
<attribute name="COMPANY" value="ADAFRUIT INDUSTRIES"/>
<attribute name="DRAWN" value="KTOWN"/>
<attribute name="REV" value="A"/>
</element>
<element name="FID3" library="microbuilder" package="FIDUCIAL_1MM" value="FIDUCIAL_1MM">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="CHECKED" value="KTOWN"/>
<attribute name="COMPANY" value="ADAFRUIT INDUSTRIES"/>
<attribute name="DRAWN" value="KTOWN"/>
<attribute name="REV" value="A"/>
</element>
<element name="R14" library="microbuilder" package="_0603MP" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$9" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="REV" value="A"/>
</element>
<element name="U$10" library="microbuilder" package="MOUNTINGHOLE_2.5_PLATED" value="MOUNTINGHOLE2.5">
<attribute name="BOM" value="EXCLUDE"/>
<attribute name="REV" value="A"/>
</element>
<element name="9-PIN-CONNECTOR" library="microbuilder" package="JST_SH9" value="">
<attribute name="NAME"/>
</element>
<element name="D1" library="microbuilder" package="SOD-123" value="MBR120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="microbuilder" package="SOT23-R" value="DMG341">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="microbuilder" package="_0603MP" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="JS102011SAQN" package="SW_JS102011SAQN" value="JS102011SAQN">
<attribute name="DESCRIPTION" value=" Slide Switch SPDT Surface Mount, Right Angle "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="401-1999-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/c-k/JS102011SAQN/401-1999-1-ND/1640114?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="C&amp;K"/>
<attribute name="MP" value="JS102011SAQN"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="STEMMA-QT" library="SM04B-SRSS-TB_LF__SN_" package="JST_SM04B-SRSS-TB(LF)(SN)" value="SM04B-SRSS-TB(LF)(SN)">
<attribute name="DESCRIPTION" value=" SH Series 1.0 mm Pitch 2 Position Single Row Side Entry Shrouded Header "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="455-1804-1-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/jst-sales-america-inc/SM04B-SRSS-TB_LF__SN_/455-1804-1-ND/926875?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="JST Sales"/>
<attribute name="MP" value="SM04B-SRSS-TB_LF__SN_"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="microbuilder" package="_0603MP" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="microbuilder" package="_0603MP" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BATTERY" library="microbuilder" package="JSTPH2" value="JSTPH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="microbuilder" package="SOT23-5" value="MCP73831T-2ACI/OT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="microbuilder" package="_0603MP" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="microbuilder" package="_0603MP" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CHG" library="adafruit" package="CHIP-LED0805" value="AMBER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="STEMMA" library="microbuilder" package="JSTPH3" value="JST PH 3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="microbuilder" package="_0603MP" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="microbuilder" package="SOD-123" value="3.6V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="TP8" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="TP1" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="TP2" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="U4" library="microbuilder" package="SOIC8_150MIL" value="2MB Flash">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="microbuilder" package="_0603MP" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$16" library="My Stuff" package="OSO_WORDMARK_THREELINE_450MIL_1000DPI" value=""/>
<element name="C9" library="microbuilder" package="_0603MP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="microbuilder" package="_0603MP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="microbuilder" package="_0603MP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="ATSAMD51G18AMUT" package="QFN48_7X7MC" value="ATSAMD51G18A-MUT">
<attribute name="BUILT_BY" value="EMA_Molly"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATSAMD51G18A-MUT"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Microchip"/>
</element>
<element name="C11" library="microbuilder" package="_0603MP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="microbuilder" package="_0603MP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="REG710NA-5_3K" package="SOT95P280X145-6N" value="REG710NA-5/3K">
<attribute name="DESCRIPTION" value=" 30-mA Switched-Cap DC-DC Converter with fixed 5-V Output 6-SOT-23 -40 to 85 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="296-26327-1-ND"/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="REG710NA-5/3K"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-6 Texas Instruments"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/REG710NA-5/3K/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="microbuilder" package="_0603MP" value=".22uF">
<attribute name="NAME"/>
<attribute name="REV" value="A"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="microbuilder" package="_0603MP" value="2.2uF">
<attribute name="NAME"/>
<attribute name="REV" value="A"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="microbuilder" package="_0603MP" value="2.2uF">
<attribute name="NAME"/>
<attribute name="REV" value="A"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="microbuilder" package="_0603MP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="microbuilder" package="_0603MP" value="5.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="microbuilder" package="_0603MP" value="5.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="My Stuff" package="SOT23-6" value="AP7332-3333W6-7SOT23">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="microbuilder" package="0805-NO" value="10uF">
<attribute name="NAME"/>
<attribute name="REV" value="A"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="microbuilder" package="_0603MP" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="microbuilder" package="_0603MP" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="microbuilder" package="_0603MP" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="adafruit" package="CHIP-LED0805" value="RED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="microbuilder" package="_0603MP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB-C" library="USB4105-GF-A" package="GCT_USB4105-GF-A" value="USB4105-GF-A">
<attribute name="DESCRIPTION" value=" USB-C (USB TYPE-C) USB 2.0 Receptacle Connector 24 (16+8 Dummy) Position Surface Mount, Right Angle; Through Hole "/>
<attribute name="DIGI-KEY_PART_NUMBER" value=""/>
<attribute name="MF" value="GCT"/>
<attribute name="MP" value="USB4105-GF-A"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/USB4105-GF-A/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="microbuilder" package="_0603MP" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="oddlyspecific" package="TL3330A" value="">
<attribute name="NAME"/>
</element>
<element name="TP3" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="U$67" library="My Stuff" package="OSO_BEAR_525X750MIL_1000DPI" value=""/>
<element name="TP4" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="TP5" library="microbuilder" package="TESTPOINT_ROUND_2MM_NO" value=""/>
<element name="B3" library="K1-5202UA" package="K1-5202UA" value="K1-5202UA"/>
<element name="B2" library="microbuilder" package="6MMX6MM_TACTILE_SMT" value="EVQQ"/>
<element name="B1" library="microbuilder" package="6MMX6MM_TACTILE_SMT" value="EVQQ"/>
</elements>
<signals>
<signal name="AVDD">
<contactref element="FFC" pad="P$6"/>
<contactref element="C17" pad="1"/>
<contactref element="FB1" pad="2"/>
</signal>
<signal name="AGND">
<contactref element="FFC" pad="P$10"/>
<contactref element="C17" pad="2"/>
<contactref element="FB2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="FFC" pad="P$9"/>
<contactref element="C18" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="FB2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="9-PIN-CONNECTOR" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="SW1" pad="3"/>
<contactref element="STEMMA-QT" pad="1"/>
<contactref element="BATTERY" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="STEMMA" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="TP1" pad="P$1"/>
<contactref element="U4" pad="4"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="18"/>
<contactref element="U3" pad="35"/>
<contactref element="U3" pad="42"/>
<contactref element="C14" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="LED" pad="C"/>
<contactref element="U3" pad="49"/>
<contactref element="C12" pad="1"/>
<contactref element="USB-C" pad="A1/B12"/>
<contactref element="USB-C" pad="G4"/>
<contactref element="USB-C" pad="G1"/>
<contactref element="USB-C" pad="B1/A12"/>
<contactref element="USB-C" pad="G3"/>
<contactref element="USB-C" pad="G2"/>
<contactref element="RESET" pad="P$2"/>
<contactref element="B3" pad="P$5"/>
<contactref element="B1" pad="A"/>
<contactref element="B1" pad="A'"/>
<contactref element="B2" pad="A"/>
<contactref element="B2" pad="A'"/>
<contactref element="R14" pad="2"/>
<contactref element="B3" pad="P$8"/>
<contactref element="B3" pad="P$7"/>
</signal>
<signal name="DISPLAY_CS">
<contactref element="FFC" pad="P$3"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="DISPLAY_MOSI">
<contactref element="FFC" pad="P$2"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="DISPLAY_SCK">
<contactref element="FFC" pad="P$1"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="5.0V">
<contactref element="FB1" pad="1"/>
<contactref element="FFC" pad="P$7"/>
<contactref element="C16" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="A0">
<contactref element="9-PIN-CONNECTOR" pad="9"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="9-PIN-CONNECTOR" pad="8"/>
<contactref element="STEMMA-QT" pad="4"/>
<contactref element="R11" pad="1"/>
<contactref element="U3" pad="22"/>
</signal>
<signal name="SDA">
<contactref element="9-PIN-CONNECTOR" pad="7"/>
<contactref element="STEMMA-QT" pad="3"/>
<contactref element="R12" pad="1"/>
<contactref element="U3" pad="21"/>
</signal>
<signal name="+3V3">
<contactref element="9-PIN-CONNECTOR" pad="1"/>
<contactref element="STEMMA-QT" pad="2"/>
<contactref element="STEMMA" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="TP5" pad="P$1"/>
<contactref element="U1" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="A1/SCK">
<contactref element="9-PIN-CONNECTOR" pad="6"/>
<contactref element="U3" pad="48"/>
</signal>
<signal name="A2/MOSI">
<contactref element="9-PIN-CONNECTOR" pad="5"/>
<contactref element="U3" pad="47"/>
</signal>
<signal name="USB_N">
<contactref element="U3" pad="33"/>
<contactref element="USB-C" pad="A7"/>
<contactref element="USB-C" pad="B7"/>
</signal>
<signal name="USB_P">
<contactref element="U3" pad="34"/>
<contactref element="USB-C" pad="A6"/>
<contactref element="USB-C" pad="B6"/>
</signal>
<signal name="SWDIO">
<contactref element="TP6" pad="P$1"/>
<contactref element="U3" pad="46"/>
</signal>
<signal name="EN2">
<contactref element="U1" pad="3"/>
<contactref element="R5" pad="1"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="V+">
<contactref element="D1" pad="C"/>
<contactref element="Q1" pad="2"/>
<contactref element="U5" pad="5"/>
<contactref element="C13" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="R4" pad="1"/>
<contactref element="TP4" pad="P$1"/>
</signal>
<signal name="VBUS">
<contactref element="D1" pad="A"/>
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="CHG" pad="A"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="USB-C" pad="B4/A9"/>
<contactref element="USB-C" pad="A4/B9"/>
</signal>
<signal name="VBAT">
<contactref element="Q1" pad="3"/>
<contactref element="U2" pad="3"/>
<contactref element="BATTERY" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="EN">
<contactref element="SW1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R8" pad="1"/>
<contactref element="CHG" pad="C"/>
</signal>
<signal name="STAT">
<contactref element="R8" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="PROG">
<contactref element="U2" pad="5"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="STEMMA_">
<contactref element="STEMMA" pad="3"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="!RESET">
<contactref element="TP8" pad="P$1"/>
<contactref element="U3" pad="40"/>
<contactref element="R7" pad="2"/>
<contactref element="RESET" pad="P$1"/>
</signal>
<signal name="STEMMA">
<contactref element="R13" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="VSW">
<contactref element="U3" pad="43"/>
</signal>
<signal name="VDDCORE1">
<contactref element="C9" pad="2"/>
<contactref element="U3" pad="41"/>
</signal>
<signal name="QSPI_SCK">
<contactref element="U3" pad="19"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="QSPI_CS">
<contactref element="U3" pad="20"/>
<contactref element="U4" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="QSPI_DATA[0]">
<contactref element="U3" pad="13"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="QSPI_DATA[1]">
<contactref element="U3" pad="14"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="QSPI_DATA[2]">
<contactref element="U3" pad="15"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="QSPI_DATA[3]">
<contactref element="U3" pad="16"/>
<contactref element="U4" pad="7"/>
</signal>
<signal name="D0/CS">
<contactref element="U3" pad="38"/>
<contactref element="9-PIN-CONNECTOR" pad="4"/>
</signal>
<signal name="D1/MISO">
<contactref element="U3" pad="37"/>
<contactref element="9-PIN-CONNECTOR" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="U5" pad="6"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U5" pad="4"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="CC1">
<contactref element="R3" pad="1"/>
<contactref element="USB-C" pad="A5"/>
</signal>
<signal name="CC2">
<contactref element="R2" pad="1"/>
<contactref element="USB-C" pad="B5"/>
</signal>
<signal name="3.3V">
<contactref element="C7" pad="2"/>
<contactref element="U3" pad="6"/>
<contactref element="C8" pad="2"/>
<contactref element="U3" pad="17"/>
<contactref element="U3" pad="36"/>
<contactref element="U3" pad="44"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="U4" pad="8"/>
<contactref element="C12" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="TP2" pad="P$1"/>
<contactref element="FFC" pad="P$8"/>
<contactref element="U1" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="SWCLK">
<contactref element="TP3" pad="P$1"/>
<contactref element="U3" pad="45"/>
</signal>
<signal name="N$1">
<contactref element="LED" pad="A"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="LED">
<contactref element="U3" pad="11"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="NW">
<contactref element="B3" pad="P$1"/>
<contactref element="U3" pad="26"/>
</signal>
<signal name="SW">
<contactref element="B3" pad="P$3"/>
<contactref element="U3" pad="28"/>
</signal>
<signal name="CENTER">
<contactref element="B3" pad="P$2"/>
<contactref element="U3" pad="27"/>
</signal>
<signal name="NE">
<contactref element="B3" pad="P$4"/>
<contactref element="U3" pad="25"/>
</signal>
<signal name="SE">
<contactref element="B3" pad="P$6"/>
<contactref element="U3" pad="29"/>
</signal>
<signal name="PREV">
<contactref element="B1" pad="B'"/>
<contactref element="U3" pad="30"/>
</signal>
<signal name="NEXT">
<contactref element="B2" pad="B"/>
<contactref element="U3" pad="24"/>
</signal>
<signal name="EXTCOMIN">
<contactref element="FFC" pad="P$4"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="DISP">
<contactref element="FFC" pad="P$5"/>
<contactref element="C18" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="U3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
