(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 72)
    (tracks 2014)
    (zones 0)
    (modules 114)
    (nets 135)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.178)
    (user_trace_width 0.254)
    (user_trace_width 0.3)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (trace_clearance 0.15)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.15)
    (segment_width 0.17)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.3)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 0.2 0.2)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 122 125)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f8_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 +2.5)
  (net 4 +1.2)
  (net 5 "Net-(C24-Pad1)")
  (net 6 "Net-(C32-Pad1)")
  (net 7 "Net-(C33-Pad2)")
  (net 8 "Net-(C34-Pad1)")
  (net 9 "Net-(CON2-Pad9)")
  (net 10 "Net-(CON2-Pad8)")
  (net 11 "Net-(CON2-Pad6)")
  (net 12 "Net-(CON2-Pad5)")
  (net 13 "Net-(CON2-Pad3)")
  (net 14 "Net-(CON2-Pad2)")
  (net 15 "Net-(CON2-Pad11)")
  (net 16 "Net-(CON2-Pad12)")
  (net 17 /SCL)
  (net 18 /SDA)
  (net 19 "Net-(CON2-Pad17)")
  (net 20 "Net-(CON2-Pad19)")
  (net 21 "Net-(D1-Pad1)")
  (net 22 /nConf)
  (net 23 +1.8)
  (net 24 "Net-(R2-Pad2)")
  (net 25 /INT)
  (net 26 "Net-(R11-Pad1)")
  (net 27 /CS)
  (net 28 "Net-(R14-Pad1)")
  (net 29 "Net-(U3-Pad4)")
  (net 30 "Net-(U4-Pad2)")
  (net 31 "Net-(U4-Pad3)")
  (net 32 "Net-(U4-Pad4)")
  (net 33 /ADAT)
  (net 34 "Net-(U4-Pad6)")
  (net 35 "Net-(U4-Pad7)")
  (net 36 "Net-(U4-Pad8)")
  (net 37 /ABCK)
  (net 38 /ALRK)
  (net 39 "Net-(U4-Pad37)")
  (net 40 "Net-(U4-Pad38)")
  (net 41 "Net-(U4-Pad39)")
  (net 42 "Net-(U4-Pad40)")
  (net 43 "Net-(U4-Pad41)")
  (net 44 "Net-(U4-Pad42)")
  (net 45 "Net-(U4-Pad43)")
  (net 46 "Net-(U4-Pad44)")
  (net 47 "Net-(U4-Pad45)")
  (net 48 "Net-(U4-Pad46)")
  (net 49 "Net-(U4-Pad47)")
  (net 50 "Net-(U4-Pad48)")
  (net 51 "Net-(U4-Pad49)")
  (net 52 "Net-(U4-Pad50)")
  (net 53 "Net-(U4-Pad52)")
  (net 54 /ADVCLK)
  (net 55 "Net-(U4-Pad54)")
  (net 56 "Net-(U4-Pad55)")
  (net 57 "Net-(U4-Pad56)")
  (net 58 "Net-(U4-Pad57)")
  (net 59 "Net-(U4-Pad58)")
  (net 60 "Net-(U4-Pad59)")
  (net 61 "Net-(U4-Pad60)")
  (net 62 "Net-(U4-Pad61)")
  (net 63 "Net-(U4-Pad62)")
  (net 64 "Net-(U4-Pad63)")
  (net 65 "Net-(U4-Pad64)")
  (net 66 /X1)
  (net 67 "Net-(U5-Pad16)")
  (net 68 /S0)
  (net 69 /S3)
  (net 70 /S2)
  (net 71 /CLK)
  (net 72 /S1)
  (net 73 "Net-(U5-Pad15)")
  (net 74 /MOSI)
  (net 75 /DCLK)
  (net 76 /MISO)
  (net 77 /VCLK)
  (net 78 "Net-(U6-Pad24)")
  (net 79 "Net-(U6-Pad52)")
  (net 80 "Net-(U6-Pad53)")
  (net 81 "Net-(U6-Pad54)")
  (net 82 "Net-(U6-Pad55)")
  (net 83 "Net-(U6-Pad89)")
  (net 84 "Net-(U6-Pad90)")
  (net 85 "Net-(U6-Pad91)")
  (net 86 "Net-(CON1-Pad3)")
  (net 87 "Net-(CON1-Pad4)")
  (net 88 "Net-(CON1-Pad6)")
  (net 89 "Net-(CON1-Pad7)")
  (net 90 "Net-(CON1-Pad9)")
  (net 91 "Net-(CON1-Pad10)")
  (net 92 "Net-(CON1-Pad12)")
  (net 93 "Net-(CON1-Pad13)")
  (net 94 "Net-(U6-Pad126)")
  (net 95 "Net-(U6-Pad127)")
  (net 96 "Net-(U6-Pad128)")
  (net 97 "Net-(U6-Pad129)")
  (net 98 "Net-(CON1-Pad15)")
  (net 99 "Net-(CON1-Pad16)")
  (net 100 "Net-(CON1-Pad18)")
  (net 101 "Net-(CON1-Pad19)")
  (net 102 "Net-(CON1-Pad21)")
  (net 103 "Net-(CON1-Pad22)")
  (net 104 "Net-(CON1-Pad28)")
  (net 105 "Net-(U8-Pad2)")
  (net 106 "Net-(U6-Pad25)")
  (net 107 /SCL_H)
  (net 108 /SDA_H)
  (net 109 "Net-(R16-Pad2)")
  (net 110 /+5)
  (net 111 /PAD1)
  (net 112 /PAD2)
  (net 113 /ESP_SCL)
  (net 114 /ESP_SDA)
  (net 115 "Net-(R7-Pad2)")
  (net 116 /nCE)
  (net 117 "Net-(CON3-Pad2)")
  (net 118 /RXD)
  (net 119 /TXD)
  (net 120 "Net-(CON3-Pad6)")
  (net 121 /SRST)
  (net 122 /HRST_OUT)
  (net 123 /HRST)
  (net 124 "Net-(U6-Pad15)")
  (net 125 "Net-(U6-Pad16)")
  (net 126 "Net-(U6-Pad18)")
  (net 127 "Net-(U6-Pad20)")
  (net 128 "Net-(U6-Pad22)")
  (net 129 "Net-(U8-Pad1)")
  (net 130 "Net-(R1-Pad2)")
  (net 131 "Net-(R18-Pad2)")
  (net 132 "Net-(C50-Pad1)")
  (net 133 /HDMI+5)
  (net 134 "Net-(CON2-Pad14)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.178)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1.2)
    (add_net +1.8)
    (add_net +2.5)
    (add_net +3V3)
    (add_net /+5)
    (add_net /ABCK)
    (add_net /ADAT)
    (add_net /ADVCLK)
    (add_net /ALRK)
    (add_net /CLK)
    (add_net /CS)
    (add_net /DCLK)
    (add_net /ESP_SCL)
    (add_net /ESP_SDA)
    (add_net /HDMI+5)
    (add_net /HRST)
    (add_net /HRST_OUT)
    (add_net /INT)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PAD1)
    (add_net /PAD2)
    (add_net /RXD)
    (add_net /S0)
    (add_net /S1)
    (add_net /S2)
    (add_net /S3)
    (add_net /SCL)
    (add_net /SCL_H)
    (add_net /SDA)
    (add_net /SDA_H)
    (add_net /SRST)
    (add_net /TXD)
    (add_net /VCLK)
    (add_net /X1)
    (add_net /nCE)
    (add_net /nConf)
    (add_net GND)
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(C33-Pad2)")
    (add_net "Net-(C34-Pad1)")
    (add_net "Net-(C50-Pad1)")
    (add_net "Net-(CON1-Pad10)")
    (add_net "Net-(CON1-Pad12)")
    (add_net "Net-(CON1-Pad13)")
    (add_net "Net-(CON1-Pad15)")
    (add_net "Net-(CON1-Pad16)")
    (add_net "Net-(CON1-Pad18)")
    (add_net "Net-(CON1-Pad19)")
    (add_net "Net-(CON1-Pad21)")
    (add_net "Net-(CON1-Pad22)")
    (add_net "Net-(CON1-Pad28)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(CON1-Pad4)")
    (add_net "Net-(CON1-Pad6)")
    (add_net "Net-(CON1-Pad7)")
    (add_net "Net-(CON1-Pad9)")
    (add_net "Net-(CON2-Pad11)")
    (add_net "Net-(CON2-Pad12)")
    (add_net "Net-(CON2-Pad14)")
    (add_net "Net-(CON2-Pad17)")
    (add_net "Net-(CON2-Pad19)")
    (add_net "Net-(CON2-Pad2)")
    (add_net "Net-(CON2-Pad3)")
    (add_net "Net-(CON2-Pad5)")
    (add_net "Net-(CON2-Pad6)")
    (add_net "Net-(CON2-Pad8)")
    (add_net "Net-(CON2-Pad9)")
    (add_net "Net-(CON3-Pad2)")
    (add_net "Net-(CON3-Pad6)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad37)")
    (add_net "Net-(U4-Pad38)")
    (add_net "Net-(U4-Pad39)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad40)")
    (add_net "Net-(U4-Pad41)")
    (add_net "Net-(U4-Pad42)")
    (add_net "Net-(U4-Pad43)")
    (add_net "Net-(U4-Pad44)")
    (add_net "Net-(U4-Pad45)")
    (add_net "Net-(U4-Pad46)")
    (add_net "Net-(U4-Pad47)")
    (add_net "Net-(U4-Pad48)")
    (add_net "Net-(U4-Pad49)")
    (add_net "Net-(U4-Pad50)")
    (add_net "Net-(U4-Pad52)")
    (add_net "Net-(U4-Pad54)")
    (add_net "Net-(U4-Pad55)")
    (add_net "Net-(U4-Pad56)")
    (add_net "Net-(U4-Pad57)")
    (add_net "Net-(U4-Pad58)")
    (add_net "Net-(U4-Pad59)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad60)")
    (add_net "Net-(U4-Pad61)")
    (add_net "Net-(U4-Pad62)")
    (add_net "Net-(U4-Pad63)")
    (add_net "Net-(U4-Pad64)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad16)")
    (add_net "Net-(U6-Pad126)")
    (add_net "Net-(U6-Pad127)")
    (add_net "Net-(U6-Pad128)")
    (add_net "Net-(U6-Pad129)")
    (add_net "Net-(U6-Pad15)")
    (add_net "Net-(U6-Pad16)")
    (add_net "Net-(U6-Pad18)")
    (add_net "Net-(U6-Pad20)")
    (add_net "Net-(U6-Pad22)")
    (add_net "Net-(U6-Pad24)")
    (add_net "Net-(U6-Pad25)")
    (add_net "Net-(U6-Pad52)")
    (add_net "Net-(U6-Pad53)")
    (add_net "Net-(U6-Pad54)")
    (add_net "Net-(U6-Pad55)")
    (add_net "Net-(U6-Pad89)")
    (add_net "Net-(U6-Pad90)")
    (add_net "Net-(U6-Pad91)")
    (add_net "Net-(U8-Pad1)")
    (add_net "Net-(U8-Pad2)")
  )
  (module Altera:altera144_wcenterpad (layer F.Cu) (tedit 5C17C258)
    (at 147.6 103.4 90)
    (attr smd)
    (fp_text reference U6 (at -10.4 -10.2 180) (layer F.SilkS))
    (fp_text value 10CL025 (at 6.32 0.11 180) (layer F.Fab))
    (pad 1 smd rect (at -10.7 -8.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at -10.7 -8.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -10.7 -7.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5))
    (pad 4 smd rect (at -10.7 -7.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -10.7 -6.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 6 smd rect (at -10.7 -6.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 74 /MOSI))
    (pad 7 smd rect (at -10.7 -5.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 68 /S0))
    (pad 8 smd rect (at -10.7 -5.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /CS))
    (pad 9 smd rect (at -10.7 -4.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R7-Pad2)"))
    (pad 10 smd rect (at -10.7 -4.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 /S1))
    (pad 11 smd rect (at -10.7 -3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /ESP_SCL))
    (pad 12 smd rect (at -10.7 -3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 /DCLK))
    (pad 13 smd rect (at -10.7 -2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 /MISO))
    (pad 14 smd rect (at -10.7 -2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /nConf))
    (pad 15 smd rect (at -10.7 -1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(U6-Pad15)"))
    (pad 16 smd rect (at -10.7 -1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U6-Pad16)"))
    (pad 17 smd rect (at -10.7 -0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 18 smd rect (at -10.7 -0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(U6-Pad18)"))
    (pad 19 smd rect (at -10.7 0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at -10.7 0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(U6-Pad20)"))
    (pad 21 smd rect (at -10.7 1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /nCE))
    (pad 22 smd rect (at -10.7 1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(U6-Pad22)"))
    (pad 23 smd rect (at -10.7 2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 /VCLK))
    (pad 24 smd rect (at -10.7 2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U6-Pad24)"))
    (pad 25 smd rect (at -10.7 3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U6-Pad25)"))
    (pad 26 smd rect (at -10.7 3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 27 smd rect (at -10.7 4.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at -10.7 4.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 114 /ESP_SDA))
    (pad 29 smd rect (at -10.7 5.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 30 smd rect (at -10.7 5.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 31 smd rect (at -10.7 6.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /PAD1))
    (pad 32 smd rect (at -10.7 6.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 112 /PAD2))
    (pad 33 smd rect (at -10.7 7.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 123 /HRST))
    (pad 34 smd rect (at -10.7 7.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 35 smd rect (at -10.7 8.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5))
    (pad 36 smd rect (at -10.7 8.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at -8.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 38 smd rect (at -8.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 39 smd rect (at -7.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U4-Pad2)"))
    (pad 40 smd rect (at -7.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 41 smd rect (at -6.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 42 smd rect (at -6.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U4-Pad64)"))
    (pad 43 smd rect (at -5.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 66 /X1))
    (pad 44 smd rect (at -5.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U4-Pad63)"))
    (pad 45 smd rect (at -4.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 46 smd rect (at -4.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U4-Pad62)"))
    (pad 47 smd rect (at -3.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 48 smd rect (at -3.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 49 smd rect (at -2.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U4-Pad61)"))
    (pad 50 smd rect (at -2.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U4-Pad60)"))
    (pad 51 smd rect (at -1.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U4-Pad59)"))
    (pad 52 smd rect (at -1.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U6-Pad52)"))
    (pad 53 smd rect (at -0.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U6-Pad53)"))
    (pad 54 smd rect (at -0.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U6-Pad54)"))
    (pad 55 smd rect (at 0.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U6-Pad55)"))
    (pad 56 smd rect (at 0.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 57 smd rect (at 1.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 58 smd rect (at 1.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U4-Pad58)"))
    (pad 59 smd rect (at 2.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U4-Pad57)"))
    (pad 60 smd rect (at 2.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U4-Pad56)"))
    (pad 61 smd rect (at 3.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 62 smd rect (at 3.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 63 smd rect (at 4.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 64 smd rect (at 4.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 65 smd rect (at 5.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U4-Pad55)"))
    (pad 66 smd rect (at 5.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U4-Pad54)"))
    (pad 67 smd rect (at 6.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U4-Pad52)"))
    (pad 68 smd rect (at 6.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U4-Pad50)"))
    (pad 69 smd rect (at 7.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U4-Pad49)"))
    (pad 70 smd rect (at 7.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 71 smd rect (at 8.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 54 /ADVCLK))
    (pad 72 smd rect (at 8.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U4-Pad48)"))
    (pad 73 smd rect (at 10.7 8.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 74 smd rect (at 10.7 8.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 75 smd rect (at 10.7 7.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5))
    (pad 76 smd rect (at 10.7 7.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U4-Pad47)"))
    (pad 77 smd rect (at 10.7 6.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U4-Pad46)"))
    (pad 78 smd rect (at 10.7 6.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 79 smd rect (at 10.7 5.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 80 smd rect (at 10.7 5.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U4-Pad45)"))
    (pad 81 smd rect (at 10.7 4.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 82 smd rect (at 10.7 4.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 83 smd rect (at 10.7 3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U4-Pad44)"))
    (pad 84 smd rect (at 10.7 3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 85 smd rect (at 10.7 2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U4-Pad43)"))
    (pad 86 smd rect (at 10.7 2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U4-Pad42)"))
    (pad 87 smd rect (at 10.7 1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U4-Pad41)"))
    (pad 88 smd rect (at 10.7 1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 /CLK))
    (pad 89 smd rect (at 10.7 0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U6-Pad89)"))
    (pad 90 smd rect (at 10.7 0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U6-Pad90)"))
    (pad 91 smd rect (at 10.7 -0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U6-Pad91)"))
    (pad 92 smd rect (at 10.7 -0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R2-Pad2)"))
    (pad 93 smd rect (at 10.7 -1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 94 smd rect (at 10.7 -1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 95 smd rect (at 10.7 -2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 96 smd rect (at 10.7 -2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 97 smd rect (at 10.7 -3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 98 smd rect (at 10.7 -3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U4-Pad40)"))
    (pad 99 smd rect (at 10.7 -4.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U4-Pad39)"))
    (pad 100 smd rect (at 10.7 -4.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U4-Pad38)"))
    (pad 101 smd rect (at 10.7 -5.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U4-Pad37)"))
    (pad 102 smd rect (at 10.7 -5.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 103 smd rect (at 10.7 -6.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /SDA))
    (pad 104 smd rect (at 10.7 -6.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 105 smd rect (at 10.7 -7.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /SCL))
    (pad 106 smd rect (at 10.7 -7.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /INT))
    (pad 107 smd rect (at 10.7 -8.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5))
    (pad 108 smd rect (at 10.7 -8.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 109 smd rect (at 8.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 110 smd rect (at 8.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 111 smd rect (at 7.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(CON1-Pad3)"))
    (pad 112 smd rect (at 7.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(CON1-Pad4)"))
    (pad 113 smd rect (at 6.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(CON1-Pad6)"))
    (pad 114 smd rect (at 6.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(CON1-Pad7)"))
    (pad 115 smd rect (at 5.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(CON1-Pad9)"))
    (pad 116 smd rect (at 5.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 117 smd rect (at 4.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 118 smd rect (at 4.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 119 smd rect (at 3.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(CON1-Pad10)"))
    (pad 120 smd rect (at 3.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(CON1-Pad12)"))
    (pad 121 smd rect (at 2.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(CON1-Pad13)"))
    (pad 122 smd rect (at 2.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 123 smd rect (at 1.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 124 smd rect (at 1.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 125 smd rect (at 0.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R18-Pad2)"))
    (pad 126 smd rect (at 0.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 94 "Net-(U6-Pad126)"))
    (pad 127 smd rect (at -0.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U6-Pad127)"))
    (pad 128 smd rect (at -0.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(U6-Pad128)"))
    (pad 129 smd rect (at -1.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(U6-Pad129)"))
    (pad 130 smd rect (at -1.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 131 smd rect (at -2.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 132 smd rect (at -2.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(CON1-Pad15)"))
    (pad 133 smd rect (at -3.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(CON1-Pad16)"))
    (pad 134 smd rect (at -3.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 135 smd rect (at -4.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(CON1-Pad18)"))
    (pad 136 smd rect (at -4.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(CON1-Pad19)"))
    (pad 137 smd rect (at -5.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(CON1-Pad21)"))
    (pad 138 smd rect (at -5.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 139 smd rect (at -6.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 140 smd rect (at -6.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 141 smd rect (at -7.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(CON1-Pad22)"))
    (pad 142 smd rect (at -7.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(CON1-Pad28)"))
    (pad 143 smd rect (at -8.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 70 /S2))
    (pad 144 smd rect (at -8.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 69 /S3))
    (pad 145 smd rect (at 0 0 90) (size 6.7 6.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (model ../../electronics/kicad/3d/smd_lqfp/tqfp-144.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Analog:LQFP-64_10x10mm_Pitch0.5mm_PAD (layer F.Cu) (tedit 5C17C1C8)
    (at 173.736 93.726 180)
    (tags "QFP 0.5 PAD")
    (attr smd)
    (fp_text reference U4 (at 7.436 3.176 180) (layer F.SilkS))
    (fp_text value ADV7513 (at -0.004 3.076 180) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -3.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at -5.7 -3.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U4-Pad2)"))
    (pad 3 smd rect (at -5.7 -2.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U4-Pad3)"))
    (pad 4 smd rect (at -5.7 -2.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at -5.7 -1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 /ADAT))
    (pad 6 smd rect (at -5.7 -1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U4-Pad6)"))
    (pad 7 smd rect (at -5.7 -0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U4-Pad7)"))
    (pad 8 smd rect (at -5.7 -0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U4-Pad8)"))
    (pad 9 smd rect (at -5.7 0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 /ABCK))
    (pad 10 smd rect (at -5.7 0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 /ALRK))
    (pad 11 smd rect (at -5.7 1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (pad 12 smd rect (at -5.7 1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C32-Pad1)"))
    (pad 13 smd rect (at -5.7 2.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C32-Pad1)"))
    (pad 14 smd rect (at -5.7 2.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R11-Pad1)"))
    (pad 15 smd rect (at -5.7 3.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C34-Pad1)"))
    (pad 16 smd rect (at -5.7 3.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CON2-Pad19)"))
    (pad 17 smd rect (at -3.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(CON2-Pad12)"))
    (pad 18 smd rect (at -3.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CON2-Pad11)"))
    (pad 19 smd rect (at -2.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C34-Pad1)"))
    (pad 20 smd rect (at -2.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(CON2-Pad9)"))
    (pad 21 smd rect (at -1.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(CON2-Pad8)"))
    (pad 22 smd rect (at -1.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(R16-Pad2)"))
    (pad 23 smd rect (at -0.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(CON2-Pad6)"))
    (pad 24 smd rect (at -0.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(CON2-Pad5)"))
    (pad 25 smd rect (at 0.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C34-Pad1)"))
    (pad 26 smd rect (at 0.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CON2-Pad3)"))
    (pad 27 smd rect (at 1.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CON2-Pad2)"))
    (pad 28 smd rect (at 1.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /INT))
    (pad 29 smd rect (at 2.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C50-Pad1)"))
    (pad 30 smd rect (at 2.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 31 smd rect (at 3.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (pad 32 smd rect (at 3.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 5.7 3.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 107 /SCL_H))
    (pad 34 smd rect (at 5.7 3.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 108 /SDA_H))
    (pad 35 smd rect (at 5.7 2.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 /SCL))
    (pad 36 smd rect (at 5.7 2.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 /SDA))
    (pad 37 smd rect (at 5.7 1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U4-Pad37)"))
    (pad 38 smd rect (at 5.7 1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U4-Pad38)"))
    (pad 39 smd rect (at 5.7 0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U4-Pad39)"))
    (pad 40 smd rect (at 5.7 0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U4-Pad40)"))
    (pad 41 smd rect (at 5.7 -0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U4-Pad41)"))
    (pad 42 smd rect (at 5.7 -0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U4-Pad42)"))
    (pad 43 smd rect (at 5.7 -1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U4-Pad43)"))
    (pad 44 smd rect (at 5.7 -1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U4-Pad44)"))
    (pad 45 smd rect (at 5.7 -2.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U4-Pad45)"))
    (pad 46 smd rect (at 5.7 -2.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U4-Pad46)"))
    (pad 47 smd rect (at 5.7 -3.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U4-Pad47)"))
    (pad 48 smd rect (at 5.7 -3.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U4-Pad48)"))
    (pad 49 smd rect (at 3.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U4-Pad49)"))
    (pad 50 smd rect (at 3.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U4-Pad50)"))
    (pad 51 smd rect (at 2.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (pad 52 smd rect (at 2.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U4-Pad52)"))
    (pad 53 smd rect (at 1.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 /ADVCLK))
    (pad 54 smd rect (at 1.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U4-Pad54)"))
    (pad 55 smd rect (at 0.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U4-Pad55)"))
    (pad 56 smd rect (at 0.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U4-Pad56)"))
    (pad 57 smd rect (at -0.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U4-Pad57)"))
    (pad 58 smd rect (at -0.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U4-Pad58)"))
    (pad 59 smd rect (at -1.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U4-Pad59)"))
    (pad 60 smd rect (at -1.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U4-Pad60)"))
    (pad 61 smd rect (at -2.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U4-Pad61)"))
    (pad 62 smd rect (at -2.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U4-Pad62)"))
    (pad 63 smd rect (at -3.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U4-Pad63)"))
    (pad 64 smd rect (at -3.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U4-Pad64)"))
    (pad 65 smd rect (at 0 0 180) (size 4.8 4.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -1 -2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 -2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 0 -2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 0 2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 1 2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 0 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -1 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -1 -1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 0 -1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 1 -1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 1 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 1 1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 0 1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -1 1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -1 2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 0 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 -1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 1 -2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 -1 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 -2 180) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (model Housings_QFP.3dshapes/LQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:2.3_hole_mount (layer F.Cu) (tedit 5BD331D9)
    (at 195.072 95.18)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad "" thru_hole circle (at -10.382 -14.53) (size 2.5 2.5) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module pads:2.3_hole_mount (layer F.Cu) (tedit 5BD331C0)
    (at 130.7592 76.5048)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad "" thru_hole circle (at 10.1608 4.1452) (size 2.5 2.5) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module jumper:DC2R019JA7R1700 (layer F.Cu) (tedit 5B8EA164)
    (at 172.4 78.2 180)
    (fp_text reference CON2 (at 0 1.9 180) (layer F.SilkS))
    (fp_text value DC2R019JA7R1700 (at 0.12 4.09 180) (layer F.Fab))
    (fp_text user %R (at 0 1.9 180) (layer F.Fab))
    (pad 19 smd rect (at -3.6 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CON2-Pad19)"))
    (pad 18 smd rect (at -3.2 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 133 /HDMI+5))
    (pad 17 smd rect (at -2.8 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(CON2-Pad17)"))
    (pad 16 smd rect (at -2.4 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 108 /SDA_H))
    (pad 15 smd rect (at -2 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 107 /SCL_H))
    (pad 14 smd rect (at -1.6 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(CON2-Pad14)"))
    (pad 13 smd rect (at -1.2 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -0.8 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(CON2-Pad12)"))
    (pad 11 smd rect (at -0.4 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CON2-Pad11)"))
    (pad 1 smd rect (at 3.6 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.2 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CON2-Pad2)"))
    (pad 3 smd rect (at 2.8 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CON2-Pad3)"))
    (pad 4 smd rect (at 2.4 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(CON2-Pad5)"))
    (pad 6 smd rect (at 1.6 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(CON2-Pad6)"))
    (pad 7 smd rect (at 1.2 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.8 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(CON2-Pad8)"))
    (pad 9 smd rect (at 0.4 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(CON2-Pad9)"))
    (pad 10 smd rect (at 0 0 180) (size 0.23 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at -5.425 2.65 180) (size 1.1 2.4) (drill oval 0.6 1.9) (layers *.Cu *.Mask F.Paste)
      (net 1 GND))
    (pad 20 thru_hole oval (at 5.425 2.65 180) (size 1.1 2.4) (drill oval 0.6 1.9) (layers *.Cu *.Mask F.Paste)
      (net 1 GND))
    (pad 20 thru_hole oval (at 5.425 0 180) (size 1.1 1.7) (drill oval 0.6 1.2) (layers *.Cu *.Mask F.Paste)
      (net 1 GND))
    (pad 20 thru_hole oval (at -5.425 0 180) (size 1.1 1.7) (drill oval 0.6 1.2) (layers *.Cu *.Mask F.Paste)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5BC9D45A)
    (at 160.8 113.2)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.1 -1.3) (layer F.SilkS))
    (fp_text value 100 (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 123 /HRST))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:2_Pads_Small (layer F.Cu) (tedit 5B8E8506)
    (at 184.776 85.388 90)
    (fp_text reference CON5 (at 1.528 0.85 180) (layer F.Fab))
    (fp_text value CONN_01X03 (at 1.52 1.78 180) (layer F.Fab))
    (pad 2 smd rect (at 0.368 1.524 90) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 121 /SRST))
    (pad 1 smd rect (at -2.032 1.524 90) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 122 /HRST_OUT))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5B8E7FFA)
    (at 134.86 122.71 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference CON3 (at 1.52 1.11 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 1.51 0.1 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(CON3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 /RXD))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 /TXD))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(CON3-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AE1CC09)
    (at 183.76 101.79)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C48 (at 3.19 -0.44 180) (layer F.SilkS))
    (fp_text value .1u (at 0 -0.025 90) (layer F.Fab))
    (fp_text user %R (at 3.19 -0.44) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:UFDFN-10_2.5x1mm (layer F.Cu) (tedit 5AB25E24)
    (at 177.173 85.2678)
    (descr http://www.semtech.com/images/datasheet/rclamp0522p_0524p.pdf)
    (fp_text reference D2 (at 0 -2) (layer F.SilkS))
    (fp_text value SP3012-04UTG (at 0.04 1.18) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 0 -0.3875) (size 0.4 0.775) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -1 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(CON2-Pad9)"))
    (pad 9 smd rect (at -0.5 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CON2-Pad11)"))
    (pad 7 smd rect (at 0.5 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(CON2-Pad12)"))
    (pad 6 smd rect (at 1 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CON2-Pad19)"))
    (pad 5 smd rect (at 1 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CON2-Pad19)"))
    (pad 4 smd rect (at 0.5 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(CON2-Pad12)"))
    (pad 2 smd rect (at -0.5 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(CON2-Pad11)"))
    (pad 3 smd rect (at 0 0.3875) (size 0.4 0.775) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(CON2-Pad9)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AD4F425)
    (at 162.8 114.6)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R17 (at 0.69 -5.32 180) (layer F.SilkS))
    (fp_text value 10K (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0.73 -5.35) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 113 /ESP_SCL))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:FPC_32 (layer F.Cu) (tedit 5AB25AF4)
    (at 127.6 97.2 270)
    (fp_text reference CON1 (at 7.9 3.4 270) (layer F.SilkS))
    (fp_text value 3-1775333-2 (at 8 4.6 270) (layer F.Fab))
    (pad 1 smd rect (at -0.003 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 77 /VCLK))
    (pad 2 smd rect (at 0.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(CON1-Pad3)"))
    (pad 4 smd rect (at 1.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(CON1-Pad4)"))
    (pad 5 smd rect (at 1.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(CON1-Pad6)"))
    (pad 7 smd rect (at 2.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(CON1-Pad7)"))
    (pad 8 smd rect (at 3.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 3.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(CON1-Pad9)"))
    (pad 10 smd rect (at 4.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(CON1-Pad10)"))
    (pad 11 smd rect (at 4.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 5.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(CON1-Pad12)"))
    (pad 13 smd rect (at 5.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(CON1-Pad13)"))
    (pad 14 smd rect (at 6.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 6.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(CON1-Pad15)"))
    (pad 16 smd rect (at 7.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(CON1-Pad16)"))
    (pad 17 smd rect (at 7.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 8.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(CON1-Pad18)"))
    (pad 19 smd rect (at 8.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(CON1-Pad19)"))
    (pad 20 smd rect (at 9.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 9.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(CON1-Pad21)"))
    (pad 22 smd rect (at 10.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(CON1-Pad22)"))
    (pad 23 smd rect (at 10.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 11.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /ABCK))
    (pad 25 smd rect (at 11.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /ADAT))
    (pad 26 smd rect (at 12.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at 12.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /ALRK))
    (pad 28 smd rect (at 13.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(CON1-Pad28)"))
    (pad 29 smd rect (at 13.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /+5))
    (pad 30 smd rect (at 14.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 31 smd rect (at 14.997 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 32 smd rect (at 15.497 0 270) (size 0.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -1.9 3.25 270) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 17.4 3.25 270) (size 1.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5B8E8FB4)
    (at 184.55 123.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 129 "Net-(U8-Pad1)"))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1D0A8)
    (at 184.55 121.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 105 "Net-(U8-Pad2)"))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1D089)
    (at 184.55 119.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 2 +3V3))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1D072)
    (at 184.55 117.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 28 "Net-(R14-Pad1)"))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1D02F)
    (at 184.55 115.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 75 /DCLK))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1D00F)
    (at 184.55 113.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 76 /MISO))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1CFB7)
    (at 184.55 111.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 74 /MOSI))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1CFA0)
    (at 184.55 109.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 2 +3V3))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5B8E825D)
    (at 168.45 123.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 119 /TXD))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5B8E8268)
    (at 168.45 121.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 118 /RXD))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1CEB4)
    (at 168.45 119.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 22 /nConf))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE72F7D)
    (at 168.45 117.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 116 /nCE))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1CE4F)
    (at 168.45 115.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 113 /ESP_SCL))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE1CE48)
    (at 168.45 113.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 114 /ESP_SDA))
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE5C2CD)
    (at 168.45 111.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module pads:2.3_hole_mount (layer F.Cu) (tedit 5B168459)
    (at 165.0492 132.518)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 -3.74) (size 2.5 2.5) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CD4)
    (at 132.575 120 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value .1u (at -0.074 0.088 180) (layer F.Fab))
    (fp_text user %R (at -2.774 -0.012 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CD1)
    (at 122.936 121.666 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.124 -1.524 180) (layer F.SilkS))
    (fp_text value .1u (at 0.034 -0.064) (layer F.Fab))
    (fp_text user %R (at 2.134 -1.514) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CCC)
    (at 122.936 118.11 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 1.71 1.464 180) (layer F.SilkS))
    (fp_text value .1u (at 0.01 -0.036 180) (layer F.Fab))
    (fp_text user %R (at 1.71 1.464 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CC5)
    (at 134.7 113.4 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value .1u (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 0.2 1.2 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CDB)
    (at 137.4 116.3 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -0.2 1.4 270) (layer F.SilkS))
    (fp_text value .1u (at 0 0) (layer F.Fab))
    (fp_text user %R (at -0.1 1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25F88)
    (at 140 117 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.01 1.3 180) (layer F.SilkS))
    (fp_text value .1u (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 0.02 1.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25F85)
    (at 143.8 117)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -0.06 -1.31) (layer F.SilkS))
    (fp_text value .1u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at -0.06 -1.31) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CE7)
    (at 151.75 116.8)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -0.04 -1.16) (layer F.SilkS))
    (fp_text value .1u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CEB)
    (at 155.45 116.8)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -0.09 -1.19) (layer F.SilkS))
    (fp_text value .1u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at -0.1 -1.2) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CEF)
    (at 158 115.8 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -0.65 -1.3 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0) (layer F.Fab))
    (fp_text user %R (at -0.65 -1.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B4C8F79)
    (at 160.02 119.126)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 3.38 -0.026) (layer F.SilkS))
    (fp_text value .1u (at -0.05 -0.033 90) (layer F.Fab))
    (fp_text user %R (at 3.38 -0.026) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CBC)
    (at 133.75 109.625 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 -1.25 180) (layer F.SilkS))
    (fp_text value .1u (at 0 -0.03 270) (layer F.Fab))
    (fp_text user %R (at -0.4 -1.23 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CB9)
    (at 133.6 105.2 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 -1.4 180) (layer F.SilkS))
    (fp_text value .1u (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 0.1 -1.3 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25B27)
    (at 133.2 102.8 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -3.2 0 270) (layer F.SilkS))
    (fp_text value .1u (at -0.1 0) (layer F.Fab))
    (fp_text user %R (at -3.2 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25B2A)
    (at 131.6 102.8 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -3 0 270) (layer F.SilkS))
    (fp_text value .1u (at -0.1 0) (layer F.Fab))
    (fp_text user %R (at -3.1 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25A78)
    (at 136.45 90.35 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 1.4 90) (layer F.SilkS))
    (fp_text value .1u (at 0.05 -0.05 180) (layer F.Fab))
    (fp_text user %R (at 0 1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25A90)
    (at 139.4 89.15 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 3.65 0 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 3.65 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB2A038)
    (at 141.375 89.15 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 3.7 0.025 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 3.7 0.025 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CA3)
    (at 146 89.3572 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 3.2572 0 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 3.2572 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CAB)
    (at 149.85 89.15 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 3.1 0 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 3.1 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CA8)
    (at 151.4 89.15 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 3.1 0 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 3.1 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25D4B)
    (at 157.2 90.7)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at -0.62 -1.28) (layer F.SilkS))
    (fp_text value .1u (at -0.01 0.02 90) (layer F.Fab))
    (fp_text user %R (at -0.6 -1.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25D3B)
    (at 159.9 92.7)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 0.91 -2.17 90) (layer F.SilkS))
    (fp_text value .1u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0.93 -2.15 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E2F)
    (at 167.7 87.3 135)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at 0 -1.25 135) (layer F.SilkS))
    (fp_text value .1u (at 0.049497 0.091924 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.272792 135) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 135) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.949999 0 135) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E73)
    (at 167.5 99.4 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at 1.75 1.15 180) (layer F.SilkS))
    (fp_text value .1u (at 0.02 -0.04 270) (layer F.Fab))
    (fp_text user %R (at 1.75 1.15 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25D2B)
    (at 161.3 103.3)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 0 -1.25) (layer F.SilkS))
    (fp_text value .1u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25D2E)
    (at 161.25 99.9)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at 0 -1.25) (layer F.SilkS))
    (fp_text value .1u (at 0.02 -0.02 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25D12)
    (at 164.625 110.625)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C28 (at 0.075 -5.025) (layer F.SilkS))
    (fp_text value .1u (at -0.025 -0.025 90) (layer F.Fab))
    (fp_text user %R (at 0.075 -5.025) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25D34)
    (at 161.7 94.2)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at -0.67 1.45) (layer F.SilkS))
    (fp_text value .1u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at -0.65 1.46) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ADDE61C)
    (at 178.625 100.8 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at 0 -1.275 90) (layer F.SilkS))
    (fp_text value .1u (at -0.02 0.045) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E69)
    (at 182.6 93)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at -1.03 -10.84) (layer F.SilkS))
    (fp_text value .1u (at -0.01 0.01 90) (layer F.Fab))
    (fp_text user %R (at -1.03 -10.83) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E65)
    (at 182.6 91.8)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at -1.11 -11) (layer F.SilkS))
    (fp_text value .1u (at -0.04 0.02 90) (layer F.Fab))
    (fp_text user %R (at -1.11 -11.02) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25AA5)
    (at 133.75 91.725 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C33 (at 3.275 0 270) (layer F.SilkS))
    (fp_text value 470p (at -0.05 -0.05) (layer F.Fab))
    (fp_text user %R (at 3.275 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C33-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E57)
    (at 182.6 89.3)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at -1.18 -11.12) (layer F.SilkS))
    (fp_text value .1u (at -0.02 0.04 90) (layer F.Fab))
    (fp_text user %R (at -1.15 -11.16) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E52)
    (at 180.4 88)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at -0.89 -2.2 90) (layer F.SilkS))
    (fp_text value .1u (at 0.03 0.05 90) (layer F.Fab))
    (fp_text user %R (at -0.89 -2.23 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C94)
    (at 155.4 79.8 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C36 (at 0 -3.2 180) (layer F.SilkS))
    (fp_text value 10u (at 0.025 0 270) (layer F.Fab))
    (fp_text user %R (at 0 -3.2 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C71)
    (at 159.4 77.5)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C37 (at 0 2.45) (layer F.SilkS))
    (fp_text value 10u (at 0 -0.025 90) (layer F.Fab))
    (fp_text user %R (at 0 2.45) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C6E)
    (at 163.45 75.6)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C38 (at 1 1.4) (layer F.SilkS))
    (fp_text value 10u (at -0.025 0.05 90) (layer F.Fab))
    (fp_text user %R (at 1 1.4) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25AE7)
    (at 130.725 92.175 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C39 (at 3.375 -0.025 270) (layer F.SilkS))
    (fp_text value 10u (at 0 0) (layer F.Fab))
    (fp_text user %R (at 3.375 -0.025 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25A5E)
    (at 125.1 93.3)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C40 (at 3.2 0.1) (layer F.SilkS))
    (fp_text value 10u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 3.2 0.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CC7)
    (at 130.6 112.7)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C42 (at 0 -1.25) (layer F.SilkS))
    (fp_text value 10u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C98)
    (at 150.95 79.125)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C43 (at -3.15 0.125) (layer F.SilkS))
    (fp_text value 10u (at 0.05 0.025 90) (layer F.Fab))
    (fp_text user %R (at -3.15 0.125) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB259FC)
    (at 132.2 85.1)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C44 (at -2.4 0.1 90) (layer F.SilkS))
    (fp_text value 10u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at -2.4 0.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25A10)
    (at 136 85.1)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C45 (at 0.925 -1.225) (layer F.SilkS))
    (fp_text value 10u (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0.925 -1.225) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:UFDFN-10_2.5x1mm (layer F.Cu) (tedit 5AB25E27)
    (at 173.99 85.2678)
    (descr http://www.semtech.com/images/datasheet/rclamp0522p_0524p.pdf)
    (fp_text reference D3 (at 0 -2) (layer F.SilkS))
    (fp_text value SP3012-04UTG (at -0.05 1.18) (layer F.Fab))
    (fp_text user %R (at 0.1 0) (layer F.Fab))
    (pad 8 smd rect (at 0 -0.3875) (size 0.4 0.775) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -1 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CON2-Pad3)"))
    (pad 9 smd rect (at -0.5 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(CON2-Pad5)"))
    (pad 7 smd rect (at 0.5 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(CON2-Pad6)"))
    (pad 6 smd rect (at 1 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(CON2-Pad8)"))
    (pad 5 smd rect (at 1 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(CON2-Pad8)"))
    (pad 4 smd rect (at 0.5 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(CON2-Pad6)"))
    (pad 2 smd rect (at -0.5 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(CON2-Pad5)"))
    (pad 3 smd rect (at 0 0.3875) (size 0.4 0.775) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CON2-Pad3)"))
  )
  (module digikey-footprints:UFDFN-10_2.5x1mm (layer F.Cu) (tedit 5AB25E2A)
    (at 170.7642 85.2678)
    (descr http://www.semtech.com/images/datasheet/rclamp0522p_0524p.pdf)
    (fp_text reference D4 (at 0 -2) (layer F.SilkS))
    (fp_text value SP3012-04UTG (at 0.03 1.16) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 0 -0.3875) (size 0.4 0.775) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -1 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 133 /HDMI+5))
    (pad 9 smd rect (at -0.5 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 108 /SDA_H))
    (pad 7 smd rect (at 0.5 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 107 /SCL_H))
    (pad 6 smd rect (at 1 -0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CON2-Pad2)"))
    (pad 5 smd rect (at 1 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CON2-Pad2)"))
    (pad 4 smd rect (at 0.5 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 107 /SCL_H))
    (pad 2 smd rect (at -0.5 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 108 /SDA_H))
    (pad 3 smd rect (at 0 0.3875) (size 0.4 0.775) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0.4375) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask)
      (net 133 /HDMI+5))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C66)
    (at 154.875 76.55 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L1 (at 4.75 0.025 270) (layer F.SilkS))
    (fp_text value 10u (at 0.05 0.075) (layer F.Fab))
    (fp_text user %R (at 4.75 0.025 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +1.8))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C67)
    (at 156.575 76.55 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L2 (at -4.85 -0.025 90) (layer F.SilkS))
    (fp_text value 10u (at 0.05 0.025 180) (layer F.Fab))
    (fp_text user %R (at -4.85 -0.025 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C34-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +1.8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C68)
    (at 159.375 75.6 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L3 (at -0.025 -3.1 180) (layer F.SilkS))
    (fp_text value 10u (at 0.05 -0.05 270) (layer F.Fab))
    (fp_text user %R (at -0.025 -3.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 +1.8))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-223 (layer F.Cu) (tedit 5AB25FA6)
    (at 126.4 88.2)
    (fp_text reference U1 (at -3.2 -3.2) (layer F.SilkS))
    (fp_text value MCP1826S-1202E/DB (at 0.1 -0.3) (layer F.Fab))
    (fp_text user %R (at -3.2 -3.2) (layer F.Fab))
    (pad 3 smd rect (at 2.3 3.1) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +1.2))
    (pad 2 smd rect (at 0 3.1) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.3 3.1) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at 0 -3.1) (size 3.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module digikey-footprints:SOT-753 (layer F.Cu) (tedit 5AB259E4)
    (at 132.4 88.2 270)
    (fp_text reference U2 (at -0.4 -2.85 270) (layer F.SilkS))
    (fp_text value MIC5219-2.5YM5-TR (at 0 -0.1 270) (layer F.Fab))
    (fp_text user %R (at 0 0.1 270) (layer F.Fab))
    (pad 5 smd rect (at -0.95 -1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 3 +2.5) (solder_mask_margin 0.07))
    (pad 4 smd rect (at 0.95 -1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C33-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at 0.95 1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 2 smd rect (at 0 1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -0.95 1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
  )
  (module digikey-footprints:SOT-753 (layer F.Cu) (tedit 5AB25FAC)
    (at 151.8 76.3 270)
    (fp_text reference U3 (at -0.25 3.25 270) (layer F.SilkS))
    (fp_text value LP5907MFX-1.8/NOPB (at 0.2 -0.13 270) (layer F.Fab))
    (fp_text user %R (at -0.2 3.25 270) (layer F.Fab))
    (pad 5 smd rect (at -0.95 -1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 23 +1.8) (solder_mask_margin 0.07))
    (pad 4 smd rect (at 0.95 -1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U3-Pad4)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at 0.95 1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 2 smd rect (at 0 1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 1 smd rect (at -0.95 1.35 270) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
  )
  (module ESP12FLAT:ESP-12_FLAT (layer F.Cu) (tedit 5C17C0BB)
    (at 176.4 123.4 180)
    (fp_text reference U8 (at -10.75 -0.55 180) (layer F.SilkS))
    (fp_text value ESP-12E (at 0.1 0.6 180) (layer F.Fab))
    (pad 1 smd rect (at -8.7615 0 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(U8-Pad1)"))
    (pad 2 smd rect (at -8.7615 2 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(U8-Pad2)"))
    (pad 3 smd rect (at -8.7615 4 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at -8.7615 6 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R14-Pad1)"))
    (pad 5 smd rect (at -8.7615 8 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 75 /DCLK))
    (pad 6 smd rect (at -8.7615 10 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 76 /MISO))
    (pad 7 smd rect (at -8.7615 12 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 74 /MOSI))
    (pad 8 smd rect (at -8.7615 14 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 16 smd rect (at 8.5615 0 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 119 /TXD))
    (pad 15 smd rect (at 8.5615 2 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 118 /RXD))
    (pad 14 smd rect (at 8.5615 4 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 22 /nConf))
    (pad 13 smd rect (at 8.5615 6 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 116 /nCE))
    (pad 12 smd rect (at 8.5615 8 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 113 /ESP_SCL))
    (pad 11 smd rect (at 8.5615 10 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 114 /ESP_SDA))
    (pad 10 smd rect (at 8.5615 12 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 8.5615 14 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5BC887A9)
    (at 164.6 111.8)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference D1 (at -0.35 -5) (layer F.SilkS))
    (fp_text value 150060BS75000 (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at -0.35 -5) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C9F)
    (at 147.55 89.3572 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.8072 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 0) (layer F.Fab))
    (fp_text user %R (at -2.8072 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25CF6)
    (at 160.782 117.094)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.018 -1.294 180) (layer F.SilkS))
    (fp_text value 10K (at 0.018 0.006 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 /nConf))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E3C)
    (at 163.225 79.9 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R5 (at -1 1.265 270) (layer F.SilkS))
    (fp_text value 2K (at 0 0) (layer F.Fab))
    (fp_text user %R (at -0.75 -1.375 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 110 /+5))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 107 /SCL_H))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E40)
    (at 163.85 84.45 315)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R6 (at 0.070711 1.343503 315) (layer F.SilkS))
    (fp_text value 2K (at 0.021213 0.077782 45) (layer F.Fab))
    (fp_text user %R (at 0.070711 1.343503 315) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 315) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 110 /+5))
    (pad 2 smd rect (at 0.949999 0 315) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 108 /SDA_H))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C80)
    (at 160.7 82.4 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.7 0.1 90) (layer F.SilkS))
    (fp_text value 2K (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at -2.75 0.125 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /SDA))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C7D)
    (at 159.1 82.4 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R9 (at -2.7 0.1 90) (layer F.SilkS))
    (fp_text value 2K (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at -2.65 0.075 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /SCL))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C24-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25C90)
    (at 151.05 82 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 1.4 90) (layer F.SilkS))
    (fp_text value 2K (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 1.4 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 /INT))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E5D)
    (at 182.6 90.5)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R11 (at -1.07 -11.05) (layer F.SilkS))
    (fp_text value 887 (at -0.01 0 90) (layer F.Fab))
    (fp_text user %R (at -1.07 -11.05) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25E4F)
    (at 181.4618 85.3348 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R12 (at 3.0748 -2.4918 270) (layer F.SilkS))
    (fp_text value 10K (at 0.01 0.02 180) (layer F.Fab))
    (fp_text user %R (at 3.0848 -2.5118 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CON2-Pad19)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B4C8F7C)
    (at 160.02 120.65 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R13 (at 0.35 -1.36) (layer F.SilkS))
    (fp_text value 10K (at 0 -0.036 270) (layer F.Fab))
    (fp_text user %R (at 0.42 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 /CS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ABA40CC)
    (at 164.4 120.6 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R14 (at -0.02 -1.35 180) (layer F.SilkS))
    (fp_text value 22 (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R14-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 /CS))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5AB25D1F)
    (at 164.6 113.2)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R15 (at 0.1 -5.2) (layer F.SilkS))
    (fp_text value 10K (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0.1 -5.2) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 114 /ESP_SDA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 5AB25F9D)
    (at 127.6 119.73 180)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U5 (at -2.96 -3.75 180) (layer F.SilkS))
    (fp_text value 664G-03LF (at -0.15 0.02 270) (layer F.Fab))
    (fp_text user %R (at -2.94 -3.69 180) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 66 /X1))
    (pad 2 smd rect (at -2.95 -1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at -2.95 -0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at -2.95 -0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 68 /S0))
    (pad 5 smd rect (at -2.95 0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.95 0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.95 1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 69 /S3))
    (pad 8 smd rect (at -2.95 2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 70 /S2))
    (pad 9 smd rect (at 2.95 2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 71 /CLK))
    (pad 10 smd rect (at 2.95 1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 72 /S1))
    (pad 11 smd rect (at 2.95 0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 12 smd rect (at 2.95 0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 2.95 -0.325 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.95 -0.975 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 15 smd rect (at 2.95 -1.625 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(U5-Pad15)"))
    (pad 16 smd rect (at 2.95 -2.275 180) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U5-Pad16)"))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5AB25F92)
    (at 154 121.6)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at 2.55 -3.05) (layer F.SilkS))
    (fp_text value MX25L1606EM1I-12G (at 0.01 0.04 90) (layer F.Fab))
    (fp_text user %R (at 2.5148 -3.0328) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /CS))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 76 /MISO))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 /MOSI))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 75 /DCLK))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:2.3_hole_mount (layer F.Cu) (tedit 5AB2C6A4)
    (at 118.4148 87.1728)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ADDE59B)
    (at 185.33 95.55)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R16 (at -3.32 -0.43) (layer F.SilkS))
    (fp_text value 2K (at -0.01 0.06 90) (layer F.Fab))
    (fp_text user %R (at -3.32 -0.43) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(R16-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:2_Pads_Small (layer F.Cu) (tedit 5B8E84F7)
    (at 184.76 90.308 90)
    (fp_text reference CON4 (at 1.528 0.85 180) (layer F.Fab))
    (fp_text value CONN_01X03 (at 1.528 1.79 180) (layer F.Fab))
    (pad 1 smd rect (at -2.032 1.524 90) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 111 /PAD1))
    (pad 2 smd rect (at 0.368 1.524 90) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 112 /PAD2))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ADDE553)
    (at 185.3 97 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C41 (at 3.26 0.54 180) (layer F.SilkS))
    (fp_text value 47p (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 3.26 0.53 180) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 /ALRK))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ADDE52B)
    (at 185.3 98.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C46 (at 2.34 -0.15 270) (layer F.SilkS))
    (fp_text value 47p (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 2.33 -0.14 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 /ABCK))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ADDE62A)
    (at 185.3 100 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C47 (at -2.6 0.68 270) (layer F.SilkS))
    (fp_text value 47p (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at -2.6 0.68 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 /ADAT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5ADDE69F)
    (at 133.8 116.3 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(R7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:.6Cast (layer F.Cu) (tedit 5AE5C29B)
    (at 168.45 109.4)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B4C944A)
    (at 149.95 118.25)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R20 (at 3.25 0.05) (layer F.SilkS))
    (fp_text value 10K (at 0.05 0.05 90) (layer F.Fab))
    (fp_text user %R (at 3.25 0.05) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 116 /nCE))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5B8E83A3)
    (at 186.84 104.2 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C49 (at -3.9 0.29 90) (layer F.SilkS))
    (fp_text value 22u (at 0 0.075 180) (layer F.Fab))
    (fp_text user %R (at -3.87 0.29 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_DIP_x2_W7.62mm_Slide_Copal_CHS-B (layer F.Cu) (tedit 5C17C07A)
    (at 180.73 105.1)
    (descr "2x-dip-switch, Slide, row spacing 7.62 mm (300 mils), Copal_CHS-B")
    (tags "DIP Switch Slide 7.62mm 300mil Copal_CHS-B")
    (attr smd)
    (fp_text reference SW1 (at -6.48 1.74) (layer F.SilkS))
    (fp_text value SW_DIP_x02 (at -2.02 1.72) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.81 -0.635) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 113 /ESP_SCL))
    (pad 3 smd rect (at 3.81 0.635) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at -3.81 0.635) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 123 /HRST))
    (pad 4 smd rect (at 3.81 -0.635) (size 1.6 0.76) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_DIP_x2_W7.62mm_Slide_Copal_CHS-B.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B8FCEC2)
    (at 183.88 86.3 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.48 -0.06) (layer F.SilkS))
    (fp_text value 470 (at -0.01 0) (layer F.Fab))
    (fp_text user %R (at -2.48 -0.04) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 122 /HRST_OUT))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(R1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B91312F)
    (at 147.81 82.01 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R18 (at -0.06 1.4 270) (layer F.SilkS))
    (fp_text value 470 (at 0 0.02) (layer F.Fab))
    (fp_text user %R (at -0.08 1.39 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 121 /SRST))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(R18-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5BA106E3)
    (at 164.81 87.84 135)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C50 (at 0.014142 -1.414214 135) (layer F.SilkS))
    (fp_text value 10u (at -0.014142 0.014142 225) (layer F.Fab))
    (fp_text user %R (at 0.028284 -1.385929 135) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 135) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C50-Pad1)"))
    (pad 2 smd rect (at 0.949999 0 135) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5BA1059D)
    (at 181.69 99.15 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L4 (at -2.7 -0.51 90) (layer F.SilkS))
    (fp_text value 10u (at 0.01 -0.02 180) (layer F.Fab))
    (fp_text user %R (at -2.71 -0.51 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(C50-Pad1)"))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:dchdmi (layer B.Cu) (tedit 0)
    (at 170.85 84 180)
    (fp_text reference LOGO (at 0 -5 180) (layer B.SilkS) hide)
    (fp_text value "" (at 0 0 180) (layer B.SilkS))
  )
  (module digikey-footprints:SOD-523 (layer F.Cu) (tedit 5C12B86F)
    (at 165.35 82.84 135)
    (fp_text reference D5 (at -2.255671 -0.021213 135) (layer F.SilkS))
    (fp_text value BAT54XV2T1G (at -0.148492 -0.601041 315) (layer F.Fab) hide)
    (fp_text user %R (at -0.025 -0.025 135) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 135) (size 0.4 0.35) (layers F.Cu F.Paste F.Mask)
      (net 133 /HDMI+5))
    (pad 2 smd rect (at 0.85 0 135) (size 0.4 0.35) (layers F.Cu F.Paste F.Mask)
      (net 110 /+5))
  )
  (module Symbols:WEEE-Logo_4.2x6mm_SilkScreen (layer F.Cu) (tedit 5C13B5ED)
    (at 165.05 94.45)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF*** (at 0.05 2.38) (layer F.SilkS) hide)
    (fp_text value WEEE-Logo_4.2x6mm_SilkScreen (at -0.1 2.31) (layer F.Fab) hide)
  )
  (gr_text + (at 164.14 81.66 90) (layer F.SilkS))
  (gr_line (start 161.559 132.432) (end 168.417 132.432) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.559 125) (end 161.559 132.432) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.568 90.658) (end 114.568 83.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 90.658) (end 114.568 90.658) (layer Edge.Cuts) (width 0.15))
  (gr_text + (at 165.45 115.7) (layer F.SilkS))
  (gr_text RST (at 188.01 84.73 90) (layer F.SilkS))
  (gr_text OPT (at 187.97 87.53 90) (layer F.SilkS))
  (gr_text @chriz2600 (at 170.8 105.11) (layer F.SilkS))
  (gr_text P2 (at 187.92 90.13 90) (layer F.SilkS))
  (gr_text P1 (at 187.92 92.39 90) (layer F.SilkS))
  (gr_text "@citrus3000psi\n" (at 169.27 103.65) (layer F.SilkS))
  (gr_text "DCHDMI 1.3a" (at 170.56 101.85) (layer F.SilkS))
  (gr_text DTR (at 147.11 118.71) (layer F.SilkS))
  (gr_text TX (at 144.68 118.68) (layer F.SilkS))
  (gr_text RX (at 142.35 118.61) (layer F.SilkS))
  (gr_text 3.3 (at 139.4 118.6) (layer F.SilkS))
  (gr_text CTS (at 137.06 118.63) (layer F.SilkS))
  (gr_text GND (at 134.5 118.6) (layer F.SilkS))
  (gr_arc (start 133.718 80.552) (end 136.968 80.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.568 83.8) (end 133.718 83.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 125) (end 122 90.658) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.968 74.672) (end 136.968 80.552) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.375 74.672) (end 136.968 74.672) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.375 78.047) (end 145.375 74.672) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.25 78.047) (end 145.375 78.047) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.25 73.672) (end 147.25 78.047) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 188.568 73.672) (end 147.25 73.672) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 188.568 125) (end 188.568 73.672) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.617 125) (end 188.568 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.617 107.797) (end 184.617 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.417 107.797) (end 184.617 107.797) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.417 132.432) (end 168.417 107.797) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 125) (end 161.559 125) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 122 125) (xy 168.4 125) (xy 168.4 107.8) (xy 184.6 107.8) (xy 184.6 125)
        (xy 188.6 125) (xy 188.6 73.7) (xy 147.3 73.7) (xy 147.3 78.1) (xy 145.4 78.1)
        (xy 145.415 74.6633) (xy 137.015 74.6633) (xy 137 79.3) (xy 136.975 80.2) (xy 136.925 80.925)
        (xy 136.8 81.6) (xy 136.5 82.3) (xy 135.9 83) (xy 134.8 83.6) (xy 133.8 83.8)
        (xy 122 83.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 122 125) (xy 168.4 125) (xy 168.4 107.8) (xy 184.6 107.8) (xy 184.6 125)
        (xy 188.6 125) (xy 188.6 73.7) (xy 147.3 73.7) (xy 147.3 78.1) (xy 145.4 78.1)
        (xy 145.415 74.6633) (xy 137.015 74.6633) (xy 137 79.3) (xy 136.975 80.2) (xy 136.925 80.975)
        (xy 136.8 81.6) (xy 136.5 82.3) (xy 135.9 83) (xy 134.8 83.6) (xy 133.8 83.8)
        (xy 122 83.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 128.96 121.44) (xy 129.12 121.78) (xy 129.04 122.08) (xy 128.65 122.22) (xy 128.35 122.03)
        (xy 128.26 121.71) (xy 128.36 121.49) (xy 128.6 121.38) (xy 128.76 121.37)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 122 125) (xy 168.4 125) (xy 168.4 107.8) (xy 184.6 107.8) (xy 184.6 125)
        (xy 188.6 125) (xy 188.6 73.7) (xy 147.3 73.7) (xy 147.3 78.1) (xy 145.4 78.1)
        (xy 145.415 74.6633) (xy 137.015 74.6633) (xy 137 79.3) (xy 137 80.225) (xy 136.925 80.85)
        (xy 136.8 81.6) (xy 136.5 82.3) (xy 135.9 83) (xy 134.8 83.6) (xy 133.8 83.8)
        (xy 122 83.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 122 125) (xy 168.4 125) (xy 168.4 107.8) (xy 184.6 107.8) (xy 184.6 125)
        (xy 188.6 125) (xy 188.6 73.7) (xy 147.3 73.7) (xy 147.3 78.1) (xy 145.4 78.1)
        (xy 145.4023 74.6633) (xy 137.0023 74.6633) (xy 137 79.3) (xy 136.975 80.225) (xy 136.9 80.95)
        (xy 136.8 81.6) (xy 136.5 82.3) (xy 135.9 83) (xy 134.8 83.6) (xy 133.8 83.8)
        (xy 122 83.8)
      )
    )
  )
)
