<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.07" y2="0" width="0" layer="20"/>
<wire x1="25.07" y1="0" x2="25.07" y2="27.957" width="0" layer="20"/>
<wire x1="25.07" y1="27.957" x2="0" y2="27.957" width="0" layer="20"/>
<wire x1="0" y1="27.957" x2="0" y2="0" width="0" layer="20"/>
<text>ZZLT</text>
<text>LTAR DISP.</text>
<text>ADAPTER</text>
<text>REV. 2</text>
<text>+</text>
<text>-</text>
<text>G</text>
<text>R</text>
<text>L</text>
<text>M</text>
</plain>
<libraries>
<library name="con-headers-jp">
<description>&lt;b&gt;Male(J), Female(P) and Pin Headers&lt;/b&gt;&lt;p&gt;Version 1.02 - 03/10/2009&lt;p&gt;
This library is a collection of various pin headers and AMP, Molex and 3M board-to-board connectors. 
This library assumes the notion of JACKS(male) and PLUGS(female) as represented by the J and P symbols.
Standard male/female pin header types are available in common 0.1" and 2 mm pitch types with alternate mirrored footprints as well.
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="SIP-100-02-40">
<description>&lt;b&gt;SIP Header&lt;/b&gt; - 0.1", 40 mil drill</description>
</package>
<package name="SIP-100-04-40Y">
<description>&lt;b&gt;SIP Header&lt;/b&gt; - 0.1", 40 mil drill</description>
</package>
</packages>
</library>
<library name="izzy">
<packages>
<package name="MOLEX-43860">
</package>
<package name="MA03-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="izzy" package="MOLEX-43860" value="MOLEX-43860"/>
<element name="P1" library="izzy" package="MA03-2" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="P2" library="con-headers-jp" package="SIP-100-02-40" value="M-1X02-SIP-100-40"/>
<element name="J2" library="con-headers-jp" package="SIP-100-04-40Y" value="F-1X04-SIP-100-40Y"/>
</elements>
<signals>
<signal name="LTAR_INPUT">
<contactref element="J1" pad="PIN7"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="PIN6"/>
<contactref element="J1" pad="PIN5"/>
<contactref element="P1" pad="3"/>
<contactref element="P1" pad="5"/>
<contactref element="P2" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="DEBUG">
<contactref element="J1" pad="PIN4"/>
<contactref element="P1" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="PIN3"/>
<contactref element="P1" pad="2"/>
</signal>
<signal name="+BAT">
<contactref element="J1" pad="PIN2"/>
<contactref element="P1" pad="1"/>
<contactref element="P2" pad="2"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
