(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 91)
    (no_connects 0)
    (area 124.384999 96.444999 153.745001 162.635001)
    (thickness 1.6)
    (drawings 46)
    (tracks 408)
    (zones 0)
    (modules 34)
    (nets 46)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.8636 0.508)
    (user_via 1.1176 0.762)
    (user_via 1.3716 1.016)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.127)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 139.065 111.125)
    (visible_elements 7FFEDF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +5V)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(F1-Pad2)")
  (net 6 "Net-(P1-Pad3)")
  (net 7 "Net-(P1-Pad5)")
  (net 8 GPIO4)
  (net 9 "Net-(P1-Pad8)")
  (net 10 "Net-(P1-Pad10)")
  (net 11 GPIO17)
  (net 12 "Net-(P1-Pad12)")
  (net 13 "Net-(P1-Pad13)")
  (net 14 "Net-(P1-Pad15)")
  (net 15 "Net-(P1-Pad16)")
  (net 16 "Net-(P1-Pad18)")
  (net 17 SPI0_MOSI)
  (net 18 SPI0_MISO)
  (net 19 "Net-(P1-Pad22)")
  (net 20 SPI0_SCLK)
  (net 21 SPI0_CS0)
  (net 22 "Net-(P1-Pad26)")
  (net 23 HAT_SDA)
  (net 24 HAT_SCL)
  (net 25 "Net-(P1-Pad29)")
  (net 26 "Net-(P1-Pad31)")
  (net 27 "Net-(P1-Pad32)")
  (net 28 "Net-(P1-Pad33)")
  (net 29 SPI1_MISO)
  (net 30 SPI1_CS0)
  (net 31 "Net-(P1-Pad37)")
  (net 32 SPI1_MOSI)
  (net 33 SPI1_SCLK)
  (net 34 "Net-(P2-Pad1)")
  (net 35 SPI0_SCLK_5)
  (net 36 SPI0_MOSI_5)
  (net 37 SPI0_CS0_5)
  (net 38 SPI1_CS0_5)
  (net 39 SPI1_SCLK_5)
  (net 40 SPI1_MOSI_5)
  (net 41 "Net-(P6-Pad4)")
  (net 42 "Net-(R5-Pad2)")
  (net 43 "Net-(P3-Pad4)")
  (net 44 "Net-(P3-Pad3)")
  (net 45 "Net-(P5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net GPIO17)
    (add_net GPIO4)
    (add_net HAT_SCL)
    (add_net HAT_SDA)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad18)")
    (add_net "Net-(P1-Pad22)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad29)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad31)")
    (add_net "Net-(P1-Pad32)")
    (add_net "Net-(P1-Pad33)")
    (add_net "Net-(P1-Pad37)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(R5-Pad2)")
    (add_net SPI0_CS0)
    (add_net SPI0_CS0_5)
    (add_net SPI0_MISO)
    (add_net SPI0_MOSI)
    (add_net SPI0_MOSI_5)
    (add_net SPI0_SCLK)
    (add_net SPI0_SCLK_5)
    (add_net SPI1_CS0)
    (add_net SPI1_CS0_5)
    (add_net SPI1_MISO)
    (add_net SPI1_MOSI)
    (add_net SPI1_MOSI_5)
    (add_net SPI1_SCLK)
    (add_net SPI1_SCLK_5)
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E858C9)
    (at 135.255 141.605)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.27) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 HAT_SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E858D0)
    (at 135.89 149.225 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 138.43 122.555)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58E85862)
    (at 143.51 120.65 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E85860)
    (at 143.51 122.555 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E858A1)
    (at 135.89 138.43 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 1.905 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E85852)
    (at 135.89 118.745)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 1.27) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58E85816)
    (at 134.62 110.49 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value "red LED" (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SMC_Standard (layer F.Cu) (tedit 58E8580D)
    (at 146.685 102.235)
    (descr "Diode SMC Standard = DO-214AB")
    (tags "Diode SMC Standard DO-214AB")
    (zone_connect 2)
    (attr smd)
    (fp_text reference D2 (at -5.715 2.54 270) (layer F.SilkS))
    (fp_text value SK520TR (at 0 5.08) (layer F.Fab))
    (pad 1 smd rect (at -3.4 0 90) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V) (zone_connect 2))
    (pad 2 smd rect (at 3.4 0 90) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2))
    (model Diodes_SMD.3dshapes/D_SMC_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS_smt_std:resistor_smt_2920 (layer F.Cu) (tedit 58E85811)
    (at 146.685 109.22)
    (zone_connect 2)
    (fp_text reference F1 (at -5.715 2.54 90) (layer F.SilkS))
    (fp_text value "2.5A 0ZCF0250FF2C" (at 0 4) (layer F.Fab))
    (pad 2 smd rect (at 3.7 0) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(F1-Pad2)") (zone_connect 2))
    (pad 1 smd rect (at -3.7 0) (size 2.3 5.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V) (zone_connect 2))
  )
  (module PJS-icons:metroid (layer F.Cu) (tedit 590FD773)
    (at 135.89 153.035 180)
    (fp_text reference icon1 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value Metroid (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad "" smd circle (at -0.635 0 180) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0.635 0 180) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0 -0.635 180) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x20_Pitch2.54mm (layer B.Cu) (tedit 58E857C2)
    (at 128.27 105.41 180)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference P1 (at 2.54 0.635 270) (layer B.SilkS))
    (fp_text value CONN_02X20 (at -1.27 -50.59 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GPIO4))
    (pad 8 thru_hole oval (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GPIO17))
    (pad 12 thru_hole oval (at -2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad16)"))
    (pad 17 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 18 thru_hole oval (at -2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(P1-Pad18)"))
    (pad 19 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 SPI0_MOSI))
    (pad 20 thru_hole oval (at -2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 SPI0_MISO))
    (pad 22 thru_hole oval (at -2.54 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(P1-Pad22)"))
    (pad 23 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 SPI0_SCLK))
    (pad 24 thru_hole oval (at -2.54 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 SPI0_CS0))
    (pad 25 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(P1-Pad26)"))
    (pad 27 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 HAT_SDA))
    (pad 28 thru_hole oval (at -2.54 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 HAT_SCL))
    (pad 29 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(P1-Pad29)"))
    (pad 30 thru_hole oval (at -2.54 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 31 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(P1-Pad31)"))
    (pad 32 thru_hole oval (at -2.54 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(P1-Pad32)"))
    (pad 33 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(P1-Pad33)"))
    (pad 34 thru_hole oval (at -2.54 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 35 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 SPI1_MISO))
    (pad 36 thru_hole oval (at -2.54 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 SPI1_CS0))
    (pad 37 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad37)"))
    (pad 38 thru_hole oval (at -2.54 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 SPI1_MOSI))
    (pad 39 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole oval (at -2.54 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 SPI1_SCLK))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01_Pitch2.54mm (layer F.Cu) (tedit 58E858E6)
    (at 139.7 149.225)
    (descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x01 2.54mm double row")
    (fp_text reference P2 (at -1.27 1.905) (layer F.SilkS))
    (fp_text value no_pop (at 1.27 2.33) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x01_Pitch2.54mm.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_4pol (layer F.Cu) (tedit 58E8587E)
    (at 150.495 115.57 270)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P3 (at 8.255 3.81 270) (layer F.SilkS))
    (fp_text value ED10563-ND (at 3.81 4.50088 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 43 "Net-(P3-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 5 "Net-(F1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 44 "Net-(P3-Pad3)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_4pol.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_4pol (layer F.Cu) (tedit 58E8587B)
    (at 150.495 126.365 270)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P4 (at 8.255 3.81 270) (layer F.SilkS))
    (fp_text value ED10563-ND (at 3.81 4.50088 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 36 SPI0_MOSI_5))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 35 SPI0_SCLK_5))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_4pol.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_4pol (layer F.Cu) (tedit 58E85877)
    (at 150.495 137.16 270)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P5 (at 8.255 3.81 270) (layer F.SilkS))
    (fp_text value ED10563-ND (at 3.81 4.50088 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 39 SPI1_SCLK_5))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 37 SPI0_CS0_5))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 45 "Net-(P5-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_4pol.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_4pol (layer F.Cu) (tedit 58E85875)
    (at 150.495 147.955 270)
    (descr "4-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P6 (at 8.255 3.81 270) (layer F.SilkS))
    (fp_text value ED10563-ND (at 3.81 4.50088 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 41 "Net-(P6-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 40 SPI1_MOSI_5))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 38 SPI1_CS0_5))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_4pol.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E858C3)
    (at 135.255 146.05)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.27) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E858BF)
    (at 135.255 144.145)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.27) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 HAT_SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E8589A)
    (at 137.16 135.89)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 SPI1_CS0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E8588D)
    (at 133.985 127 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.905 0 360) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E85897)
    (at 135.255 131.445 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R5-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E85892)
    (at 135.89 127 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.905 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 SPI0_CS0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E85814)
    (at 137.795 110.49 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E858B1)
    (at 144.145 136.525 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(P5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 139.7 113.665 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(P3-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E858B3)
    (at 144.145 140.335 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(P6-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E8581D)
    (at 139.7 117.475 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P3-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 58E8585D)
    (at 140.97 128.905)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -4.445 -4.445) (layer F.SilkS))
    (fp_text value CD4504B (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 SPI0_MOSI_5))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 SPI0_MOSI))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 SPI0_CS0_5))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 SPI0_CS0))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 SPI1_MOSI_5))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 SPI1_MOSI))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 SPI1_SCLK))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 SPI1_SCLK_5))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 SPI1_CS0))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 SPI1_CS0_5))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R5-Pad2)"))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 SPI0_SCLK))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 SPI0_SCLK_5))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58E858DF)
    (at 140.97 144.78 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 1.27 3.175 180) (layer F.SilkS))
    (fp_text value no_pop (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 HAT_SDA))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 HAT_SCL))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P2-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS-mounting:MountingHole_2-7mm (layer F.Cu) (tedit 58E6F6F8)
    (at 129.54 158.54)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference MH (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-7mm_RevA_Date21Jun2010 (at 0.09906 3.59918) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.70002 2.70002) (drill 2.70002) (layers *.Cu *.Mask F.SilkS))
  )
  (module PJS-mounting:MountingHole_2-7mm (layer F.Cu) (tedit 58E6F6A0)
    (at 129.54 100.54)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference MH (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-7mm_RevA_Date21Jun2010 (at 0.09906 3.59918) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.70002 2.70002) (drill 2.70002) (layers *.Cu *.Mask F.SilkS))
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 58CE4E7F)
    (at 140.97 138.43 180)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U3 (at 0 -2 180) (layer F.SilkS))
    (fp_text value NL27WZ17 (at 0 2 360) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(P6-Pad4)"))
    (pad 3 smd rect (at -0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(P5-Pad2)"))
    (pad 5 smd rect (at 0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 SPI0_MISO))
    (pad 6 smd rect (at 0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 SPI1_MISO))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 58CE4E7F)
    (at 136.525 115.57 180)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U4 (at 0 -2 180) (layer F.SilkS))
    (fp_text value no_pop (at 0 2 360) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P3-Pad4)"))
    (pad 3 smd rect (at -0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(P3-Pad3)"))
    (pad 5 smd rect (at 0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -0.95 0 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.95 0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 GPIO4))
    (pad 6 smd rect (at 0.95 -0.65 180) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO17))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Copyright (c) 2017 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 17.78 179.07) (layer F.Mask))
  (gr_text "Copyright (c) 2017 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 17.78 179.07) (layer B.Mask))
  (gr_text "Copyright (c) 2017 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 17.78 179.07) (layer B.SilkS))
  (gr_text "Copyright (c) 2017 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 17.78 179.07) (layer F.SilkS))
  (gr_text "Copyright (c) 2017 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 17.78 179.07) (layer B.Cu))
  (gr_text "Copyright (c) 2017 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 17.78 179.07) (layer F.Cu))
  (gr_text +5V (at 152.4 115.57 90) (layer F.SilkS))
  (gr_text Gnd (at 152.4 147.955 90) (layer F.SilkS))
  (gr_text Gnd (at 152.4 142.24 90) (layer F.SilkS))
  (gr_text Gnd (at 152.4 131.445 90) (layer F.SilkS))
  (gr_text Gnd (at 152.4 126.365 90) (layer F.SilkS))
  (gr_text Gnd (at 152.4 118.11 90) (layer F.SilkS))
  (gr_text io4 (at 152.4 120.65 90) (layer F.SilkS))
  (gr_text io17 (at 152.4 123.19 90) (layer F.SilkS))
  (gr_text 0clk (at 152.4 128.905 90) (layer F.SilkS))
  (gr_text 0mosi (at 152.4 133.985 90) (layer F.SilkS))
  (gr_text 0cs (at 152.4 137.16 90) (layer F.SilkS))
  (gr_text 0miso (at 152.4 139.7 90) (layer F.SilkS))
  (gr_text 1clk (at 152.4 144.78 90) (layer F.SilkS))
  (gr_text 1mosi (at 152.4 150.495 90) (layer F.SilkS))
  (gr_text 1cs (at 152.4 153.035 90) (layer F.SilkS))
  (gr_text 1miso (at 152.4 155.575 90) (layer F.SilkS))
  (gr_text 1miso (at 152.4 155.575 90) (layer B.SilkS))
  (gr_text 1cs (at 152.4 153.035 90) (layer B.SilkS))
  (gr_text 1mosi (at 152.4 150.495 90) (layer B.SilkS))
  (gr_text 1clk (at 152.4 144.78 90) (layer B.SilkS))
  (gr_text 0miso (at 152.4 139.7 90) (layer B.SilkS))
  (gr_text 0cs (at 152.4 137.16 90) (layer B.SilkS))
  (gr_text 0mosi (at 152.4 133.985 90) (layer B.SilkS))
  (gr_text 0clk (at 152.4 128.905 90) (layer B.SilkS))
  (gr_text io17 (at 152.4 123.19 90) (layer B.SilkS))
  (gr_text io4 (at 152.4 120.65 90) (layer B.SilkS))
  (gr_text Gnd (at 152.4 147.955 90) (layer B.SilkS))
  (gr_text Gnd (at 152.4 142.24 90) (layer B.SilkS))
  (gr_text Gnd (at 152.4 131.445 90) (layer B.SilkS))
  (gr_text Gnd (at 152.4 126.365 90) (layer B.SilkS))
  (gr_text Gnd (at 152.4 118.11 90) (layer B.SilkS))
  (gr_text +5V (at 152.4 115.57 90) (layer B.SilkS))
  (gr_text "PJS 08MAY2017" (at 146.05 161.29) (layer B.SilkS))
  (gr_text "Pi to 5V SPI breakout\nMIT licence " (at 142.875 160.02) (layer F.SilkS))
  (gr_line (start 124.46 162.56) (end 124.46 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 162.56) (end 124.46 162.56) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.67 96.52) (end 153.67 162.56) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.46 96.52) (end 153.67 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 66.04 (width 0.3) (layer F.Fab)
    (gr_text "2.6000 in" (at 162.005 129.54 90) (layer F.Fab))
    (feature1 (pts (xy 153.67 96.52) (xy 163.355 96.52)))
    (feature2 (pts (xy 153.67 162.56) (xy 163.355 162.56)))
    (crossbar (pts (xy 160.655 162.56) (xy 160.655 96.52)))
    (arrow1a (pts (xy 160.655 96.52) (xy 161.241421 97.646504)))
    (arrow1b (pts (xy 160.655 96.52) (xy 160.068579 97.646504)))
    (arrow2a (pts (xy 160.655 162.56) (xy 161.241421 161.433496)))
    (arrow2b (pts (xy 160.655 162.56) (xy 160.068579 161.433496)))
  )
  (dimension 29.21 (width 0.3) (layer F.Fab)
    (gr_text "1.1500 in" (at 139.065 168.99) (layer F.Fab))
    (feature1 (pts (xy 153.67 162.56) (xy 153.67 170.34)))
    (feature2 (pts (xy 124.46 162.56) (xy 124.46 170.34)))
    (crossbar (pts (xy 124.46 167.64) (xy 153.67 167.64)))
    (arrow1a (pts (xy 153.67 167.64) (xy 152.543496 168.226421)))
    (arrow1b (pts (xy 153.67 167.64) (xy 152.543496 167.053579)))
    (arrow2a (pts (xy 124.46 167.64) (xy 125.586504 168.226421)))
    (arrow2b (pts (xy 124.46 167.64) (xy 125.586504 167.053579)))
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 96.52) (xy 153.67 96.52) (xy 153.67 162.56) (xy 124.46 162.56) (xy 124.46 159.385)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.46 96.52) (xy 153.67 96.52) (xy 153.67 162.56) (xy 124.46 162.56) (xy 124.46 159.385)
      )
    )
  )
  (zone (net 3) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 146.685 113.03) (xy 137.795 113.03) (xy 137.795 109.22) (xy 129.54 109.22) (xy 129.54 103.505)
        (xy 137.795 103.505) (xy 137.795 99.695) (xy 146.685 99.695)
      )
    )
  )
)
