(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 197)
    (zones 0)
    (modules 50)
    (nets 23)
  )
  (page A4)
  (title_block
    (date 2019-10-27)
    (rev 04)
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.762)
    (via_min_drill 0.381)
    (uvia_size 0.762)
    (uvia_drill 0.381)
    (uvias_allowed no)
    (uvia_min_size 0.762)
    (uvia_min_drill 0.381)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.200001 3.200001)
    (pad_drill 3.200001)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 /v2)
  (net 3 GND)
  (net 4 +15V)
  (net 5 "Net-(C7-Pad2)")
  (net 6 -15V)
  (net 7 "Net-(C15-Pad2)")
  (net 8 "Net-(C15-Pad1)")
  (net 9 "Net-(D1-Pad1)")
  (net 10 "Net-(D1-Pad2)")
  (net 11 "Net-(J2-Pad2)")
  (net 12 /dU)
  (net 13 "Net-(J6-Pad2)")
  (net 14 "Net-(R1-Pad1)")
  (net 15 /v1)
  (net 16 "Net-(R10-Pad2)")
  (net 17 "Net-(R10-Pad1)")
  (net 18 "Net-(R11-Pad3)")
  (net 19 "Net-(R6-Pad1)")
  (net 20 "Net-(J10-Pad1)")
  (net 21 "Net-(R5-Pad1)")
  (net 22 "Net-(J10-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net /dU)
    (add_net /v1)
    (add_net /v2)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J10-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad3)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
  )
  (net_class +15V ""
    (clearance 0.254)
    (trace_width 1.016)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net +15V)
  )
  (net_class -15V ""
    (clearance 0.254)
    (trace_width 1.016)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net -15V)
  )
  (net_class GND ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.381)
    (add_net GND)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 180.848 104.902)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -3.683 -3.175) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5DB286BE)
    (at 114.554 132.842)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -1.7145 -3.683) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.200001 3.200001) (drill 3.200001) (layers *.Cu *.Mask))
  )
  (module FootPrints:AttractorLogo (layer F.Cu) (tedit 0)
    (at 153.924 133.35)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 1.016 -0.254) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 180.34 133.604)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -4.318 3.1115) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 114.554 104.902)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -2.0955 4.1275) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 136.153 126.746 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 2.6996 -0.0262 90) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 /v2))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 134.121 129.032)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 2.6906 0.0418 90) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 /v2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.794 125.231 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -0.263 1.524 90) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 -15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 135.89 115.561 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -0.499 -1.778 90) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 143.002 124.215 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -0.0635 1.5875 90) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 -15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 148.844 114.545 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +15V))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 133.35 111.243 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 135.382 111.243 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 1.651 90) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 164.4052 121.031)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at -0.1035 1.861) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 -15V))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 169.164 112.259 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 120.396 112.0505 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at -3.0845 0 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 122.682 112.522 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C12 (at -2.54 -0.508 180) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +15V))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 120.396 120.9405 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C13 (at -3.0845 0.254 180) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 -15V))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 122.682 120.387 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C14 (at -2.785 1.016 180) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 -15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 170.18 120.904 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C15 (at -3.1604 0.044) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(C15-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 170.171 122.936 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C16 (at -3.1514 -0.0068) (layer F.SilkS))
    (fp_text value .1uf (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C15-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF_Handsoldering (layer F.Cu) (tedit 5905D919)
    (at 160.441 117.856 270)
    (descr "Diode Mini-MELF Handsoldering")
    (tags "Diode Mini-MELF Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0.0635 -0.0235 90) (layer F.SilkS))
    (fp_text value LL4148 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2.75 0 270) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2.75 0 270) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FootPrints:CHAOS_3POS_TER (layer F.Cu) (tedit 0)
    (at 112.522 113.792 90)
    (fp_text reference J1 (at -5 0 90) (layer F.SilkS))
    (fp_text value 796689-3 (at -4.572 -5.334 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -10 0 90) (size 1.905 1.905) (drill 1.397) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -5 0 90) (size 1.905 1.905) (drill 1.397) (layers *.Cu *.Mask)
      (net 6 -15V))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.905 1.905) (drill 1.397) (layers *.Cu *.Mask)
      (net 4 +15V))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 136.144 124.46 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.7906 0.0058 90) (layer F.SilkS))
    (fp_text value 2k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 "Net-(R1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 /v2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 129.531 129.032)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0.0006 1.6418) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 125.984 118.872)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 1.778) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 /v1))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 125.975 116.84)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 /v1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 150.876 122.564 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 1.007 -1.651 90) (layer F.SilkS))
    (fp_text value 3k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 "Net-(R5-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 /v1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 147.5 126.5 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 3.04 -0.074 90) (layer F.SilkS))
    (fp_text value 3k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 "Net-(R6-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 /v2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 149.75 126.525 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at -2.761 0.11 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 153.162 120.514 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 "Net-(R5-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 /dU))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 140.462 121.412 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0.064 -1.6295 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 "Net-(J6-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 140.462 117.357 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 "Net-(R10-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FootPrints:CHAOS_2k_TRIM_POT (layer F.Cu) (tedit 0)
    (at 140.208 132.08 180)
    (fp_text reference R11 (at -0.254 -1.524) (layer F.SilkS))
    (fp_text value "64WR2KLF (2k POT)" (at -2.772 -1.524) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 3.175 180) (size 1.2192 1.2192) (drill 0.7112) (layers *.Cu *.Mask)
      (net 17 "Net-(R10-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0.635 180) (size 1.2192 1.2192) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at 0 3.175 180) (size 1.2192 1.2192) (drill 0.7112) (layers *.Cu *.Mask)
      (net 18 "Net-(R11-Pad3)"))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 158.155 118.916 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 953 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(C15-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 "Net-(J10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 171.363 116.9385 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at 0.1555 -1.865 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C15-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 161.25 123.75 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FootPrints:CHAOS_OPAMP_TL082CDR (layer F.Cu) (tedit 0)
    (at 132.588 120.396)
    (fp_text reference U1 (at -1.524 -3.556) (layer F.SilkS))
    (fp_text value TL082 (at 1.016 -3.302) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -3.048 -4.064) (layer F.SilkS))
    (fp_text user * (at -1.6129 -2.4257) (layer F.Fab))
    (pad 1 smd rect (at -2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 /v2))
    (pad 2 smd rect (at -2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R1-Pad1)"))
    (pad 3 smd rect (at -2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad2)"))
    (pad 4 smd rect (at -2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 6 -15V))
    (pad 5 smd rect (at 2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 smd rect (at 2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R1-Pad1)"))
    (pad 7 smd rect (at 2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 15 /v1))
    (pad 8 smd rect (at 2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
  )
  (module FootPrints:CHAOS_OPAMP_TL082CDR (layer F.Cu) (tedit 0)
    (at 145.542 119.38)
    (fp_text reference U2 (at -1.778 -3.556) (layer F.SilkS))
    (fp_text value TL082 (at 1.016 -3.302) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 2.9718 -0.127) (layer Cmts.User))
    (fp_text user * (at -3.302 -4.318) (layer F.SilkS))
    (fp_text user * (at -1.6129 -2.4257) (layer F.Fab))
    (pad 1 smd rect (at -2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R10-Pad2)"))
    (pad 2 smd rect (at -2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R10-Pad1)"))
    (pad 3 smd rect (at -2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J6-Pad2)"))
    (pad 4 smd rect (at -2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 6 -15V))
    (pad 5 smd rect (at 2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R6-Pad1)"))
    (pad 6 smd rect (at 2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R5-Pad1)"))
    (pad 7 smd rect (at 2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 12 /dU))
    (pad 8 smd rect (at 2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
  )
  (module FootPrints:CHAOS_OPAMP_TL082CDR (layer F.Cu) (tedit 0)
    (at 165.9782 116.884)
    (fp_text reference U3 (at -1.3862 -3.6) (layer F.SilkS))
    (fp_text value TL082 (at 1.1538 -3.092) (layer F.SilkS))
    (fp_text user * (at -1.6129 -2.4257) (layer F.Fab))
    (fp_text user * (at -2.9102 -4.108) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 8 smd rect (at 2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 4 +15V))
    (pad 7 smd rect (at 2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C15-Pad1)"))
    (pad 6 smd rect (at 2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C15-Pad2)"))
    (pad 5 smd rect (at 2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 6 -15V))
    (pad 3 smd rect (at -2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J10-Pad2)"))
    (pad 2 smd rect (at -2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
  )
  (module FootPrints:CHAOS_2PIN_100mil_HD (layer F.Cu) (tedit 0)
    (at 127 104.648 270)
    (fp_text reference J2 (at 2.069 -2.2066 90) (layer F.SilkS))
    (fp_text value TSW-102-07-F-S (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J10-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad2)"))
  )
  (module FootPrints:CHAOS_2PIN_100mil_HD (layer F.Cu) (tedit 0)
    (at 134.62 104.648 270)
    (attr virtual)
    (fp_text reference J3 (at 2.3738 -2.2986 90) (layer F.SilkS))
    (fp_text value TSW-102-07-F-S (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0.508 -0.254 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J10-Pad1)"))
  )
  (module FootPrints:CHAOS_2PIN_100mil_HD (layer F.Cu) (tedit 0)
    (at 181.864 123.444 270)
    (fp_text reference J4 (at -2.2733 -2.1971 90) (layer F.SilkS))
    (fp_text value TSW-102-07-F-S (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J10-Pad1)"))
  )
  (module FootPrints:CHAOS_2PIN_100mil_HD (layer F.Cu) (tedit 0)
    (at 181.864 114.3 270)
    (fp_text reference J5 (at -3.244 -2.1796 90) (layer F.SilkS))
    (fp_text value TSW-102-07-F-S (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0.762 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J10-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module FootPrints:CHAOS_2PIN_100mil_HD (layer F.Cu) (tedit 0)
    (at 142.24 104.648 270)
    (fp_text reference J6 (at 2.4246 -2.289 90) (layer F.SilkS))
    (fp_text value TSW-102-07-F-S (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J10-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(J6-Pad2)"))
  )
  (module FootPrints:CHAOS_2PIN_100mil_HD (layer F.Cu) (tedit 0)
    (at 169.164 104.648 270)
    (fp_text reference J7 (at 2.271 -2.2762 90) (layer F.SilkS))
    (fp_text value TSW-102-07-F-S (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J10-Pad1)"))
  )
  (module FootPrints:CHAOS_2PIN_100mil_HD (layer F.Cu) (tedit 0)
    (at 164.338 133.604 270)
    (fp_text reference J8 (at 0 0 90) (layer F.SilkS))
    (fp_text value TSW-102-07-F-S (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /dU))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module FootPrints:CHAOS_2PIN_100mil_HD (layer F.Cu) (tedit 0)
    (at 160.274 104.648 270)
    (fp_text reference J9 (at 2.2714 -2.4386 90) (layer F.SilkS))
    (fp_text value TSW-102-07-F-S (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J10-Pad1)"))
  )
  (module FootPrints:CHAOS_2PIN_100mil_HD (layer F.Cu) (tedit 0)
    (at 150.114 104.648 270)
    (fp_text reference J10 (at 1.9928 -2.508 90) (layer F.SilkS))
    (fp_text value TSW-102-07-F-S (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User))
    (fp_text user * (at 0 0 90) (layer F.SilkS))
    (fp_text user * (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J10-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(J10-Pad2)"))
  )
  (module TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 170.18 135.128)
    (descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 -2.398) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (gr_text GND (at 160.02 134.874) (layer F.SilkS))
  (gr_text du (at 159.766 132.08) (layer F.SilkS))
  (gr_text GND (at 177.546 124.714) (layer F.SilkS))
  (gr_text "Vu\n" (at 178.054 122.428) (layer F.SilkS))
  (gr_text GND (at 177.546 115.57) (layer F.SilkS))
  (gr_text Vu (at 178.054 113.284) (layer F.SilkS))
  (gr_text GND (at 164.846 106.68) (layer F.SilkS))
  (gr_text Vu (at 165.1 103.886) (layer F.SilkS))
  (gr_text GND (at 156.21 106.426) (layer F.SilkS))
  (gr_text "Vu\n" (at 156.464 103.632) (layer F.SilkS))
  (gr_text "Folding\nCircuit\n" (at 150.368 109.474) (layer F.SilkS))
  (gr_text "Negative\nResistor" (at 142.748 109.474) (layer F.SilkS))
  (gr_text Capacitor (at 134.874 108.458) (layer F.SilkS))
  (gr_text Inductor (at 127.254 108.458) (layer F.SilkS))
  (gr_text GND (at 120.65 125.73) (layer F.SilkS))
  (gr_text "-15V\n" (at 121.158 117.856) (layer F.SilkS))
  (gr_text +15V (at 121.412 115.316) (layer F.SilkS))
  (gr_text -15V (at 116.332 118.872) (layer B.CrtYd))
  (gr_text GND (at 116.332 123.698) (layer B.CrtYd))
  (gr_text "+15V\n" (at 116.332 113.792) (layer B.CrtYd))
  (gr_curve (pts (xy 185.26829 133.423556) (xy 185.26829 135.915694) (xy 183.261984 137.922) (xy 180.769846 137.922)) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 113.792 100.047264) (end 180.769846 100.047264) (layer Edge.Cuts) (width 0.4))
  (gr_curve (pts (xy 180.769846 100.047264) (xy 183.261984 100.047264) (xy 185.26829 102.05357) (xy 185.26829 104.545708)) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 185.26829 104.545708) (end 185.26829 133.423556) (layer Edge.Cuts) (width 0.4))
  (gr_curve (pts (xy 109.293556 104.545708) (xy 109.293556 102.05357) (xy 111.299862 100.047264) (xy 113.792 100.047264)) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 113.792 100.047264) (end 113.792 100.047264) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 109.293556 133.423556) (end 109.293556 104.545708) (layer Edge.Cuts) (width 0.4))
  (gr_line (start 180.769846 137.922) (end 113.792 137.922) (layer Edge.Cuts) (width 0.4))
  (gr_curve (pts (xy 113.792 137.922) (xy 111.299862 137.922) (xy 109.293556 135.915694) (xy 109.293556 133.423556)) (layer Edge.Cuts) (width 0.4))
  (gr_text "Team Controlled Chaos" (at 133.604 135.636) (layer F.SilkS))
  (gr_line (start 116.519339 102.041337) (end 116.519339 102.041337) (layer Edge.Cuts) (width 0.18288))
  (zone (net 4) (net_name +15V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1.524))
    (polygon
      (pts
        (xy 111.252 115.57) (xy 131.826 115.824) (xy 133.096 118.872) (xy 137.668 119.126) (xy 154.686 118.364)
        (xy 174.752 116.332) (xy 185.166 115.062) (xy 185.166 103.886) (xy 184.658 102.362) (xy 183.134 100.838)
        (xy 181.61 100.076) (xy 175.768 100.076) (xy 116.332 99.822) (xy 112.522 100.33) (xy 111.506 100.838)
        (xy 110.236 101.854) (xy 109.728 103.124) (xy 109.474 104.394) (xy 109.474 106.172) (xy 109.474 115.57)
      )
    )
  )
  (zone (net 6) (net_name -15V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1.524))
    (polygon
      (pts
        (xy 123.19 116.84) (xy 130.302 117.094) (xy 132.334 120.65) (xy 152.4 120.65) (xy 166.37 118.364)
        (xy 184.15 116.586) (xy 185.166 116.84) (xy 185.166 133.858) (xy 184.912 135.382) (xy 183.896 136.398)
        (xy 182.626 137.414) (xy 180.848 137.922) (xy 113.03 137.668) (xy 111.76 137.414) (xy 110.49 136.398)
        (xy 109.474 135.382) (xy 109.22 133.604) (xy 109.22 116.586) (xy 110.236 116.586)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118.872 100.076) (xy 179.324 100.076) (xy 181.102 100.076) (xy 182.372 100.33) (xy 183.388 100.838)
        (xy 184.404 101.854) (xy 184.912 103.124) (xy 185.42 104.648) (xy 185.166 133.35) (xy 184.912 135.128)
        (xy 183.896 136.906) (xy 182.626 137.668) (xy 113.284 137.922) (xy 111.252 137.414) (xy 109.982 136.144)
        (xy 109.474 134.366) (xy 109.22 133.604) (xy 109.474 103.124) (xy 109.728 102.362) (xy 110.49 101.346)
        (xy 111.252 100.838) (xy 112.014 100.584) (xy 113.538 100.076)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.792 100.076) (xy 180.594 100.076) (xy 181.864 100.33) (xy 183.134 100.838) (xy 183.896 101.346)
        (xy 184.658 102.362) (xy 185.166 103.378) (xy 185.42 104.14) (xy 185.166 133.35) (xy 185.166 134.366)
        (xy 184.912 134.874) (xy 184.658 135.636) (xy 183.896 136.652) (xy 183.134 137.414) (xy 181.864 137.668)
        (xy 181.102 137.922) (xy 113.538 137.922) (xy 111.76 137.414) (xy 110.49 136.652) (xy 109.474 135.128)
        (xy 109.22 134.112) (xy 109.474 103.632) (xy 109.728 102.362) (xy 110.744 101.346) (xy 111.252 100.838)
        (xy 112.268 100.33) (xy 113.538 100.076) (xy 113.284 100.076) (xy 113.538 100.076)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.848 137.922) (xy 113.538 137.922) (xy 112.268 137.414) (xy 110.49 136.652) (xy 109.728 134.874)
        (xy 109.22 133.604) (xy 109.22 103.886) (xy 109.474 103.124) (xy 110.236 101.6) (xy 111.506 100.584)
        (xy 113.03 100.076) (xy 114.046 100.076) (xy 180.848 100.076) (xy 182.372 100.33) (xy 183.642 101.092)
        (xy 184.15 101.6) (xy 184.658 102.362) (xy 185.166 103.632) (xy 185.166 104.394) (xy 185.166 133.35)
        (xy 184.912 134.874) (xy 184.658 135.89) (xy 183.896 136.652) (xy 182.88 137.414) (xy 181.864 137.922)
        (xy 181.102 137.922)
      )
    )
  )
)
