(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 39)
    (zones 0)
    (modules 9)
    (nets 11)
  )
  (page User 165.1 127)
  (title_block
    (date 2019-02-14)
    (rev "Ver 1.1")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (user_trace_width 1.4986)
    (trace_clearance 0.2)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(B1-Pad4)")
  (net 2 "Net-(B1-Pad2)")
  (net 3 "Net-(B1-Pad3)")
  (net 4 "Net-(B1-Pad1)")
  (net 5 "Net-(J1-Pad1)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "Net-(R1-Pad1)")
  (net 9 "Net-(R1-Pad2)")
  (net 10 "Net-(RV1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B1-Pad2)")
    (add_net "Net-(B1-Pad3)")
    (add_net "Net-(B1-Pad4)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(RV1-Pad3)")
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294E91)
    (at 18.161 25.4 270)
    (descr "Terminal Block 4Ucon ItemNo. 20193, 3 pins, pitch 3.5mm, size 11.2x7mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.4uconnector.com/online/object/4udrawing/20193.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 20193 pitch 3.5mm size 11.2x7mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J1 (at 5.08 -2.54) (layer F.SilkS))
    (fp_text value Conn (at 3.302 2.794 270) (layer F.Fab))
    (fp_text user %R (at 5.08 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(B1-Pad4)"))
    (pad 3 thru_hole circle (at 7 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:Diode_Bridge_DIP-4_W7.62mm_P5.08mm (layer F.Cu) (tedit 5C65954C)
    (at 31.115 29.591 180)
    (descr "4-lead dip package for diode bridges, row spacing 7.62 mm (300 mils), see http://cdn-reichelt.de/documents/datenblatt/A400/HDBL101G_20SERIES-TSC.pdf")
    (tags "DIL DIP PDIP 5.08mm 7.62mm 300mil")
    (fp_text reference B1 (at 3.81 5.588 180) (layer F.SilkS))
    (fp_text value DF005M-ND (at 3.81 2.54 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 5.588) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(B1-Pad4)"))
    (pad 2 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad2)"))
    (pad 3 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(B1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(B1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/Diode_Bridge_DIP-4_W7.62mm_P5.08mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 27.813 35.179 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.016 3.048) (layer F.SilkS))
    (fp_text value 470uF (at 1.778 -2.54) (layer F.Fab))
    (fp_text user %R (at 1.016 3.048) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(B1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294E91)
    (at 39.624 28.956 90)
    (descr "Terminal Block 4Ucon ItemNo. 19963, 2 pins, pitch 3.5mm, size 7.7x7mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see http://www.4uconnector.com/online/object/4udrawing/19963.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_4Ucon")
    (tags "THT Terminal Block 4Ucon ItemNo. 19963 pitch 3.5mm size 7.7x7mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J2 (at 1.778 -2.286 180) (layer F.SilkS))
    (fp_text value Conn (at 1.778 2.794 90) (layer F.Fab))
    (fp_text user %R (at 1.778 -2.286 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(B1-Pad2)"))
    (model ${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L6.6mm_D2.7mm_P2.54mm_Vertical_Vishay_IM-2 (layer F.Cu) (tedit 5C658B9A)
    (at 20.828 36.957 270)
    (descr "Inductor, Axial series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Vertical pin pitch 2.54mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (fp_text reference L1 (at 4.572 0.127) (layer F.SilkS))
    (fp_text value 22uh (at 4.064 -0.254) (layer F.Fab) hide)
    (fp_text user %R (at 4.572 0.127) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(B1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P2.54mm_Vertical_Vishay_IM-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5C6594EA)
    (at 34.036 31.369 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.715 0 -180) (layer F.SilkS))
    (fp_text value "27 Ohm" (at 4.318 0.254 -180) (layer F.Fab) hide)
    (fp_text user %R (at 5.715 0 -180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 41.021 40.767 270)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV1 (at 0.508 -1.778 270) (layer F.SilkS))
    (fp_text value "200 Ohm" (at -3.81 1.524 270) (layer F.Fab))
    (fp_text user %R (at -3.175 0.005 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at -5.08 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(RV1-Pad3)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Varistor:RV_Disc_D7mm_W4.5mm_P5mm (layer F.Cu) (tedit 5A0F68DF)
    (at 15.494 41.529 90)
    (descr "Varistor, diameter 7mm, width 4.5mm, pitch 5mm")
    (tags "varistor SIOV")
    (fp_text reference TH1 (at 3.81 -0.254 90) (layer F.SilkS))
    (fp_text value PTC (at 2.032 2.032 90) (layer F.Fab))
    (fp_text user %R (at 3.81 -0.254 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(B1-Pad4)"))
    (pad 2 thru_hole circle (at 5 2.1 90) (size 1.6 1.6) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Varistor.3dshapes/RV_Disc_D7mm_W4.5mm_P5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:TO-220-3 (layer F.Cu) (tedit 5C65897A)
    (at 35.687 40.513 90)
    (descr http://www.st.com/content/ccc/resource/technical/document/datasheet/f9/ed/f5/44/26/b9/43/a4/CD00000911.pdf/files/CD00000911.pdf/jcr:content/translations/en.CD00000911.pdf)
    (fp_text reference U1 (at 6.858 1.524 180) (layer F.SilkS))
    (fp_text value LM317T (at 2.286 -1.778 270) (layer F.Fab))
    (fp_text user %R (at 2.52 -0.01 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(B1-Pad1)"))
  )
  (gr_text "DC OUT" (at 42.418 27.305 90) (layer F.SilkS))
  (gr_text "AC INPUT" (at 15.367 28.448 90) (layer F.SilkS))
  (gr_text CR2 (at 15.494 32.512) (layer B.SilkS))
  (gr_text CR1 (at 15.494 28.956) (layer B.SilkS))
  (gr_text WHS (at 15.621 25.4) (layer B.SilkS))
  (gr_text "AC INPUT" (at 20.828 28.448 90) (layer B.SilkS))
  (gr_text "Ver 1.1\n2019-02-14\nL=1.20 W=.84" (at 27.686 26.543) (layer B.SilkS))
  (gr_text "LED Constant Current Circuit PCB-GregM" (at 31.242 42.418) (layer B.SilkS))
  (gr_line (start 13.716 22.352) (end 13.716 43.434) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 43.942 43.434) (end 13.716 43.434) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 43.942 22.352) (end 43.942 43.434) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 43.942 22.352) (end 13.716 22.352) (layer Edge.Cuts) (width 0.15))
  (gr_text + (at 37.465 28.829) (layer B.SilkS))
  (gr_text - (at 37.338 25.146) (layer B.SilkS))
  (gr_text "DC OUT" (at 42.418 27.432 90) (layer B.SilkS))
  (gr_text DF005-ND (at 27.305 27.051) (layer F.SilkS))
  (gr_text "27\nOhm" (at 34.036 28.702) (layer F.SilkS))
  (gr_text + (at 37.084 28.956) (layer F.SilkS))
  (gr_text - (at 37.338 25.146) (layer F.SilkS))
  (gr_text - (at 29.21 24.511) (layer F.SilkS))
  (gr_text ~ (at 24.384 31.75) (layer F.SilkS))
  (gr_text ~ (at 24.638 32.004) (layer F.SilkS))
  (gr_text + (at 29.464 29.464) (layer F.SilkS))
  (gr_text ~ (at 24.384 31.75) (layer F.SilkS))
  (gr_text ~ (at 24.384 32.004) (layer F.SilkS))
  (gr_text ~ (at 24.384 32.004) (layer F.SilkS))
  (zone (net 2) (net_name "Net-(B1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.196 22.098) (xy 44.196 43.688) (xy 24.511 43.815) (xy 24.511 21.971)
      )
    )
  )
)
