<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>Floral Bonnet V1.0
John 'Warthog9' Hawley
(C) 2021 CC-BY-SA 4.0</text>
<text>5V</text>
<text>GND</text>
<text>TX</text>
<text>RX</text>
<text>DTR</text>
<text>3.3V</text>
<text>5V</text>
<text>GND</text>
<text>TX</text>
<text>RX</text>
<text>DTR</text>
<text>3.3V</text>
<text>github.com/unreproducible/bonnet_floral</text>
</plain>
<libraries>
<library name="Raspberry_Pi_Zero_W_(v1.3)">
<description>&lt;Raspberry Pi Zero W (v1.3) Single-board Computers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="RASPBERRYPIZEROWV13-WOUT-RUNTV-NOMOUNT">
<description>&lt;b&gt;Raspberry Pi Zero W (v1.3)_1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-RGB-THRU@1">
<description>&lt;h3&gt;LED - RGB PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Area:5 x 5.8 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Datasheet Referenced: &lt;a href="https://www.sparkfun.com/datasheets/Components/YSL-R596CR3G4B5C-C10.pdf"&gt;YSL-R596CR3G4B5C&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED-RGB-CA&lt;/li&gt;
&lt;li&gt;LED-RGB-CC&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Artwork">
<packages>
<package name="FLORAL_SMALLER_MIRROR">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="Raspberry_Pi_Zero_W_(v1.3)" package="RASPBERRYPIZEROWV13-WOUT-RUNTV-NOMOUNT" value="RASPBERRY_PI_ZERO_W_(V1.3)-WOUT-RUNTVNOMOUNT"/>
<element name="UART" library="pinhead" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TSL2561" library="pinhead" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OLED_SCREEN" library="pinhead" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BME280" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-RGB-THRU@1" value="CLEAR">
<attribute name="PROD_ID" value="DIO-08418"/>
</element>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="SF_SKU" value="COM-00097"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="U$1" library="Artwork" package="FLORAL_SMALLER_MIRROR" value=""/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="IC1" pad="17-3.3V"/>
<contactref element="IC1" pad="1-3.3V"/>
<contactref element="TSL2561" pad="1"/>
<contactref element="BME280" pad="4"/>
<contactref element="OLED_SCREEN" pad="2"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="4-5V"/>
<contactref element="IC1" pad="2-5V"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="20-GND"/>
<contactref element="IC1" pad="30-GND"/>
<contactref element="IC1" pad="39-GND"/>
<contactref element="IC1" pad="9-GND"/>
<contactref element="IC1" pad="6-GND"/>
<contactref element="IC1" pad="25-GND"/>
<contactref element="IC1" pad="14-GND"/>
<contactref element="IC1" pad="34-GND"/>
<contactref element="UART" pad="5"/>
<contactref element="TSL2561" pad="2"/>
<contactref element="BME280" pad="3"/>
<contactref element="D1" pad="2"/>
<contactref element="OLED_SCREEN" pad="1"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="BTN_1">
<contactref element="IC1" pad="7-IO4"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="IO17">
<contactref element="IC1" pad="11-IO17"/>
</signal>
<signal name="IO27">
<contactref element="IC1" pad="13-IO27"/>
</signal>
<signal name="RGB_G">
<contactref element="IC1" pad="15-IO22"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="OLED_MOSI">
<contactref element="IC1" pad="19-IO10"/>
<contactref element="OLED_SCREEN" pad="4"/>
</signal>
<signal name="IO9">
<contactref element="IC1" pad="21-IO9"/>
</signal>
<signal name="OLED_CLK">
<contactref element="IC1" pad="23-IO11"/>
<contactref element="OLED_SCREEN" pad="3"/>
</signal>
<signal name="IO5">
<contactref element="IC1" pad="29-IO5"/>
</signal>
<signal name="IO6">
<contactref element="IC1" pad="31-IO6"/>
</signal>
<signal name="IO13">
<contactref element="IC1" pad="33-IO13"/>
</signal>
<signal name="IO19">
<contactref element="IC1" pad="35-IO19"/>
</signal>
<signal name="IO26">
<contactref element="IC1" pad="37-IO26"/>
</signal>
<signal name="IO18">
<contactref element="IC1" pad="12-IO18"/>
</signal>
<signal name="IO25">
<contactref element="IC1" pad="22-IO25"/>
</signal>
<signal name="IO7">
<contactref element="IC1" pad="26-IO7"/>
</signal>
<signal name="IO12">
<contactref element="IC1" pad="32-IO12"/>
</signal>
<signal name="IO16">
<contactref element="IC1" pad="36-IO16"/>
</signal>
<signal name="RGB_R">
<contactref element="IC1" pad="38-IO20"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="RGB_B">
<contactref element="IC1" pad="40-IO21"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="UART_DTR">
<contactref element="UART" pad="2"/>
</signal>
<signal name="UART_RXI">
<contactref element="UART" pad="3"/>
<contactref element="IC1" pad="8-IO14"/>
</signal>
<signal name="UART_TXO">
<contactref element="UART" pad="4"/>
<contactref element="IC1" pad="10-IO15"/>
</signal>
<signal name="I2C_SCL">
<contactref element="TSL2561" pad="3"/>
<contactref element="BME280" pad="2"/>
<contactref element="IC1" pad="5-IO3"/>
</signal>
<signal name="I2C_SDA">
<contactref element="TSL2561" pad="4"/>
<contactref element="BME280" pad="1"/>
<contactref element="IC1" pad="3-IO2"/>
</signal>
<signal name="TSL_INT">
<contactref element="TSL2561" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="1"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="4"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="3"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="OLED_RES">
<contactref element="OLED_SCREEN" pad="5"/>
<contactref element="IC1" pad="18-IO24"/>
</signal>
<signal name="OLED_DC">
<contactref element="OLED_SCREEN" pad="6"/>
<contactref element="IC1" pad="16-IO23"/>
</signal>
<signal name="OLED_CS">
<contactref element="OLED_SCREEN" pad="7"/>
<contactref element="IC1" pad="24-IO8"/>
</signal>
<signal name="UART_5V">
<contactref element="UART" pad="6"/>
</signal>
<signal name="UART_3.3V">
<contactref element="UART" pad="1"/>
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
