(kicad_pcb (version 4) (host pcbnew 4.0.2-4+6225~38~ubuntu14.04.1-stable)
  (general
    (links 28)
    (no_connects 0)
    (area 35.070238 27.125 76.550001 44.075)
    (thickness 2)
    (drawings 35)
    (tracks 141)
    (zones 0)
    (modules 16)
    (nets 29)
  )
  (page User 101.6 101.6)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.16)
    (user_trace_width 0.16)
    (user_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.508)
    (pad_to_mask_clearance 0.1)
    (pad_to_paste_clearance -0.003)
    (aux_axis_origin 36.15 42.6)
    (grid_origin 36.15 42.6)
    (visible_elements 7FFEFF3F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 /+5V)
  (net 2 "Net-(A1-Pad7)")
  (net 3 "Net-(A1-Pad6)")
  (net 4 "Net-(A1-Pad5)")
  (net 5 GND)
  (net 6 "Net-(A1-Pad3)")
  (net 7 "Net-(A1-Pad2)")
  (net 8 "Net-(A1-Pad1)")
  (net 9 /HD+)
  (net 10 /HD-)
  (net 11 "Net-(R1-Pad2)")
  (net 12 "Net-(Z1-Pad1)")
  (net 13 /C2CK)
  (net 14 /C2D)
  (net 15 /RX)
  (net 16 /TX)
  (net 17 "Net-(E0-Pad1)")
  (net 18 "Net-(E0-Pad10)")
  (net 19 "Net-(E0-Pad13)")
  (net 20 "Net-(E0-Pad15)")
  (net 21 "Net-(E0-Pad16)")
  (net 22 "Net-(E0-Pad17)")
  (net 23 "Net-(E0-Pad18)")
  (net 24 "Net-(E0-Pad19)")
  (net 25 "Net-(E0-Pad20)")
  (net 26 "Net-(E0-Pad21)")
  (net 27 "Net-(E0-Pad24)")
  (net 28 "Net-(E0-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5V)
    (add_net /C2CK)
    (add_net /C2D)
    (add_net /HD+)
    (add_net /HD-)
    (add_net /RX)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(E0-Pad1)")
    (add_net "Net-(E0-Pad10)")
    (add_net "Net-(E0-Pad13)")
    (add_net "Net-(E0-Pad15)")
    (add_net "Net-(E0-Pad16)")
    (add_net "Net-(E0-Pad17)")
    (add_net "Net-(E0-Pad18)")
    (add_net "Net-(E0-Pad19)")
    (add_net "Net-(E0-Pad20)")
    (add_net "Net-(E0-Pad21)")
    (add_net "Net-(E0-Pad24)")
    (add_net "Net-(E0-Pad7)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(Z1-Pad1)")
  )
  (net_class small ""
    (clearance 0.2)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5705CECD)
    (at 50.3 41.4)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 1) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5V))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5705CECA)
    (at 48.2 32.7)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.1 -1.1) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5705BCA1)
    (at 48.15 39.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-553 (layer F.Cu) (tedit 5705CEBA)
    (at 59.8 31.6)
    (descr SOT553)
    (attr smd)
    (fp_text reference Z1 (at 0.1 -0.05) (layer F.SilkS))
    (fp_text value DF5A5.6JE (at 0 1.34874) (layer F.Fab))
    (pad 1 smd rect (at -0.70104 -0.50038) (size 0.44958 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Z1-Pad1)"))
    (pad 3 smd rect (at -0.70104 0.50038) (size 0.44958 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5V))
    (pad 5 smd rect (at 0.70104 -0.50038) (size 0.44958 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 9 /HD+))
    (pad 2 smd rect (at -0.70104 0) (size 0.44958 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 4 smd rect (at 0.70104 0.50038) (size 0.44958 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 10 /HD-))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-553.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.77 0.65 0.7))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5705BD2C)
    (at 52.7 36.425 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference A1 (at -0.1 -0.05 360) (layer F.SilkS))
    (fp_text value ATECC508A (at 0 3.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(A1-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(A1-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(A1-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 5 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(A1-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(A1-Pad6)"))
    (pad 7 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(A1-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5V))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:debug (layer F.Cu) (tedit 5705CE93)
    (at 61 36.5)
    (fp_text reference C2CK1 (at 0.63 -1.5) (layer F.SilkS) hide)
    (fp_text value debug-pin (at 1.75 1.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.78 0.78) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 13 /C2CK))
  )
  (module footprints:debug (layer F.Cu) (tedit 5705CE8B)
    (at 61 34)
    (fp_text reference C2D1 (at 0.7 -5.75) (layer F.SilkS) hide)
    (fp_text value debug-pin (at 1.75 1.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.78 0.78) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 14 /C2D))
  )
  (module footprints:debug (layer F.Cu) (tedit 5705CE9A)
    (at 58.5 39)
    (fp_text reference RX1 (at 0.63 -1.5) (layer F.SilkS) hide)
    (fp_text value debug-pin (at 1.75 1.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.78 0.78) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 15 /RX))
  )
  (module footprints:debug (layer F.Cu) (tedit 5705CE9E)
    (at 58.5 36.5)
    (fp_text reference TX1 (at 0.63 -1.5) (layer F.SilkS) hide)
    (fp_text value debug-pin (at 1.75 1.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.78 0.78) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 16 /TX))
  )
  (module footprints:debug (layer F.Cu) (tedit 5705D08F)
    (at 58.5 34)
    (fp_text reference GND1 (at 0.63 -1.5) (layer F.SilkS) hide)
    (fp_text value debug-pin (at 1.75 1.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.78 0.78) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
  )
  (module footprints:QSOP-24_3.9x8.7mm_Pitch0.635mm_fat (layer F.Cu) (tedit 571C16FD)
    (at 59.75 37.35 180)
    (descr "SSOP24: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot556-1_po.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference E0 (at 0 -0.45 180) (layer F.SilkS))
    (fp_text value EFM8UB1_24pin (at 0 5.4 180) (layer F.Fab))
    (pad 1 smd rect (at -2.6 -3.4925 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(E0-Pad1)"))
    (pad 2 smd rect (at -2.6 -2.8575 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(A1-Pad6)"))
    (pad 3 smd rect (at -2.6 -2.2225 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(A1-Pad5)"))
    (pad 4 smd rect (at -2.6 -1.5875 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 5 smd rect (at -2.6 -0.9525 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 /HD+))
    (pad 6 smd rect (at -2.6 -0.3175 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 10 /HD-))
    (pad 7 smd rect (at -2.6 0.3175 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(E0-Pad7)"))
    (pad 8 smd rect (at -2.6 0.9525 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(E0-Pad7)"))
    (pad 9 smd rect (at -2.6 1.5875 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5V))
    (pad 10 smd rect (at -2.6 2.2225 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(E0-Pad10)"))
    (pad 11 smd rect (at -2.6 2.8575 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 13 /C2CK))
    (pad 12 smd rect (at -2.6 3.4925 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 14 /C2D))
    (pad 13 smd rect (at 2.6 3.4925 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(E0-Pad13)"))
    (pad 14 smd rect (at 2.6 2.8575 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(E0-Pad13)"))
    (pad 15 smd rect (at 2.6 2.2225 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(E0-Pad15)"))
    (pad 16 smd rect (at 2.6 1.5875 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(E0-Pad16)"))
    (pad 17 smd rect (at 2.6 0.9525 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(E0-Pad17)"))
    (pad 18 smd rect (at 2.6 0.3175 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(E0-Pad18)"))
    (pad 19 smd rect (at 2.6 -0.3175 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(E0-Pad19)"))
    (pad 20 smd rect (at 2.6 -0.9525 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(E0-Pad20)"))
    (pad 21 smd rect (at 2.6 -1.5875 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(E0-Pad21)"))
    (pad 22 smd rect (at 2.6 -2.2225 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 15 /RX))
    (pad 23 smd rect (at 2.6 -2.8575 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 16 /TX))
    (pad 24 smd rect (at 2.6 -3.4925 180) (size 1.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(E0-Pad24)"))
    (model Housings_SSOP.3dshapes/SSOP-24_3.9x8.7mm_Pitch0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:u2f-button (layer F.Cu) (tedit 571CDF8F)
    (at 43.9 36.45 90)
    (attr smd)
    (fp_text reference SW1 (at 0.15 0.09 90) (layer F.SilkS))
    (fp_text value SW_PUSH (at -0.28 3.13 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -1.56 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(E0-Pad13)"))
    (pad 1 smd rect (at 3.6 -1.56 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(E0-Pad13)"))
    (pad 2 smd rect (at 3.6 1.44 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at -3.6 1.44 90) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
  )
  (module footprints:LED-0606 (layer F.Cu) (tedit 5686CF1E)
    (at 48.1 36.25)
    (attr smd)
    (fp_text reference RGB1 (at 0.07546 -1.90872) (layer F.SilkS))
    (fp_text value CA_RGB (at 0.0145 1.70824) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.43 -0.72) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(E0-Pad18)"))
    (pad 2 smd rect (at 0.42 -0.72) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(E0-Pad19)"))
    (pad 3 smd rect (at 0.42 0.73) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(E0-Pad20)"))
    (pad 4 smd rect (at -0.43 0.73) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad2)"))
  )
  (module footprints:u2f-fiducial (layer F.Cu) (tedit 571CE320)
    (at 36.15 42.6)
    (fp_text reference F1 (at 0.1 -1.4) (layer F.SilkS) hide)
    (fp_text value u2f-fiducial (at 5.3848 -1.4986) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.508) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 1.016) (clearance 1.016))
  )
  (module footprints:u2f-fiducial (layer F.Cu) (tedit 571CE320)
    (at 36.15 29.9)
    (fp_text reference F2 (at 0.1 -1.4) (layer F.SilkS) hide)
    (fp_text value u2f-fiducial (at 5.3848 -1.4986) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.508) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 1.016) (clearance 1.016))
  )
  (module footprints:u2f-fiducial (layer F.Cu) (tedit 571CE320)
    (at 63.35 29.9)
    (fp_text reference F3 (at 0.1 -1.4) (layer F.SilkS) hide)
    (fp_text value u2f-fiducial (at 5.3848 -1.4986) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.508) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 1.016) (clearance 1.016))
  )
  (gr_line (start 75.75 42.25) (end 64.25 42.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.75 30.25) (end 64.25 30.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.25 43.5) (end 64.25 42.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 35.25 43.5) (end 64.25 43.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 35.25 29) (end 35.25 43.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.25 29) (end 35.25 29) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.25 30.25) (end 64.25 29) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text u2fzero.com (at 43.3 42.2) (layer F.SilkS))
  (gr_text "U2F Zero" (at 42.4 30.4) (layer F.SilkS))
  (gr_circle (center 38.6 36.25) (end 40.85 36.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.75 42.25) (end 75.75 30.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "GND\n" (at 64.45 40.05) (layer Cmts.User))
  (gr_text D+ (at 64.5 37.6) (layer Cmts.User))
  (gr_text D- (at 64.35 35.35) (layer Cmts.User))
  (gr_text +5v (at 64.3 33) (layer Cmts.User))
  (zone (net 1) (net_name /+5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.75 33.75) (xy 66.55 33.75) (xy 66.55 31.75) (xy 74.75 31.75) (xy 74.75 33.75)
      )
    )
  )
  (zone (net 9) (net_name /HD+) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.25 38.4) (xy 66.55 38.4) (xy 66.55 36.4) (xy 74.25 36.4) (xy 74.25 38.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.55 31.75) (xy 74.75 31.75) (xy 74.75 33.75) (xy 66.55 33.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.25 38.4) (xy 74.25 36.4) (xy 66.55 36.4) (xy 66.55 38.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.25 36.1) (xy 66.55 36.1) (xy 66.55 34.1) (xy 74.25 34.1) (xy 74.25 36.1)
      )
    )
  )
  (zone (net 10) (net_name /HD-) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.25 36.1) (xy 66.55 36.1) (xy 66.55 34.1) (xy 74.25 34.1) (xy 74.25 36.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.55 38.75) (xy 66.55 40.75) (xy 74.75 40.75) (xy 74.75 38.75)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.15 30.35) (xy 66 30.35) (xy 66 38.75) (xy 74.75 38.75) (xy 74.75 40.75)
        (xy 66 40.75) (xy 66 42.15) (xy 64.15 42.15) (xy 64.15 43.4) (xy 35.35 43.4)
        (xy 35.35 29.1) (xy 64.15 29.1) (xy 64.15 30.35)
      )
    )
  )
)
