(kicad_pcb (version 20171130) (host pcbnew no-vcs-found-7586afd~61~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 60)
    (zones 0)
    (modules 3)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 +3V3)
  (net 4 SS)
  (net 5 MOSI)
  (net 6 MISO)
  (net 7 SCLK)
  (net 8 "Net-(U1-Pad9)")
  (net 9 "Net-(U1-Pad8)")
  (net 10 GDO0)
  (net 11 "Net-(U1-Pad5)")
  (net 12 "Net-(U1-Pad4)")
  (net 13 "Net-(U1-Pad3)")
  (net 14 "Net-(U1-Pad2)")
  (net 15 "Net-(U1-Pad6)")
  (net 16 "Net-(U2-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GDO0)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad4)")
    (add_net SCLK)
    (add_net SS)
  )
  (module lib:CC1101-868MHz-Module (layer B.Cu) (tedit 5A42B5C7)
    (at 136.906 59.69 180)
    (descr http://www.digirf.com/XWFU/2013/4f3751b81deca976.pdf)
    (fp_text reference U2 (at 0 0 180) (layer B.SilkS))
    (fp_text value CC1101-868MHz-Module (at 0 11 180) (layer B.Fab))
    (pad ANT smd oval (at -5.715 9.525 90) (size 1.75 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad ANT thru_hole circle (at -5.715 8.89 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 12 smd oval (at 7.62 -0.635 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd oval (at 7.62 -1.905 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd oval (at 7.62 -3.175 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd oval (at 7.62 -4.445 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 8 smd oval (at 7.62 -5.715 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 7 smd oval (at 7.62 -6.985 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 6 smd oval (at -7.62 -6.985 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 SS))
    (pad 5 smd oval (at -7.62 -5.715 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 10 GDO0))
    (pad 4 smd oval (at -7.62 -4.445 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(U2-Pad4)"))
    (pad 3 smd oval (at -7.62 -3.175 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 MISO))
    (pad 2 smd oval (at -7.62 -1.905 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 7 SCLK))
    (pad 1 smd oval (at -7.62 -0.635 180) (size 1.75 0.7) (layers B.Cu B.Paste B.Mask)
      (net 5 MOSI))
  )
  (module lib:microduino (layer F.Cu) (tedit 5A364307)
    (at 136.8425 60.0075)
    (tags "foont print ruotato mettere i comp su F Cu")
    (fp_text reference U1 (at 0 -7.62) (layer F.SilkS) hide)
    (fp_text value Microduino (at 0 0) (layer F.SilkS) hide)
    (fp_text user GND (at 8.255 -12.7 90) (layer B.SilkS))
    (fp_text user RST (at 8.255 -10.16 90) (layer B.SilkS))
    (fp_text user D6 (at 8.255 -7.62 90) (layer B.SilkS))
    (fp_text user D5 (at 8.255 -5.08 90) (layer B.SilkS))
    (fp_text user D4 (at 8.255 -2.54 90) (layer B.SilkS))
    (fp_text user D3 (at 8.255 0 90) (layer F.SilkS))
    (fp_text user D1 (at 8.255 5.08 90) (layer F.SilkS))
    (fp_text user D0 (at 8.255 6.985 90) (layer F.SilkS))
    (fp_text user RX (at 12.065 7.62 90) (layer B.SilkS))
    (fp_text user TX (at 12.065 5.715 90) (layer B.SilkS))
    (fp_text user A5 (at 4.445 7.62 90) (layer B.SilkS))
    (fp_text user A4 (at 2.54 7.62 90) (layer B.SilkS))
    (fp_text user A3 (at 0 7.62 90) (layer B.SilkS))
    (fp_text user A2 (at -2.54 7.62 90) (layer F.SilkS))
    (fp_text user A1 (at -4.445 7.62 90) (layer F.SilkS))
    (fp_text user D12 (at -8.255 5.08 90) (layer F.SilkS))
    (fp_text user D9 (at -8.255 -2.54 90) (layer B.SilkS))
    (fp_text user D8 (at -8.255 -5.08 90) (layer B.SilkS))
    (fp_text user D7 (at -8.255 -7.62 90) (layer B.SilkS))
    (fp_text user 3V3 (at -8.255 -10.16 90) (layer B.SilkS))
    (fp_text user 5V (at -8.255 -12.7 90) (layer B.SilkS))
    (fp_text user SCK (at -12.065 7.62 90) (layer B.SilkS))
    (fp_text user SO (at -12.065 5.08 90) (layer B.SilkS))
    (fp_text user SI (at -12.065 2.54 90) (layer B.SilkS))
    (fp_text user SS (at -12.065 0 90) (layer B.SilkS))
    (fp_text user SDA (at 2.54 12.065 180) (layer F.SilkS))
    (fp_text user SCL (at 5.08 12.065 180) (layer B.SilkS))
    (fp_text user SDA (at 2.54 12.065 180) (layer B.SilkS))
    (fp_text user SCL (at 5.08 12.065 180) (layer F.SilkS))
    (fp_text user SS (at -12.065 0 90) (layer F.SilkS))
    (fp_text user SI (at -12.065 2.54 90) (layer F.SilkS))
    (fp_text user SO (at -12.065 5.08 90) (layer F.SilkS))
    (fp_text user SCK (at -12.065 7.62 90) (layer F.SilkS))
    (fp_text user 5V (at -8.255 -12.7 90) (layer F.SilkS))
    (fp_text user 3V3 (at -8.255 -10.16 90) (layer F.SilkS))
    (fp_text user D7 (at -8.255 -7.62 90) (layer F.SilkS))
    (fp_text user D8 (at -8.255 -5.08 90) (layer F.SilkS))
    (fp_text user D9 (at -8.255 -2.54 90) (layer F.SilkS))
    (fp_text user D10 (at -8.255 0 90) (layer F.SilkS))
    (fp_text user D11 (at -8.255 2.54 90) (layer F.SilkS))
    (fp_text user D13 (at -8.255 7.62 90) (layer F.SilkS))
    (fp_text user REF (at -5.715 5.08 90) (layer F.SilkS))
    (fp_text user A0 (at -6.35 7.62 90) (layer F.SilkS))
    (fp_text user A1 (at -4.445 7.62 90) (layer B.SilkS))
    (fp_text user A2 (at -2.54 7.62 90) (layer B.SilkS))
    (fp_text user A3 (at 0 7.62 90) (layer F.SilkS))
    (fp_text user A4 (at 2.54 7.62 90) (layer F.SilkS))
    (fp_text user A5 (at 4.445 7.62 90) (layer F.SilkS))
    (fp_text user A6 (at 6.35 7.62 270) (layer F.SilkS))
    (fp_text user A7 (at 5.715 5.08 90) (layer F.SilkS))
    (fp_text user TX (at 12.065 5.715 90) (layer F.SilkS))
    (fp_text user RX (at 12.065 7.62 90) (layer F.SilkS))
    (fp_text user D2 (at 8.255 2.54 90) (layer F.SilkS))
    (fp_text user D4 (at 8.255 -2.54 90) (layer F.SilkS))
    (fp_text user D5 (at 8.255 -5.08 90) (layer F.SilkS))
    (fp_text user D6 (at 8.255 -7.62 90) (layer F.SilkS))
    (fp_text user RST (at 8.255 -10.16 90) (layer F.SilkS))
    (fp_text user GND (at 8.255 -12.7 90) (layer F.SilkS))
    (pad 9 thru_hole circle (at 10.16 7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad9)"))
    (pad 8 thru_hole circle (at 10.16 5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U1-Pad8)"))
    (pad 7 thru_hole circle (at 10.16 2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 GDO0))
    (pad 6 thru_hole circle (at 10.16 0) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at 10.16 -2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at 10.16 -5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U1-Pad4)"))
    (pad 3 thru_hole circle (at 10.16 -7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at 10.16 -10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U1-Pad2)"))
    (pad 1 thru_hole circle (at 10.16 -12.7) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 10.16 -12.7) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole circle (at 10.16 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 10.16 -10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 -7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at 10.16 -5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 -2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 10.16 0) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at 10.16 2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 GDO0))
    (pad 8 thru_hole circle (at 10.16 5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 10.16 7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad9)"))
    (pad 11 thru_hole circle (at 7.62 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at 5.08 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 2.54 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 0 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole circle (at -2.54 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at -5.08 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at -7.62 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at -10.16 10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at -10.16 7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 7 SCLK))
    (pad 20 thru_hole circle (at -10.16 5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 6 MISO))
    (pad 21 thru_hole circle (at -10.16 2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 5 MOSI))
    (pad 22 thru_hole circle (at -10.16 0) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 SS))
    (pad 23 thru_hole circle (at -10.16 -2.54) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 24 thru_hole circle (at -10.16 -5.08) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole circle (at -10.16 -7.62) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole circle (at -10.16 -10.16) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 27 thru_hole circle (at -10.16 -12.7) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module lib:SMA_EDGE (layer F.Cu) (tedit 5A3642DC)
    (at 136.906 48.514)
    (fp_text reference J1 (at 0 -6.35) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at 0 -6.35 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -4.064 -1.7653) (size 5.08 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.064 -1.7653) (size 5.08 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -1.7653) (size 1.27 3.5) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -4.064 -1.7653) (size 5.08 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.064 -1.7653) (size 5.08 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -1.7653) (size 1.27 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (gr_line (start 149.5425 71.9455) (end 149.5425 45.6565) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.9045 72.7075) (end 148.6535 72.7075) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.1425 45.5295) (end 124.1425 71.8185) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.7805 44.7675) (end 125.0315 44.7675) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124.968 71.882) (end 124.9045 72.7075) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 148.717 71.882) (end 149.5425 71.9455) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 148.717 45.593) (end 148.7805 44.7675) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124.968 45.593) (end 124.1425 45.5295) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.333 45.0215) (xy 149.225 45.0215) (xy 149.225 72.4535) (xy 124.3965 72.4535)
      )
    )
  )
)
