(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 75)
    (zones 0)
    (modules 3)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (user_trace_width 0.4572)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /DAT1)
  (net 2 /DAT0)
  (net 3 /GND)
  (net 4 /CLK)
  (net 5 /3V3)
  (net 6 /CMD)
  (net 7 /DAT3)
  (net 8 /DAT2)
  (net 9 "Net-(J2-Pad10)")
  (net 10 /29)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /29)
    (add_net /3V3)
    (add_net /CLK)
    (add_net /CMD)
    (add_net /DAT0)
    (add_net /DAT1)
    (add_net /DAT2)
    (add_net /DAT3)
    (add_net /GND)
    (add_net "Net-(J2-Pad10)")
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 131.2926 97.79)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value CARD_DETECT (at 0 1.9) (layer F.SilkS))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 10 /29) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 9 "Net-(J2-Pad10)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Connector_Card:microSD_HC_Hirose_DM3D-SF (layer F.Cu) (tedit 5B82D16A)
    (at 130.8608 86.36 180)
    (descr "Micro SD, SMD, right-angle, push-pull (https://media.digikey.com/PDF/Data%20Sheets/Hirose%20PDFs/DM3D-SF.pdf)")
    (tags "Micro SD")
    (attr smd)
    (fp_text reference J2 (at -0.025 -7.625) (layer F.SilkS) hide)
    (fp_text value Micro_SD_Card_Det (at -0.025 6.975) (layer F.Fab))
    (fp_text user KEEPOUT (at -0.725 -4.8) (layer Cmts.User))
    (fp_text user %R (at -0.025 1.475) (layer F.Fab))
    (fp_text user KEEPOUT (at -0.275 -0.525) (layer Cmts.User))
    (pad 10 smd rect (at 5.575 -5.45 180) (size 1 1.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad10)"))
    (pad 11 smd rect (at 5.625 5.225 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 1 smd rect (at 3.175 5.35 180) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /DAT2))
    (pad 2 smd rect (at 2.075 5.35 180) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 7 /DAT3))
    (pad 3 smd rect (at 0.975 5.35 180) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 6 /CMD))
    (pad 4 smd rect (at -0.125 5.35 180) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /3V3))
    (pad 5 smd rect (at -1.225 5.35 180) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /CLK))
    (pad 6 smd rect (at -2.325 5.35 180) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 7 smd rect (at -3.425 5.35 180) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /DAT0))
    (pad 11 smd rect (at 5.975 -3.025 180) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 9 smd rect (at -5.65 -3.875 180) (size 1.45 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 11 smd rect (at -5.975 -2.375 180) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 11 smd rect (at -5.725 5.225 180) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /GND))
    (pad 8 smd rect (at -4.525 5.35 180) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /DAT1))
    (model ${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3D-SF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 139.7 81.28)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x09 (at 0 22.65) (layer F.Fab))
    (fp_text user %R (at 0 10.16 90) (layer F.Fab))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /29))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /DAT2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DAT3))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CMD))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /3V3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /CLK))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /DAT0))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /DAT1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 140.97 80.01) (end 140.97 102.87) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.19 80.01) (end 140.97 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.19 102.87) (end 123.19 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 140.97 102.87) (end 123.19 102.87) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.818602 87.9602) (xy 135.818602 85.852) (xy 127.208002 85.852) (xy 127.208002 87.9602)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.2766 92.0242) (xy 130.2766 90.17) (xy 132.8674 90.1446) (xy 132.8928 92.202) (xy 130.2766 92.1766)
        (xy 130.2766 92.1258)
      )
    )
  )
  (zone (net 3) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.24 78.74) (xy 121.92 78.74) (xy 121.92 104.14) (xy 142.24 104.14)
      )
    )
  )
)
