(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 9)
    (no_connects 0)
    (area 124.384999 63.424999 202.005001 95.325001)
    (thickness 1.6)
    (drawings 21)
    (tracks 23)
    (zones 0)
    (modules 7)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4064)
    (user_trace_width 0.4064)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad2)")
  (net 2 "Net-(BT1-Pad1)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(R1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5A985833)
    (at 135.89 77.47 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 0 -3 270) (layer F.SilkS))
    (fp_text value 150 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 4 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal.wrl
      (at (xyz -0.315 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery_Holders:Keystone_106_1x20mm-CoinCell (layer B.Cu) (tedit 5A983818)
    (at 171.45 78.74)
    (descr http://www.keyelco.com/product-pdf.cfm?p=720)
    (tags "Keystone type 106 battery holder")
    (fp_text reference BT1 (at -1.25 4.5) (layer B.SilkS))
    (fp_text value Battery_Cell (at 15 -15) (layer B.Fab))
    (fp_text user + (at 2.75 0) (layer B.SilkS))
    (pad 2 thru_hole circle (at 20 0) (size 3 3) (drill 1.17) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model Battery_Holders.3dshapes/Keystone_106_1x20mm-CoinCell.wrl
      (at (xyz 0.6 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57FE943C)
    (at 129.54 67.31)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.6) (layer F.SilkS))
    (fp_text value LED (at 0 1.7) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at -1.65 0 180) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_D5.0mm_FlatTop (layer F.Cu) (tedit 5A98393C)
    (at 128.27 78.74 90)
    (descr "LED, Round, FlatTop, diameter 5.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-483GDT(Ver.15B).pdf")
    (tags "LED Round FlatTop diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 6.35 0 180) (layer F.SilkS))
    (fp_text value IR (at 1.27 4.01 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 142.24 67.31)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 0 (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5AA1AEC0)
    (at 133.35 92.71 180)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 -2 180) (layer F.SilkS))
    (fp_text value SW_Push (at 3.175 6.985 360) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)"))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(BT1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SigmaLogo:SigmaDesign (layer F.Cu) (tedit 0)
    (at 157.48 80.01 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (gr_text POWER (at 136.525 90.805 90) (layer F.SilkS))
  (gr_text "IR LED FLASHLIGHT" (at 160.02 67.31) (layer B.SilkS))
  (dimension 77.47 (width 0.3) (layer Dwgs.User)
    (gr_text "77.470 mm" (at 163.195 58.34) (layer Dwgs.User))
    (feature1 (pts (xy 201.93 63.5) (xy 201.93 56.99)))
    (feature2 (pts (xy 124.46 63.5) (xy 124.46 56.99)))
    (crossbar (pts (xy 124.46 59.69) (xy 201.93 59.69)))
    (arrow1a (pts (xy 201.93 59.69) (xy 200.803496 60.276421)))
    (arrow1b (pts (xy 201.93 59.69) (xy 200.803496 59.103579)))
    (arrow2a (pts (xy 124.46 59.69) (xy 125.586504 60.276421)))
    (arrow2b (pts (xy 124.46 59.69) (xy 125.586504 59.103579)))
  )
  (gr_line (start 201.93 66.04) (end 201.93 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 199.39 66.04) (end 199.39 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127 66.04) (end 124.46 66.04) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127 92.71) (end 127 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 95.25) (end 127 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 199.39 92.71) (end 201.93 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 63.5) (end 199.39 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.46 66.04) (end 124.46 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 199.39 95.25) (end 128.27 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 201.93 92.71) (end 201.93 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
)
