(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.051)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C3-Pad1)")
  (net 3 "Net-(C4-Pad1)")
  (net 4 "+3.3V")
  (net 5 "+1V1")
  (net 6 "Net-(C13-Pad1)")
  (net 7 "Net-(C16-Pad2)")
  (net 8 "Net-(C17-Pad2)")
  (net 9 "/ADC_AVDD")
  (net 10 "Net-(D3-Pad2)")
  (net 11 "Net-(FB2-Pad1)")
  (net 12 "Net-(FB3-Pad1)")
  (net 13 "/UART0_RX")
  (net 14 "/UART0_TX")
  (net 15 "/SWCLK")
  (net 16 "/SWDIO")
  (net 17 "/NRST")
  (net 18 "Vbus")
  (net 19 "Net-(J3-Pad2)")
  (net 20 "Net-(J3-Pad3)")
  (net 21 "unconnected-(J3-Pad4)")
  (net 22 "Net-(R2-Pad2)")
  (net 23 "/LED")
  (net 24 "/QSPI_SS_N")
  (net 25 "Net-(R10-Pad2)")
  (net 26 "/PDM+")
  (net 27 "Net-(R13-Pad1)")
  (net 28 "Net-(R14-Pad1)")
  (net 29 "/BTN")
  (net 30 "/SD")
  (net 31 "unconnected-(U3-Pad9)")
  (net 32 "unconnected-(U3-Pad11)")
  (net 33 "unconnected-(U3-Pad12)")
  (net 34 "unconnected-(U3-Pad13)")
  (net 35 "unconnected-(U3-Pad14)")
  (net 36 "unconnected-(U3-Pad15)")
  (net 37 "unconnected-(U3-Pad16)")
  (net 38 "unconnected-(U3-Pad17)")
  (net 39 "unconnected-(U3-Pad18)")
  (net 40 "unconnected-(U3-Pad27)")
  (net 41 "unconnected-(U3-Pad28)")
  (net 42 "unconnected-(U3-Pad29)")
  (net 43 "unconnected-(U3-Pad30)")
  (net 44 "unconnected-(U3-Pad31)")
  (net 45 "unconnected-(U3-Pad32)")
  (net 46 "unconnected-(U3-Pad40)")
  (net 47 "unconnected-(U3-Pad41)")
  (net 48 "unconnected-(U3-Pad4)")
  (net 49 "unconnected-(U3-Pad5)")
  (net 50 "/POT")
  (net 51 "unconnected-(U3-Pad6)")
  (net 52 "unconnected-(U3-Pad7)")
  (net 53 "/QSPI_SD3")
  (net 54 "/QSPI_SCLK")
  (net 55 "/QSPI_SD0")
  (net 56 "/QSPI_SD2")
  (net 57 "/QSPI_SD1")
  (net 58 "unconnected-(U4-Pad2)")
  (net 59 "Net-(C24-Pad1)")
  (net 60 "Net-(C26-Pad1)")
  (net 61 "unconnected-(U3-Pad8)")
  (net 62 "/Vraw")
  (net 63 "/Vbat")
  (net 64 "Net-(L1-Pad2)")
  (net 65 "unconnected-(U3-Pad39)")
  (net 66 "/Vbat_sw")
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.84 115.316 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.17) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/PDM+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 114.046 109.347)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 1.587 0) (layer "F.SilkS"))
    (fp_text value "27.5" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(R14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 129.125 122.687 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0.894 -1.49 90) (layer "F.SilkS"))
    (fp_text value "Speaker" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(C26-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(C24-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 139.197 122.682 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0.889 -1.773 90) (layer "F.SilkS"))
    (fp_text value "Battery" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "/Vbat") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.634 115.062)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0.635 -1.27) (layer "F.SilkS"))
    (fp_text value "10uf" (at 16.759 -6.858) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.114 110.236 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 1.651 -0.005 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+1V1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.188 122.428)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 1.397 -0.127) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.998 103.505 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C25" (at -1.27 0 180) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 114.046 108.331)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 1.651 0) (layer "F.SilkS"))
    (fp_text value "27.5" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J3-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 130.781 119.977 -90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB3" (at -0.47 -1.045 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(FB3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(C24-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.892 110.236 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C21" (at 1.651 0.122 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 129.1082 103.505 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 1.8796 -0.0762 90) (layer "F.SilkS"))
    (fp_text value "LED Green" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 124.079 122.682 -90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0.889 -1.651 90) (layer "F.SilkS"))
    (fp_text value "SWD" (at 0 12.49 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.08) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/SWCLK") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/SWDIO") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/NRST") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.34 120.462 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C26" (at 1.721 0.066) (layer "F.SilkS"))
    (fp_text value "220pf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(C26-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.426 112.014)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 1.397 0) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.537 116.614 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 1.171 -0.127 180) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_CK_KMR2" (layer "F.Cu")
    (tedit 5A02FC95)
    (at 119.126 119.126 180)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 0 0) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.45) (layer "F.Fab"))
    (pad "1" smd rect (at 2.05 -0.8 180) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/NRST") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at -2.05 -0.8 180) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.05 0.8 180) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.05 0.8 180) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.step"
      (offset (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.537 119.634 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 1.397 -0.127 90) (layer "F.SilkS"))
    (fp_text value "27pf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "emeb_library:SON65P200X200X80-7N" (layer "F.Cu")
    (tedit 6386320F)
    (at 125.857 108.966)
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0.292 -1.7134) (layer "F.SilkS"))
    (fp_text value "TPS61291DRVR" (at 5.9816 1.7134) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.025 -0.65) (size 0.66 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(L1-Pad2)") (pinfunction "SW") (pintype "input"))
    (pad "2" smd rect locked (at -1.025 0) (size 0.66 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "VOUT") (pintype "output"))
    (pad "3" smd rect locked (at -1.025 0.65) (size 0.66 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/Vraw") (pinfunction "VIN") (pintype "input"))
    (pad "4" smd rect locked (at 1.025 0.65) (size 0.66 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "EN/BYP") (pintype "input"))
    (pad "5" smd rect locked (at 1.025 0) (size 0.66 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSEL") (pintype "input"))
    (pad "6" smd rect locked (at 1.025 -0.65) (size 0.66 0.32) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd rect locked (at 0 0 90) (size 1.6 1) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "EXP") (pintype "power_in"))
    (model ":3dmodels:TPS61291DRVR.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 129.765 119.977 -90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB2" (at -0.47 1.114 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(FB2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(C26-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.558 117.983 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C20" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_CK_KMR2" (layer "F.Cu")
    (tedit 5A02FC95)
    (at 103.505 111.633 -90)
    (descr "CK components KMR2 tactile switch http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW3" (at 0 -0.127 90) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 2.55 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.45 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.05 -0.8 270) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(R10-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 2.05 -0.8 270) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(R10-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.05 0.8 270) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.05 0.8 270) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_PTS645.step"
      (offset (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.555 111.953 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -0.574 -1.397 90) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/Vraw") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.321 111.506)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C22" (at 1.646 0) (layer "F.SilkS"))
    (fp_text value "1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "emeb_library:RP2040" (layer "F.Cu")
    (tedit 0)
    (at 110.0886 116.7384)
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -4.6786 -1.9304) (layer "F.SilkS"))
    (fp_text value "RP2040" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -4.445 -2.8) (layer "F.SilkS"))
    (fp_text user "0.032in/0.813mm" (at -3.4036 -6.4516) (layer "Dwgs.User"))
    (fp_text user "0.007in/0.178mm" (at -6.4516 3.4036) (layer "Dwgs.User"))
    (fp_text user "0.016in/0.4mm" (at -5.4356 -2.4) (layer "Dwgs.User"))
    (fp_text user "0.268in/6.807mm" (at 8.9916 0.635) (layer "Dwgs.User"))
    (fp_text user "0.126in/3.2mm" (at 0 4.6482) (layer "Dwgs.User"))
    (fp_text user "0.268in/6.807mm" (at 0 8.9916) (layer "Dwgs.User"))
    (fp_text user "0.126in/3.2mm" (at 4.6482 -0.635) (layer "Dwgs.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at -2.9972 -2.8) (layer "F.Fab"))
    (fp_text user "*" (at -2.9972 -2.8) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.4036 -2.6 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "2" smd rect locked (at -3.4036 -2.200001 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/UART0_TX") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "3" smd rect locked (at -3.4036 -1.799999 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/UART0_RX") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "4" smd rect locked (at -3.4036 -1.4 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "unconnected-(U3-Pad4)") (pinfunction "GPIO2") (pintype "bidirectional+no_connect"))
    (pad "5" smd rect locked (at -3.4036 -1.000001 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "unconnected-(U3-Pad5)") (pinfunction "GPIO3") (pintype "bidirectional+no_connect"))
    (pad "6" smd rect locked (at -3.4036 -0.599999 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "unconnected-(U3-Pad6)") (pinfunction "GPIO4") (pintype "bidirectional+no_connect"))
    (pad "7" smd rect locked (at -3.4036 -0.2 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "unconnected-(U3-Pad7)") (pinfunction "GPIO5") (pintype "bidirectional+no_connect"))
    (pad "8" smd rect locked (at -3.4036 0.2 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "unconnected-(U3-Pad8)") (pinfunction "GPIO6") (pintype "bidirectional+no_connect"))
    (pad "9" smd rect locked (at -3.4036 0.599999 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "unconnected-(U3-Pad9)") (pinfunction "GPIO7") (pintype "bidirectional+no_connect"))
    (pad "10" smd rect locked (at -3.4036 1.000001 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "11" smd rect locked (at -3.4036 1.4 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "unconnected-(U3-Pad11)") (pinfunction "GPIO8") (pintype "bidirectional+no_connect"))
    (pad "12" smd rect locked (at -3.4036 1.799999 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "unconnected-(U3-Pad12)") (pinfunction "GPIO9") (pintype "bidirectional+no_connect"))
    (pad "13" smd rect locked (at -3.4036 2.200001 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "unconnected-(U3-Pad13)") (pinfunction "GPIO10") (pintype "bidirectional+no_connect"))
    (pad "14" smd rect locked (at -3.4036 2.6 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(U3-Pad14)") (pinfunction "GPIO11") (pintype "bidirectional+no_connect"))
    (pad "15" smd rect locked (at -2.6 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "unconnected-(U3-Pad15)") (pinfunction "GPIO12") (pintype "bidirectional+no_connect"))
    (pad "16" smd rect locked (at -2.200001 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "unconnected-(U3-Pad16)") (pinfunction "GPIO13") (pintype "bidirectional+no_connect"))
    (pad "17" smd rect locked (at -1.799999 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "unconnected-(U3-Pad17)") (pinfunction "GPIO14") (pintype "bidirectional+no_connect"))
    (pad "18" smd rect locked (at -1.4 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(U3-Pad18)") (pinfunction "GPIO15") (pintype "bidirectional+no_connect"))
    (pad "19" smd rect locked (at -1.000001 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "TESTEN") (pintype "unspecified"))
    (pad "20" smd rect locked (at -0.599999 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C4-Pad1)") (pinfunction "XIN") (pintype "unspecified"))
    (pad "21" smd rect locked (at -0.2 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(R2-Pad2)") (pinfunction "XOUT") (pintype "output"))
    (pad "22" smd rect locked (at 0.2 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "23" smd rect locked (at 0.599999 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+1V1") (pinfunction "DVDD") (pintype "power_in"))
    (pad "24" smd rect locked (at 1.000001 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/SWCLK") (pinfunction "SWCLK") (pintype "unspecified"))
    (pad "25" smd rect locked (at 1.4 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/SWDIO") (pinfunction "SWDIO") (pintype "unspecified"))
    (pad "26" smd rect locked (at 1.799999 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/NRST") (pinfunction "RUN") (pintype "unspecified"))
    (pad "27" smd rect locked (at 2.200001 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(U3-Pad27)") (pinfunction "GPIO16") (pintype "bidirectional+no_connect"))
    (pad "28" smd rect locked (at 2.6 3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "unconnected-(U3-Pad28)") (pinfunction "GPIO17") (pintype "bidirectional+no_connect"))
    (pad "29" smd rect locked (at 3.4036 2.6 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "unconnected-(U3-Pad29)") (pinfunction "GPIO18") (pintype "bidirectional+no_connect"))
    (pad "30" smd rect locked (at 3.4036 2.200001 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "unconnected-(U3-Pad30)") (pinfunction "GPIO19") (pintype "bidirectional+no_connect"))
    (pad "31" smd rect locked (at 3.4036 1.799999 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "unconnected-(U3-Pad31)") (pinfunction "GPIO20") (pintype "bidirectional+no_connect"))
    (pad "32" smd rect locked (at 3.4036 1.4 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "unconnected-(U3-Pad32)") (pinfunction "GPIO21") (pintype "bidirectional+no_connect"))
    (pad "33" smd rect locked (at 3.4036 1.000001 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "34" smd rect locked (at 3.4036 0.599999 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/LED") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "35" smd rect locked (at 3.4036 0.2 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/BTN") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "36" smd rect locked (at 3.4036 -0.2 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/SD") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "37" smd rect locked (at 3.4036 -0.599999 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/PDM+") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "38" smd rect locked (at 3.4036 -1.000001 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/POT") (pinfunction "GPIO26/ADC0") (pintype "bidirectional"))
    (pad "39" smd rect locked (at 3.4036 -1.4 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "unconnected-(U3-Pad39)") (pinfunction "GPIO27/ADC1") (pintype "bidirectional+no_connect"))
    (pad "40" smd rect locked (at 3.4036 -1.799999 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "unconnected-(U3-Pad40)") (pinfunction "GPIO28/ADC2") (pintype "bidirectional+no_connect"))
    (pad "41" smd rect locked (at 3.4036 -2.200001 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "unconnected-(U3-Pad41)") (pinfunction "GPIO29/ADC3") (pintype "bidirectional+no_connect"))
    (pad "42" smd rect locked (at 3.4036 -2.6 90) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "43" smd rect locked (at 2.6 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/ADC_AVDD") (pinfunction "ADC_AVDD") (pintype "power_in"))
    (pad "44" smd rect locked (at 2.200001 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "VREG_VIN") (pintype "unspecified"))
    (pad "45" smd rect locked (at 1.799999 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+1V1") (pinfunction "VREG_VOUT") (pintype "output"))
    (pad "46" smd rect locked (at 1.4 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(R14-Pad1)") (pinfunction "USB_DM") (pintype "unspecified"))
    (pad "47" smd rect locked (at 1.000001 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(R13-Pad1)") (pinfunction "USB_DP") (pintype "unspecified"))
    (pad "48" smd rect locked (at 0.599999 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "USB_VDD") (pintype "power_in"))
    (pad "49" smd rect locked (at 0.2 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "IOVDD") (pintype "power_in"))
    (pad "50" smd rect locked (at -0.2 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+1V1") (pinfunction "DVDD") (pintype "power_in"))
    (pad "51" smd rect locked (at -0.599999 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/QSPI_SD3") (pinfunction "QSPI_SD3") (pintype "bidirectional"))
    (pad "52" smd rect locked (at -1.000001 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/QSPI_SCLK") (pinfunction "QSPI_SCLK") (pintype "unspecified"))
    (pad "53" smd rect locked (at -1.4 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/QSPI_SD0") (pinfunction "QSPI_SD0") (pintype "bidirectional"))
    (pad "54" smd rect locked (at -1.799999 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/QSPI_SD2") (pinfunction "QSPI_SD2") (pintype "bidirectional"))
    (pad "55" smd rect locked (at -2.200001 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/QSPI_SD1") (pinfunction "QSPI_SD1") (pintype "bidirectional"))
    (pad "56" smd rect locked (at -2.6 -3.4036) (size 0.1778 0.8128) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/QSPI_SS_N") (pinfunction "QSPI_SS_N") (pintype "unspecified"))
    (pad "57" smd rect locked (at 0 0) (size 3.2004 3.2004) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "/home/ericb/Engineering/KBADC/kicad/3Dmodels/QFN56_7X7_RPI.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Taiyo-Yuden_MD-2020" (layer "F.Cu")
    (tedit 5990349C)
    (at 122.428 108.926 90)
    (descr "Inductor, Taiyo Yuden, MD series, Taiyo-Yuden_MD-2020, 2.0mmx2.0mm")
    (tags "inductor taiyo-yuden md smd")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at 0.849 -1.651 90) (layer "F.SilkS"))
    (fp_text value "3.3uH" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.675 0 90) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/Vraw") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0.675 0 90) (size 0.65 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(L1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Taiyo-Yuden_MD-2020.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.216 123.444)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 1.369 0 180) (layer "F.SilkS"))
    (fp_text value "27pf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.321 112.522)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C19" (at 1.646 0) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/ADC_AVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_Micro-B_Amphenol_10103594-0001LF_Horizontal" (layer "F.Cu")
    (tedit 5A1DC0BD)
    (at 116.078 104.648 180)
    (descr "Micro USB Type B 10103594-0001LF, http://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10103594.pdf")
    (tags "USB USB_B USB_micro USB_OTG")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at -4.445 2.159) (layer "F.SilkS"))
    (fp_text value "USB_B_Micro" (at -0.025 4.435) (layer "F.Fab"))
    (fp_text user "PCB edge" (at -0.025 2.235) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at -0.025 -0.015) (layer "F.Fab"))
    (pad "1" smd rect (at -1.325 -1.765 270) (size 1.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Vbus") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at -0.675 -1.765 270) (size 1.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J3-Pad2)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" smd rect (at -0.025 -1.765 270) (size 1.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(J3-Pad3)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" smd rect (at 0.625 -1.765 270) (size 1.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "unconnected-(J3-Pad4)") (pinfunction "ID") (pintype "passive+no_connect"))
    (pad "5" smd rect (at 1.275 -1.765 270) (size 1.65 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "6" smd rect (at -2.875 -1.865 180) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.445 -1.885 270) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -2.975 -0.565 180) (size 1.825 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.755 1.115 270) (size 1.7 1.35) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.395 -1.885 270) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 2.875 -1.885 180) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -2.755 0.185 180) (size 1.35 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 2.725 0.185 180) (size 1.35 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 2.975 -0.565 180) (size 1.825 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -0.985 1.385 270) (size 2.5 1.43) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.705 1.115 270) (size 1.7 1.35) (drill oval 1.2 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 0.935 1.385 270) (size 2.5 1.43) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10103594-0001LF_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.003 110.236 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 1.651 0.122 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 109.987 121.92 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at -0.381 0.767 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.003 121.92 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -0.127 -0.884 90) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+1V1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SON:WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4.3mm" (layer "F.Cu")
    (tedit 5DC5FB10)
    (at 106.68 105.156)
    (descr "WSON, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf (page 68)), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "WSON NoLead")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at -4.064 -2.54) (layer "F.SilkS"))
    (fp_text value "W25Q32JVZPIQ" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.85 -1.075) (size 1.37 1.73) (layers "F.Paste") (roundrect_rratio 0.182482))
    (pad "" smd roundrect (at 0.85 1.075) (size 1.37 1.73) (layers "F.Paste") (roundrect_rratio 0.182482))
    (pad "" smd roundrect (at -0.85 1.075) (size 1.37 1.73) (layers "F.Paste") (roundrect_rratio 0.182482))
    (pad "" smd roundrect (at 0.85 -1.075) (size 1.37 1.73) (layers "F.Paste") (roundrect_rratio 0.182482))
    (pad "1" smd roundrect (at -2.7 -1.905) (size 0.75 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/QSPI_SS_N") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd roundrect (at -2.7 -0.635) (size 0.75 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/QSPI_SD1") (pinfunction "DO(IO1)") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.7 0.635) (size 0.75 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/QSPI_SD2") (pinfunction "IO2") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.7 1.905) (size 0.75 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.7 1.905) (size 0.75 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/QSPI_SD0") (pinfunction "DI(IO0)") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.7 0.635) (size 0.75 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/QSPI_SCLK") (pinfunction "CLK") (pintype "input"))
    (pad "7" smd roundrect (at 2.7 -0.635) (size 0.75 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/QSPI_SD3") (pinfunction "IO3") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.7 -1.905) (size 0.75 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (pad "9" smd rect (at 0 0) (size 3.4 4.3) (layers "F.Cu" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SON.3dshapes/WSON-8-1EP_3x3mm_P0.5mm_EP1.6x2.0mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1.9 1.6 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.426 110.49 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -1.397 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/QSPI_SS_N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 103.378 118.872 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0.889 -1.397) (layer "F.SilkS"))
    (fp_text value "Serial" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/UART0_RX") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/UART0_TX") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-8_3x3mm_P0.65mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 130.302 116.078 -90)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -2.55 90) (layer "F.SilkS"))
    (fp_text value "PAM8302AAD" (at -0.635 0.127 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.15 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/SD") (pinfunction "~{SD}") (pintype "input"))
    (pad "2" smd rect (at -2.15 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "unconnected-(U4-Pad2)") (pinfunction "NC") (pintype "no_connect"))
    (pad "3" smd rect (at -2.15 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C16-Pad2)") (pinfunction "IN+") (pintype "input"))
    (pad "4" smd rect (at -2.15 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C17-Pad2)") (pinfunction "IN-") (pintype "input"))
    (pad "5" smd rect (at 2.15 0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(FB2-Pad1)") (pinfunction "OUT+") (pintype "output"))
    (pad "6" smd rect (at 2.15 0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "7" smd rect (at 2.15 -0.325 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect (at 2.15 -0.975 270) (size 1.1 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(FB3-Pad1)") (pinfunction "OUT-") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.189 113.792)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 0.889) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_Tactile_SPST_Angled_PTS645Vx83-2LFS" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 147.066 116.851 -90)
    (descr "tactile switch SPST right angle, PTS645VL83-2 LFS")
    (tags "tactile switch SPST angled PTS645VL83-2 LFS C&K Button")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW4" (at 2.25 1.68 90) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 2.25 5.38988 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.25 1.68 90) (layer "F.Fab"))
    (pad "" thru_hole circle (at -1.25 2.49 270) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.76 2.49 270) (size 2.1 2.1) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.75 1.75) (drill 0.99) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.5 0 270) (size 1.75 1.75) (drill 0.99) (layers *.Cu *.Mask)
      (net 29 "/BTN") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_Tactile_SPST_Angled_PTS645Vx83-2LFS.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.426 109.474 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -1.651 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/QSPI_SS_N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.094 113.792 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -1.397 0.635) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.936 117.094)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -0.635 -0.889) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.189 118.364)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0.099 -0.889) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.277 120.462)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C24" (at 1.581 -0.066) (layer "F.SilkS"))
    (fp_text value "220pf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(C24-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 114.305 110.617)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C23" (at 1.646 0) (layer "F.SilkS"))
    (fp_text value "1uf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+1V1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 119.253 109.728)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 1.27 1.143) (layer "F.SilkS"))
    (fp_text value "BAT54C" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Vbus") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/Vbat_sw") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/Vraw") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 103.929 122.428)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 2.497 -0.889) (layer "F.SilkS"))
    (fp_text value "Crystal_4pin_SMD" (at 0 2.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 0.85) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.1 0.85) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "3" smd rect (at 1.1 -0.85) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C4-Pad1)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.1 -0.85) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.428 105.156 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 1.905 90) (layer "F.SilkS"))
    (fp_text value "22uf" (at 0 2.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 125.796 113.157)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 113.924 112.014 90)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB1" (at 0.254 -0.767 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/ADC_AVDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "emeb_library:RV12" (layer "B.Cu")
    (tedit 0)
    (at 138.43 106.109 180)
    (property "Sheetfile" "buddhabox.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV1" (at 0 0.5 unlocked) (layer "B.SilkS"))
    (fp_text value "RV12" (at 0 -1 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at -8.2 -4 135) (size 3.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "/Vbat") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 8.2 -4 225) (size 3.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 66 "/Vbat_sw") (pinfunction "2") (pintype "passive"))
    (pad "3" smd roundrect (at -4.25 -7 205) (size 2.5 2.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" smd roundrect (at 0 -8.4 180) (size 2.5 2.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "/POT") (pinfunction "4") (pintype "passive"))
    (pad "5" smd roundrect (at 4.25 -7 155) (size 2.5 2.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "5") (pintype "passive"))
  )
  (footprint "emeb_library:avatar" (layer "B.Cu")
    (tedit 0)
    (at 111.633 111.252 180)
    (attr through_hole)
    (fp_text reference "Ref**" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "Val**" (at 0 0) (layer "B.SilkS") hide)
  )
  (gr_line (start 142.875 101.6) (end 145.034 101.6) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 149.86 124.46) (end 101.6 124.46) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 145.034 101.6) (end 146.558 103.124) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 101.6 101.6) (end 133.985 101.6) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 142.875 101.6) (mid 138.43 112.526458) (end 133.985 101.6) (layer "Edge.Cuts") (width 0.15))
  (gr_circle (center 126.492 103.886) (end 127.762 103.886) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_line (start 101.6 124.46) (end 101.6 101.6) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 149.86 110.49) (end 149.86 124.46) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 146.558 103.124) (end 146.558 107.188) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 149.86 110.49) (end 146.558 107.188) (layer "Edge.Cuts") (width 0.15))
  (gr_circle (center 141.986 116.84) (end 143.256 116.84) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_text "Buddhabox V0.1\n(c) 2022 E. Brombaugh" (at 128.016 116.84) (layer "B.SilkS"))
  (gr_text "TX" (at 103.3272 114.6556) (layer "F.SilkS"))
  (gr_text "Buddhabox" (at 137.414 114.3) (layer "F.SilkS"))
  (gr_text "Spkr-" (at 133.858 122.555 90) (layer "F.SilkS"))
  (gr_text "Spkr+" (at 127 122.555 90) (layer "F.SilkS"))
  (gr_text "RX" (at 102.108 118.872 90) (layer "F.SilkS"))
  (gr_text "3V Battery\n(-) (+)" (at 137.922 120.142) (layer "F.SilkS"))
  (gr_text "USR" (at 130.3274 103.759 90) (layer "F.SilkS"))
  (gr_text "SWD" (at 124.714 120.777) (layer "F.SilkS"))
  (gr_text "BOOT" (at 103.378 108.458) (layer "F.SilkS"))
  (gr_text "RST" (at 119.126 117.221) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.479 124.079)
        (xy 101.981 124.079)
        (xy 101.981 101.981)
        (xy 149.479 101.981)
      )
    )
  )
)
