(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 0)
    (no_connects 0)
    (area 151.054999 67.234999 174.065001 80.085001)
    (thickness 1.6)
    (drawings 20)
    (tracks 26)
    (zones 0)
    (modules 2)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 2.5)
    (user_trace_width 5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 5A19F7A7)
    (at 74.676 104.14 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference REF** (at 0 -1.27 270) (layer F.SilkS) hide)
    (fp_text value SOIC-8-N (at 0 1.27 270) (layer F.Fab) hide)
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5A19FB7B)
    (at 65.786 109.728 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Pin_Header_Straight_1x08_Pitch2.54mm (at 0 20.11 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.89 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 32bitfun.com (at 74.676 112.141) (layer B.SilkS))
  (gr_text "SOIC8 Adapter" (at 74.676 103.124) (layer B.SilkS))
  (gr_line (start 63.246 103.124) (end 63.246 113.284) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.106 103.124) (end 86.106 113.284) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.566 100.584) (end 65.786 100.584) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 65.786 103.124) (end 63.246 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 83.566 103.124) (end 83.566 100.584) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.246 113.284) (end 86.106 113.284) (layer Edge.Cuts) (width 0.15))
  (gr_text 1 (at 73.152 102.743) (layer F.SilkS))
  (gr_text 4 (at 73.152 105.664) (layer F.SilkS))
  (gr_text 5 (at 76.2 105.664) (layer F.SilkS))
  (gr_text 8 (at 76.2 102.743) (layer F.SilkS))
  (gr_text 8 (at 83.566 112.268) (layer F.SilkS))
  (gr_text 7 (at 81.026 112.268) (layer F.SilkS))
  (gr_text 6 (at 78.486 112.268) (layer F.SilkS))
  (gr_text 5 (at 75.946 112.268) (layer F.SilkS))
  (gr_text 4 (at 73.406 112.268) (layer F.SilkS))
  (gr_text 3 (at 70.866 112.268) (layer F.SilkS))
  (gr_text 2 (at 68.326 112.268) (layer F.SilkS))
  (gr_text 1 (at 65.786 112.268) (layer F.SilkS))
)
