(kicad_pcb (version 20171130) (host pcbnew 5.0.2-5.fc29)
  (general
    (thickness 1.6)
    (drawings 37)
    (tracks 117)
    (zones 0)
    (modules 7)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010b0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /D2)
  (net 3 /MISO)
  (net 4 /MOSI)
  (net 5 /SCK)
  (net 6 /NSS)
  (net 7 /RST)
  (net 8 /D5)
  (net 9 /D1)
  (net 10 /D0)
  (net 11 +3V3)
  (net 12 /D4)
  (net 13 /D3)
  (net 14 "Net-(J3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /NSS)
    (add_net /RST)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(J3-Pad1)")
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5EC6A283)
    (at 138.43 106.1975 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.43 270) (layer B.SilkS) hide)
    (fp_text value 100k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 /RST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RFM9X:RFM9X-SMD-Fixed locked (layer F.Cu) (tedit 5EC6A100)
    (at 143.495 106.06)
    (fp_text reference U1 (at 0 -9.5) (layer F.SilkS) hide)
    (fp_text value RFM9X (at 0 7) (layer F.SilkS))
    (pad 1 smd rect (at -7 -7) (size 3 1.3) (drill (offset -0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 7 -7) (size 3 1.3) (drill (offset 0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 /D2))
    (pad 2 smd rect (at -7 -5) (size 3 1.3) (drill (offset -0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 /MISO))
    (pad 3 smd rect (at -7 -3) (size 3 1.3) (drill (offset -0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 4 smd rect (at -7 -1) (size 3 1.3) (drill (offset -0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 5 smd rect (at -7 1) (size 3 1.3) (drill (offset -0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 6 /NSS))
    (pad 6 smd rect (at -7 3) (size 3 1.3) (drill (offset -0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 /RST))
    (pad 7 smd rect (at -7 5) (size 3 1.3) (drill (offset -0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 8 /D5))
    (pad 8 smd rect (at -7 7) (size 3 1.3) (drill (offset -0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 7 -5) (size 3 1.3) (drill (offset 0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 9 /D1))
    (pad 11 smd rect (at 7 -3) (size 3 1.3) (drill (offset 0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 10 /D0))
    (pad 12 smd rect (at 7 -1) (size 3 1.3) (drill (offset 0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 13 smd rect (at 7 1) (size 3 1.3) (drill (offset 0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 12 /D4))
    (pad 14 smd rect (at 7 3) (size 3 1.3) (drill (offset 0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 13 /D3))
    (pad 15 smd rect (at 7 5) (size 3 1.3) (drill (offset 0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 7 7) (size 3 1.3) (drill (offset 0.5 0)) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J3-Pad1)"))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5EC56EE7)
    (at 154.7875 102.235)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 +3V3))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:SMA_Amphenol_132134-11_Vertical locked (layer F.Cu) (tedit 5EC56F1C)
    (at 161.925 106.045)
    (descr https://www.amphenolrf.com/downloads/dl/file/id/3406/product/2975/132134_11_customer_drawing.pdf)
    (tags "SMA THT Female Jack Vertical ExtendedLegs")
    (zone_connect 2)
    (fp_text reference J3 (at 0 -4.75) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at 0 5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers *.Cu *.Mask)
      (net 14 "Net-(J3-Pad1)") (zone_connect 2))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-11_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical locked (layer F.Cu) (tedit 5EC56F13)
    (at 135.89 117.475 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 15.03 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.35 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /D5))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /D4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /D3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /D2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /D1))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /D0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical locked (layer F.Cu) (tedit 5EC56EC8)
    (at 135.89 94.615 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (zone_connect 2)
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x07 (at 0 17.57 90) (layer F.Fab) hide)
    (fp_text user %R (at 3.175 7.62 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RST) (zone_connect 2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /MISO) (zone_connect 2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /MOSI) (zone_connect 2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SCK) (zone_connect 2))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /NSS) (zone_connect 2))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3V3) (zone_connect 2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 159.385 99.06 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 270) (layer F.Fab) hide)
  )
  (gr_text "RFM9X\nBREAKOUT" (at 154.305 116.84) (layer F.SilkS))
  (gr_text DIO5 (at 135.89 115.57) (layer F.SilkS))
  (gr_text "DIO0\n" (at 148.59 115.57) (layer F.SilkS))
  (gr_text DIO1 (at 146.05 115.57) (layer F.SilkS))
  (gr_text DIO2 (at 143.51 115.57) (layer F.SilkS))
  (gr_text "DIO3\n" (at 140.97 115.57) (layer F.SilkS))
  (gr_text DIO4 (at 138.43 115.57) (layer F.SilkS))
  (gr_text 3V3 (at 151.13 96.52 180) (layer F.SilkS))
  (gr_text "GND\n" (at 148.59 96.52 180) (layer F.SilkS))
  (gr_text "NSS\n" (at 146.05 96.52 180) (layer F.SilkS))
  (gr_text SCK (at 143.51 96.52 180) (layer F.SilkS))
  (gr_text "MOSI\n" (at 140.97 96.52 180) (layer F.SilkS))
  (gr_text "MISO\n" (at 138.43 96.52 180) (layer F.SilkS))
  (gr_text "RST\n" (at 135.89 96.52 180) (layer F.SilkS))
  (gr_text JASONPAX.TECH (at 155.575 107.315 270) (layer F.SilkS))
  (gr_line (start 158.75 118.745) (end 133.35 118.745) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 167.005 110.49) (end 158.75 118.745) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 167.005 101.6) (end 167.005 110.49) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 158.75 93.345) (end 167.005 101.6) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.35 93.345) (end 158.75 93.345) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.35 118.745) (end 133.35 93.345) (layer Edge.Cuts) (width 0.2))
  (dimension 8.255 (width 0.3) (layer F.CrtYd)
    (gr_text "8.255 mm" (at 157.7975 119.575) (layer F.CrtYd))
    (feature1 (pts (xy 161.925 105.41) (xy 161.925 118.061421)))
    (feature2 (pts (xy 153.67 105.41) (xy 153.67 118.061421)))
    (crossbar (pts (xy 153.67 117.475) (xy 161.925 117.475)))
    (arrow1a (pts (xy 161.925 117.475) (xy 160.798496 118.061421)))
    (arrow1b (pts (xy 161.925 117.475) (xy 160.798496 116.888579)))
    (arrow2a (pts (xy 153.67 117.475) (xy 154.796504 118.061421)))
    (arrow2b (pts (xy 153.67 117.475) (xy 154.796504 116.888579)))
  )
  (dimension 11.43 (width 0.3) (layer F.CrtYd)
    (gr_text "11.430 mm" (at 124.265 111.76 270) (layer F.CrtYd))
    (feature1 (pts (xy 143.51 117.475) (xy 125.778579 117.475)))
    (feature2 (pts (xy 143.51 106.045) (xy 125.778579 106.045)))
    (crossbar (pts (xy 126.365 106.045) (xy 126.365 117.475)))
    (arrow1a (pts (xy 126.365 117.475) (xy 125.778579 116.348496)))
    (arrow1b (pts (xy 126.365 117.475) (xy 126.951421 116.348496)))
    (arrow2a (pts (xy 126.365 106.045) (xy 125.778579 107.171504)))
    (arrow2b (pts (xy 126.365 106.045) (xy 126.951421 107.171504)))
  )
  (dimension 22.86 (width 0.3) (layer F.CrtYd)
    (gr_text "22.860 mm" (at 118.536203 106.045 90) (layer F.CrtYd))
    (feature1 (pts (xy 135.255 94.615) (xy 120.049782 94.615)))
    (feature2 (pts (xy 135.255 117.475) (xy 120.049782 117.475)))
    (crossbar (pts (xy 120.636203 117.475) (xy 120.636203 94.615)))
    (arrow1a (pts (xy 120.636203 94.615) (xy 121.222624 95.741504)))
    (arrow1b (pts (xy 120.636203 94.615) (xy 120.049782 95.741504)))
    (arrow2a (pts (xy 120.636203 117.475) (xy 121.222624 116.348496)))
    (arrow2b (pts (xy 120.636203 117.475) (xy 120.049782 116.348496)))
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 93.345) (xy 158.75 93.345) (xy 167.005 101.6) (xy 167.005 110.49) (xy 158.75 118.745)
        (xy 133.35 118.745)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 93.345) (xy 158.75 93.345) (xy 161.925 96.52) (xy 167.005 101.6) (xy 167.005 105.41)
        (xy 167.005 110.49) (xy 163.195 114.3) (xy 158.75 118.745) (xy 133.35 118.745)
      )
    )
  )
)
