(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 63)
    (no_connects 0)
    (area -9.284 -53.352701 34.149 53.352701)
    (thickness 1.6)
    (drawings 20)
    (tracks 96)
    (zones 0)
    (modules 27)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.0508)
    (uvia_drill 0.0254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 +12V)
  (net 7 -12V)
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(D2-Pad1)")
  (net 10 "Net-(P3-Pad5)")
  (net 11 "Net-(P4-Pad5)")
  (net 12 "Net-(P5-Pad2)")
  (net 13 "Net-(P5-Pad3)")
  (net 14 "Net-(P6-Pad2)")
  (net 15 "Net-(P6-Pad3)")
  (net 16 "Net-(P3-Pad1)")
  (net 17 "Net-(P4-Pad1)")
  (net 18 "Net-(P5-Pad1)")
  (net 19 "Net-(P6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.0508)
    (uvia_drill 0.0254)
    (add_net +12V)
    (add_net -12V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad5)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
  )
  (module nearness:0805 (layer F.Cu) (tedit 5A49B1D3)
    (at 28.8925 -20.6375)
    (fp_text reference R16 (at 0 1.5875) (layer F.SilkS))
    (fp_text value 100k (at 0 1.905) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P5-Pad2)"))
  )
  (module nearness:0603 (layer F.Cu) (tedit 59C70EBF)
    (at 25.4 -33.02 180)
    (fp_text reference C1 (at 2.2225 0 270) (layer F.SilkS))
    (fp_text value 22p (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.8 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
  )
  (module nearness:0603 (layer F.Cu) (tedit 59CB911D)
    (at 25.4 33.02)
    (fp_text reference C2 (at -2.2225 0 90) (layer F.SilkS))
    (fp_text value 22p (at 0 1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.8 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 5A49B20C)
    (at 27.305 -2.54 180)
    (fp_text reference C3 (at -2.54 0 270) (layer F.SilkS))
    (fp_text value 22u (at 0 1.905 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +12V))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module nearness:0805 (layer F.Cu) (tedit 5A49B210)
    (at 27.305 2.54)
    (fp_text reference C4 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 22u (at 0 1.905) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 -12V))
  )
  (module nearness:0603 (layer F.Cu) (tedit 5A49ACC1)
    (at 20.955 -30.7975 90)
    (fp_text reference C5 (at 2.2225 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 +12V))
    (pad 2 smd rect (at 0.8 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module nearness:0603 (layer F.Cu) (tedit 59C70EBC)
    (at 29.845 -24.765 270)
    (fp_text reference C6 (at -2.2225 0 360) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 -12V))
  )
  (module nearness:0603 (layer F.Cu) (tedit 5A49AE03)
    (at 29.845 30.7975 270)
    (fp_text reference C7 (at 2.2225 0 360) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 +12V))
    (pad 2 smd rect (at 0.8 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module nearness:0603 (layer F.Cu) (tedit 59CB911B)
    (at 20.955 24.765 90)
    (fp_text reference C8 (at -2.2225 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 -12V))
  )
  (module nearness:SOD-123 (layer F.Cu) (tedit 59ACF59B)
    (at 27.305 -5.08 180)
    (fp_text reference D1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1N5819HW (at 0 1.905 180) (layer F.Fab))
    (pad 1 smd rect (at -1.9 0 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 6 +12V))
    (pad 2 smd rect (at 1.9 0 180) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad2)"))
  )
  (module nearness:SOD-123 (layer F.Cu) (tedit 59ACF59D)
    (at 27.305 5.08)
    (fp_text reference D2 (at 0 0) (layer F.SilkS))
    (fp_text value 1N5819HW (at 0 1.905) (layer F.Fab))
    (pad 1 smd rect (at -1.9 0) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.9 0) (size 1.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 -12V))
  )
  (module nearness:SOIC-8 (layer F.Cu) (tedit 59AD2098)
    (at 25.4 -26.9875)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value LME49720 (at 0 5.08) (layer F.Fab))
    (pad 1 smd rect (at -1.905 3) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at -0.635 3) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P3-Pad1)"))
    (pad 3 smd rect (at 0.635 3) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.905 3) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 7 -12V))
    (pad 5 smd rect (at 1.905 -3) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.635 -3) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at -0.635 -3) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (pad 8 smd rect (at -1.905 -3) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 6 +12V))
  )
  (module nearness:SOIC-8 (layer F.Cu) (tedit 59CB953A)
    (at 25.4 26.9875 180)
    (fp_text reference U2 (at 0 0 180) (layer F.SilkS))
    (fp_text value LME49720 (at 0 5.08 180) (layer F.Fab))
    (pad 1 smd rect (at -1.905 3 180) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P6-Pad1)"))
    (pad 2 smd rect (at -0.635 3 180) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P4-Pad1)"))
    (pad 3 smd rect (at 0.635 3 180) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.905 3 180) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 7 -12V))
    (pad 5 smd rect (at 1.905 -3 180) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.635 -3 180) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at -0.635 -3 180) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (pad 8 smd rect (at -1.905 -3 180) (size 0.65 2) (layers F.Cu F.Paste F.Mask)
      (net 6 +12V))
  )
  (module nearness:Pin_1x5 (layer F.Cu) (tedit 59ACF43A)
    (at 25.4 -42.2275 90)
    (fp_text reference P3 (at 0 -7.62 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X05 (at 0 7.62 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(P3-Pad5)"))
  )
  (module nearness:Pin_1x5 (layer F.Cu) (tedit 59ACF434)
    (at 25.4 42.2275 90)
    (fp_text reference P4 (at 0 -7.62 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X05 (at 0 7.62 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(P4-Pad5)"))
  )
  (module nearness:Pin_1x3 (layer F.Cu) (tedit 59ACFAE8)
    (at 22.86 -12.065)
    (fp_text reference P5 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 5.08) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(P5-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(P5-Pad3)"))
  )
  (module nearness:Pin_1x3 (layer F.Cu) (tedit 59ACFAED)
    (at 22.86 12.065 180)
    (fp_text reference P6 (at 0 -5.08 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(P6-Pad1)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(P6-Pad2)"))
    (pad 3 thru_hole circle (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(P6-Pad3)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 5A49B1CE)
    (at 24.13 -20.6375 180)
    (fp_text reference R15 (at 0 -1.5875 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.905 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P5-Pad1)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 59CB9553)
    (at 26.67 20.6375)
    (fp_text reference R17 (at 0 -1.5875 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.905) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P6-Pad1)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 59CB9551)
    (at 21.9075 20.6375 180)
    (fp_text reference R18 (at 0 1.5875 360) (layer F.SilkS))
    (fp_text value 100k (at 0 1.905 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P6-Pad2)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 59AD2308)
    (at 20.955 -26.3525 90)
    (fp_text reference R19 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.905 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 59AE7F5B)
    (at 29.845 26.3525 270)
    (fp_text reference R20 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value 100k (at 0 1.905 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P6-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 59C70C73)
    (at 26.9875 -36.5125 90)
    (fp_text reference R21 (at 2.54 0 360) (layer F.SilkS))
    (fp_text value 100k (at 0 1.905 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P3-Pad5)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 59CB9118)
    (at 23.8125 36.5125 270)
    (fp_text reference R22 (at 2.54 0 360) (layer F.SilkS))
    (fp_text value 100k (at 0 1.905 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P4-Pad5)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 59CB96FB)
    (at 23.8125 -36.5125 90)
    (fp_text reference R23 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.905 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 1 0 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P3-Pad5)"))
  )
  (module nearness:0805 (layer F.Cu) (tedit 59CB9114)
    (at 26.9875 36.5125 270)
    (fp_text reference R24 (at 2.54 0 360) (layer F.SilkS))
    (fp_text value 1k (at 0 1.905 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1 0 270) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P4-Pad5)"))
  )
  (module nearness:Eurorack_2x5 (layer B.Cu) (tedit 5A487B11)
    (at 21.59 0 180)
    (fp_text reference P7 (at -5.08 0 180) (layer B.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -10.16 180) (layer B.Fab))
    (fp_text user -12V (at -5.08 -5.08 180) (layer B.SilkS))
    (fp_text user +12V (at -5.08 5.08 180) (layer B.SilkS) hide)
    (pad 3 thru_hole circle (at -1.27 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at -1.27 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -1.27 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -1.27 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad1)"))
    (pad 1 thru_hole circle (at 1.27 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(D2-Pad1)"))
  )
  (gr_line (start 18.415 44.1325) (end 18.415 -44.1325) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 32.385 44.1325) (end 18.415 44.1325) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 32.385 -44.1325) (end 32.385 44.1325) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 18.415 -44.1325) (end 32.385 -44.1325) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_text -6dB (at 30.48 13.335 90) (layer F.SilkS))
  (gr_text -6dB (at 30.48 -13.335 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.923 -43.6245) (xy 31.877 -43.6245) (xy 31.877 43.6245) (xy 18.923 43.6245)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.923 -43.6245) (xy 31.877 -43.6245) (xy 31.877 43.6245) (xy 18.923 43.6245)
      )
    )
  )
)
