(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 343)
    (zones 0)
    (modules 40)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.15)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 1)
    (via_drill 0.5)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 50.8 153.67)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x210fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "prototype_osh"))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad48)")
  (net 2 "Net-(U1-Pad46)")
  (net 3 "Net-(U1-Pad45)")
  (net 4 "Net-(U1-Pad41)")
  (net 5 "Net-(U1-Pad39)")
  (net 6 "Net-(U1-Pad38)")
  (net 7 "Net-(U1-Pad37)")
  (net 8 "Net-(U1-Pad28)")
  (net 9 "Net-(U1-Pad27)")
  (net 10 "Net-(U1-Pad26)")
  (net 11 "Net-(U1-Pad25)")
  (net 12 "Net-(U1-Pad22)")
  (net 13 "Net-(U1-Pad16)")
  (net 14 "Net-(U1-Pad15)")
  (net 15 "Net-(U1-Pad12)")
  (net 16 "Net-(U1-Pad11)")
  (net 17 "Net-(U1-Pad4)")
  (net 18 GND)
  (net 19 +5V)
  (net 20 "Net-(C2-Pad1)")
  (net 21 "Net-(C3-Pad1)")
  (net 22 +3V3)
  (net 23 "Net-(C6-Pad2)")
  (net 24 "Net-(J1-Pad4)")
  (net 25 /D+)
  (net 26 /D-)
  (net 27 /MOSI)
  (net 28 /SCK)
  (net 29 /MISO)
  (net 30 /TX2)
  (net 31 /RX2)
  (net 32 /TX3)
  (net 33 /RX3)
  (net 34 "Net-(U5-Pad5)")
  (net 35 "Net-(U5-Pad4)")
  (net 36 "Net-(U5-Pad1)")
  (net 37 /SDA)
  (net 38 /SCL)
  (net 39 +12V)
  (net 40 /SAMD_Reset)
  (net 41 "Net-(R4-Pad2)")
  (net 42 /PA02_AIN0)
  (net 43 /PA02_AIN2)
  (net 44 /PA02_AIN3)
  (net 45 /PA02_AIN4)
  (net 46 /PA02_AIN5)
  (net 47 "Net-(U1-Pad14)")
  (net 48 /PA02_AIN10)
  (net 49 "Net-(Q1-Pad2)")
  (net 50 "Net-(Q1-Pad1)")
  (net 51 /PID_base)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.25)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D+)
    (add_net /D-)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PA02_AIN0)
    (add_net /PA02_AIN10)
    (add_net /PA02_AIN2)
    (add_net /PA02_AIN3)
    (add_net /PA02_AIN4)
    (add_net /PA02_AIN5)
    (add_net /PID_base)
    (add_net /RX2)
    (add_net /RX3)
    (add_net /SAMD_Reset)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX2)
    (add_net /TX3)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad5)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 54.9 150.17)
    (fp_text reference H6 (at 5.25 1) (layer F.SilkS))
    (fp_text value 4mm_hole (at 7.5 -0.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 54.9 92.17)
    (fp_text reference H-1 (at 5 1.25) (layer F.SilkS))
    (fp_text value 4mm_hole (at 6.5 -0.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 95.3 121.42)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 750 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /PID_base))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-3 (layer F.Cu) (tedit 5A02FF57)
    (at 96.05 125.67)
    (descr SOT-89-3)
    (tags SOT-89-3)
    (attr smd)
    (fp_text reference Q1 (at 0.45 -3.2) (layer F.SilkS))
    (fp_text value Q_NPN_BCE (at 0.45 3.25) (layer F.Fab))
    (fp_text user %R (at 0.38 0 90) (layer F.Fab))
    (pad 2 smd trapezoid (at -0.0762 0 90) (size 1.5 1) (rect_delta 0 0.7 ) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 1.3335 0 270) (size 2.2 1.84) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Q1-Pad2)"))
    (pad 3 smd rect (at -1.48 1.5 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at -1.3335 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Q1-Pad2)"))
    (pad 1 smd rect (at -1.48 -1.5 270) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(Q1-Pad1)"))
    (pad 2 smd trapezoid (at 2.667 0 270) (size 1.6 0.85) (rect_delta 0 0.6 ) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 88.3 144.92 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /SAMD_Reset))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /MOSI))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /SCK))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /MISO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 73.02 101.695 90)
    (fp_text reference U8 (at 2.775 -2.47 90) (layer F.SilkS))
    (fp_text value 5V (at 0.025 3.25 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 +12V) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V) (solder_mask_margin 0.07))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 73.05 98.92 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 1.75) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 73.05 104.42 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1uF (at 0 -1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fireboard:CO (layer B.Cu) (tedit 5D139581)
    (at 108.8 122.17 180)
    (fp_text reference U5 (at 0 31.5) (layer B.SilkS))
    (fp_text value CO (at 0 32.5) (layer B.Fab))
    (fp_text user "Bottom Components Width 2.5mm" (at 0 24.25) (layer B.SilkS))
    (fp_text user "Board Width 1.6mm" (at 0 25.75) (layer B.SilkS))
    (fp_text user "Top Components Width 9mm" (at 0 27.5) (layer B.SilkS))
    (fp_text user "Total Width 13mm" (at 0 30) (layer B.SilkS))
    (pad 8 thru_hole circle (at 8.79 -26.352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 +3V3))
    (pad 7 thru_hole circle (at 6.25 -26.352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 +3V3))
    (pad 6 thru_hole circle (at 3.71 -26.352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 5 thru_hole circle (at 1.17 -26.352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(U5-Pad5)"))
    (pad 4 thru_hole circle (at -1.37 -26.352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U5-Pad4)"))
    (pad 3 thru_hole circle (at -3.91 -26.352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 /RX3))
    (pad 2 thru_hole circle (at -6.45 -26.352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 /TX3))
    (pad 1 thru_hole circle (at -8.99 -26.352 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(U5-Pad1)"))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 81.55 101.67 180)
    (fp_text reference D1 (at 0.025 -3.375) (layer F.SilkS))
    (fp_text value D_Schottky_AAK (at -2.5 0 270) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95 180) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 180) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0 180) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 +12V) (solder_mask_margin 0.07))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 64.8 97.67 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0.75 -7.5 90) (layer F.SilkS))
    (fp_text value Link (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /SCL))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /SDA))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 +12V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Wuerth_614105150721_Vertical (layer F.Cu) (tedit 5A142044)
    (at 61.3 144.67 180)
    (descr "USB Micro-B receptacle, through-hole, vertical, http://katalog.we-online.de/em/datasheet/614105150721.pdf")
    (tags "usb micro receptacle vertical")
    (fp_text reference J1 (at 1.3 -2.48) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 1.3 2.92) (layer F.Fab))
    (fp_text user %R (at 1.3 0.22) (layer F.Fab))
    (pad 6 thru_hole oval (at 4.875 0.22 180) (size 0.85 1.85) (drill oval 0.35 1.35) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 6 thru_hole oval (at -2.275 0.22 180) (size 0.85 1.85) (drill oval 0.35 1.35) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 5 thru_hole circle (at 2.6 0 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 4 thru_hole circle (at 1.95 1 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 1.3 0 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask)
      (net 25 /D+))
    (pad 2 thru_hole circle (at 0.65 1 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask)
      (net 26 /D-))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask)
      (net 19 +5V))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Wuerth_614105150721_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Tactile_SMD_6x6mm_PTS645 (layer F.Cu) (tedit 5AF35643)
    (at 76.05 134.17)
    (descr http://www.ckswitches.com/media/1471/pts645.pdf)
    (fp_text reference S1 (at 0 -4.27) (layer F.SilkS))
    (fp_text value KS-01Q-01 (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 3 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R4-Pad2)"))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 76.8 101.67 90)
    (fp_text reference U7 (at 3 2.5 90) (layer F.SilkS))
    (fp_text value 5V (at 1 -2.5 90) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 +12V) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0 90) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 +5V) (solder_mask_margin 0.07))
  )
  (module fireboard:CO2 (layer F.Cu) (tedit 5D163504)
    (at 152.8 121.17)
    (fp_text reference U6 (at 0 -2.802) (layer F.SilkS))
    (fp_text value CO2 (at 0 -3.802) (layer F.Fab))
    (fp_text user "Board Width 1.5mm" (at 0 -28.25) (layer F.SilkS))
    (fp_text user "Botom Componets Width 3mm" (at 0 -26.75) (layer F.SilkS))
    (fp_text user "Top Componets Width 8mm" (at 0 -29.75) (layer F.SilkS))
    (fp_text user "Total Width 13mm" (at 0 -31.5) (layer F.SilkS))
    (pad 5 thru_hole circle (at 9.144 23.368) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /SDA))
    (pad "" thru_hole circle (at -25.25 -22.25) (size 5 5) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 25.25 22.25) (size 5 5) (drill 3.2) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 11.62 23.368) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 /SCL))
    (pad 3 thru_hole circle (at 14.16 23.368) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 +12V))
    (pad 2 thru_hole circle (at 16.7 23.368) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1 thru_hole circle (at 19.24 23.35) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 +3V3))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 72.8 129.92 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.5) (layer F.SilkS))
    (fp_text value 22R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /SAMD_Reset))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 79.05 129.92)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /SAMD_Reset))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 76.8 98.92 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 1.75) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 76.8 104.42 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1uF (at 0 -1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 121.8 125.67)
    (fp_text reference OUT (at 0 4) (layer F.SilkS))
    (fp_text value 4mm_hole (at 0 5.5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 121.8 114.17)
    (fp_text reference IN (at 0 4) (layer F.SilkS))
    (fp_text value 4mm_hole (at 0 5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 80.3 150.17)
    (fp_text reference H5 (at 5.25 1) (layer F.SilkS))
    (fp_text value 4mm_hole (at 7.5 -0.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 122.8 150.17)
    (fp_text reference H4 (at 4.75 1.25) (layer F.SilkS))
    (fp_text value 4mm_hole (at 6.5 -0.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 178.8 150.17)
    (fp_text reference H3 (at -4.5 1.25) (layer F.SilkS))
    (fp_text value 4mm_hole (at -7 -0.4) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 178.8 92.17)
    (fp_text reference H2 (at -4.5 1.25) (layer F.SilkS))
    (fp_text value 4mm_hole (at -7 -0.4) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 80.3 92.17)
    (fp_text reference H0 (at 5 1.25) (layer F.SilkS))
    (fp_text value 4mm_hole (at 6.5 -0.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module fireboard:4mm_hole (layer F.Cu) (tedit 5D161793)
    (at 122.8 92.17)
    (fp_text reference H1 (at 5.25 1) (layer F.SilkS))
    (fp_text value 4mm_hole (at 7 -0.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 5 5) (drill 4) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 78.3 143.92 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -2.88 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 112.05 111.17 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3 0 90) (layer F.SilkS))
    (fp_text value 12.5pF (at 0 -1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 113.3 111.17 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 3 0 90) (layer F.SilkS))
    (fp_text value 12.5pF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 72.8 143.92 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -2.75 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 3 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 112.3 132.17 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 4.7k (at -2.5 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /SCL))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 109.3 132.17 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 4.7k (at -2.5 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /SDA))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_3215-2Pin_3.2x1.5mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 113.05 108.17)
    (descr "SMD Crystal FC-135 https://support.epson.biz/td/api/doc_check.php?dl=brief_FC-135R_en.pdf")
    (tags "SMD SMT Crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 2) (layer F.SilkS))
    (fp_text value 32.86MHz (at 0.5 3.5) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at -1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C3-Pad1)"))
    (pad 1 smd rect (at 1.25 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3215-2Pin_3.2x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fireboard:PID-AH (layer B.Cu) (tedit 5D13BF07)
    (at 87.8 121.67)
    (fp_text reference U4 (at 0 5.588) (layer B.SilkS))
    (fp_text value PID-AH (at 0 7.366) (layer B.Fab))
    (pad 3 thru_hole circle (at 2.54 3.81) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 49 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole circle (at 0 -3.81) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 42 /PA02_AIN0))
    (pad 1 thru_hole circle (at -2.54 3.81) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 19 +5V))
  )
  (module fireboard:LOX-02-S (layer B.Cu) (tedit 5D1379BC)
    (at 67.3 119.67)
    (fp_text reference U3 (at 0 1.27) (layer B.SilkS))
    (fp_text value LOX-02-S (at 0 2.54) (layer B.Fab))
    (pad 4 thru_hole circle (at -2.54 7) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /TX2))
    (pad 3 thru_hole circle (at 0 7) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /RX2))
    (pad 2 thru_hole circle (at -2.54 -5.7) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1 thru_hole circle (at 2.54 -5.7) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 +5V))
  )
  (module digikey-footprints:SOT-23-3 (layer F.Cu) (tedit 59D275F3)
    (at 75.59 144.04)
    (fp_text reference U2 (at 0.025 -2.87) (layer F.SilkS))
    (fp_text value 3.3V (at -0.04 2.88) (layer F.Fab))
    (fp_text user %R (at -0.125 0.15) (layer F.Fab))
    (pad 1 smd rect (at -1.05 -0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.05 0.95) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 +12V) (solder_mask_margin 0.07))
    (pad 3 smd rect (at 1.05 0) (size 1.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3) (solder_mask_margin 0.07))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 118.05 120.67 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 3 0 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 "Net-(C6-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 104.3 112.67 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100uF (at -0.5 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 +3V3))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-48_7x7mm_P0.5mm (layer F.Cu) (tedit 5A02F146)
    (at 109.13 120.69 270)
    (descr "48 LEAD TQFP 7x7mm (see MICREL TQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -6 90) (layer F.SilkS))
    (fp_text value ATSAMD21G18A-AUT (at 0 6.52 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at -4.35 -2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -4.35 -1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 /PA02_AIN0))
    (pad 4 smd rect (at -4.35 -1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -4.35 -0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 6 smd rect (at -4.35 -0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 7 smd rect (at -4.35 0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 /PA02_AIN2))
    (pad 8 smd rect (at -4.35 0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 /PA02_AIN3))
    (pad 9 smd rect (at -4.35 1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 /PA02_AIN4))
    (pad 10 smd rect (at -4.35 1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 /PA02_AIN5))
    (pad 11 smd rect (at -4.35 2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -4.35 2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at -2.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 /PID_base))
    (pad 14 smd rect (at -2.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at -1.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at -1.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at -0.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 18 smd rect (at -0.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 19 smd rect (at 0.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /MOSI))
    (pad 20 smd rect (at 0.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /SCK))
    (pad 21 smd rect (at 1.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 /MISO))
    (pad 22 smd rect (at 1.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 2.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /TX2))
    (pad 24 smd rect (at 2.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /RX2))
    (pad 25 smd rect (at 4.35 2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 4.35 2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at 4.35 1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 4.35 1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at 4.35 0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /TX3))
    (pad 30 smd rect (at 4.35 0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 /RX3))
    (pad 31 smd rect (at 4.35 -0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 /SDA))
    (pad 32 smd rect (at 4.35 -0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 /SCL))
    (pad 33 smd rect (at 4.35 -1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /D-))
    (pad 34 smd rect (at 4.35 -1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 /D+))
    (pad 35 smd rect (at 4.35 -2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 36 smd rect (at 4.35 -2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 37 smd rect (at 2.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 2.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad38)"))
    (pad 39 smd rect (at 1.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad39)"))
    (pad 40 smd rect (at 1.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 /SAMD_Reset))
    (pad 41 smd rect (at 0.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad41)"))
    (pad 42 smd rect (at 0.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 43 smd rect (at -0.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C6-Pad2)"))
    (pad 44 smd rect (at -0.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 +3V3))
    (pad 45 smd rect (at -1.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad45)"))
    (pad 46 smd rect (at -1.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad46)"))
    (pad 47 smd rect (at -2.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 /PA02_AIN10))
    (pad 48 smd rect (at -2.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U1-Pad48)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-48_7x7mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 54.9 150.17) (end 56.9 150.17) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 54.9 92.17) (end 56.9 92.17) (layer Edge.Cuts) (width 0.05))
  (gr_text "LAWRENCE FACTORY" (at 106.8 99.67) (layer F.SilkS))
  (gr_text "FIREBOARD\nPROTOTYPE" (at 106.8 95.17) (layer F.SilkS))
  (gr_circle (center 121.8 125.67) (end 123.8 125.67) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 121.8 114.17) (end 123.8 114.17) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 122.8 92.17) (end 124.8 92.17) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 80.3 92.17) (end 82.3 92.17) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 80.3 150.17) (end 82.3 150.17) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 122.8 150.17) (end 124.8 150.17) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 178.8 150.17) (end 180.8 150.17) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 178.8 92.17) (end 180.8 92.67) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50.8 88.67) (end 50.8 153.67) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 181.3 88.67) (end 50.8 88.67) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 181.3 153.67) (end 181.3 88.67) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 50.8 153.67) (end 181.3 153.67) (layer Edge.Cuts) (width 0.12))
)
