(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.59)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (33 "F.Adhes" user "F.Adhesive")
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J8-Pad1)")
  (net 2 "Net-(J9-Pad1)")
  (net 3 "Net-(Q1-Pad1)")
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 86.36 53.34)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "BATT+" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 83.82 55.88)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "PB+" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J9-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 86.4616 55.9816 180)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at -0.254 2.286 180) (layer "F.SilkS"))
    (fp_text value "Q_PMOS_GDS" (at 0 2.5 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J8-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(J9-Pad1)") (pinfunction "S") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 54.61)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 83.82 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 83.82 46.99)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (net 3 "Net-(Q1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 87.63 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 92.8116 55.9816 180)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at -0.254 2.286 180) (layer "F.SilkS"))
    (fp_text value "Q_PMOS_GDS" (at 0 2.5 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J8-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(J9-Pad1)") (pinfunction "S") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 46.99)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 86.6775 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 90.17 53.34)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "SW" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 55.5625)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 92.8116 49.6316 180)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at -0.254 2.286 180) (layer "F.SilkS"))
    (fp_text value "Q_PMOS_GDS" (at 0 2.5 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J8-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(J9-Pad1)") (pinfunction "S") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 56.515)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 82.8675 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 93.345 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 90.17 49.53)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "PB+" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 48.895)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 85.725 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 46.0375)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 92.3925 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 94.2975 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 47.9425)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 57.4675)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 52.705)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 90.4875 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 49.8475)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 50.8)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 92.71 46.99)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "BATT+" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 89.535 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 53.6575)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 86.36 46.99)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "BATT+" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 83.82 53.34)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "SW" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(Q1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 88.5825 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 83.82 49.53)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "PB+" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 90.17 46.99)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "SW" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 91.44 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 90.17 55.88)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "PB+" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 92.71 53.34)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "BATT+" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers F&B.Cu *.Mask)
      (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "drill:drill" (layer "F.Cu")
    (tedit 0)
    (at 84.7725 51.7525)
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "drill" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 0.01 0.01) (drill 0.635) (layers "F.Cu"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 86.4616 49.6316 180)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at -0.254 2.286 180) (layer "F.SilkS"))
    (fp_text value "Q_PMOS_GDS" (at 0 2.5 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect locked (at -1 0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J8-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(J9-Pad1)") (pinfunction "S") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 92.7608 56.0324 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "100k" (at 0 -1.43) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 86.36 49.6824 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "100k" (at 0 -1.43) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 86.4108 56.0324 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "100k" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Q1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 92.7608 49.6824 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "/net/cytocin/raid/home/hubbe/hack/teensy/lightsaber/fet_breakout/graflex_helper_board.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "100k" (at 0 -1.43) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "B.Cu" "B.Mask") (roundrect_rratio 0.25)
      (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 88.265 57.785) (end 88.9 57.785) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 94.615 45.72) (end 94.615 51.435) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 82.55 57.785) (end 82.55 52.07) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 94.615 52.07) (end 94.615 57.785) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 88.265 45.72) (end 88.9 45.72) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 82.55 51.435) (end 82.55 45.72) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 94.615 51.435) (end 94.615 52.07) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 88.9 45.72) (end 94.615 45.72) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 94.615 57.785) (end 88.9 57.785) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 82.55 45.72) (end 88.265 45.72) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 88.265 57.785) (end 82.55 57.785) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 82.55 52.07) (end 82.55 51.435) (layer "Edge.Cuts") (width 0.15))
)
