(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 49)
    (zones 0)
    (modules 7)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 1)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.75 1)
    (user_via 4 3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad10)")
  (net 7 "Net-(J1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
    (add_net VCC)
  )
  (module custom:ph2.0_6 (layer F.Cu) (tedit 5C7A8677)
    (at 80.01 120.19)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J7 (at 31 -4) (layer F.SilkS) hide)
    (fp_text value Conn_01x12_Male (at 31 7) (layer F.Fab))
    (fp_text user %R (at 31 5) (layer F.Fab))
    (pad 11 thru_hole rect (at 60 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 12 thru_hole oval (at 62 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 9 thru_hole rect (at 48 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 10 thru_hole oval (at 50 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 7 thru_hole rect (at 36 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 8 thru_hole oval (at 38 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 6 thru_hole oval (at 26 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 thru_hole rect (at 24 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 4 thru_hole oval (at 14 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 3 thru_hole rect (at 12 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:ph2.0_6 (layer F.Cu) (tedit 5C7A8677)
    (at 80.01 111.3)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J4 (at 31 -4) (layer F.SilkS) hide)
    (fp_text value Conn_01x12_Male (at 31 7) (layer F.Fab))
    (fp_text user %R (at 31 5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole rect (at 12 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 4 thru_hole oval (at 14 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 5 thru_hole rect (at 24 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 6 thru_hole oval (at 26 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 8 thru_hole oval (at 38 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 7 thru_hole rect (at 36 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 10 thru_hole oval (at 50 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 9 thru_hole rect (at 48 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 12 thru_hole oval (at 62 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 11 thru_hole rect (at 60 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:ph2.0_6 (layer F.Cu) (tedit 5C7A8677)
    (at 80.01 102.41)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J3 (at 31 -4) (layer F.SilkS) hide)
    (fp_text value Conn_01x12_Male (at 31 7) (layer F.Fab))
    (fp_text user %R (at 31 5) (layer F.Fab))
    (pad 11 thru_hole rect (at 60 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 12 thru_hole oval (at 62 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 9 thru_hole rect (at 48 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 10 thru_hole oval (at 50 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 7 thru_hole rect (at 36 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 8 thru_hole oval (at 38 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 6 thru_hole oval (at 26 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 thru_hole rect (at 24 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 4 thru_hole oval (at 14 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 3 thru_hole rect (at 12 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:ph2.0_6 (layer F.Cu) (tedit 5C7A8677)
    (at 80.01 93.52)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J2 (at 31 -4) (layer F.SilkS) hide)
    (fp_text value Conn_01x12_Male (at 31 7) (layer F.Fab))
    (fp_text user %R (at 31 5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole rect (at 12 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 4 thru_hole oval (at 14 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 5 thru_hole rect (at 24 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 6 thru_hole oval (at 26 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 8 thru_hole oval (at 38 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 7 thru_hole rect (at 36 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 10 thru_hole oval (at 50 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 9 thru_hole rect (at 48 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 12 thru_hole oval (at 62 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 11 thru_hole rect (at 60 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:ph2.0_6 (layer F.Cu) (tedit 5C7A8677)
    (at 80.01 84.63)
    (descr "JST PH series connector, B2B-PH-K, top entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J1 (at 31 -4) (layer F.SilkS) hide)
    (fp_text value Conn_01x12_Male (at 31 7) (layer F.Fab))
    (fp_text user %R (at 31 5) (layer F.Fab))
    (pad 11 thru_hole rect (at 60 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 12 thru_hole oval (at 62 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 9 thru_hole rect (at 48 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 10 thru_hole oval (at 50 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 7 thru_hole rect (at 36 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 8 thru_hole oval (at 38 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 6 thru_hole oval (at 26 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 thru_hole rect (at 24 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 4 thru_hole oval (at 14 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 3 thru_hole rect (at 12 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B2B-PH-K_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:balance_plug (layer F.Cu) (tedit 5BAFA1EB)
    (at 99.933415 76.145683 90)
    (fp_text reference J6 (at 0 10.16 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x07_Female (at 0 -8.89 90) (layer F.Fab))
    (pad 1 smd roundrect (at 0 7.62 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 2 smd roundrect (at 0 5.08 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad10)"))
    (pad 3 smd roundrect (at 0 2.54 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pad8)"))
    (pad 4 smd roundrect (at 0 0 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 smd roundrect (at 0 -2.54 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(J1-Pad4)"))
    (pad 6 smd roundrect (at 0 -5.08 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad2)"))
    (pad 7 smd roundrect (at 0 -7.62 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
  )
  (module custom:xt60_pad (layer F.Cu) (tedit 5BAFA200)
    (at 124.963415 76.145683 90)
    (fp_text reference J5 (at 0 0.762 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Female (at 0 -0.762 90) (layer F.Fab))
    (pad 1 smd roundrect (at 0 3.6 90) (size 4 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VCC))
    (pad 2 smd roundrect (at 0 -3.6 90) (size 4 4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
  )
  (gr_text "1s Charging Board" (at 103.5 107) (layer B.SilkS))
  (gr_text "Created by Phobos" (at 103.5 115.8) (layer B.SilkS))
  (gr_text + (at 128.438415 79.645683 90) (layer F.SilkS))
  (gr_text + (at 107.563415 78.895683 180) (layer F.SilkS))
  (gr_text - (at 121.313415 79.645683 180) (layer F.SilkS))
  (gr_text - (at 92.313415 78.895683 180) (layer F.SilkS))
  (gr_line (start 77.9 123.1) (end 77.9 74.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.1 123.1) (end 77.9 123.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.9 74.1) (end 144.1 74.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.1 123.1) (end 144.1 74.1) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name "Net-(J1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 81.4 83.8) (xy 92.6 83.8) (xy 92.6 121) (xy 81.4 121)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pad4)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 93.4 83.8) (xy 104.6 83.8) (xy 104.6 121) (xy 93.4 121)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pad6)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 105.4 83.8) (xy 116.6 83.8) (xy 116.6 121) (xy 105.4 121)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pad8)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 117.4 83.8) (xy 128.6 83.8) (xy 128.6 121) (xy 117.4 121)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pad10)") (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 129.4 83.8) (xy 140.6 83.8) (xy 140.6 121) (xy 129.4 121)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 105 74) (xy 105 123.25) (xy 144.25 123.25) (xy 144.25 74)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 105 74) (xy 77.75 74) (xy 77.75 123.25) (xy 105 123.25)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 77.75 74) (xy 144.25 74) (xy 144.25 123.25) (xy 77.75 123.25)
      )
    )
  )
)
