(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.646)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0254)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.524)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0254)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "./")
		)
	)
	(net 0 "")
	(net 1 "DRAIN")
	(net 2 "+24V")
	(net 3 "GND")
	(net 4 "BASE")
	(net 5 "D11")
	(net 6 "GATE")
	(net 7 "RMB-")
	(net 8 "VCC")
	(net 9 "MOSI")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 128.425 117.49 -90)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "H5"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PinHeader_1x05_P2.54mm_Vertical"
			(at 0 12.49 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "VCC")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "RMB-")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "VCC")
		)
		(pad "4" thru_hole rect
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "5" thru_hole rect
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 113.77 101.29 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
		(property "Reference" "0.1uf"
			(at 2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "C_Disc_D7.0mm_W2.5mm_P5.00mm"
			(at 2.5 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "VCC")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "RMB-")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 120.64 101.3 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "100K"
			(at 5.08 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GATE")
		)
		(pad "2" thru_hole rect
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92L_HandSolder"
		(layer "F.Cu")
		(at 115.11 117.48 90)
		(descr "TO-92L leads in-line (large body variant of TO-92), also known as TO-226, wide, drill 0.75mm, hand-soldering variant with enlarged pads (see https://www.diodes.com/assets/Package-Files/TO92L.pdf and http://www.ti.com/lit/an/snoa059/snoa059.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "2N2222"
			(at 1.27 -3.8 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TO-92L_HandSolder"
			(at 1.27 2.79 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92L_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.1 1.8)
			(drill 0.75
				(offset 0 0.4)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "2" thru_hole roundrect
			(at 1.27 -1.27 90)
			(size 1.1 1.8)
			(drill 0.75
				(offset 0 -0.4)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "BASE")
		)
		(pad "3" thru_hole roundrect
			(at 2.54 0 90)
			(size 1.1 1.8)
			(drill 0.75
				(offset 0 0.4)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 7 "RMB-")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92L.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 113.67 109.345)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "SOL IN"
			(at 2.2 1.14 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PinHeader_1x02_P2.54mm_Vertical"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+24V")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 126.93 111.81 90)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "1N4001"
			(at 5.58 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 5.08 2.47 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 -90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.1 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 90)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+24V")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "DRAIN")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 123.75 111.46 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "1K"
			(at 5.08 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 5.08 2.37 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MOSI")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GATE")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 117.51 101.58 -90)
		(descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "1N4001"
			(at 5.58 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 5.08 2.47 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.1 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 5.47 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "VCC")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "RMB-")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 131.17 106.83 180)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "IRL540"
			(at 2.06 2.55 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "PinHeader_1x03_P2.54mm_Vertical"
			(at 0 7.41 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "DRAIN")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GATE")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 -5.08 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 118.27 114.68)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "1K"
			(at 5.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "BASE")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "D11")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 131.35 117.48 180)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "H4"
			(at 0 -2.33 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PinHeader_1x04_P2.54mm_Vertical"
			(at 0 9.95 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "D11")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MOSI")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 2 2)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+24V")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 2 2)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "DRAIN")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 112.04 99.97)
		(end 133.04 118.97)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "4\n"
		(at 128.82 116.61 0)
		(layer "B.SilkS")
	)
	(gr_text "FEEDBACK4IR v1.1"
		(at 122.42 104.89 0)
		(layer "B.SilkS")
	)
	(gr_text "6"
		(at 130.43 114.48 90)
		(layer "B.SilkS")
	)
	(gr_text "5"
		(at 130.46 117.05 90)
		(layer "B.SilkS")
	)
	(gr_text "VCC"
		(at 124.38 116.68 0)
		(layer "B.SilkS")
	)
	(gr_text "8"
		(at 130.46 109.43 90)
		(layer "B.SilkS")
	)
	(gr_text "7"
		(at 130.43 111.95 90)
		(layer "B.SilkS")
	)
	(gr_text "1:SOL-\n2:SOL+\n3:RMB-\n4:RMB+"
		(at 128.4 109.66 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 121.85 116.65 0)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 114.68 109.71 -90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 119.38 116.65 0)
		(layer "B.SilkS")
	)
	(gr_text "2\n"
		(at 114.63 112.28 270)
		(layer "B.SilkS")
	)
	(gr_text "5:RMB Signal\n6:SOL Signal\n7:SOL Output\n8:SOL Output"
		(at 123.4 109.64 0)
		(layer "B.SilkS")
	)
	(gr_text "3"
		(at 126.25 116.63 0)
		(layer "B.SilkS")
	)
	(gr_text "\n"
		(at 128.76 108.74 270)
		(layer "B.SilkS")
	)
	(gr_text "IRL540"
		(at 129.685992 106.998027 90)
		(layer "F.SilkS")
	)
	(zone
		(net 3)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 111.79 99.59) (xy 133.36 99.62) (xy 133.29 119.08) (xy 111.83 119.19)
			)
		)
	)
)