(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "User" 215.9 139.7)
  (title_block
    (title "CC Monitor")
    (date "2023-02-18")
    (rev "1.0")
    (company "CC-SA 4.0")
    (comment 2 "(c) 2023")
    (comment 3 "Wolfgang Friedrich")
    (comment 4 "Pier42 Electronics Design")
  )
  (layers
    (0 "F.Cu" jumper)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 150 86)
    (grid_origin 150 86)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/")
    )
  )
  (net 0 "")
  (net 1 "VBUS")
  (net 2 "GND")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "/+3.3V")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "/CC1_L")
  (net 7 "/CC2_L")
  (net 8 "/CC1")
  (net 9 "/D-")
  (net 10 "/D+")
  (net 11 "/SBU1")
  (net 12 "/CC2")
  (net 13 "/SBU2")
  (net 14 "Net-(R3-Pad2)")
  (net 15 "Net-(R5-Pad2)")
  (net 16 "unconnected-(U4-Pad5)")
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.3 72.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Description" "CAP CER 1UF 10% 50V X5R 0603")
    (property "LCSC #" "C90540")
    (property "Mfr1" "FH")
    (property "Mfr1 PN" "0603B105K500NT")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -0.1 1.65) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.55) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "P42:USB_C_Receptacle_Molex_213716-0001" (layer "F.Cu")
    (tedit 5BCCCD93)
    (at 157.65 80.5 -90)
    (descr "USB 2.0 Type C Receptacle, https://gct.co/Files/Drawings/USB4085.pdf")
    (tags "USB Type-C Receptacle Through-hole Right angle")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -1.8 -90) (layer "F.SilkS"))
    (fp_text value "USB_C" (at 2.2 3.95) (layer "F.Fab") hide)
    (fp_text user "PCB Edge" (at 0 6.1 -90) (layer "Dwgs.User") hide)
    (fp_text user "${REFERENCE}" (at 0 4.025 -90) (layer "F.Fab"))
    (pad "A1" thru_hole circle (at -2.975 0 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" thru_hole circle (at -2.125 0 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" thru_hole circle (at -1.275 0 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 8 "/CC1") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" thru_hole circle (at -0.425 0 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 9 "/D-") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" thru_hole circle (at 0.425 0 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 10 "/D+") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" thru_hole circle (at 1.275 0 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 "/SBU1") (pinfunction "SBU1") (pintype "bidirectional"))
    (pad "A9" thru_hole circle (at 2.125 0 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" thru_hole circle (at 2.975 0 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" thru_hole circle (at 2.975 1.35 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" thru_hole circle (at 2.125 1.35 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" thru_hole circle (at 1.275 1.35 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 12 "/CC2") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" thru_hole circle (at 0.425 1.35 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 9 "/D-") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" thru_hole circle (at -0.425 1.35 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 10 "/D+") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" thru_hole circle (at -1.275 1.35 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 13 "/SBU2") (pinfunction "SBU2") (pintype "bidirectional"))
    (pad "B9" thru_hole circle (at -2.125 1.35 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" thru_hole circle (at -2.975 1.35 270) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 4.65 270) (size 1.3 2.5) (drill oval 0.7 1.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 0.5 270) (size 1.3 3.2) (drill oval 0.7 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 4.65 270) (size 1.3 2.5) (drill oval 0.7 1.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 0.5 270) (size 1.3 3.2) (drill oval 0.7 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "O:/Wolfgang/My Projects/KiCAD_Libraries/3D Models/2137160001.stp"
      (offset (xyz 0 -3.55 1.17))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 180))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 172.5 66.75 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Description" "RES 15K 1% 0.1W 0603")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "15K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.05 -1.6 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/CC2_L") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 161.65 83.5)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP1" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "VBUS" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-89-3" (layer "F.Cu")
    (tedit 5C33D6E8)
    (at 153.3 68.5 180)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags "SOT-89-3")
    (property "Description" "IC, LDO, 3.3V 100mA, SOT89")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0.4 3.2) (layer "F.SilkS"))
    (fp_text value "HT7533-1" (at 0.3 3.5) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.5 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.65 -1.5 180) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd custom (at -1.5625 0 180) (size 1.475 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VBUS") (pinfunction "VIN") (pintype "power_in") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 3.8625 0.8665)
            (xy 0.7375 0.8665)
            (xy 0.7375 -0.8665)
            (xy 3.8625 -0.8665)
          ) (width 0) (fill yes))
      ))
    (pad "3" smd rect (at -1.65 1.5 180) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C5-Pad1)") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 162.5 70.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Description" "RES 10K 1% 0.1W 0603")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.15 -1.3 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-666" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 167.5 76)
    (descr "SOT666")
    (tags "SOT-666")
    (property "LCSC #" "C2827693")
    (property "Mfr" "ST Micro")
    (property "Mfr PN" "USBLC6-2P6")
    (property "Mfr1" "TECH PUBLIC")
    (property "Mfr1 PN" "USBLC6-2P6")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -1.75) (layer "F.SilkS"))
    (fp_text value "USBLC6-2" (at 0 1.75 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.9 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 -0.5375) (size 0.5 0.375) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/CC2") (pinfunction "I/O1") (pintype "passive"))
    (pad "2" smd rect (at -0.925 0) (size 0.65 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd rect (at -0.85 0.5375) (size 0.5 0.375) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/CC1") (pinfunction "I/O2") (pintype "passive"))
    (pad "4" smd rect (at 0.85 0.5375) (size 0.5 0.375) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/CC1") (pinfunction "I/O2") (pintype "passive"))
    (pad "5" smd rect (at 0.925 0) (size 0.65 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "unconnected-(U4-Pad5)") (pinfunction "VBUS") (pintype "passive+no_connect"))
    (pad "6" smd rect (at 0.85 -0.5375) (size 0.5 0.375) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/CC2") (pinfunction "I/O1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-666.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 159.05 68.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Description" "RES 0R 1% 1A 0603")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 2.5 -0.05 90) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2 0.15 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 177.95 68.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Description" "CAP CER 1UF 10% 50V X5R 0603")
    (property "LCSC #" "C90540")
    (property "Mfr1" "FH")
    (property "Mfr1 PN" "0603B105K500NT")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -2.6 0.05 90) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -2.2 -0.15 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 175.95 68.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Description" "RES 0R 1% 1A 0603")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.6 0.05 90) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 2.2 0.15 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 180.75 57.25)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 172.86 60.6 90)
    (descr "Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x02 2.54mm double row")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -0.5 -2.16 90) (layer "F.SilkS"))
    (fp_text value "CC2" (at 5 -2.46 90) (layer "F.SilkS"))
    (fp_text user "${VALUE}" (at 5.01176 -2.46151 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.31 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/CC2_L") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/CC2_L") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 170.25 64.5)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP2" (at 0.85 -1.448) (layer "F.SilkS"))
    (fp_text value "3.3V" (at 2.55 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.05 -1.4) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "/+3.3V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 162.5 66.75 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Description" "RES 15K 1% 0.1W 0603")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 1.5 90) (layer "F.SilkS"))
    (fp_text value "15K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.3 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/CC1_L") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" (layer "F.Cu")
    (tedit 56DDBCCA)
    (at 154.25 57.25)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 4.2) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 165 72.75)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP3" (at -2.4 -0.05) (layer "F.SilkS"))
    (fp_text value "CC1" (at -1.4 1.75) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -0.5 1.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "/CC1") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Diode_SMD:D_SMB" (layer "F.Cu")
    (tedit 58645DF3)
    (at 167.5 83.5)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (property "Description" "DIODE TVS 33V 38.6V SMB")
    (property "LCSC #" "C173526")
    (property "Mfr" "Littlefuse")
    (property "Mfr PN" "SZ1SMB33AT3G")
    (property "Mfr1" "MDD（Microdiode Electronics）")
    (property "Mfr1 PN" "SMBJ33A")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -3) (layer "F.SilkS"))
    (fp_text value "33V" (at 0 3.1) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -3) (layer "F.Fab"))
    (pad "1" smd rect (at -2.15 0) (size 2.5 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VBUS") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd rect (at 2.15 0) (size 2.5 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 167.5 68.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Description" "IC, OPAMP, 20MHz, 10V/usec, rail, SOIC-8")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 3.5) (layer "F.SilkS"))
    (fp_text value "TSV992IDT" (at 0 3.4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/CC1_L") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R3-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/CC1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/CC2") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(R5-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/CC2_L") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/+3.3V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 157.05 68.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Description" "CAP CER 1UF 10% 50V X5R 0603")
    (property "LCSC #" "C90540")
    (property "Mfr1" "FH")
    (property "Mfr1 PN" "0603B105K500NT")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -2.6 -0.15 90) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -2.2 -0.05 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 170 72.75)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP4" (at 2.5 0.15) (layer "F.SilkS"))
    (fp_text value "CC2" (at 1.4 1.75) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.5 1.75) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "/CC2") (pinfunction "1") (pintype "passive"))
  )
  (footprint "P42:logo_small_Fab" (layer "F.Cu")
    (tedit 5CBD1A28)
    (at 197.394111 103.323715)
    (attr through_hole)
    (fp_text reference "G***" (at 3.8 -3.2) (layer "F.Fab") hide)
    (fp_text value "LOGO" (at 5.2 -1.1) (layer "F.Fab") hide)
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 167.5 64.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Description" "CAP CER 1UF 10% 50V X5R 0603")
    (property "LCSC #" "C90540")
    (property "Mfr1" "FH")
    (property "Mfr1 PN" "0603B105K500NT")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 1.5) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.4) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 159.6 60.6 90)
    (descr "Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x02 2.54mm double row")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -0.5 -2.2 90) (layer "F.SilkS"))
    (fp_text value "CC1" (at 5 5.2 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.31 1.27) (layer "F.Fab"))
    (fp_text user "${VALUE}" (at 5 5.2 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/CC1_L") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/CC1_L") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 172.5 70.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Description" "RES 10K 1% 0.1W 0603")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 1.5 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.05 1.6 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D1.0mm_Drill0.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 164.75 64.5)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "TP5" (at -0.95 -1.5) (layer "F.SilkS"))
    (fp_text value "GND" (at -2.55 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -1.05 -1.45) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-89-3" (layer "F.Cu")
    (tedit 5C33D6E8)
    (at 181.7 68.5)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags "SOT-89-3")
    (property "Description" "IC, LINEAR, 3.3V 100mA, SOT89")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0.3 -3.5) (layer "F.SilkS"))
    (fp_text value "L78L33" (at 0.3 3.5) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.5 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.65 -1.5) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C2-Pad1)") (pinfunction "OUT") (pintype "power_out"))
    (pad "2" smd custom (at -1.5625 0) (size 1.475 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 3.8625 0.8665)
            (xy 0.7375 0.8665)
            (xy 0.7375 -0.8665)
            (xy 3.8625 -0.8665)
          ) (width 0) (fill yes))
      ))
    (pad "3" smd rect (at -1.65 1.5) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VBUS") (pinfunction "IN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "P42:USB_C_Receptacle_Molex_213716-0001" (layer "F.Cu")
    (tedit 5BCCCD93)
    (at 177.35 80.5 90)
    (descr "USB 2.0 Type C Receptacle, https://gct.co/Files/Drawings/USB4085.pdf")
    (tags "USB Type-C Receptacle Through-hole Right angle")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -0.7 -1.85 90) (layer "F.SilkS"))
    (fp_text value "USB_C" (at -2.9 4.05 180) (layer "F.Fab") hide)
    (fp_text user "PCB Edge" (at 0 6.1 90) (layer "Dwgs.User") hide)
    (fp_text user "${REFERENCE}" (at 0 4.025 90) (layer "F.Fab"))
    (pad "A1" thru_hole circle (at -2.975 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" thru_hole circle (at -2.125 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" thru_hole circle (at -1.275 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 8 "/CC1") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" thru_hole circle (at -0.425 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 9 "/D-") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" thru_hole circle (at 0.425 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 10 "/D+") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" thru_hole circle (at 1.275 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 "/SBU1") (pinfunction "SBU1") (pintype "bidirectional"))
    (pad "A9" thru_hole circle (at 2.125 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" thru_hole circle (at 2.975 0 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" thru_hole circle (at 2.975 1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" thru_hole circle (at 2.125 1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" thru_hole circle (at 1.275 1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 12 "/CC2") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" thru_hole circle (at 0.425 1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 9 "/D-") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" thru_hole circle (at -0.425 1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 10 "/D+") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" thru_hole circle (at -1.275 1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 13 "/SBU2") (pinfunction "SBU2") (pintype "bidirectional"))
    (pad "B9" thru_hole circle (at -2.125 1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 "VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" thru_hole circle (at -2.975 1.35 90) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 4.65 90) (size 1.3 2.5) (drill oval 0.7 1.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.32 0.5 90) (size 1.3 3.2) (drill oval 0.7 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 4.65 90) (size 1.3 2.5) (drill oval 0.7 1.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 4.32 0.5 90) (size 1.3 3.2) (drill oval 0.7 2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "O:/Wolfgang/My Projects/KiCAD_Libraries/3D Models/2137160001.stp"
      (offset (xyz 0 -3.55 1.17))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 180))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.7 72.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Description" "CAP CER 1UF 10% 50V X5R 0603")
    (property "LCSC #" "C90540")
    (property "Mfr1" "FH")
    (property "Mfr1 PN" "0603B105K500NT")
    (property "Sheetfile" "CC_Monitor_ver1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 1.65) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.43) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.1 1.35) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "P42:logo_small" (layer "B.Cu")
    (tedit 5BD5F218)
    (at 171.6 77.1 180)
    (attr through_hole)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "P42:Pier42_5.4mmx3.0mm" (layer "B.Cu")
    (tedit 5D0AED7D)
    (at 171.6 66.7 180)
    (attr through_hole)
    (fp_text reference "G***" (at -4.107996 0.186267) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at -3.62849 0.124967) (layer "B.SilkS") hide)
  )
  (gr_rect (start 150 86) (end 185 53) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "     (c) 2023\nCC Monitor rev1" (at 167.4 68.3) (layer "B.SilkS"))
  (gr_text "CC Monitor rev1" (at 167.3 78.5) (layer "F.SilkS"))
  (gr_text "PCB Specification:\n2 Layer\n1.6 mm Thickness\nSoldermask Blue\nTrace 8 mil / Crearance: 7 mil\nCopper 1 oz thickness\nPlating: Lead-free HASL\n" (at 30.4 47.6) (layer "Eco1.User"))
  (dimension (type aligned) (layer "F.Fab")
    (pts (xy 185 86) (xy 185 53))
    (height 6)
    (gr_text "33.0 mm" (at 189.2 69.5 90) (layer "F.Fab"))
    (format (units 3) (units_format 1) (precision 1))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.Fab")
    (pts (xy 150 86) (xy 185 86))
    (height 5.6)
    (gr_text "35.0 mm" (at 167.5 89.8) (layer "F.Fab"))
    (format (units 3) (units_format 1) (precision 1))
    (style (thickness 0.2) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 1) (net_name "VBUS") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 177.35 85.5)
        (xy 157.65 85.5)
        (xy 157.65 81.35)
        (xy 177.35 81.35)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 184 85)
        (xy 151 85)
        (xy 151 54)
        (xy 184 54)
      )
    )
  )
)
