<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="25.3899875" x2="0" y2="3.81" width="0" layer="20"/>
<wire x1="0" y1="3.81" x2="3.81" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.81" y1="0" x2="96.52" y2="0" width="0" layer="20"/>
<wire x1="96.52" y1="0" x2="100.33" y2="3.81" width="0" layer="20" curve="90"/>
<wire x1="100.33" y1="3.81" x2="100.33" y2="25.3899875" width="0" layer="20"/>
<wire x1="100.33" y1="25.3899875" x2="96.5199875" y2="29.2" width="0" layer="20" curve="90"/>
<wire x1="3.8100125" y1="29.2" x2="0" y2="25.3899875" width="0" layer="20" curve="90"/>
<wire x1="44.45" y1="34.4932" x2="55.88" y2="34.4932" width="0" layer="20" curve="-180" cap="flat"/>
<wire x1="39.751" y1="29.2" x2="44.45" y2="34.4932" width="0" layer="20" curve="90" cap="flat"/>
<wire x1="60.579" y1="29.2" x2="55.88" y2="34.4932" width="0" layer="20" curve="-90" cap="flat"/>
<wire x1="3.81" y1="29.2" x2="39.751" y2="29.2" width="0" layer="20"/>
<wire x1="60.579" y1="29.2" x2="96.52" y2="29.2" width="0" layer="20"/>
<text>Luminardo</text>
<text>RESET</text>
</plain>
<libraries>
<library name="magictale">
<packages>
<package name="MT_LOGO_COMPACT">
</package>
<package name="CONN_HEADER_1X04">
</package>
<package name="CONN_HEADER_2X03">
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
</package>
<package name="CONN_HEADER_2X07_F_MIRR">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="TO-92-AMMO">
</package>
<package name="EKMB_PIR">
</package>
<package name="CONN_HEADER_1X03">
</package>
<package name="USB-A-VER">
<description>&lt;b&gt;USB connector&lt;/b&gt; with shield&lt;p&gt;</description>
</package>
<package name="CONN_HEADER_2X04">
</package>
<package name="CONN_USB_MINI_RA">
</package>
<package name="SOD123">
<description>SOD-123 0.91x1.22 mm pad</description>
</package>
<package name="SO08_POWER_PAD">
</package>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package E&lt;/b&gt;</description>
</package>
<package name="MBH6045C">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="XTAL_4X6">
<description>3.6mm * 6mm dimension &lt;br&gt;
12MHz available</description>
</package>
<package name="CONN_HEADER_1X02">
</package>
<package name="SO014">
</package>
<package name="TQFP32-08">
</package>
<package name="BATTCOM_20MM_PTH">
</package>
<package name="PJ-012A">
</package>
<package name="TL3330AF260QG">
</package>
</packages>
</library>
<library name="holes">
<packages>
<package name="3,3-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.3 mm, round</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="FIDUCIAL_1MM">
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="XTAL3215">
</package>
</packages>
</library>
<library name="Seeeduino_v3.0">
<description>Generated from &lt;b&gt;Seeeduino v3.0.brd&lt;/b&gt;&lt;p&gt;
by exp-project-lbr.ulp</description>
<packages>
<package name="LOGO_OSHW_FILLX200_NOTEXT">
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SSOP-28">
<description>SSOP28</description>
</package>
<package name="SOT-23">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PTC-1206">
</package>
</packages>
</library>
<library name="CH_misc_IC">
<description>Micsellaneous IC named by function rather than manufacturer</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="TKJMixed">
<packages>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;44-lead Thin Quad Flat Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="P8" library="magictale" package="CONN_HEADER_2X07_F_MIRR" value="VFDCTRL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="F_PIN" value="1"/>
<attribute name="L_PIN" value="13"/>
<attribute name="DIGIKEY" value="OR1103-ND "/>
</element>
<element name="H2" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="H4" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="U$" library="magictale" package="MT_LOGO_COMPACT" value="MT_LOGOCOMPACT">
<attribute name="PCBREV" value="REV 2.1, 2016.11.09"/>
<attribute name="URL" value="http://magictale.com"/>
<attribute name="LICENSE" value="CC3.0"/>
<attribute name="PROJECT" value="Luminardo"/>
</element>
<element name="FIDUTIAL1" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="FIDUTIAL3" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="FIDUTIAL2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="FIDUTIAL4" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="P2" library="magictale" package="CONN_HEADER_1X04" value="SERIAL1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="F_PIN" value="1"/>
<attribute name="L_PIN" value="4"/>
<attribute name="DIGIKEY" value="SAM1034-02-ND"/>
</element>
<element name="P4" library="magictale" package="CONN_HEADER_1X04" value="I2C">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="F_PIN" value="1"/>
<attribute name="L_PIN" value="4"/>
<attribute name="DIGIKEY" value="SAM1034-02-ND"/>
</element>
<element name="P6" library="magictale" package="CONN_HEADER_2X03" value="ISP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="F_PIN" value="1"/>
<attribute name="L_PIN" value="5"/>
<attribute name="DIGIKEY" value="609-3210-ND"/>
</element>
<element name="R2" library="magictale" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT10K0CT-ND"/>
</element>
<element name="C3" library="magictale" package="C1206" value="18pF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="1276-1844-1-ND"/>
</element>
<element name="C5" library="magictale" package="C1206" value="18pF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="1276-1844-1-ND"/>
</element>
<element name="C2" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="C6" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="C11" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="R7" library="magictale" package="R1206" value="1K5">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RNCP1206FTD1K50CT-ND"/>
</element>
<element name="R9" library="magictale" package="R1206" value="1K5">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RNCP1206FTD1K50CT-ND"/>
</element>
<element name="U$3" library="Seeeduino_v3.0" package="LOGO_OSHW_FILLX200_NOTEXT" value=""/>
<element name="B1" library="magictale" package="BATTCOM_20MM_PTH" value="">
<attribute name="DIGIKEY" value="BS-3-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="magictale" package="SO08" value="DS1338SO08">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="DS1338Z-33+-ND"/>
</element>
<element name="Y3" library="adafruit" package="XTAL3215" value="32768 kHz">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="300-8816-1-ND"/>
</element>
<element name="C16" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="U6" library="dp_devices" package="SSOP-28" value="FT232RL">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="768-1007-1-ND"/>
</element>
<element name="H1" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="H3" library="holes" package="3,3-PAD" value="MOUNT-PAD-ROUND3.3"/>
<element name="P5" library="magictale" package="CONN_USB_MINI_RA" value="USB2Serial">
<attribute name="DIGIKEY" value="732-2735-ND"/>
<attribute name="NAME"/>
</element>
<element name="C15" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="C13" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="C12" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="LD1" library="adafruit" package="CHIPLED_1206" value="TX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="160-1737-1-ND"/>
</element>
<element name="LD2" library="adafruit" package="CHIPLED_1206" value="RX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="160-1737-1-ND"/>
</element>
<element name="R10" library="magictale" package="R1206" value="1K">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT1K00CT-ND"/>
</element>
<element name="R11" library="magictale" package="R1206" value="1K">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT1K00CT-ND"/>
</element>
<element name="R12" library="magictale" package="R1206" value="1K">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT1K00CT-ND"/>
</element>
<element name="R13" library="magictale" package="R1206" value="1K">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT1K00CT-ND"/>
</element>
<element name="C14" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="C8" library="magictale" package="C1206" value="18pF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="1276-1844-1-ND"/>
</element>
<element name="C9" library="magictale" package="C1206" value="18pF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="1276-1844-1-ND"/>
</element>
<element name="R3" library="magictale" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT10K0CT-ND"/>
</element>
<element name="R4" library="magictale" package="R1206" value="33 1%">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT33R0"/>
</element>
<element name="R5" library="magictale" package="R1206" value="33 1%">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT33R0"/>
</element>
<element name="R1" library="magictale" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT10K0CT-ND"/>
</element>
<element name="F1" library="SparkFun-PowerIC" package="PTC-1206" value="PTCSMD">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="507-1798-1-ND"/>
</element>
<element name="U4" library="CH_misc_IC" package="SOT23-5" value="NCP380HSN05AAT1G">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="NCP380HSN05AAT1GOSCT-ND"/>
</element>
<element name="U2" library="magictale" package="TQFP32-08" value="MAX3421E">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="MAX3421EEHJ+-ND"/>
</element>
<element name="P1" library="magictale" package="USB-A-VER" value="USB Host">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="DIGIKEY" value="1175-1265-ND"/>
<attribute name="NAME"/>
</element>
<element name="R8" library="magictale" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT10K0CT-ND"/>
</element>
<element name="C1" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="C4" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="D1" library="TKJMixed" package="SOD123" value="PMEG2010-ER">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="568-6504-1-ND"/>
</element>
<element name="U5" library="magictale" package="SO014" value="74AHC125">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="296-4530-1-ND"/>
</element>
<element name="D2" library="TKJMixed" package="SOD123" value="PMEG2010-ER">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="568-6504-1-ND"/>
</element>
<element name="U1" library="magictale" package="TO-92-AMMO" value="DS18B20">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="DS18B20+T&amp;RCT-ND"/>
</element>
<element name="R6" library="magictale" package="R1206" value="4K7">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT4K70CT-ND"/>
</element>
<element name="Q1" library="dp_devices" package="SOT-23" value="DMG2307L-7">
<attribute name="DIGIKEY" value="DMG2307L-7DICT-ND"/>
<attribute name="NAME"/>
</element>
<element name="R14" library="magictale" package="R1206" value="100K">
<attribute name="DIGIKEY" value="RMCF1206JT100KCT-ND"/>
<attribute name="NAME"/>
</element>
<element name="P10" library="magictale" package="EKMB_PIR" value="PIR SNR">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="255-3074-ND"/>
<attribute name="F_PIN" value="1"/>
<attribute name="L_PIN" value="3"/>
</element>
<element name="P3" library="magictale" package="CONN_HEADER_1X03" value="E_SNR">
<attribute name="NAME"/>
<attribute name="F_PIN" value="1"/>
<attribute name="L_PIN" value="3"/>
<attribute name="DIGIKEY" value="SAM1034-02-ND"/>
</element>
<element name="P7" library="magictale" package="CONN_HEADER_2X04" value="PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="F_PIN" value="1"/>
<attribute name="L_PIN" value="7"/>
<attribute name="DIGIKEY" value="609-3235-ND"/>
</element>
<element name="P9" library="magictale" package="CONN_HEADER_2X03" value="SPI">
<attribute name="F_PIN" value="1"/>
<attribute name="L_PIN" value="5"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="609-3210-ND"/>
</element>
<element name="U3" library="TKJMixed" package="TQFP44" value="ATMEGA1284PA">
<attribute name="OC_NEWARK" value=""/>
<attribute name="MPN" value="ATMEGA1284P-10AU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="ATMEGA1284P-AURCT-ND"/>
</element>
<element name="U8" library="magictale" package="SO08_POWER_PAD" value="LM22675">
<attribute name="DIGIKEY" value="LM22675MR-5.0/NOPB-ND"/>
<attribute name="NAME"/>
</element>
<element name="C17" library="magictale" package="C1206" value="10nF">
<attribute name="DIGIKEY" value="399-1234-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="ZD1" library="magictale" package="SOD123" value="1N5819">
<attribute name="DIGIKEY" value="1N5819HW-FDICT-ND "/>
<attribute name="NAME"/>
</element>
<element name="C20" library="magictale" package="C1206" value="1uF">
<attribute name="DIGIKEY" value="587-1434-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C18" library="magictale" package="PANASONIC_C" value="56uF">
<attribute name="DIGIKEY" value="P16502CT-ND"/>
<attribute name="NAME"/>
</element>
<element name="L1" library="magictale" package="MBH6045C" value="22uH">
<attribute name="DIGIKEY" value="490-13129-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="U9" library="magictale" package="SOT223" value="LD1117">
<attribute name="DIGIKEY" value="497-1241-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C21" library="magictale" package="C1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="445-14296-1-ND"/>
</element>
<element name="C22" library="magictale" package="C1206" value="10uF">
<attribute name="DIGIKEY" value="1276-3044-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="Y2" library="magictale" package="XTAL_4X6" value="12MHz">
<attribute name="DIGIKEY" value="535-9836-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="R15" library="magictale" package="R1206" value="10K">
<attribute name="NAME"/>
<attribute name="DIGIKEY" value="RMCF1206JT10K0CT-ND"/>
</element>
<element name="P11" library="magictale" package="CONN_HEADER_1X02" value="SERIAL 0">
<attribute name="F_PIN" value="1"/>
<attribute name="DIGIKEY" value="SAM1034-01-ND"/>
</element>
<element name="Y1" library="magictale" package="XTAL_4X6" value="10MHz">
<attribute name="DIGIKEY" value="535-9833-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="magictale" package="PJ-012A" value="PJ-012A">
<attribute name="DIGIKEY" value="CP-012A-ND"/>
<attribute name="NAME"/>
</element>
<element name="FIDUTIAL5" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="FIDUTIAL6" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="R16" library="magictale" package="R1206" value="33K">
<attribute name="DIGIKEY" value="RMCF1206JT33K0CT-ND"/>
<attribute name="NAME"/>
</element>
<element name="R17" library="magictale" package="R1206" value="10K">
<attribute name="DIGIKEY" value="RMCF1206JT10K0CT-ND"/>
<attribute name="NAME"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="DIGIKEY" value="399-8269-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C19" library="SparkFun-Capacitors" package="EIA3216" value="4.7uF">
<attribute name="DIGIKEY" value="399-3696-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="EIA3216" value="4.7uF">
<attribute name="DIGIKEY" value="399-3696-1-ND"/>
<attribute name="NAME"/>
</element>
<element name="SW1" library="magictale" package="TL3330AF260QG" value="RESET">
<attribute name="DIGIKEY" value="EG4389CT-ND"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C6" pad="1"/>
<contactref element="P8" pad="4"/>
<contactref element="P2" pad="4"/>
<contactref element="P4" pad="4"/>
<contactref element="P6" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U7" pad="4"/>
<contactref element="B1" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="U6" pad="25"/>
<contactref element="U6" pad="7"/>
<contactref element="U6" pad="18"/>
<contactref element="U6" pad="21"/>
<contactref element="U6" pad="26"/>
<contactref element="C15" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="P5" pad="5"/>
<contactref element="U4" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="19"/>
<contactref element="P1" pad="4"/>
<contactref element="P1" pad="S2"/>
<contactref element="P1" pad="S1"/>
<contactref element="C11" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U5" pad="7"/>
<contactref element="U5" pad="13"/>
<contactref element="U5" pad="12"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="P3" pad="3"/>
<contactref element="P7" pad="7"/>
<contactref element="P7" pad="8"/>
<contactref element="P9" pad="6"/>
<contactref element="U3" pad="18"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="28"/>
<contactref element="U3" pad="39"/>
<contactref element="U3" pad="39"/>
<contactref element="U3" pad="28"/>
<contactref element="U3" pad="18"/>
<contactref element="U3" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="U8" pad="BODY@1"/>
<contactref element="U8" pad="6"/>
<contactref element="U8" pad="BODY@1"/>
<contactref element="U8" pad="6"/>
<contactref element="C20" pad="1"/>
<contactref element="ZD1" pad="A"/>
<contactref element="C18" pad="-"/>
<contactref element="U9" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="P5" pad="S1"/>
<contactref element="P5" pad="S2"/>
<contactref element="P5" pad="S4"/>
<contactref element="P5" pad="S3"/>
<contactref element="P10" pad="3"/>
<contactref element="R16" pad="1"/>
<contactref element="C10" pad="C"/>
<contactref element="C19" pad="C"/>
<contactref element="C7" pad="C"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="S0"/>
<contactref element="SW1" pad="S1"/>
</signal>
<signal name="RESET">
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="U2" pad="12"/>
<contactref element="U5" pad="6"/>
<contactref element="U3" pad="4"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="U2" pad="13"/>
<contactref element="U5" pad="3"/>
<contactref element="P9" pad="3"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="P6" pad="1"/>
<contactref element="U2" pad="15"/>
<contactref element="P9" pad="1"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="RX-I">
<contactref element="R10" pad="1"/>
<contactref element="U3" pad="9"/>
<contactref element="P11" pad="1"/>
</signal>
<signal name="TX-O">
<contactref element="R11" pad="1"/>
<contactref element="U3" pad="10"/>
<contactref element="P11" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="P4" pad="3"/>
<contactref element="R9" pad="2"/>
<contactref element="U7" pad="6"/>
<contactref element="U3" pad="19"/>
</signal>
<signal name="SDA">
<contactref element="P4" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="U7" pad="5"/>
<contactref element="U3" pad="20"/>
</signal>
<signal name="L_SNR">
<contactref element="P8" pad="12"/>
<contactref element="U3" pad="30"/>
</signal>
<signal name="IR_REC">
<contactref element="P8" pad="1"/>
<contactref element="U3" pad="36"/>
</signal>
<signal name="SPKR">
<contactref element="P8" pad="3"/>
<contactref element="U3" pad="43"/>
</signal>
<signal name="R">
<contactref element="P8" pad="10"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="G">
<contactref element="P8" pad="8"/>
<contactref element="U3" pad="15"/>
</signal>
<signal name="B">
<contactref element="P8" pad="6"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="XTAL1">
<contactref element="C3" pad="2"/>
<contactref element="U3" pad="7"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="XTAL2">
<contactref element="C5" pad="2"/>
<contactref element="U3" pad="8"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="Y3" pad="P$2"/>
<contactref element="U7" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="Y3" pad="P$1"/>
<contactref element="U7" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="B1" pad="1"/>
<contactref element="U7" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="P5" pad="3"/>
<contactref element="U6" pad="15"/>
</signal>
<signal name="N$5">
<contactref element="P5" pad="2"/>
<contactref element="U6" pad="16"/>
</signal>
<signal name="N$8">
<contactref element="U6" pad="5"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U6" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LD1" pad="C"/>
<contactref element="U6" pad="23"/>
</signal>
<signal name="N$10">
<contactref element="U6" pad="22"/>
<contactref element="LD2" pad="C"/>
</signal>
<signal name="N$11">
<contactref element="LD1" pad="A"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="LD2" pad="A"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U6" pad="2"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="SS">
<contactref element="U2" pad="14"/>
<contactref element="R3" pad="2"/>
<contactref element="U3" pad="44"/>
</signal>
<signal name="+3V3">
<contactref element="R2" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="P4" pad="1"/>
<contactref element="P2" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="U6" pad="4"/>
<contactref element="C13" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="U2" pad="23"/>
<contactref element="R3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="U6" pad="19"/>
<contactref element="C15" pad="2"/>
<contactref element="U5" pad="14"/>
<contactref element="U7" pad="8"/>
<contactref element="C16" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="P3" pad="1"/>
<contactref element="P7" pad="3"/>
<contactref element="P7" pad="4"/>
<contactref element="P10" pad="1"/>
<contactref element="P9" pad="2"/>
<contactref element="U3" pad="17"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="38"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="17"/>
<contactref element="U3" pad="38"/>
<contactref element="U3" pad="27"/>
<contactref element="U9" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="U9" pad="4"/>
<contactref element="C10" pad="A"/>
</signal>
<signal name="+5V">
<contactref element="P6" pad="2"/>
<contactref element="U4" pad="5"/>
<contactref element="U6" pad="20"/>
<contactref element="C12" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="Q1" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="P7" pad="5"/>
<contactref element="P7" pad="6"/>
<contactref element="U8" pad="4"/>
<contactref element="L1" pad="2"/>
<contactref element="C18" pad="+"/>
<contactref element="U9" pad="3"/>
<contactref element="C21" pad="2"/>
</signal>
<signal name="MAX_INT">
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="18"/>
<contactref element="U3" pad="21"/>
</signal>
<signal name="N$20">
<contactref element="P5" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="C9" pad="2"/>
<contactref element="U2" pad="24"/>
<contactref element="Y2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="C8" pad="2"/>
<contactref element="U2" pad="25"/>
<contactref element="Y2" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="U2" pad="21"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="20"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="P1" pad="3"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="P1" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="U4" pad="1"/>
<contactref element="P1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C7" pad="A"/>
</signal>
<signal name="OVRLD">
<contactref element="U4" pad="3"/>
<contactref element="U2" pad="26"/>
</signal>
<signal name="USB_EN">
<contactref element="R8" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="SCK_5V">
<contactref element="U5" pad="2"/>
<contactref element="P6" pad="3"/>
</signal>
<signal name="RES_5V">
<contactref element="U5" pad="5"/>
<contactref element="P6" pad="5"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="4"/>
<contactref element="U5" pad="10"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="MOSI_5V">
<contactref element="U5" pad="9"/>
<contactref element="P6" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="D1" pad="A"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="D2" pad="A"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="TEMP">
<contactref element="U1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="P3" pad="2"/>
<contactref element="U3" pad="37"/>
</signal>
<signal name="RTC_INT">
<contactref element="U7" pad="7"/>
<contactref element="U3" pad="41"/>
</signal>
<signal name="PIR">
<contactref element="U3" pad="42"/>
<contactref element="P10" pad="2"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="PWR_IN">
<contactref element="P7" pad="1"/>
<contactref element="U8" pad="7"/>
<contactref element="D2" pad="C"/>
<contactref element="C20" pad="2"/>
<contactref element="P7" pad="2"/>
<contactref element="C19" pad="A"/>
</signal>
<signal name="V_DI">
<contactref element="P8" pad="7"/>
<contactref element="U3" pad="22"/>
</signal>
<signal name="V_CLK">
<contactref element="P8" pad="9"/>
<contactref element="U3" pad="33"/>
</signal>
<signal name="V_CS">
<contactref element="P8" pad="11"/>
<contactref element="U3" pad="32"/>
</signal>
<signal name="V_PWR">
<contactref element="P8" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="V_SHDN">
<contactref element="P8" pad="14"/>
<contactref element="U3" pad="35"/>
</signal>
<signal name="V_PWR_EN">
<contactref element="Q1" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="U3" pad="34"/>
</signal>
<signal name="SS2">
<contactref element="P9" pad="5"/>
<contactref element="U3" pad="31"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U3" pad="29"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="V_DO">
<contactref element="U3" pad="23"/>
<contactref element="P8" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="U3" pad="1"/>
<contactref element="U5" pad="8"/>
<contactref element="U2" pad="16"/>
<contactref element="P9" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="U8" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="C17" pad="2"/>
<contactref element="L1" pad="1"/>
<contactref element="U8" pad="8"/>
<contactref element="ZD1" pad="C"/>
</signal>
<signal name="RX1-I">
<contactref element="U3" pad="11"/>
<contactref element="P2" pad="2"/>
</signal>
<signal name="TX1-O">
<contactref element="U3" pad="12"/>
<contactref element="P2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
