(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.567)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" power)
		(2 "In2.Cu" power)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0254)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.2021)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.9906)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.2021)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0254)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 113.2 133)
		(pcbplotparams
			(layerselection 0x0001008_7ffffff8)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 2.000000)
			(dashed_line_gap_ratio 1.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GNDA")
	(net 2 "Net-(U1-SET)")
	(net 3 "Net-(U2-SET)")
	(net 4 "+3V0")
	(net 5 "+14V0")
	(net 6 "Net-(U3-SET)")
	(net 7 "-14V0")
	(net 8 "Net-(U7-REFIO)")
	(net 9 "Net-(U8-REFIO)")
	(net 10 "+3.3V")
	(net 11 "Net-(C49-Pad1)")
	(net 12 "Net-(C49-Pad2)")
	(net 13 "+15V")
	(net 14 "-15V")
	(net 15 "Net-(U9-Ain+)")
	(net 16 "Net-(U9-Ain-)")
	(net 17 "/+15V Supply")
	(net 18 "/-15V Supply")
	(net 19 "Net-(U7-IOUTB)")
	(net 20 "Net-(U7-IOUTA)")
	(net 21 "/S.LATCH_X")
	(net 22 "/S.LATCH_Y")
	(net 23 "/S.LATCH_A")
	(net 24 "/S.WRITE_A")
	(net 25 "/S.CLK_D")
	(net 26 "/S.CLK_A")
	(net 27 "Net-(U8-IOUTB)")
	(net 28 "Net-(U8-IOUTA)")
	(net 29 "Net-(D1-A)")
	(net 30 "Net-(J5-In)")
	(net 31 "Net-(D6-K)")
	(net 32 "/D-1")
	(net 33 "/D-2")
	(net 34 "/D-3")
	(net 35 "/D-4")
	(net 36 "/D-5")
	(net 37 "/D-6")
	(net 38 "/D-7")
	(net 39 "/D-8")
	(net 40 "Net-(D7-COM)")
	(net 41 "Net-(U19-SET)")
	(net 42 "unconnected-(J2-Pin_2-Pad2)")
	(net 43 "/D-9")
	(net 44 "/D-10")
	(net 45 "/D-11")
	(net 46 "/D-12")
	(net 47 "/D-13")
	(net 48 "/D-14")
	(net 49 "/D-15")
	(net 50 "unconnected-(J2-Pin_19-Pad19)")
	(net 51 "unconnected-(J2-Pin_20-Pad20)")
	(net 52 "Net-(D8-K)")
	(net 53 "unconnected-(J3-Pin_1-Pad1)")
	(net 54 "unconnected-(J3-Pin_19-Pad19)")
	(net 55 "unconnected-(J3-Pin_20-Pad20)")
	(net 56 "Net-(D8-A)")
	(net 57 "unconnected-(J3-Pin_2-Pad2)")
	(net 58 "Net-(U13-+)")
	(net 59 "unconnected-(J4-Pin_19-Pad19)")
	(net 60 "unconnected-(J4-Pin_20-Pad20)")
	(net 61 "Net-(J6-In)")
	(net 62 "Net-(J7-Pin_1)")
	(net 63 "Net-(U14-+)")
	(net 64 "Net-(U15--)")
	(net 65 "Net-(U16--)")
	(net 66 "Net-(J7-Pin_2)")
	(net 67 "Net-(J7-Pin_3)")
	(net 68 "Net-(J7-Pin_4)")
	(net 69 "Net-(J8-In)")
	(net 70 "unconnected-(J4-Pin_1-Pad1)")
	(net 71 "Net-(U1-ILIM)")
	(net 72 "Net-(U2-ILIM)")
	(net 73 "/Y-14")
	(net 74 "/Y-13")
	(net 75 "/Y-12")
	(net 76 "/Y-11")
	(net 77 "/Y-10")
	(net 78 "/Y-9")
	(net 79 "/Y-8")
	(net 80 "/Y-7")
	(net 81 "/Y-6")
	(net 82 "/Y-5")
	(net 83 "/Y-4")
	(net 84 "/Y-3")
	(net 85 "/Y-2")
	(net 86 "/Y-1")
	(net 87 "unconnected-(U14-NC-Pad5)")
	(net 88 "unconnected-(U15-NC-Pad5)")
	(net 89 "unconnected-(U16-NC-Pad5)")
	(net 90 "Net-(U1-PGFB)")
	(net 91 "Net-(U2-PGFB)")
	(net 92 "Net-(U3-ILIM)")
	(net 93 "/X-14")
	(net 94 "/X-13")
	(net 95 "/X-12")
	(net 96 "/X-11")
	(net 97 "/X-10")
	(net 98 "/X-9")
	(net 99 "/X-8")
	(net 100 "/X-7")
	(net 101 "/X-6")
	(net 102 "/X-5")
	(net 103 "/X-4")
	(net 104 "/X-3")
	(net 105 "/X-2")
	(net 106 "/X-1")
	(net 107 "Net-(U3-PGFB)")
	(net 108 "/A-1")
	(net 109 "/A-2")
	(net 110 "/A-3")
	(net 111 "/A-4")
	(net 112 "/A-5")
	(net 113 "/A-6")
	(net 114 "/A-7")
	(net 115 "/A-8")
	(net 116 "/A-9")
	(net 117 "/A-10")
	(net 118 "/A-11")
	(net 119 "/A-12")
	(net 120 "/A-13")
	(net 121 "/A-14")
	(net 122 "/A-15")
	(net 123 "Net-(U7-FS_ADJ)")
	(net 124 "Net-(U8-FS_ADJ)")
	(net 125 "Net-(R34-Pad2)")
	(net 126 "Net-(R35-Pad2)")
	(net 127 "Net-(U11-+)")
	(net 128 "Net-(U11--)")
	(net 129 "Net-(U12-+)")
	(net 130 "Net-(U12--)")
	(net 131 "Net-(U11-Vout-)")
	(net 132 "Net-(U11-Vout+)")
	(net 133 "Net-(U10-+)")
	(net 134 "Net-(U10--)")
	(net 135 "Net-(U12-Vout-)")
	(net 136 "Net-(U12-Vout+)")
	(net 137 "Net-(R60-Pad2)")
	(net 138 "Net-(C74-Pad1)")
	(net 139 "Net-(U16-+)")
	(net 140 "unconnected-(U3-VIOC-Pad7)")
	(net 141 "unconnected-(U4-2Q7-Pad22)")
	(net 142 "unconnected-(U4-2Q8-Pad23)")
	(net 143 "unconnected-(U4-2D8-Pad26)")
	(net 144 "unconnected-(U5-2Q7-Pad22)")
	(net 145 "unconnected-(U5-2Q8-Pad23)")
	(net 146 "unconnected-(U5-2D8-Pad26)")
	(net 147 "unconnected-(U6-2Q8-Pad23)")
	(net 148 "unconnected-(U7-SLEEP-Pad15)")
	(net 149 "unconnected-(U8-SLEEP-Pad15)")
	(net 150 "unconnected-(U10-PD-Pad7)")
	(net 151 "unconnected-(U11-PD-Pad7)")
	(net 152 "unconnected-(U12-PD-Pad7)")
	(net 153 "unconnected-(U13-VOS-Pad1)")
	(net 154 "unconnected-(U13-NC-Pad5)")
	(net 155 "unconnected-(U13-VOS-Pad8)")
	(net 156 "unconnected-(U14-VOS-Pad1)")
	(net 157 "unconnected-(U14-VOS-Pad8)")
	(net 158 "unconnected-(U15-VOS-Pad1)")
	(net 159 "unconnected-(U15-VOS-Pad8)")
	(net 160 "unconnected-(U16-VOS-Pad1)")
	(net 161 "unconnected-(U16-VOS-Pad8)")
	(net 162 "unconnected-(U6-2D8-Pad26)")
	(net 163 "Net-(U17--)")
	(net 164 "Net-(U17-+)")
	(net 165 "Net-(U18--)")
	(net 166 "unconnected-(U17-VOS-Pad1)")
	(net 167 "unconnected-(U17-NC-Pad5)")
	(net 168 "unconnected-(U17-VOS-Pad8)")
	(net 169 "unconnected-(U18-VOS-Pad1)")
	(net 170 "unconnected-(U18-NC-Pad5)")
	(net 171 "unconnected-(U18-VOS-Pad8)")
	(net 172 "Net-(D5-K)")
	(net 173 "Net-(D2-K)")
	(net 174 "Net-(D4-K)")
	(net 175 "Net-(D3-K)")
	(net 176 "Net-(D4-A)")
	(net 177 "Net-(D5-A)")
	(net 178 "Net-(D6-A)")
	(net 179 "unconnected-(J4-Pin_17-Pad17)")
	(net 180 "Net-(R75-Pad1)")
	(net 181 "Net-(R30-Pad2)")
	(net 182 "Net-(R72-Pad2)")
	(net 183 "Net-(R74-Pad2)")
	(net 184 "Net-(R77-Pad2)")
	(net 185 "Net-(R79-Pad2)")
	(net 186 "Net-(RV2-Pad2)")
	(net 187 "Net-(U18-+)")
	(net 188 "Net-(R75-Pad2)")
	(net 189 "Net-(R59-Pad2)")
	(net 190 "unconnected-(J4-Pin_2-Pad2)")
	(net 191 "Net-(R29-Pad2)")
	(net 192 "Net-(R65-Pad2)")
	(net 193 "Net-(R68-Pad2)")
	(net 194 "Net-(R76-Pad2)")
	(net 195 "Net-(R80-Pad2)")
	(net 196 "Net-(R81-Pad1)")
	(net 197 "Net-(R81-Pad2)")
	(net 198 "Net-(U19-ILIM)")
	(net 199 "Net-(U19-PGFB)")
	(net 200 "Net-(RV5-Pad2)")
	(net 201 "Net-(D9-K)")
	(net 202 "Net-(J1-Pin_2)")
	(net 203 "Net-(J1-Pin_3)")
	(net 204 "Net-(J1-Pin_4)")
	(net 205 "Net-(R64-Pad1)")
	(net 206 "Net-(R90-Pad2)")
	(net 207 "Net-(R91-Pad2)")
	(net 208 "Net-(R94-Pad1)")
	(net 209 "Net-(R95-Pad1)")
	(net 210 "Net-(RV7-Pad2)")
	(net 211 "Net-(RV3-Pad1)")
	(net 212 "Net-(U10-Vocm)")
	(net 213 "Net-(R27-Pad2)")
	(net 214 "+5VA")
	(net 215 "+5VD")
	(net 216 "/+5V Supply")
	(net 217 "Net-(U13--)")
	(net 218 "Net-(U14--)")
	(net 219 "Net-(JP5-C)")
	(net 220 "Net-(JP6-C)")
	(net 221 "Net-(JP7-C)")
	(net 222 "unconnected-(J2-Pin_5-Pad5)")
	(net 223 "/PG+14A")
	(net 224 "/PG3.3A")
	(net 225 "/PG-14A")
	(net 226 "/PG3.3D")
	(net 227 "/Power Good")
	(net 228 "Net-(Q1-B)")
	(net 229 "Net-(Q2-B)")
	(net 230 "Net-(Q3-B)")
	(net 231 "Net-(Q4-B)")
	(net 232 "Net-(R24-Pad2)")
	(net 233 "Net-(R25-Pad2)")
	(net 234 "Net-(R26-Pad2)")
	(net 235 "Net-(R97-Pad2)")
	(net 236 "unconnected-(U20-Pad8)")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 159.86 125.88 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 174.71 83.97 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A106051CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/CRG0603ZR/2380828"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Differential output current limiting (or not)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "Net-(J7-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 136 "Net-(U12-Vout+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 164.5 99.91 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "25"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "13-RP0603BRD0725RLCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/yageo/RP0603BRD0725RL/16916489"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC output load"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U7-IOUTA)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 164.46 66.7)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "33k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3ARB333V/3073660"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets voltage reference"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P33KBDCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(U1-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 192.67 108.94 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R71"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "20k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20118CT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PB3B2002V/6212901"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC offset preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 193 "Net-(R68-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 164.6 78.94 90)
		(property "Reference" "GNDA8"
			(at 0.65 -2.71 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 170.73 126.48)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R58"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "500"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "541-3301-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/vishay-dale/TNPU0603500RAZEN00/6615936"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Part of gain circuit on ADC buffer op amp responsible for video signal in"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 133 "Net-(U10-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "Net-(D7-COM)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias"
		(layer "F.Cu")
		(at 152.902344 62.65 -90)
		(descr "MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf#page=24), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U19"
			(at 0 -2.95 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT3045"
			(at 0 2.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT3045.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT3045IMSE#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT3045IMSE-TRPBF/6235368"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.41 -0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.41 0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 -0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.15 -1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 215 "+5VD")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.15 -0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 215 "+5VD")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.15 -0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 215 "+5VD")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.15 0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 224 "/PG3.3A")
			(pinfunction "EN/UV")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.15 0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 226 "/PG3.3D")
			(pinfunction "PG")
			(pintype "open_collector")
		)
		(pad "6" smd roundrect
			(at -2.15 1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 198 "Net-(U19-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.15 1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 199 "Net-(U19-PGFB)")
			(pinfunction "PGFB")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.15 0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "Net-(U19-SET)")
			(pinfunction "SET")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 2.15 0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 2.15 -0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "OUTS")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.15 -0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "12" smd roundrect
			(at 2.15 -1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "13" thru_hole circle
			(at -0.5 -1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at -0.5 0 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at -0.5 1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.5 2.5)
			(layers "B.Cu")
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.65 2.85)
			(layers "F.Cu" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 -1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 0 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 165.13 55.79)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "+5VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
		(layer "F.Cu")
		(at 117.9068 75.12215 -90)
		(descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U20"
			(at 0 -3.45 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "7421"
			(at 0 3.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74hcs21.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "296-SN74HCS21PWRCT-ND"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/SN74HCS21PWR/12165103"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "Net-(R24-Pad2)")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 233 "Net-(R25-Pad2)")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at -2.8625 0 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 234 "Net-(R26-Pad2)")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8625 0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 235 "Net-(R97-Pad2)")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 227 "/Power Good")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.8625 1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.8625 1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 236 "unconnected-(U20-Pad8)")
			(pintype "output+no_connect")
		)
		(pad "9" smd roundrect
			(at 2.8625 1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.8625 0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.8625 0 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "12" smd roundrect
			(at 2.8625 -0.65 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 2.8625 -1.3 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.8625 -1.95 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 187.37 58 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1516-QBLP601D-OCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/qt-brightek-qtb/QBLP601D-O/13278855"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "-15V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 155.89 61.37 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R100"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good LED driver"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33	"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 231 "Net-(Q4-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 226 "/PG3.3D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:C_1210_3225_Kelvin_Connections"
		(layer "F.Cu")
		(at 179.74 65.15 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 -2.3 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at -0.1 2.9 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:C_1210_3225_Kelvin_Connections"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-CL32B106KAJ4PNECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL32B106KAJ4PNE/11487783?s=N4IgTCBcDaIMIBkDMYBCBGADANgNIEEApAFgAUA5AAhAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 -0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at -1.475 0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 -0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 173.98 98.38 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R51"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A106051CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/CRG0603ZR/2380828"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Differential output current limiting (or not)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 131 "Net-(U11-Vout-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "Net-(J7-Pin_4)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 166.15 111.84 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C85"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 166.15 93.78 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C63"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 185.67 93.78)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 182.95 95.86)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R60"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.82K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB1821V/2026770"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC single ended gain resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P1.82KDBCT-ND "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 218 "Net-(U14--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 137 "Net-(R60-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 176.61 55.77)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+15V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 170.71 87.59)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.99K"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/vishay-dale/TNPW12064K99BYEN/9562428"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Differential gain resistor, sets ratio between single ended and differential output range"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.52"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "541-9840-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 130 "Net-(U12--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 136 "Net-(U12-Vout+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 167.1 119.49)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_A-1"
			(at 1.41 0.57 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 126 "Net-(R35-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 170.71 97.17)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.99K"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/vishay-dale/TNPW12064K99BYEN/9562428"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Differential gain resistor, sets ratio between single ended and differential output range"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.52"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "541-9840-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 127 "Net-(U11-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 131 "Net-(U11-Vout-)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 159.35 95.78 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 142.64 111.76 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C81"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:MountingHole_3.5mm_Pad_Via_CrtYd"
		(layer "F.Cu")
		(at 117.2 129 90)
		(descr "Mounting Hole 3.5mm with Courtyard for Washers + Tolerance")
		(tags "mounting hole 3.5mm Courtyard")
		(property "Reference" "H1"
			(at 0 -4.5 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:MountingHole_3.5mm_Pad_Via_CrtYd"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.625 0 90)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" connect rect
			(at -2.5 -0.75 90)
			(size 5 8.5)
			(layers "F.Cu" "F.Mask")
		)
		(pad "1" connect rect
			(at -2.5 -0.75 90)
			(size 5 8.5)
			(layers "B.Cu" "B.Mask")
		)
		(pad "1" thru_hole circle
			(at -1.856155 -1.856155 90)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 1.856155 90)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" connect rect
			(at -0.750003 -2.5 180)
			(size 5 8.499994)
			(layers "F.Cu" "F.Mask")
		)
		(pad "1" connect rect
			(at -0.750003 -2.5 180)
			(size 5 8.499994)
			(layers "B.Cu" "B.Mask")
		)
		(pad "1" thru_hole circle
			(at 0 -2.625 90)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 7 7)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.625 90)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 -1.856155 90)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 1.856155 90)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.625 0 90)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(layer "F.Cu")
		(at 197.03 82.84 90)
		(property "Reference" "GNDA1"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 152.04 119.89 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(layer "F.Cu")
		(at 197.53 106.79 90)
		(property "Reference" "GNDA12"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:Reduced_pads_R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 180.39 96.04)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R73"
			(at 2.54 -1.92 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 2.54 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:Reduced_pads_R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "DNP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Optional axial resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 218 "Net-(U14--)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(R60-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 169.8 109.89 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.32k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P2.32KDBCT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB2321V/2026779"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC gain preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 191 "Net-(R29-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 189.67 108.94)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R68"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "12k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20094CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PB3B1202V/6212877"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC offset preset"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 193 "Net-(R68-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 165.35 125.36 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C52"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-2016-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B225KP8NFNC/3887674?s=N4IgTCBcDaIMIBkCMAGAQmMBWA0gBQA4A5AMSJAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "Net-(U10-Vocm)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:SOT-416"
		(layer "F.Cu")
		(at 182.56 63.81 -90)
		(descr "SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf")
		(tags "SOT-416")
		(property "Reference" "Q1"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MMBT3904TT1G"
			(at 0 2.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOT-416"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mmbt3904tt1-d.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "MMBT3904TT1GOSCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/onsemi/MMBT3904TT1G/919603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.65 -0.5 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 228 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.65 0.5 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.65 0 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "Net-(D5-K)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/2SK3019TL.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 183.71 90.88)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R77"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20122CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PB3B2202V/6212905"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC offset preset"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 184 "Net-(R77-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 166.02 122.74)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "25"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "13-RP0603BRD0725RLCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/yageo/RP0603BRD0725RL/16916489"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC input load"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U9-Ain+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "Net-(R34-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 194.3148 77.689)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_X_Out1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 189 "Net-(R59-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 163.94 125.16)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Vcom1"
			(at 2.6 2.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 212 "Net-(U10-Vocm)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 178.52 82.49 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R56"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J4K99BTD/9479768"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Input summing to single-ended stage"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 165 "Net-(U18--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "Net-(U13-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 189.96 126.37 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R90"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "14k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "10-ERA-3ARB1402VCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3ARB1402V/6049053"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC offset preset"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 206 "Net-(R90-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 177.77 80.28)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R52"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J4K99BTD/9479768"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Input summing to single-ended stage"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "Net-(U12-Vout-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 217 "Net-(U13--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:IDC-Header_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
		(locked yes)
		(layer "F.Cu")
		(at 117.2 96.14)
		(descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
		(property "Reference" "J3"
			(at 1.38 -1.76 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 1.27 28.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:IDC-Header_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "WM20559-ND"
			(at -1.1332 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at -1.1332 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/molex/0878342019/3303513?s=N4IgTCBcDaILIHsA2BTAHgAgAwA4DsOAzACxhYCMAnCALoC%2BQA"
			(at -1.1332 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 53 "unconnected-(J3-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(J3-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/D-1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/D-2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/D-3")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/D-4")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/D-5")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/D-6")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/D-7")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/D-8")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(J3-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(J3-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 172.48 84.99 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C70"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 175.09 116.98 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C65"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 182.56 126.41 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R64"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "500"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20KBECT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3ARW203V/3073699"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.05%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC Gain preset"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 205 "Net-(R64-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U15--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 178.18 126.405 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R96"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "DNP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Optional ADC attenuator feedback resistor (why?)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 138 "Net-(C74-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U15--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 161.42 61.04 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "750"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3EKF7500V/196472"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets power regulator current limit"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P750HCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "Net-(U1-ILIM)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 164.71 119.09 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C49-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(C49-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:MountingHole_3.5mm_Pad_Via_CrtYd"
		(locked yes)
		(layer "F.Cu")
		(at 209.2 57 -90)
		(descr "Mounting Hole 3.5mm with Courtyard for Washers + Tolerance")
		(tags "mounting hole 3.5mm Courtyard")
		(property "Reference" "H2"
			(at 0 -4.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:MountingHole_3.5mm_Pad_Via_CrtYd"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.625 0 270)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" connect rect
			(at -2.5 -0.75 270)
			(size 5 8.5)
			(layers "F.Cu" "F.Mask")
		)
		(pad "1" connect rect
			(at -2.5 -0.75 270)
			(size 5 8.5)
			(layers "B.Cu" "B.Mask")
		)
		(pad "1" thru_hole circle
			(at -1.856155 -1.856155 270)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 1.856155 270)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" connect rect
			(at -0.750003 -2.5)
			(size 5 8.499994)
			(layers "F.Cu" "F.Mask")
		)
		(pad "1" connect rect
			(at -0.750003 -2.5)
			(size 5 8.499994)
			(layers "B.Cu" "B.Mask")
		)
		(pad "1" thru_hole circle
			(at 0 -2.625 270)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 7 7)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.625 270)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 -1.856155 270)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 1.856155 270)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.625 0 270)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 165.42 115.38 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C58"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1945-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B105KP8NFNC/3887603?s=N4IgTCBcDaIMIBkCMAGAQqgrAaQAoA4A5AMUJAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C49-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 142.8 127.2 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 149.41 111.84)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C80"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 159.4575 57.34 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 215 "+5VD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 194.3148 97.329)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Y_Offset1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 163 "Net-(U17--)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias"
		(layer "F.Cu")
		(at 175.882344 62.65 -90)
		(descr "MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf#page=24), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U2"
			(at 0 -2.95 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT3045"
			(at 0 2.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT3045.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT3045IMSE#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT3045IMSE-TRPBF/6235368"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.41 -0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.41 0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 -0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.15 -1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+15V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.15 -0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+15V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.15 -0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+15V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.15 0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+15V")
			(pinfunction "EN/UV")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.15 0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 223 "/PG+14A")
			(pinfunction "PG")
			(pintype "open_collector")
		)
		(pad "6" smd roundrect
			(at -2.15 1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "Net-(U2-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.15 1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 91 "Net-(U2-PGFB)")
			(pinfunction "PGFB")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.15 0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U2-SET)")
			(pinfunction "SET")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 2.15 0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 2.15 -0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "OUTS")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.15 -0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "12" smd roundrect
			(at 2.15 -1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "13" thru_hole circle
			(at -0.5 -1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at -0.5 0 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at -0.5 1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.5 2.5)
			(layers "B.Cu")
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.65 2.85)
			(layers "F.Cu" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 -1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 0 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 183.95 114.67 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C53"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 152.89 57.97 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R85"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.99k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3EKF4991V/196341"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good pullup"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P4.99KHCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 215 "+5VD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 226 "/PG3.3D")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 157.35 61.13 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R86"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.3k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P3.3KGCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEYJ332V/135886?s=N4IgTCBcDaIAoGYB0CDSBxAwgFQLQDkAREAXQF8g"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets LED brightness"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 215 "+5VD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "Net-(D8-A)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(layer "F.Cu")
		(at 180.1075 130.35)
		(property "Reference" "GNDA10"
			(at 0 -1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 170.2 121.99 -90)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U10"
			(at 0 -3.4 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AD8137YRZ"
			(at 0 3.4 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-AD8137YRZ-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/AD8137YRZ/669749"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.614 -1.905 270)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 134 "Net-(U10--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.614 -0.635 270)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "Net-(U10-Vocm)")
			(pinfunction "Vocm")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.614 0.635 270)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.614 1.905 270)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "Net-(R35-Pad2)")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 2.614 1.905 270)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "Net-(R34-Pad2)")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at 2.614 0.635 270)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at 2.614 -0.635 270)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 150 "unconnected-(U10-PD-Pad7)")
			(pinfunction "PD")
			(pintype "input+no_connect")
		)
		(pad "8" smd roundrect
			(at 2.614 -1.905 270)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 133 "Net-(U10-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 192.69 75.9)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP-2"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 7 "-14V0")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
		(layer "F.Cu")
		(at 184.71 105.56 90)
		(descr "Potentiometer, vertical, Bourns 3224W, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
		(tags "Potentiometer vertical Bourns 3224W")
		(property "Reference" "RV5"
			(at 0 -3.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "20K"
			(at 0 3.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/3224.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "118-3224W-1-203ECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/bourns-inc/3224W-1-203E/225661"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.6 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+14V0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 1.45 90)
			(size 2 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 200 "Net-(RV5-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "-14V0")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224W_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/3D Models/3224W-1-203E.stp"
			(offset
				(xyz -1.2 -0.64 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 157.33 111.84 90)
		(property "Reference" "GNDA2"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 154.34 57.35)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_D3.1"
			(at 2 -0.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 215 "+5VD")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 162.83 100.6647)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_IA_Y1"
			(at 1.3716 -4.0782 45)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 20 "Net-(U7-IOUTA)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 161.84 81.11)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 172.76 109.89)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R81"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.82K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A140440CT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J1K82BTD/9480388"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC gain adjustable preset"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 196 "Net-(R81-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 197 "Net-(R81-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 139.27 78.48 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C68"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 194.34 103.35 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C82"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 162.83 102.1647)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_IB_Y1"
			(at 1.524 3.7958 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 19 "Net-(U7-IOUTB)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 158.86 89.18 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 193.92 57.34 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 14 "-15V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 187.04 126.37 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R91"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "12.1k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P12.1KDBCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB1212V/2026845"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC offset preset"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 207 "Net-(R91-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 142.64 93.7 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C83"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 119.85 66.28295 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good load"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33	"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 225 "/PG-14A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "Net-(R24-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 173.52 111.84)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C86"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 172.76 108.43 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R76"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.75k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P4.75KDBCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB4751V/2026809"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC gain preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 194 "Net-(R76-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(layer "F.Cu")
		(at 179.69 57.34 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -2.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at 0 2.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-CL32B106KAJ4PNECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL32B106KAJ4PNE/11487783?s=N4IgTCBcDaIMIBkDMYBCBGADANgNIEEApAFgAUA5AAhAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 13 "+15V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 121.412 77.49215 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 146.02 93.78 -90)
		(property "Reference" "GNDD3"
			(at 0 -1.2 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 187.38 82.09 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C72"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 161.08 87.65 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(U8-REFIO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.92 61.03 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R84"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB152V/1465858"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets power regulator current limit"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P1.5KDBCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 198 "Net-(U19-ILIM)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:TSSOP-48_6.1x12.5mm_P0.5mm"
		(layer "F.Cu")
		(at 145.8348 83.559 180)
		(descr "TSSOP, 48 Pin (JEDEC MO-153 Var ED https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U4"
			(at 0.0048 -5.571 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SN74ALVCH16374DGGR"
			(at 0 7.2 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "296-1144-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/texas-instruments/SN74ALVCH16374DGGR/276787"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.8125 -5.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "1OE")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.8125 -5.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 106 "/X-1")
			(pinfunction "1Q1")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -3.8125 -4.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 105 "/X-2")
			(pinfunction "1Q2")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -3.8125 -4.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -3.8125 -3.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "/X-3")
			(pinfunction "1Q3")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -3.8125 -3.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "/X-4")
			(pinfunction "1Q4")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -3.8125 -2.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at -3.8125 -2.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 102 "/X-5")
			(pinfunction "1Q5")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at -3.8125 -1.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 101 "/X-6")
			(pinfunction "1Q6")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -3.8125 -1.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -3.8125 -0.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "/X-7")
			(pinfunction "1Q7")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at -3.8125 -0.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "/X-8")
			(pinfunction "1Q8")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at -3.8125 0.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "/X-9")
			(pinfunction "2Q1")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at -3.8125 0.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "/X-10")
			(pinfunction "2Q2")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at -3.8125 1.2485 180)
			(size 1.275 0.297)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -3.8125 1.7525 180)
			(size 1.275 0.305)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 96 "/X-11")
			(pinfunction "2Q3")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at -3.8125 2.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 95 "/X-12")
			(pinfunction "2Q4")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at -3.8125 2.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at -3.8125 3.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 94 "/X-13")
			(pinfunction "2Q5")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at -3.8125 3.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 93 "/X-14")
			(pinfunction "2Q6")
			(pintype "output")
		)
		(pad "21" smd roundrect
			(at -3.8125 4.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "22" smd roundrect
			(at -3.8125 4.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "unconnected-(U4-2Q7-Pad22)")
			(pinfunction "2Q7")
			(pintype "output+no_connect")
		)
		(pad "23" smd roundrect
			(at -3.8125 5.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 142 "unconnected-(U4-2Q8-Pad23)")
			(pinfunction "2Q8")
			(pintype "output+no_connect")
		)
		(pad "24" smd roundrect
			(at -3.8125 5.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "2OE")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 3.8125 5.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/S.LATCH_X")
			(pinfunction "2LE")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 3.8125 5.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 143 "unconnected-(U4-2D8-Pad26)")
			(pinfunction "2D8")
			(pintype "input+no_connect")
		)
		(pad "27" smd roundrect
			(at 3.8125 4.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/D-15")
			(pinfunction "2D7")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 3.8125 4.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" smd roundrect
			(at 3.8125 3.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/D-14")
			(pinfunction "2D6")
			(pintype "input")
		)
		(pad "30" smd roundrect
			(at 3.8125 3.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/D-13")
			(pinfunction "2D5")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at 3.8125 2.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "32" smd roundrect
			(at 3.8125 2.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/D-12")
			(pinfunction "2D4")
			(pintype "input")
		)
		(pad "33" smd roundrect
			(at 3.8125 1.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "/D-11")
			(pinfunction "2D3")
			(pintype "input")
		)
		(pad "34" smd roundrect
			(at 3.8125 1.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "35" smd roundrect
			(at 3.8125 0.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/D-10")
			(pinfunction "2D2")
			(pintype "input")
		)
		(pad "36" smd roundrect
			(at 3.8125 0.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/D-9")
			(pinfunction "2D1")
			(pintype "input")
		)
		(pad "37" smd roundrect
			(at 3.8125 -0.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/D-8")
			(pinfunction "1D8")
			(pintype "input")
		)
		(pad "38" smd roundrect
			(at 3.8125 -0.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/D-7")
			(pinfunction "1D7")
			(pintype "input")
		)
		(pad "39" smd roundrect
			(at 3.8125 -1.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" smd roundrect
			(at 3.8125 -1.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/D-6")
			(pinfunction "1D6")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at 3.8125 -2.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/D-5")
			(pinfunction "1D5")
			(pintype "input")
		)
		(pad "42" smd roundrect
			(at 3.8125 -2.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "43" smd roundrect
			(at 3.8125 -3.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/D-4")
			(pinfunction "1D4")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at 3.8125 -3.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/D-3")
			(pinfunction "1D3")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at 3.8125 -4.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "46" smd roundrect
			(at 3.8125 -4.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/D-2")
			(pinfunction "1D2")
			(pintype "input")
		)
		(pad "47" smd roundrect
			(at 3.8125 -5.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/D-1")
			(pinfunction "1D1")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at 3.8125 -5.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "/S.LATCH_X")
			(pinfunction "1LE")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-48_6.1x12.5mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:SOT-416"
		(layer "F.Cu")
		(at 159.55 63.75 -90)
		(descr "SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf")
		(tags "SOT-416")
		(property "Reference" "Q4"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MMBT3904TT1G"
			(at 0 2.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOT-416"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mmbt3904tt1-d.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "MMBT3904TT1GOSCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/onsemi/MMBT3904TT1G/919603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.65 -0.5 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 231 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.65 0.5 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.65 0 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "Net-(D8-K)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/2SK3019TL.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(layer "F.Cu")
		(at 168.21 57.34 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -2.3 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at 0 2.3 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-CL32B106KAJ4PNECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL32B106KAJ4PNE/11487783?s=N4IgTCBcDaIMIBkDMYBCBGADANgNIEEApAFgAUA5AAhAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 214 "+5VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:TSSOP-48_6.1x12.5mm_P0.5mm"
		(layer "F.Cu")
		(at 145.8307 119.9608)
		(descr "TSSOP, 48 Pin (JEDEC MO-153 Var ED https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U6"
			(at 0 -7.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SN74ALVCH16374DGGR"
			(at 0 7.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "296-1144-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/texas-instruments/SN74ALVCH16374DGGR/276787"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.8125 -5.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/S.WRITE_A")
			(pinfunction "1OE")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.8125 -5.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/D-1")
			(pinfunction "1Q1")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -3.8125 -4.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/D-2")
			(pinfunction "1Q2")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -3.8125 -4.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -3.8125 -3.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/D-3")
			(pinfunction "1Q3")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -3.8125 -3.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/D-4")
			(pinfunction "1Q4")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -3.8125 -2.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at -3.8125 -2.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/D-5")
			(pinfunction "1Q5")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at -3.8125 -1.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/D-6")
			(pinfunction "1Q6")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -3.8125 -1.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -3.8125 -0.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/D-7")
			(pinfunction "1Q7")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at -3.8125 -0.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/D-8")
			(pinfunction "1Q8")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at -3.8125 0.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/D-9")
			(pinfunction "2Q1")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at -3.8125 0.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/D-10")
			(pinfunction "2Q2")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at -3.8125 1.2485)
			(size 1.275 0.297)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -3.8125 1.7525)
			(size 1.275 0.305)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "/D-11")
			(pinfunction "2Q3")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at -3.8125 2.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/D-12")
			(pinfunction "2Q4")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at -3.8125 2.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at -3.8125 3.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/D-13")
			(pinfunction "2Q5")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at -3.8125 3.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/D-14")
			(pinfunction "2Q6")
			(pintype "output")
		)
		(pad "21" smd roundrect
			(at -3.8125 4.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "22" smd roundrect
			(at -3.8125 4.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/D-15")
			(pinfunction "2Q7")
			(pintype "output")
		)
		(pad "23" smd roundrect
			(at -3.8125 5.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 147 "unconnected-(U6-2Q8-Pad23)")
			(pinfunction "2Q8")
			(pintype "output+no_connect")
		)
		(pad "24" smd roundrect
			(at -3.8125 5.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/S.WRITE_A")
			(pinfunction "2OE")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 3.8125 5.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/S.LATCH_A")
			(pinfunction "2LE")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 3.8125 5.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 162 "unconnected-(U6-2D8-Pad26)")
			(pinfunction "2D8")
			(pintype "input+no_connect")
		)
		(pad "27" smd roundrect
			(at 3.8125 4.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "/A-15")
			(pinfunction "2D7")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 3.8125 4.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" smd roundrect
			(at 3.8125 3.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 121 "/A-14")
			(pinfunction "2D6")
			(pintype "input")
		)
		(pad "30" smd roundrect
			(at 3.8125 3.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 120 "/A-13")
			(pinfunction "2D5")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at 3.8125 2.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "32" smd roundrect
			(at 3.8125 2.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "/A-12")
			(pinfunction "2D4")
			(pintype "input")
		)
		(pad "33" smd roundrect
			(at 3.8125 1.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "/A-11")
			(pinfunction "2D3")
			(pintype "input")
		)
		(pad "34" smd roundrect
			(at 3.8125 1.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "35" smd roundrect
			(at 3.8125 0.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 117 "/A-10")
			(pinfunction "2D2")
			(pintype "input")
		)
		(pad "36" smd roundrect
			(at 3.8125 0.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "/A-9")
			(pinfunction "2D1")
			(pintype "input")
		)
		(pad "37" smd roundrect
			(at 3.8125 -0.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 115 "/A-8")
			(pinfunction "1D8")
			(pintype "input")
		)
		(pad "38" smd roundrect
			(at 3.8125 -0.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 114 "/A-7")
			(pinfunction "1D7")
			(pintype "input")
		)
		(pad "39" smd roundrect
			(at 3.8125 -1.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" smd roundrect
			(at 3.8125 -1.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 113 "/A-6")
			(pinfunction "1D6")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at 3.8125 -2.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "/A-5")
			(pinfunction "1D5")
			(pintype "input")
		)
		(pad "42" smd roundrect
			(at 3.8125 -2.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "43" smd roundrect
			(at 3.8125 -3.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 111 "/A-4")
			(pinfunction "1D4")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at 3.8125 -3.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 110 "/A-3")
			(pinfunction "1D3")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at 3.8125 -4.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "46" smd roundrect
			(at 3.8125 -4.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 109 "/A-2")
			(pinfunction "1D2")
			(pintype "input")
		)
		(pad "47" smd roundrect
			(at 3.8125 -5.25)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 108 "/A-1")
			(pinfunction "1D1")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at 3.8125 -5.75)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/S.LATCH_A")
			(pinfunction "1LE")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-48_6.1x12.5mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 146.1 127.2 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Pullup for output enable on ADC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/S.WRITE_A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 164.5 102.92 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "25"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "13-RP0603BRD0725RLCT-ND"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/yageo/RP0603BRD0725RL/16916489"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC output load"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U7-IOUTB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 162.83 84.1047)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_IB_X1"
			(at 1.5748 3.9116 135)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 27 "Net-(U8-IOUTB)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 162.31 115.48 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 172.9 67 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "392K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3EKF3923V/196332"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets Power Good level"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P392KHCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 91 "Net-(U2-PGFB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 185.13 55.76)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LI0603G221R-10"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "240-2368-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/laird-signal-integrity-products/LI0603G221R-10/710125"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/-15V Supply")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "-15V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 179.64 126.405 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R95"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2K"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J2K0BTD/9480392"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC Gain preset"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A140444CT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 209 "Net-(R95-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U15--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal_Flipable"
		(layer "F.Cu")
		(at 201.2 117.5 -90)
		(descr "http://www.farnell.com/datasheets/612848.pdf")
		(tags "BNC Amphenol Horizontal")
		(property "Reference" "J8"
			(at 0.06 -2.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "Coaxial Con Amphenol 031-5538-10RFX"
			(at 0 6 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal_Flipable"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "ARF1691-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/amphenol-rf/031-5538-10RFX/2041817"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(J8-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -5.08 -5.08 270)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 -5.08 270)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/31-5538-10RFX.stp"
			(offset
				(xyz 0 -1.15 1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(layer "F.Cu")
		(at 154.73 77.66 90)
		(property "Reference" "GNDD8"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 175.94 66.7)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "140k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RN73C1J140KBTD/6557649"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets voltage reference"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A124703CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ".0625"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U2-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 161.84 99.17)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.9275 58 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.3k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P3.3KGCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEYJ332V/135886?s=N4IgTCBcDaIAoGYB0CDSBxAwgFQLQDkAREAXQF8g"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "5%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets LED brightness"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 173 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 190.47 111.84 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C89"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMF"
		(layer "F.Cu")
		(at 146.5 75.84)
		(descr "Diode SMF (DO-219AB), http://www.vishay.com/docs/95572/smf_do-219ab.pdf")
		(tags "Diode SMF (DO-214AB)")
		(property "Reference" "D12"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMF20A"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smf4l_datasheet.pdf.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "18-SMF4L20AT1GCT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/SMF4L20AT1G/21320688"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMF*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.45 0)
			(size 1.3 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 1 "GNDA")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.45 0)
			(size 1.3 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 18 "/-15V Supply")
			(pinfunction "A2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMF.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 170.01 93.78 -90)
		(property "Reference" "GNDD5"
			(at 0 -1.2 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 164.5 84.86 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "25"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "13-RP0603BRD0725RLCT-ND"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/yageo/RP0603BRD0725RL/16916489"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC output load"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U8-IOUTB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 188.8 57.3 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP-1"
			(at 0 -1.448 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 14 "-15V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 153.41 68.6)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 41 "Net-(U19-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 198.29 127.52)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_In1"
			(at 0.45 -5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 69 "Net-(J8-In)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 179.52 115.72 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U15"
			(at 0 -3.4 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1363"
			(at 0 3.4 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1363fa.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT1363CS8#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT1363CS8-TRPBF/958986"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.614 -1.905 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 158 "unconnected-(U15-VOS-Pad1)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(pad "2" smd roundrect
			(at -2.614 -0.635 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U15--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.614 0.635 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "Net-(U10-Vocm)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.614 1.905 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.614 1.905 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 88 "unconnected-(U15-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd roundrect
			(at 2.614 0.635 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 138 "Net-(C74-Pad1)")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at 2.614 -0.635 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.614 -1.905 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 159 "unconnected-(U15-VOS-Pad8)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMF"
		(layer "F.Cu")
		(at 135.9 75.84)
		(descr "Diode SMF (DO-219AB), http://www.vishay.com/docs/95572/smf_do-219ab.pdf")
		(tags "Diode SMF (DO-214AB)")
		(property "Reference" "D10"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMF20A"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smf4l_datasheet.pdf.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "18-SMF4L20AT1GCT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/SMF4L20AT1G/21320688"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMF*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.45 0)
			(size 1.3 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 216 "/+5V Supply")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.45 0)
			(size 1.3 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 1 "GNDA")
			(pinfunction "A2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMF.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 118.37 66.26295 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good load"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33	"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 224 "/PG3.3A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 234 "Net-(R26-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 172.4 114.58 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-2016-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B225KP8NFNC/3887674?s=N4IgTCBcDaIMIBkCMAGAQmMBWA0gBQA4A5AMSJAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "Net-(U10-Vocm)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 164.5 81.85 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "25"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "13-RP0603BRD0725RLCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/yageo/RP0603BRD0725RL/16916489"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC output load"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U8-IOUTA)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 182.44 57.34 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 13 "+15V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Logo_11.4x12mm_SilkScreen"
		(layer "F.Cu")
		(at 126.972141 130.715932)
		(descr "Open Source Hardware Logo")
		(tags "Logo OSHW")
		(property "Reference" "OSHW_logo_front"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Logo_11.4x12mm_SilkScreen"
			(at 1.226752 1.724504 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 173.95 96.13)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Y_A1"
			(at 0 -4.0132 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 131 "Net-(U11-Vout-)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 157.33 93.78 90)
		(property "Reference" "GNDD7"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 165.85 57.38)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_A3.1"
			(at -2.2 -0.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 214 "+5VA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 176.25 82.35)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R53"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J4K99BTD/9479768"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Input summing to single-ended stage"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 136 "Net-(U12-Vout+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "Net-(U13-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 161.4 58 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R89"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.3k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P3.3KGCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEYJ332V/135886?s=N4IgTCBcDaIAoGYB0CDSBxAwgFQLQDkAREAXQF8g"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets LED brightness"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 201 "Net-(D9-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 197 72 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R62"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A106051CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/CRG0603ZR/2380828"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Output current limiting (or not) on DAC single ended"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 189 "Net-(R59-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "Net-(J5-In)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 182.95 77.8)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R59"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.82K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB1821V/2026770"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC single ended gain resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P1.82KDBCT-ND "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 217 "Net-(U13--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 189 "Net-(R59-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 188.09 55.76 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "-15V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 179.17 102.76 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C71"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 194.3148 95.749)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Y_Out1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 137 "Net-(R60-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:Nidec SP4T CS-4-14NTA"
		(layer "F.Cu")
		(at 190.41 105.61 -90)
		(property "Reference" "SW3"
			(at -3.25 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 4.05 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:Nidec SP4T CS-4-14NTA"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/cs-4.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "563-1037-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/nidec-components-corporation/CS-4-14NTA/948348"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.15 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.3 -2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.3 2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 192 "Net-(R65-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 193 "Net-(R68-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.3 2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 200 "Net-(RV5-Pad2)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "C" smd rect
			(at 0 -2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "Net-(U17-+)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "NC" smd rect
			(at -1.35 -2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KIPRJMOD}/3D Models/CS-4-14NTA.stp"
			(offset
				(xyz 0 0 2.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 173.65 55.77)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LI0603G221R-10"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "240-2368-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/laird-signal-integrity-products/LI0603G221R-10/710125"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/+15V Supply")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+15V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 159.35 77.72 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 176.25 100.41)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R55"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J4K99BTD/9479768"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Input summing to single-ended stage"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 132 "Net-(U11-Vout+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "Net-(U14-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 178.52 100.55 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R57"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J4K99BTD/9479768"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Input summing to single-ended stage"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 163 "Net-(U17--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "Net-(U14-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 174.71 102.03)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A106051CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/CRG0603ZR/2380828"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Differential output current limiting (or not)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 132 "Net-(U11-Vout+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "Net-(J7-Pin_3)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 190.9 99.31 90)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U17"
			(at 0 -3.4 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1363"
			(at 0 3.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1363fa.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT1363CS8#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT1363CS8-TRPBF/958986"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.614 -1.905 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 166 "unconnected-(U17-VOS-Pad1)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(pad "2" smd roundrect
			(at -2.614 -0.635 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 163 "Net-(U17--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.614 0.635 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 164 "Net-(U17-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.614 1.905 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.614 1.905 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "unconnected-(U17-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd roundrect
			(at 2.614 0.635 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 163 "Net-(U17--)")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at 2.614 -0.635 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.614 -1.905 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 168 "unconnected-(U17-VOS-Pad8)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 164.51 97.09 90)
		(property "Reference" "GNDA16"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:CAP_20SVPF120M"
		(layer "F.Cu")
		(at 153.99 73.3 180)
		(property "Reference" "C10"
			(at 0.525 -4.335 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 uF"
			(at 0 4.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:CAP_20SVPF120M"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/os-con/models/20SVPF120M"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P16498CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/20SVPF120M/4204830"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.8 0 180)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2.8 0 180)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "${KIPRJMOD}/3D Models/20SVPF120M.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 183.62 54.2 90)
		(property "Reference" "GNDA13"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 183.71 108.94)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R65"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20122CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PB3B2202V/6212905"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC offset preset"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 192 "Net-(R65-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 160.25 113.9)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Clk_A1"
			(at 2 -1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 26 "/S.CLK_A")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
		(layer "F.Cu")
		(at 176.74 89.82 90)
		(descr "Potentiometer, vertical, Bourns 3224W, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
		(tags "Potentiometer vertical Bourns 3224W")
		(property "Reference" "RV1"
			(at -1.6 -5.75 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "20K"
			(at 0 3.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/3224.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "3224W-202ECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/bourns-inc/3224W-1-202E/225658"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.6 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 1.45 90)
			(size 2 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 188 "Net-(R75-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224W_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/3D Models/3224W-1-203E.stp"
			(offset
				(xyz -1.2 -0.64 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:TSSOP-48_6.1x12.5mm_P0.5mm"
		(layer "F.Cu")
		(at 145.8348 101.619 180)
		(descr "TSSOP, 48 Pin (JEDEC MO-153 Var ED https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U5"
			(at 0 -7.2 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SN74ALVCH16374DGGR"
			(at 0 7.2 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:TSSOP-48_6.1x12.5mm_P0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "296-1144-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/texas-instruments/SN74ALVCH16374DGGR/276787"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.8125 -5.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "1OE")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.8125 -5.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 86 "/Y-1")
			(pinfunction "1Q1")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -3.8125 -4.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 85 "/Y-2")
			(pinfunction "1Q2")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -3.8125 -4.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -3.8125 -3.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 84 "/Y-3")
			(pinfunction "1Q3")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -3.8125 -3.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 83 "/Y-4")
			(pinfunction "1Q4")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -3.8125 -2.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at -3.8125 -2.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "/Y-5")
			(pinfunction "1Q5")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at -3.8125 -1.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "/Y-6")
			(pinfunction "1Q6")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -3.8125 -1.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -3.8125 -0.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "/Y-7")
			(pinfunction "1Q7")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at -3.8125 -0.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "/Y-8")
			(pinfunction "1Q8")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at -3.8125 0.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "/Y-9")
			(pinfunction "2Q1")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at -3.8125 0.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "/Y-10")
			(pinfunction "2Q2")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at -3.8125 1.2485 180)
			(size 1.275 0.297)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -3.8125 1.7525 180)
			(size 1.275 0.305)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "/Y-11")
			(pinfunction "2Q3")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at -3.8125 2.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "/Y-12")
			(pinfunction "2Q4")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at -3.8125 2.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at -3.8125 3.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "/Y-13")
			(pinfunction "2Q5")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at -3.8125 3.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "/Y-14")
			(pinfunction "2Q6")
			(pintype "output")
		)
		(pad "21" smd roundrect
			(at -3.8125 4.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "22" smd roundrect
			(at -3.8125 4.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 144 "unconnected-(U5-2Q7-Pad22)")
			(pinfunction "2Q7")
			(pintype "output+no_connect")
		)
		(pad "23" smd roundrect
			(at -3.8125 5.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 145 "unconnected-(U5-2Q8-Pad23)")
			(pinfunction "2Q8")
			(pintype "output+no_connect")
		)
		(pad "24" smd roundrect
			(at -3.8125 5.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "2OE")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 3.8125 5.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/S.LATCH_Y")
			(pinfunction "2LE")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 3.8125 5.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "unconnected-(U5-2D8-Pad26)")
			(pinfunction "2D8")
			(pintype "input+no_connect")
		)
		(pad "27" smd roundrect
			(at 3.8125 4.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/D-15")
			(pinfunction "2D7")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 3.8125 4.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" smd roundrect
			(at 3.8125 3.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/D-14")
			(pinfunction "2D6")
			(pintype "input")
		)
		(pad "30" smd roundrect
			(at 3.8125 3.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/D-13")
			(pinfunction "2D5")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at 3.8125 2.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "32" smd roundrect
			(at 3.8125 2.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/D-12")
			(pinfunction "2D4")
			(pintype "input")
		)
		(pad "33" smd roundrect
			(at 3.8125 1.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "/D-11")
			(pinfunction "2D3")
			(pintype "input")
		)
		(pad "34" smd roundrect
			(at 3.8125 1.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "35" smd roundrect
			(at 3.8125 0.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "/D-10")
			(pinfunction "2D2")
			(pintype "input")
		)
		(pad "36" smd roundrect
			(at 3.8125 0.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/D-9")
			(pinfunction "2D1")
			(pintype "input")
		)
		(pad "37" smd roundrect
			(at 3.8125 -0.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/D-8")
			(pinfunction "1D8")
			(pintype "input")
		)
		(pad "38" smd roundrect
			(at 3.8125 -0.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/D-7")
			(pinfunction "1D7")
			(pintype "input")
		)
		(pad "39" smd roundrect
			(at 3.8125 -1.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" smd roundrect
			(at 3.8125 -1.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/D-6")
			(pinfunction "1D6")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at 3.8125 -2.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/D-5")
			(pinfunction "1D5")
			(pintype "input")
		)
		(pad "42" smd roundrect
			(at 3.8125 -2.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "43" smd roundrect
			(at 3.8125 -3.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "/D-4")
			(pinfunction "1D4")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at 3.8125 -3.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "/D-3")
			(pinfunction "1D3")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at 3.8125 -4.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "46" smd roundrect
			(at 3.8125 -4.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "/D-2")
			(pinfunction "1D2")
			(pintype "input")
		)
		(pad "47" smd roundrect
			(at 3.8125 -5.25 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/D-1")
			(pinfunction "1D1")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at 3.8125 -5.75 180)
			(size 1.275 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "/S.LATCH_Y")
			(pinfunction "1LE")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-48_6.1x12.5mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 191.81 61.13 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "13k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P13KGCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEYJ133V/135680"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets LED brightness"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 178 "Net-(D6-A)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 181.79 61.12 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1516-QBLP601D-OCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/qt-brightek-qtb/QBLP601D-O/13278855"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 172 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 177 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 187.45 79.07 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C57"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.92 64 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R88"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3ARB103V/3073635"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets Power Good level"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBDCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 199 "Net-(U19-PGFB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 187.42 66.7)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "140k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RN73C1J140KBTD/6557649"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets voltage reference"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A124703CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ".0625"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U3-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 184.38 61 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J1K0BTD/9479919"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets power regulator current limit"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND "
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 92 "Net-(U3-ILIM)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 182.95 81.25)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U13"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1363"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1363fa.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT1363CS8#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT1363CS8-TRPBF/958986"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.614 -1.905)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 153 "unconnected-(U13-VOS-Pad1)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(pad "2" smd roundrect
			(at -2.614 -0.635)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 217 "Net-(U13--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.614 0.635)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "Net-(U13-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.614 1.905)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.614 1.905)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 154 "unconnected-(U13-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd roundrect
			(at 2.614 0.635)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 189 "Net-(R59-Pad2)")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at 2.614 -0.635)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.614 -1.905)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 155 "unconnected-(U13-VOS-Pad8)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 181.19 75.9)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP+2"
			(at 1.5 -1.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 5 "+14V0")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:CAP_20SVPF120M"
		(layer "F.Cu")
		(at 176.98 73.3 180)
		(property "Reference" "C8"
			(at 0.525 -4.335 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 uF"
			(at 0 4.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:CAP_20SVPF120M"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/os-con/models/20SVPF120M"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P16498CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/20SVPF120M/4204830"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.8 0 180)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+14V0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2.8 0 180)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "${KIPRJMOD}/3D Models/20SVPF120M.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Scan Generator:SOT-416"
		(layer "F.Cu")
		(at 194.05 63.77 -90)
		(descr "SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf")
		(tags "SOT-416")
		(property "Reference" "Q3"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MMBT3904TT1G"
			(at 0 2.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOT-416"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mmbt3904tt1-d.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "MMBT3904TT1GOSCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/onsemi/MMBT3904TT1G/919603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.65 -0.5 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 230 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.65 0.5 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.65 0 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(D6-K)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/2SK3019TL.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 166.72 102.16)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "301"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1712-RA73F1J226RBTDCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RA73F1J226RBTD/16030916"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets differential output voltage range"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U7-IOUTB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 128 "Net-(U11--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:Nidec SP4T CS-4-14NTA"
		(layer "F.Cu")
		(at 165.12 89.85 90)
		(property "Reference" "SW1"
			(at -3.25 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 4.05 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:Nidec SP4T CS-4-14NTA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/cs-4.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "563-1037-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/nidec-components-corporation/CS-4-14NTA/948348"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.15 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.3 -2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 181 "Net-(R30-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.3 2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 182 "Net-(R72-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 183 "Net-(R74-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.3 2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 180 "Net-(R75-Pad1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "C" smd rect
			(at 0 -2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 124 "Net-(U8-FS_ADJ)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "NC" smd rect
			(at -1.35 -2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KIPRJMOD}/3D Models/CS-4-14NTA.stp"
			(offset
				(xyz 0 0 2.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 187.87 68.6)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 6 "Net-(U3-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:nanographs small"
		(layer "F.Cu")
		(at 193.248857 130.473844)
		(property "Reference" "front_logo"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "nanographs small"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 172.76 90.37 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R72"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.75k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P4.75KDBCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB4751V/2026809"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC gain preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 182 "Net-(R72-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 158.86 107.24 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:Nidec SP4T CS-4-14NTA"
		(layer "F.Cu")
		(at 190.41 87.55 -90)
		(property "Reference" "SW2"
			(at -3.25 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 4.05 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:Nidec SP4T CS-4-14NTA"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/cs-4.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "563-1037-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/nidec-components-corporation/CS-4-14NTA/948348"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.15 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.3 -2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.3 2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 184 "Net-(R77-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "Net-(R79-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.3 2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 186 "Net-(RV2-Pad2)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "C" smd rect
			(at 0 -2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 187 "Net-(U18-+)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "NC" smd rect
			(at -1.35 -2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KIPRJMOD}/3D Models/CS-4-14NTA.stp"
			(offset
				(xyz 0 0 2.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 175.86 57.99 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good pullup"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+15V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 223 "/PG+14A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 158.1 75.9)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP+3.2"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 10 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 169.8 108.43 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R80"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "Assortment"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC gain preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 195 "Net-(R80-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
		(layer "F.Cu")
		(at 184.71 87.5 90)
		(descr "Potentiometer, vertical, Bourns 3224W, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
		(tags "Potentiometer vertical Bourns 3224W")
		(property "Reference" "RV2"
			(at 0 -3.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "20K"
			(at 0 3.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/3224.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "118-3224W-1-203ECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/bourns-inc/3224W-1-203E/225661"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.6 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+14V0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 1.45 90)
			(size 2 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 186 "Net-(RV2-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "-14V0")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224W_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/3D Models/3224W-1-203E.stp"
			(offset
				(xyz -1.2 -0.64 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 170.96 57.34 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 214 "+5VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 178.32 111.84 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C87"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 180.33 61.12 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "13k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P13KGCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEYJ133V/135680"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets LED brightness"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+15V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 177 "Net-(D5-A)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 173.95 78.07)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_X_A1"
			(at -0.1016 -4.4704 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 135 "Net-(U12-Vout-)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 166.72 100.66)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "301"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1712-RA73F1J226RBTDCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RA73F1J226RBTD/16030916"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets differential output voltage range"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U7-IOUTA)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 127 "Net-(U11-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:C_1210_3225_Kelvin_Connections"
		(layer "F.Cu")
		(at 191.22 65.15 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 -2.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at -0.1 2.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:C_1210_3225_Kelvin_Connections"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-CL32B106KAJ4PNECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL32B106KAJ4PNE/11487783?s=N4IgTCBcDaIMIBkDMYBCBGADANgNIEEApAFgAUA5AAhAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 -0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at -1.475 0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 -0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 169.8 90.37 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R74"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "Assortment"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC gain preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 183 "Net-(R74-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 171.75 116.04)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R49"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J4K99BTD/9479768"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Part of ADC gain circuit responsible for Vcom"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 134 "Net-(U10--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "Net-(U10-Vocm)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:Nidec SP4T CS-4-14NTA"
		(layer "F.Cu")
		(at 176.9 121.67)
		(property "Reference" "SW6"
			(at -3.25 0 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 4.05 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:Nidec SP4T CS-4-14NTA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/cs-4.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "563-1037-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/nidec-components-corporation/CS-4-14NTA/948348"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.15 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.3 -2.25 180)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 211 "Net-(RV3-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.3 2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 209 "Net-(R95-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 208 "Net-(R94-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.3 2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 205 "Net-(R64-Pad1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "C" smd rect
			(at 0 -2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "Net-(C74-Pad1)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "NC" smd rect
			(at -1.35 -2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KIPRJMOD}/3D Models/CS-4-14NTA.stp"
			(offset
				(xyz 0 0 2.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 190.47 93.78 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 152.67 107.24 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 194.34 85.29 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C56"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 184.775 127.16)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R67"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.99K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J4K99BTD/9479768"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC offset summing"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139820CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U15--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "Net-(J8-In)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:SOT-416"
		(layer "F.Cu")
		(at 171.09 63.78 -90)
		(descr "SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf")
		(tags "SOT-416")
		(property "Reference" "Q2"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MMBT3904TT1G"
			(at 0 2.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOT-416"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mmbt3904tt1-d.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "MMBT3904TT1GOSCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/onsemi/MMBT3904TT1G/919603"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.65 -0.5 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 229 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.65 0.5 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.65 0 270)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 174 "Net-(D4-K)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/2SK3019TL.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Scan Generator:C_1210_3225_Kelvin_Connections"
		(layer "F.Cu")
		(at 156.76 65.15 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -2.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at -0.1 2.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:C_1210_3225_Kelvin_Connections"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-CL32B106KAJ4PNECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL32B106KAJ4PNE/11487783?s=N4IgTCBcDaIMIBkDMYBCBGADANgNIEEApAFgAUA5AAhAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 -0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at -1.475 0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 -0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 197.75 89.73 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R63"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A106051CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/CRG0603ZR/2380828"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Output current limiting (or not) on DAC single ended"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 137 "Net-(R60-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(J6-In)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 164.71 117.59 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C54"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-2016-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B225KP8NFNC/3887674?s=N4IgTCBcDaIMIBkCMAGAQmMBWA0gBQA4A5AMSJAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C49-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(C49-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 181.64 111.84 90)
		(property "Reference" "GNDA6"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 177.77 98.34)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R54"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J4K99BTD/9479768"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Input summing to single-ended stage"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 131 "Net-(U11-Vout-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 218 "Net-(U14--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 163.96 115.38 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C59"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1945-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B105KP8NFNC/3887603?s=N4IgTCBcDaIMIBkCMAGAQqgrAaQAoA4A5AMUJAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(C49-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 178.87 61.37 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good LED driver"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33	"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 223 "/PG+14A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 228 "Net-(Q1-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(layer "F.Cu")
		(at 203.49 127.15)
		(property "Reference" "GNDA11"
			(at 0 -1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 170.71 79.11)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.99K"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/vishay-dale/TNPW12064K99BYEN/9562428"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Differential gain resistor, sets ratio between single ended and differential output range"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.52"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "541-9840-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 129 "Net-(U12-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 135 "Net-(U12-Vout-)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
		(layer "F.Cu")
		(at 176.74 107.88 90)
		(descr "Potentiometer, vertical, Bourns 3224W, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
		(tags "Potentiometer vertical Bourns 3224W")
		(property "Reference" "RV6"
			(at 0 -3.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "20K"
			(at 0 3.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/3224.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "3224W-202ECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/bourns-inc/3224W-1-202E/225658"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.6 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 1.45 90)
			(size 2 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "Net-(R81-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224W_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/3D Models/3224W-1-203E.stp"
			(offset
				(xyz -1.2 -0.64 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 173.98 80.32 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A106051CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/CRG0603ZR/2380828"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Differential output current limiting (or not)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "Net-(J7-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "Net-(U12-Vout-)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 121.4628 74.28295)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "PowerGood1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 227 "/Power Good")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
		(layer "F.Cu")
		(at 182 121.12 -90)
		(descr "Potentiometer, vertical, Bourns 3224W, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
		(tags "Potentiometer vertical Bourns 3224W")
		(property "Reference" "RV3"
			(at 0 -3.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2K"
			(at 0 3.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/3224.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "3224W-202ECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/bourns-inc/3224W-1-202E/225658"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.6 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.25 -1.45 270)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 211 "Net-(RV3-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 1.45 270)
			(size 2 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 211 "Net-(RV3-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.25 -1.45 270)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(U15--)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224W_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/3D Models/3224W-1-203E.stp"
			(offset
				(xyz -1.2 -0.64 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 153.6275 55.76)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 215 "+5VD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 190.35 61.37 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R98"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good LED driver"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33	"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 225 "/PG-14A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 230 "Net-(Q3-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 181.89 93.81 90)
		(property "Reference" "GNDA4"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 172.9 63.99 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3ARB103V/3073635"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets Power Good level"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBDCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 91 "Net-(U2-PGFB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 167.39 61.37 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R99"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good LED driver"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33	"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 229 "Net-(Q2-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 224 "/PG3.3A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 193.41 111.84 90)
		(property "Reference" "GNDA7"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:R_0603_1608Metric 2 pos sellector"
		(layer "F.Cu")
		(at 154.07 91.84 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "JP7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Jumper_3_Bridged12"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:R_0603_1608Metric 2 pos sellector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P0.0GCT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEY0R00V/135656"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*3Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.6 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.05 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 221 "Net-(JP7-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.7 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 187.45 97.13 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C60"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 177.33 57.44)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP+1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 13 "+15V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 186.71 90.88 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R78"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "13k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20098CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PB3B1302V/6212881"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC offset preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 184 "Net-(R77-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 169.485 111.84 90)
		(property "Reference" "GNDA5"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 182.95 99.31)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U14"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1363"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1363fa.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT1363CS8#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT1363CS8-TRPBF/958986"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.614 -1.905)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 156 "unconnected-(U14-VOS-Pad1)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(pad "2" smd roundrect
			(at -2.614 -0.635)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 218 "Net-(U14--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.614 0.635)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "Net-(U14-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.614 1.905)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.614 1.905)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 87 "unconnected-(U14-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd roundrect
			(at 2.614 0.635)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 137 "Net-(R60-Pad2)")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at 2.614 -0.635)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.614 -1.905)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 157 "unconnected-(U14-VOS-Pad8)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 174.98 126.67 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R61"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "500"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "541-3301-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/vishay-dale/TNPU0603500RAZEN00/6615936"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Pre-clamping part of gain circuit on ADC buffer op amp responsible for video signal in"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "a problem"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 40 "Net-(D7-COM)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.243902)
			(net 138 "Net-(C74-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 151.6 124.04)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_ADC_MSB1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 121 "/A-14")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 174.28 103.95)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Y_B1"
			(at 0.1016 3.7572 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 132 "Net-(U11-Vout+)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 174.28 85.89)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_X_B1"
			(at 0 3.9116 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 136 "Net-(U12-Vout+)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:Cable Pinout 1-8 Front"
		(layer "F.Cu")
		(at 114.7826 107.569)
		(property "Reference" "REF**"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Cable Pinout 1-8 Front"
			(at 0 -1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Scan Generator:Cable Pinout 1-8 Front"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "D8"
			(at 0 8.89 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D2"
			(at 0 -6.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D1"
			(at 0 -8.89 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D6"
			(at 0 3.81 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D4"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D7"
			(at 0 6.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D3"
			(at 0 -3.81 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D5"
			(at 0 1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 194.34 126.37 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "37.4k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20150CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PB3B3742V/6212933"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC offset preset"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 213 "Net-(R27-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:IDC-Header_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
		(locked yes)
		(layer "F.Cu")
		(at 127.36 96.14)
		(descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
		(property "Reference" "J4"
			(at 1.38 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 1.27 28.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:IDC-Header_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "WM20559-ND"
			(at -1.1332 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at -1.1332 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/molex/0878342019/3303513?s=N4IgTCBcDaILIHsA2BTAHgAgAwA4DsOAzACxhYCMAnCALoC%2BQA"
			(at -1.1332 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 70 "unconnected-(J4-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 190 "unconnected-(J4-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/D-9")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/D-10")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/D-11")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/D-12")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/D-13")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/D-14")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/D-15")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 179 "unconnected-(J4-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(J4-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "unconnected-(J4-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_0.75mm_Mask1.5mm"
		(layer "F.Cu")
		(at 124.11 56.62)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "FID3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Fiducial:Fiducial_0.75mm_Mask1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 166.02 121.24)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "25"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "13-RP0603BRD0725RLCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/yageo/RP0603BRD0725RL/16916489"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC input load"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U9-Ain-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "Net-(R35-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 160.66 54.2 90)
		(property "Reference" "GNDA14"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 151.5 97.61)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Y_MSB1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 73 "/Y-14")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 149.92 66.99 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R87"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "82.5k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB8252V/2026921"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets Power Good level"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P82.5KDBCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 199 "Net-(U19-PGFB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(layer "F.Cu")
		(at 140.08 125.91)
		(property "Reference" "GNDD1"
			(at 0 -1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(layer "F.Cu")
		(at 184.36 75.27)
		(property "Reference" "GNDA3"
			(at 0 -1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 170.2 117.54)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C67"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 191.42 126.37 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R92"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10.5k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139980CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J10K5BTD/9479928"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC offset preset"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 206 "Net-(R90-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 168.85 61.12 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.3k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P3.3KGCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEYJ332V/135886?s=N4IgTCBcDaIAoGYB0CDSBxAwgFQLQDkAREAXQF8g"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets LED brightness"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "+5VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 176 "Net-(D4-A)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 186.15 124.29)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Offset1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 65 "Net-(U16--)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 151.4275 58 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1516-QBLP601D-OCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/qt-brightek-qtb/QBLP601D-O/13278855"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 173 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 215 "+5VD")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 152.67 89.18 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 169.55 75.9)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP+3.1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 4 "+3V0")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:R_0603_1608Metric 2 pos sellector"
		(layer "F.Cu")
		(at 154.02 109.9 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "JP5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Jumper_3_Bridged12"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:R_0603_1608Metric 2 pos sellector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P0.0GCT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEY0R00V/135656"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*3Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.6 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.05 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 219 "Net-(JP5-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.7 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 163.81 121.99 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "12 pF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "CL10C471JB8NNNC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1168-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10C471JB8NNNC/3886826"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC input bandwidth"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U9-Ain+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U9-Ain-)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 172.76 91.83)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R75"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.82K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A140440CT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J1K82BTD/9480388"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC gain adjustable preset"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 180 "Net-(R75-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 188 "Net-(R75-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 172.48 99.765 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C69"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 161.1864 101.4147 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C-Opt"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "Assortment"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC output bandwidth"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U7-IOUTB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U7-IOUTA)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 184.02 124.33)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Sum1"
			(at -0.7092 -1.7308 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 64 "Net-(U15--)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 152.96 66.7)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R83"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "33k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3ARB333V/3073660"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets voltage reference"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P33KBDCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "Net-(U19-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
		(layer "F.Cu")
		(at 187.35 121.07 90)
		(descr "Potentiometer, vertical, Bourns 3224W, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
		(tags "Potentiometer vertical Bourns 3224W")
		(property "Reference" "RV7"
			(at 0 -3.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "20K"
			(at 0 3.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/3224.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "118-3224W-1-203ECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/bourns-inc/3224W-1-203E/225661"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.6 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "+14V0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 1.45 90)
			(size 2 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 210 "Net-(RV7-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.25 -1.45 90)
			(size 1.3 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "-14V0")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224W_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/3D Models/3224W-1-203E.stp"
			(offset
				(xyz -1.2 -0.64 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:MountingHole_3.5mm_Pad_Via_CrtYd"
		(layer "F.Cu")
		(at 209.2 129 180)
		(descr "Mounting Hole 3.5mm with Courtyard for Washers + Tolerance")
		(tags "mounting hole 3.5mm Courtyard")
		(property "Reference" "H4"
			(at 0 -4.5 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:MountingHole_3.5mm_Pad_Via_CrtYd"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.625 0 180)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" connect rect
			(at -2.5 -0.75 180)
			(size 5 8.5)
			(layers "F.Cu" "F.Mask")
		)
		(pad "1" connect rect
			(at -2.5 -0.75 180)
			(size 5 8.5)
			(layers "B.Cu" "B.Mask")
		)
		(pad "1" thru_hole circle
			(at -1.856155 -1.856155 180)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 1.856155 180)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" connect rect
			(at -0.750003 -2.5 270)
			(size 5 8.499994)
			(layers "F.Cu" "F.Mask")
		)
		(pad "1" connect rect
			(at -0.750003 -2.5 270)
			(size 5 8.499994)
			(layers "B.Cu" "B.Mask")
		)
		(pad "1" thru_hole circle
			(at 0 -2.625 180)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 7 7)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.625 180)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 -1.856155 180)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 1.856155 180)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.625 0 180)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 164.36 58 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.99k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3EKF4991V/196341"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good pullup"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P4.99KHCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "+5VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 224 "/PG3.3A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 162.9 58 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D9"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1516-QBLP601D-OCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/qt-brightek-qtb/QBLP601D-O/13278855"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 201 "Net-(D9-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "+5VA")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 170.31 61.12 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D4"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1516-QBLP601D-OCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/qt-brightek-qtb/QBLP601D-O/13278855"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 174 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 176 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 192.88 126.37 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10.2k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139979CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J10K2BTD/9479927"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC offset preset"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 213 "Net-(R27-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:TSSOP-28_4.4x9.7mm_P0.65mm"
		(layer "F.Cu")
		(at 156.5 83.35)
		(descr "TSSOP, 28 Pin (JEDEC MO-153 Var AE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U8"
			(at 0 -5.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AD9744ARUZ"
			(at 0 5.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9744.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-AD9744ARUZ-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/AD9744ARUZ/936549"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x9.7mm*P0.65mm*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.943 -4.225)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 93 "/X-14")
			(pinfunction "D13")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.943 -3.575)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 94 "/X-13")
			(pinfunction "D12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.943 -2.925)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 95 "/X-12")
			(pinfunction "D11")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.943 -2.275)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 96 "/X-11")
			(pinfunction "D10")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.943 -1.625)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "/X-10")
			(pinfunction "D9")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.943 -0.975)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "/X-9")
			(pinfunction "D8")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.943 -0.326)
			(size 1.314 0.398)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 99 "/X-8")
			(pinfunction "D7")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.943 0.325)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "/X-7")
			(pinfunction "D6")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -2.943 0.975)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 101 "/X-6")
			(pinfunction "D5")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -2.943 1.625)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 102 "/X-5")
			(pinfunction "D4")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -2.943 2.275)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 103 "/X-4")
			(pinfunction "D3")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -2.943 2.925)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 104 "/X-3")
			(pinfunction "D2")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at -2.943 3.575)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 105 "/X-2")
			(pinfunction "D1")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at -2.943 4.225)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 106 "/X-1")
			(pinfunction "D0")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at 2.943 4.225)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 149 "unconnected-(U8-SLEEP-Pad15)")
			(pinfunction "SLEEP")
			(pintype "input+no_connect")
		)
		(pad "16" smd roundrect
			(at 2.943 3.575)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "REFLO")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at 2.943 2.925)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(U8-REFIO)")
			(pinfunction "REFIO")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 2.943 2.275)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 124 "Net-(U8-FS_ADJ)")
			(pinfunction "FS_ADJ")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at 2.943 1.625)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "20" smd roundrect
			(at 2.943 0.975)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "21" smd roundrect
			(at 2.943 0.325)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U8-IOUTB)")
			(pinfunction "IOUTB")
			(pintype "output")
		)
		(pad "22" smd roundrect
			(at 2.943 -0.326)
			(size 1.314 0.398)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U8-IOUTA)")
			(pinfunction "IOUTA")
			(pintype "output")
		)
		(pad "23" smd roundrect
			(at 2.943 -0.975)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "24" smd roundrect
			(at 2.943 -1.625)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "AVDD")
			(pintype "power_in")
		)
		(pad "25" smd roundrect
			(at 2.943 -2.275)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 221 "Net-(JP7-C)")
			(pinfunction "MODE")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 2.943 -2.925)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "DGND")
			(pintype "power_in")
		)
		(pad "27" smd roundrect
			(at 2.943 -3.575)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at 2.943 -4.225)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/S.CLK_D")
			(pinfunction "CLK")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:01550900M"
		(layer "F.Cu")
		(at 141.2 69.28 -90)
		(descr "01550900M-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "FH2"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fuse_Holder"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "Scan Generator:01550900M"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_154_154t_154l_154tl_datasheet.pdf.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "F1889-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/01550900M/2519878?s=N4IgTCBcDaIAwEYCsS4E45wLYgLoF8g"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.19 0)
			(size 3.81 4.24)
			(layers "F.Cu" "F.Mask")
			(net 204 "Net-(J1-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.19 0)
			(size 3.81 4.24)
			(layers "F.Cu" "F.Mask")
			(net 17 "/+15V Supply")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/01550900M.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 162.17 55.79)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LI0603G221R-10"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "240-2368-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/laird-signal-integrity-products/LI0603G221R-10/710125"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 216 "/+5V Supply")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "+5VA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 184.38 67 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "392K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3EKF3923V/196332"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets Power Good level"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P392KHCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "Net-(U3-PGFB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(layer "F.Cu")
		(at 191.17 57.34 90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 0 -2.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at 0 2.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-CL32B106KAJ4PNECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL32B106KAJ4PNE/11487783?s=N4IgTCBcDaIMIBkDMYBCBGADANgNIEEApAFgAUA5AAhAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 14 "-15V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 193.41 93.78 90)
		(property "Reference" "GNDD6"
			(at 0 -3.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 178.32 93.78 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 167.1 124.49)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_A+1"
			(at 0.07 3.41 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 125 "Net-(R34-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 117.78 69.35295 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R97"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good load"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33	"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 226 "/PG3.3D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 235 "Net-(R97-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 161.42 64 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3ARB103V/3073635"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets Power Good level"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBDCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 90 "Net-(U1-PGFB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 184.77 125.7)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R66"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.99K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J4K99BTD/9479768"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC offset summing"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139820CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U15--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "Net-(U16--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 164.53 129.36)
		(property "Reference" "GNDA9"
			(at 0 -1.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 161.35 93.78)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C64"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(layer "F.Cu")
		(at 195.08 54.22 90)
		(property "Reference" "GNDA17"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:HVSSOP-8-1_Expanded_Thermal_Pad_P0.65mm_EP1.57x1.89mm_ThermalVias"
		(layer "F.Cu")
		(at 170 101.41 90)
		(descr "HVSSOP, 8 Pin (https://www.ti.com/lit/ds/symlink/tpa6110a2.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HVSSOP SO")
		(property "Reference" "U11"
			(at 0 -3.81 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "THS4151"
			(at 0 2.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:HVSSOP-8-1_Expanded_Thermal_Pad_P0.65mm_EP1.57x1.89mm_ThermalVias"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ths4150.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "296-10054-5-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/texas-instruments/THS4151ID/380601"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 0 90)
			(size 1.41 1.7)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.15 -0.975 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 128 "Net-(U11--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.15 -0.325 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "Vocm")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.15 0.325 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.15 0.975 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 132 "Net-(U11-Vout+)")
			(pinfunction "Vout+")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 2.15 0.975 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 131 "Net-(U11-Vout-)")
			(pinfunction "Vout-")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at 2.15 0.325 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at 2.15 -0.325 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 151 "unconnected-(U11-PD-Pad7)")
			(pinfunction "PD")
			(pintype "input+no_connect")
		)
		(pad "8" smd roundrect
			(at 2.15 -0.975 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 127 "Net-(U11-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "9" thru_hole circle
			(at -0.485 -1.25 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at -0.485 0 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at -0.485 1.25 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 0 0 90)
			(size 1.57 3.1)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "9" smd rect
			(at 0 0 90)
			(size 1.57 3.1)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "9" thru_hole circle
			(at 0.485 -1.25 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at 0.485 0 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at 0.485 1.25 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(model "${KIPRJMOD}/3D Models/THS4150_DGN0008D.stp"
			(offset
				(xyz 0 0 0.59)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 151.5 79.55)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_X_MSB1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 93 "/X-14")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:Cable Pinout Ctrl Front"
		(layer "F.Cu")
		(at 124.5616 74.549)
		(property "Reference" "REF**"
			(at -2.286 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Cable Pinout Ctrl Front"
			(at -2.286 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Scan Generator:Cable Pinout Ctrl Front"
			(at -2.286 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -2.286 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at -2.286 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "ALa"
			(at 0 1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "ACl"
			(at 0 6.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "YLa"
			(at 0 -3.81 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "PG"
			(at 0 -11.43 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "AWr"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "XLa"
			(at 0 -6.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "DCl"
			(at 0 3.81 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
	)
	(footprint "Scan Generator:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal_Flipable"
		(layer "F.Cu")
		(at 201.2 87.5 -90)
		(descr "http://www.farnell.com/datasheets/612848.pdf")
		(tags "BNC Amphenol Horizontal")
		(property "Reference" "J6"
			(at 0.23 -3.02 90)
			(layer "F.SilkS")
		)
		(property "Value" "Coaxial Con Amphenol 031-5538-10RFX"
			(at 0 6 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal_Flipable"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "ARF1691-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/amphenol-rf/031-5538-10RFX/2041817"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(J6-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -5.08 -5.08 270)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 -5.08 270)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/31-5538-10RFX.stp"
			(offset
				(xyz 0 -1.15 1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 136.2 78.18)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C73"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias"
		(layer "F.Cu")
		(at 187.362344 62.65 -90)
		(descr "MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf#page=24), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U3"
			(at 0 -2.95 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT3094_MSE"
			(at 0 2.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT3094.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT3094EMSE#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT3094EMSE-TRPBF/9606784"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.41 -0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.41 0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 -0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.15 -1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "-15V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.15 -0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "-15V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.15 -0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 223 "/PG+14A")
			(pinfunction "EN/UV")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.15 0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 225 "/PG-14A")
			(pinfunction "PG")
			(pintype "open_collector")
		)
		(pad "5" smd roundrect
			(at -2.15 0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "Net-(U3-PGFB)")
			(pinfunction "PGFB")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.15 1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 92 "Net-(U3-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.15 1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "unconnected-(U3-VIOC-Pad7)")
			(pinfunction "VIOC")
			(pintype "output+no_connect")
		)
		(pad "8" smd roundrect
			(at 2.15 0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U3-SET)")
			(pinfunction "SET")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 2.15 0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 2.15 -0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "OUTS")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.15 -0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "12" smd roundrect
			(at 2.15 -1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "13" thru_hole circle
			(at -0.5 -1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 14 "-15V")
			(pinfunction "IN_Pad")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at -0.5 0 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 14 "-15V")
			(pinfunction "IN_Pad")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at -0.5 1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 14 "-15V")
			(pinfunction "IN_Pad")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.5 2.5)
			(layers "B.Cu")
			(net 14 "-15V")
			(pinfunction "IN_Pad")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.65 2.85)
			(layers "F.Cu" "F.Mask")
			(net 14 "-15V")
			(pinfunction "IN_Pad")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 -1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 14 "-15V")
			(pinfunction "IN_Pad")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 0 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 14 "-15V")
			(pinfunction "IN_Pad")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 14 "-15V")
			(pinfunction "IN_Pad")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 115.91 80.12 90)
		(property "Reference" "GNDD4"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 172.48 81.705 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C77"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 189.67 90.88)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R79"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "12k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20094CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PB3B1202V/6212877"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC offset preset"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 185 "Net-(R79-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 161.08 105.71 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U7-REFIO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 179.17 84.7 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C79"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 142.61 90.79 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias"
		(layer "F.Cu")
		(at 164.402344 62.65 -90)
		(descr "MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf#page=24), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U1"
			(at -1.6948 -2.95 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT3045"
			(at 0 2.95 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT3045.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT3045IMSE#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT3045IMSE-TRPBF/6235368"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.41 -0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.41 0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 -0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.41 0.71 270)
			(size 0.69 1.19)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.15 -1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "+5VA")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.15 -0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "+5VA")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.15 -0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "+5VA")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.15 0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "+5VA")
			(pinfunction "EN/UV")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.15 0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 224 "/PG3.3A")
			(pinfunction "PG")
			(pintype "open_collector")
		)
		(pad "6" smd roundrect
			(at -2.15 1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "Net-(U1-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.15 1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 90 "Net-(U1-PGFB)")
			(pinfunction "PGFB")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.15 0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(U1-SET)")
			(pinfunction "SET")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 2.15 0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 2.15 -0.325 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "OUTS")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.15 -0.975 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "12" smd roundrect
			(at 2.15 -1.625 270)
			(size 1.45 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "13" thru_hole circle
			(at -0.5 -1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at -0.5 0 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at -0.5 1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.5 2.5)
			(layers "B.Cu")
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 0 0 270)
			(size 1.65 2.85)
			(layers "F.Cu" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 -1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 0 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 0.5 1 270)
			(size 0.5 0.5)
			(drill 0.254)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:MountingHole_3.5mm_Pad_Via_CrtYd"
		(layer "F.Cu")
		(at 117.2 57)
		(descr "Mounting Hole 3.5mm with Courtyard for Washers + Tolerance")
		(tags "mounting hole 3.5mm Courtyard")
		(property "Reference" "H3"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:MountingHole_3.5mm_Pad_Via_CrtYd"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.625 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" connect rect
			(at -2.5 -0.75)
			(size 5 8.5)
			(layers "F.Cu" "F.Mask")
		)
		(pad "1" connect rect
			(at -2.5 -0.75)
			(size 5 8.5)
			(layers "B.Cu" "B.Mask")
		)
		(pad "1" thru_hole circle
			(at -1.856155 -1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at -1.856155 1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" connect rect
			(at -0.750003 -2.5 90)
			(size 5 8.499994)
			(layers "F.Cu" "F.Mask")
		)
		(pad "1" connect rect
			(at -0.750003 -2.5 90)
			(size 5 8.499994)
			(layers "B.Cu" "B.Mask")
		)
		(pad "1" thru_hole circle
			(at 0 -2.625)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 7 7)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 0 2.625)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 -1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 1.856155 1.856155)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole circle
			(at 2.625 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 161.1864 83.3547 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C55"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C-Opt"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "Assortment"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC output bandwidth"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U8-IOUTB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U8-IOUTA)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_0.75mm_Mask1.5mm"
		(layer "F.Cu")
		(at 136.31 122.88)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "FID1"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Fiducial:Fiducial_0.75mm_Mask1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
		)
	)
	(footprint "Scan Generator:Nidec SP4T CS-4-14NTA"
		(layer "F.Cu")
		(at 165.12 107.91 90)
		(property "Reference" "SW4"
			(at -3.25 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 4.05 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:Nidec SP4T CS-4-14NTA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/cs-4.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "563-1037-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/nidec-components-corporation/CS-4-14NTA/948348"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.15 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.3 -2.25 270)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 191 "Net-(R29-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.3 2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 194 "Net-(R76-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 195 "Net-(R80-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.3 2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 196 "Net-(R81-Pad1)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "C" smd rect
			(at 0 -2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 123 "Net-(U7-FS_ADJ)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "NC" smd rect
			(at -1.35 -2.25 90)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KIPRJMOD}/3D Models/CS-4-14NTA.stp"
			(offset
				(xyz 0 0 2.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 175.12 114.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Range1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 138 "Net-(C74-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 158.81 61.13 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D8"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1516-QBLP601D-OCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/qt-brightek-qtb/QBLP601D-O/13278855"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "Net-(D8-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "Net-(D8-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 161.42 67 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "82.5k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB8252V/2026921"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets Power Good level"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P82.5KDBCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 90 "Net-(U1-PGFB)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 168.4 116.04)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J1K0BTD/9479919"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Feedback on ADC buffer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "Net-(R35-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 134 "Net-(U10--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_0.75mm_Mask1.5mm"
		(layer "F.Cu")
		(at 203.56 59.52)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "FID2"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Fiducial:Fiducial_0.75mm_Mask1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 184.38 64 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3ARB103V/3073635"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets Power Good level"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBDCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 107 "Net-(U3-PGFB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 185.67 111.84)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C88"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:Nidec SP4T CS-4-14NTA"
		(layer "F.Cu")
		(at 192.5 121.62)
		(property "Reference" "SW5"
			(at -3.25 0 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 4.05 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:Nidec SP4T CS-4-14NTA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/cs-4.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "563-1037-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/nidec-components-corporation/CS-4-14NTA/948348"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -4.15 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.3 -2.25 180)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 213 "Net-(R27-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.3 2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 206 "Net-(R90-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 207 "Net-(R91-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.3 2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 210 "Net-(RV7-Pad2)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "C" smd rect
			(at 0 -2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "Net-(U16-+)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "NC" smd rect
			(at -1.35 -2.25)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KIPRJMOD}/3D Models/CS-4-14NTA.stp"
			(offset
				(xyz 0 0 2.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 150.6675 55.76)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LI0603G221R-10"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "240-2368-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/laird-signal-integrity-products/LI0603G221R-10/710125"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 216 "/+5V Supply")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 215 "+5VD")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 170.71 105.65)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.99K"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/vishay-dale/TNPW12064K99BYEN/9562428"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Differential gain resistor, sets ratio between single ended and differential output range"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.52"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "541-9840-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 128 "Net-(U11--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 132 "Net-(U11-Vout+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 119.25 69.35215 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good load"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33	"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 223 "/PG+14A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 233 "Net-(R25-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:LQFP-48_7x7mm_P0.5mm"
		(layer "F.Cu")
		(at 157.9275 119.9927 180)
		(descr "LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U9"
			(at 0 -5.85 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LTC2246HLX#PBF"
			(at 0 5.85 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:LQFP-48_7x7mm_P0.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "LTC2246HLX#PBF-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LTC2246HLX-PBF/1931208"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.25 -2.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -4.25 -2.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U9-Ain+)")
			(pinfunction "Ain+")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -4.25 -1.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U9-Ain-)")
			(pinfunction "Ain-")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -4.25 -1.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -4.25 -0.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C49-Pad1)")
			(pinfunction "REFH")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -4.25 -0.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C49-Pad1)")
			(pinfunction "REFH")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -4.25 0.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(C49-Pad2)")
			(pinfunction "REFL")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -4.25 0.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(C49-Pad2)")
			(pinfunction "REFL")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at -4.25 1.2485 180)
			(size 1.3 0.297)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at -4.25 1.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -4.25 2.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -4.25 2.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at -2.75 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at -2.25 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "/S.CLK_A")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at -1.75 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -1.25 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "SHDIN")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at -0.75 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at -0.25 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at 0.25 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 108 "/A-1")
			(pinfunction "D0")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at 0.75 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 109 "/A-2")
			(pinfunction "D1")
			(pintype "output")
		)
		(pad "21" smd roundrect
			(at 1.25 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 110 "/A-3")
			(pinfunction "D2")
			(pintype "output")
		)
		(pad "22" smd roundrect
			(at 1.75 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 111 "/A-4")
			(pinfunction "D3")
			(pintype "output")
		)
		(pad "23" smd roundrect
			(at 2.25 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 112 "/A-5")
			(pinfunction "D4")
			(pintype "output")
		)
		(pad "24" smd roundrect
			(at 2.75 4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "25" smd roundrect
			(at 4.25 2.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "26" smd roundrect
			(at 4.25 2.2565 180)
			(size 1.3 0.313)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 113 "/A-6")
			(pinfunction "D5")
			(pintype "output")
		)
		(pad "27" smd roundrect
			(at 4.25 1.7525 180)
			(size 1.3 0.305)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 114 "/A-7")
			(pinfunction "D6")
			(pintype "output")
		)
		(pad "28" smd roundrect
			(at 4.25 1.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 115 "/A-8")
			(pinfunction "D7")
			(pintype "output")
		)
		(pad "29" smd roundrect
			(at 4.25 0.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "30" smd roundrect
			(at 4.25 0.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "0GND")
			(pintype "power_in")
		)
		(pad "31" smd roundrect
			(at 4.25 -0.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "0VDD")
			(pintype "passive")
		)
		(pad "32" smd roundrect
			(at 4.25 -0.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "33" smd roundrect
			(at 4.25 -1.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 116 "/A-9")
			(pinfunction "D8")
			(pintype "output")
		)
		(pad "34" smd roundrect
			(at 4.25 -1.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 117 "/A-10")
			(pinfunction "D9")
			(pintype "output")
		)
		(pad "35" smd roundrect
			(at 4.25 -2.25 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 118 "/A-11")
			(pinfunction "D10")
			(pintype "output")
		)
		(pad "36" smd roundrect
			(at 4.25 -2.75 180)
			(size 1.3 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "37" smd roundrect
			(at 2.75 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "38" smd roundrect
			(at 2.25 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 119 "/A-12")
			(pinfunction "D11")
			(pintype "output")
		)
		(pad "39" smd roundrect
			(at 1.75 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 120 "/A-13")
			(pinfunction "D12")
			(pintype "output")
		)
		(pad "40" smd roundrect
			(at 1.2485 -4.25 180)
			(size 0.297 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 121 "/A-14")
			(pinfunction "D13")
			(pintype "output")
		)
		(pad "41" smd roundrect
			(at 0.75 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 122 "/A-15")
			(pinfunction "OF")
			(pintype "output")
		)
		(pad "42" smd roundrect
			(at 0.25 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 220 "Net-(JP6-C)")
			(pinfunction "MODE")
			(pintype "input")
		)
		(pad "43" smd roundrect
			(at -0.25 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "SENSE")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at -0.75 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "Net-(U10-Vocm)")
			(pinfunction "VCM")
			(pintype "output")
		)
		(pad "45" smd roundrect
			(at -1.25 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "Net-(U10-Vocm)")
			(pinfunction "VCM")
			(pintype "output")
		)
		(pad "46" smd roundrect
			(at -1.75 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "47" smd roundrect
			(at -2.25 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "48" smd roundrect
			(at -2.75 -4.25 180)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-48_7x7mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 145.26 111.84 90)
		(property "Reference" "GNDD2"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:CAP_20SVPF120M"
		(layer "F.Cu")
		(at 188.46 73.3)
		(property "Reference" "C9"
			(at 0.525 -4.335 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 uF"
			(at 0 4.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:CAP_20SVPF120M"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/os-con/models/20SVPF120M"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P16498CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/20SVPF120M/4204830"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.8 0)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2.8 0)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "-14V0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "${KIPRJMOD}/3D Models/20SVPF120M.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMF"
		(layer "F.Cu")
		(at 141.2 75.84)
		(descr "Diode SMF (DO-219AB), http://www.vishay.com/docs/95572/smf_do-219ab.pdf")
		(tags "Diode SMF (DO-214AB)")
		(property "Reference" "D11"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMF20A"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diodes/littelfuse_tvs_diode_smf4l_datasheet.pdf.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "18-SMF4L20AT1GCT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/SMF4L20AT1G/21320688"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMF*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.45 0)
			(size 1.3 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 17 "/+15V Supply")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.45 0)
			(size 1.3 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1923076923)
			(net 1 "GNDA")
			(pinfunction "A2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMF.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:01550900M"
		(layer "F.Cu")
		(at 146.5 69.28 -90)
		(descr "01550900M-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "FH3"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fuse_Holder"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "Scan Generator:01550900M"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_154_154t_154l_154tl_datasheet.pdf.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "F1889-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/01550900M/2519878?s=N4IgTCBcDaIAwEYCsS4E45wLYgLoF8g"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.19 0)
			(size 3.81 4.24)
			(layers "F.Cu" "F.Mask")
			(net 202 "Net-(J1-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.19 0)
			(size 3.81 4.24)
			(layers "F.Cu" "F.Mask")
			(net 18 "/-15V Supply")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/01550900M.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Scan Generator:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal_Flipable"
		(layer "F.Cu")
		(at 201.2 68.5 -90)
		(descr "http://www.farnell.com/datasheets/612848.pdf")
		(tags "BNC Amphenol Horizontal")
		(property "Reference" "J5"
			(at 6.45 1.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "Coaxial Con Amphenol 031-5538-10RFX"
			(at 0 6 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal_Flipable"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" " ~"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "ARF1691-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/amphenol-rf/031-5538-10RFX/2041817"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J5-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -5.08 -5.08 270)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.6 2.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.08 -5.08 270)
			(size 3.5 7)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/31-5538-10RFX.stp"
			(offset
				(xyz 0 -1.15 1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 174.4 58 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1516-QBLP601D-OCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/qt-brightek-qtb/QBLP601D-O/13278855"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 175 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "+15V")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 152.02 95.86)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 176.39 68.6)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 3 "Net-(U2-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 152.04 77.8)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 176.72 126.405 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C74"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "Assortment"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 138 "Net-(C74-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U15--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 188.5 126.37 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R93"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "18.7k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P18.7KDBCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB1872V/2026861"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC offset preset"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 207 "Net-(R91-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 170.91 127.75)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Clamped1"
			(at -0.1524 2.6416 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 40 "Net-(D7-COM)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:Cable Pinout 9-16 Front"
		(layer "F.Cu")
		(at 124.8156 107.569)
		(property "Reference" "REF**"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Cable Pinout 9-16 Front"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Scan Generator:Cable Pinout 9-16 Front"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "D11"
			(at 0 -3.81 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D13"
			(at 0 1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D9"
			(at 0 -8.89 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D15"
			(at 0 6.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D12"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D14"
			(at 0 3.81 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D10"
			(at 0 -6.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D16"
			(at 0 8.89 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 164.91 68.6)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 2 "Net-(U1-SET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2173913043)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 150.93 91.05)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_Clk_D2"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 25 "/S.CLK_D")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:CAP_20SVPF120M"
		(layer "F.Cu")
		(at 165.5 73.3 180)
		(property "Reference" "C7"
			(at 0.525 -4.335 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100 uF"
			(at 0 4.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:CAP_20SVPF120M"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://industrial.panasonic.com/ww/products/pt/os-con/models/20SVPF120M"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P16498CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/20SVPF120M/4204830"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.8 0 180)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+3V0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2.8 0 180)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "${KIPRJMOD}/3D Models/20SVPF120M.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 193.27 61.17 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D6"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1516-QBLP601D-OCT-ND"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/qt-brightek-qtb/QBLP601D-O/13278855"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "Net-(D6-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 178 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 166.72 82.6)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "301"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1712-RA73F1J226RBTDCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RA73F1J226RBTD/16030916"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets differential output voltage range"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U8-IOUTA)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 129 "Net-(U12-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 192.67 90.88 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R82"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "20k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20118CT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PB3B2002V/6212901"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC offset preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 185 "Net-(R79-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 142.61 108.85)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 173.52 93.78)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C62"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 189.905 115.72 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U16"
			(at 0 -3.4 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1363"
			(at 0 3.4 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1363fa.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT1363CS8#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT1363CS8-TRPBF/958986"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.614 -1.905 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 160 "unconnected-(U16-VOS-Pad1)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(pad "2" smd roundrect
			(at -2.614 -0.635 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "Net-(U16--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.614 0.635 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 139 "Net-(U16-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.614 1.905 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.614 1.905 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 89 "unconnected-(U16-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd roundrect
			(at 2.614 0.635 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "Net-(U16--)")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at 2.614 -0.635 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.614 -1.905 180)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 161 "unconnected-(U16-VOS-Pad8)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 162.83 82.6047)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_IA_X1"
			(at -0.0508 -6.2484 45)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 28 "Net-(U8-IOUTA)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:Reduced_pads_R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 180.39 77.98)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R70"
			(at 2.54 -1.92 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 2.54 1.92 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:Reduced_pads_R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "DNP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Optional axial resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 217 "Net-(U13--)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 189 "Net-(R59-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 161.35 111.84)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C84"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 194.3148 79.269)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP_X_Offset1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D1.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 165 "Net-(U18--)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:HVSSOP-8-1_Expanded_Thermal_Pad_P0.65mm_EP1.57x1.89mm_ThermalVias"
		(layer "F.Cu")
		(at 170 83.35 90)
		(descr "HVSSOP, 8 Pin (https://www.ti.com/lit/ds/symlink/tpa6110a2.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "HVSSOP SO")
		(property "Reference" "U12"
			(at 0 -3.81 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "THS4151"
			(at 0 2.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:HVSSOP-8-1_Expanded_Thermal_Pad_P0.65mm_EP1.57x1.89mm_ThermalVias"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ths4150.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "296-10054-5-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/texas-instruments/THS4151ID/380601"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at 0 0 90)
			(size 1.41 1.7)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.15 -0.975 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 130 "Net-(U12--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.15 -0.325 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "Vocm")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.15 0.325 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.15 0.975 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 136 "Net-(U12-Vout+)")
			(pinfunction "Vout+")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 2.15 0.975 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 135 "Net-(U12-Vout-)")
			(pinfunction "Vout-")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at 2.15 0.325 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at 2.15 -0.325 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 152 "unconnected-(U12-PD-Pad7)")
			(pinfunction "PD")
			(pintype "input+no_connect")
		)
		(pad "8" smd roundrect
			(at 2.15 -0.975 90)
			(size 1.45 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 129 "Net-(U12-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "9" thru_hole circle
			(at -0.485 -1.25 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at -0.485 0 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at -0.485 1.25 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 0 0 90)
			(size 1.57 3.1)
			(property pad_prop_heatsink)
			(layers "F.Cu")
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "9" smd rect
			(at 0 0 90)
			(size 1.57 3.1)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "9" thru_hole circle
			(at 0.485 -1.25 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at 0.485 0 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at 0.485 1.25 90)
			(size 0.6 0.6)
			(drill 0.3)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "TP")
			(pintype "power_in")
		)
		(model "${KIPRJMOD}/3D Models/THS4150_DGN0008D.stp"
			(offset
				(xyz 0 0 0.59)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 190.9 81.25 90)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U18"
			(at 0 -3.4 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1363"
			(at 0 3.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1363fa.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-LT1363CS8#TRPBFCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/LT1363CS8-TRPBF/958986"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.614 -1.905 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 169 "unconnected-(U18-VOS-Pad1)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(pad "2" smd roundrect
			(at -2.614 -0.635 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 165 "Net-(U18--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.614 0.635 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 187 "Net-(U18-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.614 1.905 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.614 1.905 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 170 "unconnected-(U18-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd roundrect
			(at 2.614 0.635 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 165 "Net-(U18--)")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at 2.614 -0.635 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.614 -1.905 90)
			(size 1.672 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 171 "unconnected-(U18-VOS-Pad8)")
			(pinfunction "VOS")
			(pintype "input+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 149.41 93.78)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C75"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-3178-1-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL31B475KAHNNWE/3888836?s=N4IgTCBcDaIMIBkDMBGAQgFgOwFYDSAggBIByJA6iALoC%2BQA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 10 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 172.9 58 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "13k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P13KGCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEYJ133V/135680"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets LED brightness"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 175 "Net-(D3-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 181.1 126.405 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R94"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3EKF1001V/196032"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "ADC Gain preset"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P1.00KHCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 208 "Net-(R94-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U15--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 167.7075 126.47)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J1K0BTD/9479919"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Feedback on ADC buffer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 125 "Net-(R34-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 133 "Net-(U10-+)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 166.72 84.1)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "301"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1712-RA73F1J226RBTDCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RA73F1J226RBTD/16030916"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets differential output voltage range"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U8-IOUTB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 130 "Net-(U12--)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 194.34 114.67 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C61"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(layer "F.Cu")
		(at 149.95 54.21 90)
		(property "Reference" "GNDD9"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 172.9 61.02 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RQ73C1J1K0BTD/9479919"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "1%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets power regulator current limit"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.15"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "A139971CT-ND "
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "Net-(U2-ILIM)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:01550900M"
		(layer "F.Cu")
		(at 135.9 69.28 -90)
		(descr "01550900M-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "FH1"
			(at -0.815 -0.155 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fuse_Holder"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "Scan Generator:01550900M"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_154_154t_154l_154tl_datasheet.pdf.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "F1889-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/littelfuse-inc/01550900M/2519878?s=N4IgTCBcDaIAwEYCsS4E45wLYgLoF8g"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.19 0)
			(size 3.81 4.24)
			(layers "F.Cu" "F.Mask")
			(net 203 "Net-(J1-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.19 0)
			(size 3.81 4.24)
			(layers "F.Cu" "F.Mask")
			(net 216 "/+5V Supply")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/01550900M.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Scan Generator:GND Test Point WIth Dimensions"
		(locked yes)
		(layer "F.Cu")
		(at 172.14 54.23 90)
		(property "Reference" "GNDA15"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 2.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:GND Test Point WIth Dimensions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "NA"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 -2.55 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1 1)
			(drill 0.4)
			(property pad_prop_testpoint)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Scan Generator:C_1210_3225_Kelvin_Connections"
		(layer "F.Cu")
		(at 168.26 65.15 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -2.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at -0.1 2.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:C_1210_3225_Kelvin_Connections"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-CL32B106KAJ4PNECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL32B106KAJ4PNE/11487783?s=N4IgTCBcDaIMIBkDMYBCBGADANgNIEEApAFgAUA5AAhAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 -0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at -1.475 0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 -0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0.75 270)
			(size 1.15 1.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+3V0")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 169.8 91.83 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.32k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P2.32KDBCT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB2321V/2026779"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC gain preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 181 "Net-(R30-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:TSSOP-28_4.4x9.7mm_P0.65mm"
		(layer "F.Cu")
		(at 156.5 101.41)
		(descr "TSSOP, 28 Pin (JEDEC MO-153 Var AE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U7"
			(at 0 -5.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AD9744ARUZ"
			(at 0 5.8 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9744.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "505-AD9744ARUZ-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/analog-devices-inc/AD9744ARUZ/936549"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x9.7mm*P0.65mm*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.943 -4.225)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "/Y-14")
			(pinfunction "D13")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.943 -3.575)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "/Y-13")
			(pinfunction "D12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.943 -2.925)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "/Y-12")
			(pinfunction "D11")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.943 -2.275)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 76 "/Y-11")
			(pinfunction "D10")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.943 -1.625)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 77 "/Y-10")
			(pinfunction "D9")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.943 -0.975)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "/Y-9")
			(pinfunction "D8")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.943 -0.326)
			(size 1.314 0.398)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 79 "/Y-8")
			(pinfunction "D7")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.943 0.325)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 80 "/Y-7")
			(pinfunction "D6")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -2.943 0.975)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 81 "/Y-6")
			(pinfunction "D5")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -2.943 1.625)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 82 "/Y-5")
			(pinfunction "D4")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -2.943 2.275)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 83 "/Y-4")
			(pinfunction "D3")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -2.943 2.925)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 84 "/Y-3")
			(pinfunction "D2")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at -2.943 3.575)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 85 "/Y-2")
			(pinfunction "D1")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at -2.943 4.225)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 86 "/Y-1")
			(pinfunction "D0")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at 2.943 4.225)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 148 "unconnected-(U7-SLEEP-Pad15)")
			(pinfunction "SLEEP")
			(pintype "input+no_connect")
		)
		(pad "16" smd roundrect
			(at 2.943 3.575)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "REFLO")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at 2.943 2.925)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U7-REFIO)")
			(pinfunction "REFIO")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 2.943 2.275)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 123 "Net-(U7-FS_ADJ)")
			(pinfunction "FS_ADJ")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at 2.943 1.625)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "20" smd roundrect
			(at 2.943 0.975)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "21" smd roundrect
			(at 2.943 0.325)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U7-IOUTB)")
			(pinfunction "IOUTB")
			(pintype "output")
		)
		(pad "22" smd roundrect
			(at 2.943 -0.326)
			(size 1.314 0.398)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U7-IOUTA)")
			(pinfunction "IOUTA")
			(pintype "output")
		)
		(pad "23" smd roundrect
			(at 2.943 -0.975)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "24" smd roundrect
			(at 2.943 -1.625)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "AVDD")
			(pintype "power_in")
		)
		(pad "25" smd roundrect
			(at 2.943 -2.275)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 219 "Net-(JP5-C)")
			(pinfunction "MODE")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 2.943 -2.925)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "DGND")
			(pintype "power_in")
		)
		(pad "27" smd roundrect
			(at 2.943 -3.575)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+3.3V")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at 2.943 -4.225)
			(size 1.314 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "/S.CLK_D")
			(pinfunction "CLK")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-28_4.4x9.7mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:IDC-Header_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
		(locked yes)
		(layer "F.Cu")
		(at 127.36 60.58)
		(descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
		(property "Reference" "J2"
			(at 1.34 -1.67 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 1.27 28.96 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:IDC-Header_2x10_P2.54mm_Vertical_No_Pin_1_Mark"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "WM20559-ND"
			(at -1.1332 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at -1.1332 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/molex/0878342019/3303513?s=N4IgTCBcDaILIHsA2BTAHgAgAwA4DsOAzACxhYCMAnCALoC%2BQA"
			(at -1.1332 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 10 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(J2-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 227 "/Power Good")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 222 "unconnected-(J2-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/S.LATCH_X")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/S.LATCH_Y")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/S.WRITE_A")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/S.LATCH_A")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/S.CLK_D")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/S.CLK_A")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(J2-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(J2-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:R_0603_1608Metric 2 pos sellector"
		(layer "F.Cu")
		(at 155.46 127.78 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "JP6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Jumper_3_Bridged12"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:R_0603_1608Metric 2 pos sellector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P0.0GCT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEY0R00V/135656"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*3Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.6 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V0")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.05 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 220 "Net-(JP6-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.7 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 187.38 100.15 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C78"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 172.48 103.05 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C76"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 185.87 58 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "13k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P13KGCT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3GEYJ133V/135680"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Sets LED brightness"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:Female M8 Right Angle Panel Mount Connector"
		(layer "F.Cu")
		(at 205.2 102.5 90)
		(property "Reference" "J7"
			(at 0 -4.1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Shielded"
			(at 0 -8.05 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:Female M8 Right Angle Panel Mount Connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.binder-usa.com/us-en/products/automation-technology/m8/86-6618-1121-00004-m8-female-panel-mount-connector-4-shieldable-tht-ip67-m10x075-front-fastened"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1SH*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -5.95 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 1.7 0.5 90)
			(size 1.7 1.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(J7-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.075 -1.45 90)
			(size 1.7 1.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(J7-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -1.7 0.5 90)
			(size 1.7 1.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(J7-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -1.075 -1.45 90)
			(size 1.7 1.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(J7-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole roundrect
			(at -6.25 0 90)
			(size 2 4)
			(drill oval 1 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.4)
			(net 1 "GNDA")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "5" thru_hole roundrect
			(at 6.25 0 90)
			(size 2 4)
			(drill oval 1 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.4)
			(net 1 "GNDA")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/86_6618_1121_00004.stp"
			(offset
				(xyz 0 -3.19 6.28)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 184.387344 58 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PA3J103V/5035971"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "meh - 5%"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "Power Good pullup"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.33"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P10KBZCT-ND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 225 "/PG-14A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(layer "F.Cu")
		(at 156.7075 57.34 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -2.3 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10u"
			(at 0 2.3 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-CL32B106KAJ4PNECT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL32B106KAJ4PNE/11487783?s=N4IgTCBcDaIMIBkDMYBCBGADANgNIEEApAFgAUA5AAhAF0BfIA"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 215 "+5VD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 186.71 108.94 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R69"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "13k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "P20098CT-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-PB3B1302V/6212881"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" "DAC offset preset"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "-14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 192 "Net-(R65-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 185.47 116.77 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C66"
			(at 0 -1.43 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1 uF"
			(at 0 1.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1276-1006-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B104KA8NNNC/3886664"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+14V0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Scan Generator:SOT-416"
		(layer "F.Cu")
		(at 173.05 127.31 90)
		(descr "SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf")
		(tags "SOT-416")
		(property "Reference" "D7"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SS423(TE85L,F)"
			(at 0 2.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:SOT-416"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/1SS423_datasheet_en_20220720.pdf?did=4401&prodName=1SS423"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK Part Number" "1SS423(TE85LF)CT-ND "
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.digikey.com/en/products/detail/toshiba-semiconductor-and-storage/1SS423-TE85L-F/4305011"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.65 -0.5 90)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GNDA")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.65 0.5 90)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+3V0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.65 0 90)
			(size 0.6 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(D7-COM)")
			(pinfunction "COM")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/2SK3019TL.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Scan Generator:M8 Right Angle Panel Mount Connector"
		(layer "F.Cu")
		(at 141.2 61 180)
		(property "Reference" "J1"
			(at 0.01 3.15 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Shielded"
			(at 0 -8.05 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Scan Generator:M8 Right Angle Panel Mount Connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Is Good" "Y"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Order Link" "https://www.binder-usa.com/us-en/products/automation-technology/m8/86-6319-1121-00004-m8-male-panel-mount-connector-4-shieldable-tht-ip67-front-fastened"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tolerance" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Context" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1SH*")
		(sheetname "Root")
		(sheetfile "Open Beam Interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -5.95 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -1.7 0.5 180)
			(size 1.7 1.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDA")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1.075 -1.45 180)
			(size 1.7 1.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 202 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 1.7 0.5 180)
			(size 1.7 1.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 1.075 -1.45 180)
			(size 1.7 1.7)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 204 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole roundrect
			(at -6.25 0 180)
			(size 2 4)
			(drill oval 1 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.4)
			(net 1 "GNDA")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "5" thru_hole roundrect
			(at 6.25 0 180)
			(size 2 4)
			(drill oval 1 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.4)
			(net 1 "GNDA")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/3D Models/09-3421-82-04.STP"
			(offset
				(xyz 0 -3.19 6.28)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(footprint "Scan Generator:Cable Pinout 9-16 Back"
		(layer "B.Cu")
		(at 124.82 107.57 180)
		(property "Reference" "D9-D16_silk_labels"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Cable Pinout 9-16 Back"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "D11"
			(at 0 3.81 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D13"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D12"
			(at 0 1.27 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D9"
			(at 0 8.89 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D10"
			(at 0 6.35 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D16"
			(at 0 -8.89 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D14"
			(at 0 -3.81 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D15"
			(at 0 -6.35 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
	)
	(footprint "Scan Generator:Cable Pinout 1-8 Back"
		(layer "B.Cu")
		(at 114.787 107.57 180)
		(property "Reference" "D1-D8_silk_labels"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Cable Pinout 1-8 Back"
			(at 0 1 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "D2"
			(at 0 6.35 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D1"
			(at 0 8.89 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D3"
			(at 0 3.81 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D5"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D7"
			(at 0 -6.35 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D4"
			(at 0 1.27 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D6"
			(at 0 -3.81 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D8"
			(at 0 -8.89 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
	)
	(footprint "Scan Generator:Scan Gen Art 2"
		(layer "B.Cu")
		(at 177.013351 92.258459 -90)
		(property "Reference" "scanning_art"
			(at 0 0.5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Scan Gen Art 2"
			(at 0 -1 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
	)
	(footprint "Symbol:OSHW-Logo_11.4x12mm_SilkScreen"
		(layer "B.Cu")
		(at 149.65 124.76 -90)
		(descr "Open Source Hardware Logo")
		(tags "Logo OSHW")
		(property "Reference" "OSHW_logo_back"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Value" "OSHW-Logo_11.4x12mm_SilkScreen"
			(at 0.75 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Scan Generator:Cable Pinout Ctrl Back"
		(layer "B.Cu")
		(at 122.28175 74.55 180)
		(property "Reference" "ctrl_silk_labels"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Cable Pinout Ctrl Back"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "A Write"
			(at 0 1.27 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "X Latch"
			(at 0 6.35 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Pwr Good"
			(at 0 11.43 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "A Clock"
			(at 0 -6.35 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Y Latch"
			(at 0 3.81 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "A Latch"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "D Clock"
			(at 0 -3.81 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
	)
	(footprint "Scan Generator:Offset and Scale Drawing"
		(layer "B.Cu")
		(at 150.19 84.87 -90)
		(property "Reference" "offset_scale_single_diff_drawing"
			(at 0 0.5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Offset and Scale Drawing"
			(at 0 -1 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "Differential"
			(at 8.4 -1.6 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Single Ended"
			(at 7.7 4.9 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "+"
			(at 9.6 2.1 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "-"
			(at 9.6 -5.2 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "-"
			(at 9.6 0.6 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "+"
			(at 9.6 -3.7 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Scale"
			(at 0.2 5.1 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "Offset"
			(at -12.7 5.1 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
	)
	(footprint "Scan Generator:Nanographs Big"
		(layer "B.Cu")
		(at 139.015723 95.532108 -90)
		(property "Reference" "back_logo"
			(at 0 0.5 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Nanographs Big"
			(at 0 -1 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
	)
	(footprint "Scan Generator:Portland Oregon Stag Sign"
		(layer "B.Cu")
		(at 149.841773 111.021859 -90)
		(property "Reference" "PDX_sign"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_line
		(start 113.2 129)
		(end 113.2 57)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.2 53)
		(end 209.2 53)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 213.2 57)
		(end 213.2 129)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 209.2 53)
		(mid 212.080236 54.119764)
		(end 213.2 57)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 117.2 133)
		(mid 114.371573 131.828427)
		(end 113.2 129)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 213.2 129)
		(mid 212.028427 131.828427)
		(end 209.2 133)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 209.2 133)
		(end 117.2 133)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 113.2 57)
		(mid 114.371573 54.171573)
		(end 117.2 53)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_text "Designed and manufactured by:"
		(at 135.08 67.540001 90)
		(layer "B.SilkS")
	)
	(gr_text "Differential\nX&Y"
		(at 197.04 102.5 90)
		(layer "B.SilkS")
	)
	(gr_text "Detector"
		(at 197 117.52 90)
		(layer "B.SilkS")
	)
	(gr_text "Made   in"
		(at 145.801773 105.531859 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 145.03 58.82 90)
		(layer "B.SilkS")
	)
	(gr_text "-15"
		(at 143.95 64.21 90)
		(layer "B.SilkS")
	)
	(gr_text "Power\nIn"
		(at 141.23 57.07 90)
		(layer "B.SilkS")
	)
	(gr_text "Y"
		(at 197.04 87.5 90)
		(layer "B.SilkS")
	)
	(gr_text "+5"
		(at 137.43 58.75 90)
		(layer "B.SilkS")
	)
	(gr_text "+15"
		(at 138.35 64.21 90)
		(layer "B.SilkS")
	)
	(gr_text "X"
		(at 197.22 68.5 90)
		(layer "B.SilkS")
	)
	(gr_text "Open Beam Interface"
		(at 164.043351 55.788459 90)
		(layer "B.SilkS")
	)
	(gr_text "by"
		(at 163.79 131.7 0)
		(layer "F.SilkS")
	)
	(gr_text "Mode"
		(at 155.34 126.71 0)
		(layer "F.SilkS")
	)
	(gr_text "DAC Scale"
		(at 179.68 89.83 90)
		(layer "F.SilkS")
	)
	(gr_text "Isabel Burgos\nAdam McCombs\n"
		(at 165.64 129.04 0)
		(layer "F.SilkS")
	)
	(gr_text "Buffer"
		(at 166.83 114.7 0)
		(layer "F.SilkS")
	)
	(gr_text "+3.0V Digital"
		(at 159.47 76.8 90)
		(layer "F.SilkS")
	)
	(gr_text "DAC Scale"
		(at 179.68 107.89 90)
		(layer "F.SilkS")
	)
	(gr_text "In"
		(at 165.31 59.55 0)
		(layer "F.SilkS")
	)
	(gr_text "Data"
		(at 133.25 81.09 0)
		(layer "F.SilkS")
	)
	(gr_text "Detector"
		(at 150.54 115 0)
		(layer "F.SilkS")
	)
	(gr_text "Out"
		(at 183.06 61.91 90)
		(layer "F.SilkS")
	)
	(gr_text "Offset"
		(at 194.78 101.9 90)
		(layer "F.SilkS")
	)
	(gr_text "X"
		(at 197.12 68.5 90)
		(layer "F.SilkS")
	)
	(gr_text "Digital"
		(at 144.83 109.76 0)
		(layer "F.SilkS")
	)
	(gr_text "Analog"
		(at 156.52 109.88 0)
		(layer "F.SilkS")
	)
	(gr_text "Power Good\n&&&& Gate"
		(at 113.83 64.15 0)
		(layer "F.SilkS")
	)
	(gr_text "Mode"
		(at 154.03 108.82 0)
		(layer "F.SilkS")
	)
	(gr_text "Analog"
		(at 156.52 91.82 0)
		(layer "F.SilkS")
	)
	(gr_text "Open Beam Interface\nrevA4 2025-07-01"
		(at 144.37 129.04 0)
		(layer "F.SilkS")
	)
	(gr_text "Out"
		(at 160.08 61.85 90)
		(layer "F.SilkS")
	)
	(gr_text "Analog"
		(at 157.88 127.95 0)
		(layer "F.SilkS")
	)
	(gr_text "+5.0"
		(at 137.11 62.34 90)
		(layer "F.SilkS")
	)
	(gr_text "Differential"
		(at 161.14 78.31 0)
		(layer "F.SilkS")
	)
	(gr_text "+14.0V Analog"
		(at 182.51 76.8 90)
		(layer "F.SilkS")
	)
	(gr_text "Scale"
		(at 179.73 125.04 0)
		(layer "F.SilkS")
	)
	(gr_text "Diff"
		(at 198.43 102.53 90)
		(layer "F.SilkS")
	)
	(gr_text "Single\nEnded"
		(at 175.5 97.73 0)
		(layer "F.SilkS")
	)
	(gr_text "Offset"
		(at 186.96 125.03 0)
		(layer "F.SilkS")
	)
	(gr_text "In"
		(at 188.27 59.55 0)
		(layer "F.SilkS")
	)
	(gr_text "X"
		(at 151.54 84.26 0)
		(layer "F.SilkS")
	)
	(gr_text "Y"
		(at 197.24 87.49 90)
		(layer "F.SilkS")
	)
	(gr_text "Out"
		(at 194.54 61.89 90)
		(layer "F.SilkS")
	)
	(gr_text "Bus"
		(at 133.25 83.05 0)
		(layer "F.SilkS")
	)
	(gr_text "Y"
		(at 151.54 102.32 0)
		(layer "F.SilkS")
	)
	(gr_text "-14.0V Analog"
		(at 193.99 76.8 90)
		(layer "F.SilkS")
	)
	(gr_text "Detector"
		(at 198.61 126.88 90)
		(layer "F.SilkS")
	)
	(gr_text "Digital"
		(at 144.83 91.7 0)
		(layer "F.SilkS")
	)
	(gr_text "VCOM"
		(at 163.26 128.12 0)
		(layer "F.SilkS")
	)
	(gr_text "Single\nEnded"
		(at 175.5 79.67 0)
		(layer "F.SilkS")
	)
	(gr_text "+3.0V Analog"
		(at 170.98 76.8 90)
		(layer "F.SilkS")
	)
	(gr_text "Differential"
		(at 161.14 96.37 0)
		(layer "F.SilkS")
	)
	(gr_text "Mode"
		(at 154.03 90.76 0)
		(layer "F.SilkS")
	)
	(gr_text "-15.0"
		(at 145.6 62.14 90)
		(layer "F.SilkS")
	)
	(gr_text "+15.0"
		(at 138.88 62.42 110)
		(layer "F.SilkS")
	)
	(gr_text "X&Y"
		(at 201.91 102.48 90)
		(layer "F.SilkS")
	)
	(gr_text "Offset"
		(at 194.78 83.84 90)
		(layer "F.SilkS")
	)
	(gr_text "Clamp"
		(at 172.79 123.38 -90)
		(layer "F.SilkS")
	)
	(gr_text "Out"
		(at 171.58 61.97 90)
		(layer "F.SilkS")
	)
	(gr_text "In"
		(at 153.81 59.55 0)
		(layer "F.SilkS")
	)
	(gr_text "In"
		(at 176.79 59.55 0)
		(layer "F.SilkS")
	)
	(gr_text "Digital"
		(at 147.72 127.97 0)
		(layer "F.SilkS")
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Dwgs.User")
		(pts
			(xy 213.2 129) (xy 213.2 57)
		)
		(height 34)
		(gr_text "72.0000 mm"
			(locked yes)
			(at 245.4 93 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 213.9 68.5) (xy 213.9 87.5)
		)
		(height -15.3)
		(gr_text "19.0000 mm"
			(at 227.4 78 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(locked yes)
		(layer "Dwgs.User")
		(pts
			(xy 217.2 53) (xy 217.2 133)
		)
		(height -25)
		(gr_text "80.0000 mm"
			(locked yes)
			(at 240.4 93 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 213.9 87.5) (xy 213.9 102.5)
		)
		(height -15.3)
		(gr_text "15.0000 mm"
			(at 227.4 95 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 213.9 102.5) (xy 213.9 117.5)
		)
		(height -15.3)
		(gr_text "15.0000 mm"
			(at 227.4 110 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 213.9 129) (xy 213.9 117.5)
		)
		(height 15.3)
		(gr_text "11.5000 mm"
			(at 231.65 121.31 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 213.9 68.5) (xy 213.9 57)
		)
		(height 15.3)
		(gr_text "11.5000 mm"
			(at 231.65 64.91 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 113.2 133) (xy 213.2 133)
		)
		(height 3.518)
		(gr_text "100.0000 mm"
			(at 163.2 134.718 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 117.2 129) (xy 209.2 129)
		)
		(height 11.461999)
		(gr_text "92.0000 mm"
			(at 163.2 138.661999 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 117.2 129) (xy 127.2 127)
		)
		(height 14.75)
		(orientation 0)
		(gr_text "10.0000 mm"
			(at 122.27 145.77 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 113.2 133) (xy 113.2 119)
		)
		(height -2.42)
		(orientation 1)
		(gr_text "14.0000 mm"
			(at 108.72 126.06 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 112.2 57) (xy 112.15 61)
		)
		(height -6.7)
		(orientation 1)
		(gr_text "4.0000 mm"
			(at 103.84 58.52 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 113.2 51.5) (xy 141.2 51.5)
		)
		(height -8.2)
		(orientation 0)
		(gr_text "28.0000 mm"
			(at 127.2 41.5 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 201.2 52.4) (xy 209.2 52)
		)
		(height -9.8)
		(orientation 0)
		(gr_text "8.0000 mm"
			(at 205.38 40.53 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.3)
			(arrow_length 1.27)
			(text_position_mode 2)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 3)
		(net_name "Net-(U2-SET)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 19)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 174.79 64.05) (xy 174.69 64.15) (xy 174.69 65.7) (xy 174.19 66.2) (xy 174.19 69.35) (xy 174.49 69.65)
				(xy 175.34 69.65) (xy 175.64 69.35) (xy 175.64 66.2) (xy 175.14 65.7) (xy 175.14 64.15) (xy 175.04 64.05)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDA")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 156.81 63.3) (xy 157.16 62.95) (xy 157.98 62.95) (xy 159.46 64.43) (xy 159.46 69.3) (xy 159.11 69.65)
				(xy 153.56 69.65) (xy 153.31 69.35) (xy 153.31 66.4) (xy 153.51 66.2) (xy 154.96 66.2) (xy 155.16 66.4)
				(xy 155.16 67.15) (xy 155.41 67.4) (xy 158.06 67.4) (xy 158.31 67.15) (xy 158.31 64.75) (xy 157.91 64.35)
				(xy 157.16 64.35) (xy 156.81 64)
			)
		)
	)
	(zone
		(net 7)
		(net_name "-14V0")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 18)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 188.07 64.2) (xy 188.27 64) (xy 189.42 64) (xy 189.92 64.5) (xy 192.32 64.5) (xy 192.62 64.8)
				(xy 192.62 67.05) (xy 192.42 67.25) (xy 191.42 67.25) (xy 191.22 67.05) (xy 191.22 66.1) (xy 190.97 65.85)
				(xy 190.27 65.85) (xy 190.017692 65.6) (xy 188.27 65.6) (xy 188.07 65.4)
			)
		)
	)
	(zone
		(net 10)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 18)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 153.61 64.2) (xy 153.81 64) (xy 154.96 64) (xy 155.46 64.5) (xy 157.86 64.5) (xy 158.16 64.8)
				(xy 158.16 67.05) (xy 157.96 67.25) (xy 156.96 67.25) (xy 156.76 67.05) (xy 156.76 66.1) (xy 156.51 65.85)
				(xy 155.81 65.85) (xy 155.557692 65.6) (xy 153.81 65.6) (xy 153.61 65.4)
			)
		)
	)
	(zone
		(net 217)
		(net_name "Net-(U13--)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 179.89 77.98) (xy 179.89 78.38) (xy 179.63 78.64) (xy 181.26 78.64) (xy 181.59 78.42) (xy 181.31 78.42)
				(xy 180.8 77.9)
			)
		)
	)
	(zone
		(net 14)
		(net_name "-15V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 185.27 55.3) (xy 185.52 55.05) (xy 187.92 55.05) (xy 188.17 55.3) (xy 188.17 56.1) (xy 188.52 56.45)
				(xy 189.27 56.45) (xy 189.62 56.1) (xy 189.62 55.3) (xy 189.87 55.05) (xy 194.72 55.05) (xy 194.97 55.3)
				(xy 194.97 56.9) (xy 194.62 57.25) (xy 189.97 57.25) (xy 189.67 57.55) (xy 189.67 59.65) (xy 189.42 59.9)
				(xy 189.42 61) (xy 189.17 61.25) (xy 188.21 61.25) (xy 188.02 61.06) (xy 188.02 59.2) (xy 188.02 58.3)
				(xy 187.67 57.95) (xy 186.97 57.95) (xy 186.62 57.6) (xy 186.62 56.7) (xy 186.32 56.4) (xy 185.52 56.4)
				(xy 185.27 56.15)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDA")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 179.79 63.3) (xy 180.14 62.95) (xy 180.99 62.95) (xy 182.44 64.4) (xy 182.44 69.3) (xy 182.09 69.65)
				(xy 176.54 69.65) (xy 176.29 69.35) (xy 176.29 66.4) (xy 176.49 66.2) (xy 177.94 66.2) (xy 178.14 66.4)
				(xy 178.14 67.15) (xy 178.39 67.4) (xy 181.04 67.4) (xy 181.29 67.15) (xy 181.29 64.75) (xy 180.89 64.35)
				(xy 180.14 64.35) (xy 179.79 64)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDA")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.31 63.3) (xy 168.66 62.95) (xy 169.5 62.95) (xy 170.96 64.41) (xy 170.96 69.3) (xy 170.61 69.65)
				(xy 165.06 69.65) (xy 164.81 69.35) (xy 164.81 66.4) (xy 165.01 66.2) (xy 166.46 66.2) (xy 166.66 66.4)
				(xy 166.66 67.15) (xy 166.91 67.4) (xy 169.56 67.4) (xy 169.81 67.15) (xy 169.81 64.75) (xy 169.41 64.35)
				(xy 168.66 64.35) (xy 168.31 64)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(U3-SET)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 19)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 186.27 64.05) (xy 186.17 64.15) (xy 186.17 65.7) (xy 185.67 66.2) (xy 185.67 69.35) (xy 185.97 69.65)
				(xy 186.82 69.65) (xy 187.12 69.35) (xy 187.12 66.2) (xy 186.62 65.7) (xy 186.62 64.15) (xy 186.52 64.05)
			)
		)
	)
	(zone
		(net 218)
		(net_name "Net-(U14--)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 179.89 96.04) (xy 179.89 96.44) (xy 179.63 96.7) (xy 181.26 96.7) (xy 181.59 96.48) (xy 181.31 96.48)
				(xy 180.8 95.96)
			)
		)
	)
	(zone
		(net 215)
		(net_name "+5VD")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150.81 55.3) (xy 151.06 55.05) (xy 153.46 55.05) (xy 153.71 55.3) (xy 153.71 56.1) (xy 154.06 56.45)
				(xy 154.81 56.45) (xy 155.16 56.1) (xy 155.16 55.3) (xy 155.41 55.05) (xy 160.26 55.05) (xy 160.51 55.3)
				(xy 160.51 56.9) (xy 160.16 57.25) (xy 155.51 57.25) (xy 155.21 57.55) (xy 155.21 59.65) (xy 155.21 60.75)
				(xy 154.71 61.25) (xy 153.11 61.25) (xy 152.96 61.1) (xy 152.96 59.8) (xy 153.56 59.2) (xy 153.56 58.3)
				(xy 153.21 57.95) (xy 151.082166 57.95) (xy 150.81 57.678865)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+14V0")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 175.34 65.7) (xy 175.84 65.7) (xy 176.19 66.05) (xy 176.19 69.9) (xy 175.89 70.2) (xy 173.94 70.2)
				(xy 173.64 69.9) (xy 173.64 65.95) (xy 173.89 65.7) (xy 174.49 65.7) (xy 174.04 66.15) (xy 174.04 69.45)
				(xy 174.39 69.8) (xy 175.44 69.8) (xy 175.79 69.45) (xy 175.79 66.15)
			)
		)
	)
	(zone
		(net 137)
		(net_name "Net-(R60-Pad2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.98 96.04) (xy 185.965 96.045) (xy 186.76 95.25) (xy 185.22 95.25) (xy 184.99 95.48) (xy 184.42 95.48)
			)
		)
	)
	(zone
		(net 7)
		(net_name "-14V0")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 186.82 65.7) (xy 187.32 65.7) (xy 187.67 66.05) (xy 187.67 69.9) (xy 187.37 70.2) (xy 185.42 70.2)
				(xy 185.12 69.9) (xy 185.12 65.95) (xy 185.37 65.7) (xy 185.97 65.7) (xy 185.52 66.15) (xy 185.52 69.45)
				(xy 185.87 69.8) (xy 186.92 69.8) (xy 187.27 69.45) (xy 187.27 66.15)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDA")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 191.27 63.3) (xy 191.62 62.95) (xy 192.46 62.95) (xy 193.92 64.41) (xy 193.92 69.3) (xy 193.57 69.65)
				(xy 188.02 69.65) (xy 187.77 69.35) (xy 187.77 66.4) (xy 187.97 66.2) (xy 189.42 66.2) (xy 189.62 66.4)
				(xy 189.62 67.15) (xy 189.87 67.4) (xy 192.52 67.4) (xy 192.77 67.15) (xy 192.77 64.75) (xy 192.37 64.35)
				(xy 191.62 64.35) (xy 191.27 64)
			)
		)
	)
	(zone
		(net 189)
		(net_name "Net-(R59-Pad2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.025)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.98 77.98) (xy 185.965 77.985) (xy 186.76 77.19) (xy 185.22 77.19) (xy 184.99 77.42) (xy 184.42 77.42)
			)
		)
	)
	(zone
		(net 10)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 152.36 65.7) (xy 152.86 65.7) (xy 153.21 66.05) (xy 153.21 69.9) (xy 152.91 70.2) (xy 150.96 70.2)
				(xy 150.66 69.9) (xy 150.66 65.95) (xy 150.91 65.7) (xy 151.51 65.7) (xy 151.06 66.15) (xy 151.06 69.45)
				(xy 151.41 69.8) (xy 152.46 69.8) (xy 152.81 69.45) (xy 152.81 66.15)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+3V0")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 18)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 165.11 64.2) (xy 165.31 64) (xy 166.46 64) (xy 166.96 64.5) (xy 169.36 64.5) (xy 169.66 64.8)
				(xy 169.66 67.05) (xy 169.46 67.25) (xy 168.46 67.25) (xy 168.26 67.05) (xy 168.26 66.1) (xy 168.01 65.85)
				(xy 167.31 65.85) (xy 167.057692 65.6) (xy 165.31 65.6) (xy 165.11 65.4)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(U1-SET)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 19)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 163.31 64.05) (xy 163.21 64.15) (xy 163.21 65.7) (xy 162.71 66.2) (xy 162.71 69.35) (xy 163.01 69.65)
				(xy 163.86 69.65) (xy 164.16 69.35) (xy 164.16 66.2) (xy 163.66 65.7) (xy 163.66 64.15) (xy 163.56 64.05)
			)
		)
	)
	(zone
		(net 214)
		(net_name "+5VA")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 162.31 55.3) (xy 162.56 55.05) (xy 164.96 55.05) (xy 165.21 55.3) (xy 165.21 56.1) (xy 165.56 56.45)
				(xy 166.31 56.45) (xy 166.66 56.1) (xy 166.66 55.3) (xy 166.91 55.05) (xy 171.66 55.05) (xy 171.99 55.38)
				(xy 171.99 56.92) (xy 171.66 57.25) (xy 167.01 57.25) (xy 166.71 57.55) (xy 166.71 59.65) (xy 166.46 59.9)
				(xy 166.46 61) (xy 166.21 61.25) (xy 164.61 61.25) (xy 164.46 61.1) (xy 164.46 59.8) (xy 165.06 59.2)
				(xy 165.06 58.3) (xy 164.71 57.95) (xy 162.6 57.95) (xy 162.317021 57.667021)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+3V0")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 163.86 65.7) (xy 164.36 65.7) (xy 164.71 66.05) (xy 164.71 69.9) (xy 164.41 70.2) (xy 162.46 70.2)
				(xy 162.16 69.9) (xy 162.16 65.95) (xy 162.41 65.7) (xy 163.01 65.7) (xy 162.56 66.15) (xy 162.56 69.45)
				(xy 162.91 69.8) (xy 163.96 69.8) (xy 164.31 69.45) (xy 164.31 66.15)
			)
		)
	)
	(zone
		(net 41)
		(net_name "Net-(U19-SET)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 19)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.81 64.05) (xy 151.71 64.15) (xy 151.71 65.7) (xy 151.21 66.2) (xy 151.21 69.35) (xy 151.51 69.65)
				(xy 152.36 69.65) (xy 152.66 69.35) (xy 152.66 66.2) (xy 152.16 65.7) (xy 152.16 64.15) (xy 152.06 64.05)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+3V0")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 161.83 115.8) (xy 162.79 115.8) (xy 162.94 115.95) (xy 162.94 118.29) (xy 162.78 118.45) (xy 161.4 118.45)
				(xy 161.24 118.29) (xy 161.24 117.11) (xy 161.68 116.67) (xy 161.68 115.95)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+14V0")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 18)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 176.59 64.2) (xy 176.79 64) (xy 177.94 64) (xy 178.44 64.5) (xy 180.84 64.5) (xy 181.14 64.8)
				(xy 181.14 67.05) (xy 180.94 67.25) (xy 179.94 67.25) (xy 179.74 67.05) (xy 179.74 66.1) (xy 179.49 65.85)
				(xy 178.79 65.85) (xy 178.537692 65.6) (xy 176.79 65.6) (xy 176.59 65.4)
			)
		)
	)
	(zone
		(net 13)
		(net_name "+15V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 173.79 55.3) (xy 174.04 55.05) (xy 176.44 55.05) (xy 176.69 55.3) (xy 176.69 56.1) (xy 177.04 56.45)
				(xy 177.79 56.45) (xy 178.14 56.1) (xy 178.14 55.3) (xy 178.39 55.05) (xy 183.24 55.05) (xy 183.49 55.3)
				(xy 183.49 56.9) (xy 183.14 57.25) (xy 178.49 57.25) (xy 178.19 57.55) (xy 178.19 59.65) (xy 177.94 59.9)
				(xy 177.94 61) (xy 177.69 61.25) (xy 176.09 61.25) (xy 175.94 61.1) (xy 175.94 59.8) (xy 176.54 59.2)
				(xy 176.54 58.3) (xy 176.19 57.95) (xy 174.118332 57.95) (xy 173.79 57.602354)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(locked yes)
		(layers "F&B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.0256)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 213.2 133) (xy 213.2 53) (xy 113.2 53) (xy 113.2 133)
			)
		)
		(polygon
			(pts
				(xy 211.2 131) (xy 211.2 55) (xy 115.2 55) (xy 115.2 131)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDA")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 115.2 55) (xy 133.13 55) (xy 133.13 70.37) (xy 160.59 70.37) (xy 160.59 77.02) (xy 160.73 77.16)
				(xy 160.73 80.74) (xy 160.19 81.28) (xy 157.22 81.28) (xy 156.21 82.29) (xy 156.21 94.81) (xy 156.51 95.11)
				(xy 160.46 95.11) (xy 160.76 95.41) (xy 160.76 98.67) (xy 160.07 99.36) (xy 156.6 99.36) (xy 156.21 99.75)
				(xy 156.21 110.4) (xy 155.8 110.81) (xy 153.1 110.81) (xy 152.64 111.27) (xy 152.64 131) (xy 115.2 131)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDA")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 152.84 111.48) (xy 153.31 111.01) (xy 155.89 111.01) (xy 156.4 110.5) (xy 156.4 99.86) (xy 156.7 99.56)
				(xy 160.17 99.56) (xy 160.96 98.77) (xy 160.96 95.31) (xy 160.56 94.91) (xy 156.71 94.91) (xy 156.41 94.61)
				(xy 156.41 82.39) (xy 157.32 81.48) (xy 160.28 81.48) (xy 160.93 80.83) (xy 160.93 77.04) (xy 160.79 76.9)
				(xy 160.79 70.37) (xy 133.13 70.37) (xy 133.13 55) (xy 211.2 55) (xy 211.2 131) (xy 152.84 131)
			)
		)
	)
	(zone
		(net 10)
		(net_name "+3.3V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 152.64 130.7) (xy 152.34 131) (xy 141.9 131) (xy 141.4 130.5) (xy 141.4 77.05) (xy 154.86 77.05)
				(xy 155.16 76.75) (xy 155.16 64.8) (xy 155.46 64.5) (xy 159.16 64.5) (xy 159.46 64.8) (xy 159.46 76.75)
				(xy 160 77.05) (xy 160.55 77.05) (xy 160.73 77.23) (xy 160.73 80.74) (xy 160.19 81.28) (xy 157.22 81.28)
				(xy 156.21 82.29) (xy 156.21 94.65) (xy 156.67 95.11) (xy 160.46 95.11) (xy 160.76 95.41) (xy 160.76 99.06)
				(xy 160.46 99.36) (xy 156.5 99.36) (xy 156.21 99.65) (xy 156.21 110.4) (xy 155.8 110.81) (xy 153.1 110.81)
				(xy 152.64 111.27)
			)
		)
	)
	(zone
		(net 14)
		(net_name "-15V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 16)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.62 63.4) (xy 189 63.4) (xy 189.65 62.705944) (xy 195.1 62.7) (xy 195.1 57.93) (xy 194.59 57.42)
				(xy 185.31 57.42) (xy 183.62 59.11)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+3V0")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.66 73.3) (xy 166.659744 64.800256) (xy 166.96 64.5) (xy 170.66 64.5) (xy 170.960021 64.8)
				(xy 170.96 76.3) (xy 170.41 76.85) (xy 168.7 76.85) (xy 166.14 79.41) (xy 166.14 111.44) (xy 174.28 119.58)
				(xy 174.28 130.69) (xy 173.97 131) (xy 153.14 131) (xy 152.84 130.7) (xy 152.84 111.48) (xy 153.31 111.01)
				(xy 155.89 111.01) (xy 156.4 110.5) (xy 156.4 99.86) (xy 156.7 99.56) (xy 160.64 99.56) (xy 160.96 99.24)
				(xy 160.96 95.31) (xy 160.56 94.91) (xy 156.81 94.91) (xy 156.41 94.51) (xy 156.41 82.39) (xy 157.32 81.48)
				(xy 160.28 81.48) (xy 160.93 80.83) (xy 160.93 77.47) (xy 161.35 77.05) (xy 162.91 77.05)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+14V0")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 178.44 64.5) (xy 182.14 64.5) (xy 182.44 64.8) (xy 182.44 76.75) (xy 182.74 77.05) (xy 188.38 77.05)
				(xy 189.42 78.09) (xy 189.42 82.355) (xy 189.12 82.655) (xy 186.565 82.655) (xy 185.22 81.31) (xy 173.34 81.31)
				(xy 172.94 81.71) (xy 172.94 83.75) (xy 174.8 85.61) (xy 184.44 85.61) (xy 184.74 85.91) (xy 184.74 87)
				(xy 184.44 87.3) (xy 182.65 87.3) (xy 182.26 87.69) (xy 182.26 89.2) (xy 182.64 89.58) (xy 189.1 89.58)
				(xy 189.4 89.88) (xy 189.4 91.1) (xy 189.1 91.4) (xy 188.59 91.4) (xy 188.29 91.1) (xy 188.29 90.61)
				(xy 187.88 90.2) (xy 186.68 90.2) (xy 185.72 91.16) (xy 185.72 95.39) (xy 188.52 98.19) (xy 188.52 100.4)
				(xy 188.22 100.7) (xy 186.57 100.7) (xy 185.24 99.37) (xy 173.35 99.37) (xy 172.95 99.77) (xy 172.95 100.54)
				(xy 176.14 103.73) (xy 184.42 103.73) (xy 184.72 104.03) (xy 184.72 105.2) (xy 184.42 105.5) (xy 182.77 105.5)
				(xy 182.26 106.01) (xy 182.26 106.96) (xy 182.81 107.51) (xy 189.1 107.51) (xy 189.4 107.81) (xy 189.4 109.14)
				(xy 189.1 109.44) (xy 188.59 109.44) (xy 188.29 109.14) (xy 188.29 108.57) (xy 187.89 108.17) (xy 186.06 108.17)
				(xy 184.74 109.49) (xy 182.84 109.49) (xy 182.44 109.89) (xy 182.44 114.37) (xy 182.84 114.77) (xy 186.71 114.77)
				(xy 187.01 115.07) (xy 187.01 120.67) (xy 186.71 120.97) (xy 184.97 120.97) (xy 184.61 121.33) (xy 184.61 123.31)
				(xy 187.67 126.37) (xy 187.67 127.44) (xy 188.08 127.85) (xy 188.92 127.85) (xy 189.33 127.44) (xy 189.33 126.44)
				(xy 189.63 126.14) (xy 190.29 126.14) (xy 190.59 126.44) (xy 190.59 127.54) (xy 190.89 127.84) (xy 191.85 127.84)
				(xy 192.24 127.45) (xy 192.24 126.45) (xy 192.54 126.15) (xy 193.21 126.15) (xy 193.51 126.45) (xy 193.51 127.79)
				(xy 193.81 128.09) (xy 194.65 128.09) (xy 194.95 128.39) (xy 194.95 130.7) (xy 194.65 131) (xy 174.78 131)
				(xy 174.48 130.7) (xy 174.48 119.48) (xy 166.34 111.34) (xy 166.34 79.51) (xy 168.8 77.05) (xy 177.84 77.05)
				(xy 178.14 76.75) (xy 178.14 64.8)
			)
		)
	)
	(zone
		(net 7)
		(net_name "-14V0")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.92 64.5) (xy 193.62 64.5) (xy 193.92 64.8) (xy 193.92 77.05) (xy 194.95 78.08) (xy 194.95 127.59)
				(xy 194.65 127.89) (xy 193.91 127.89) (xy 193.71 127.69) (xy 193.71 126.35) (xy 193.31 125.95) (xy 192.44 125.95)
				(xy 192.04 126.35) (xy 192.04 127.34) (xy 191.74 127.64) (xy 190.99 127.64) (xy 190.79 127.44) (xy 190.79 126.34)
				(xy 190.39 125.94) (xy 189.53 125.94) (xy 189.13 126.34) (xy 189.13 127.34) (xy 188.83 127.64) (xy 188.17 127.64)
				(xy 187.87 127.34) (xy 187.87 126.3) (xy 184.81 123.22) (xy 184.81 121.37) (xy 185.01 121.17) (xy 186.81 121.17)
				(xy 187.21 120.77) (xy 187.21 114.97) (xy 186.81 114.57) (xy 182.94 114.57) (xy 182.64 114.27) (xy 182.64 109.99)
				(xy 182.94 109.69) (xy 184.84 109.69) (xy 186.16 108.37) (xy 187.79 108.37) (xy 188.09 108.67) (xy 188.09 109.24)
				(xy 188.49 109.64) (xy 189.2 109.64) (xy 189.6 109.24) (xy 189.6 107.71) (xy 189.2 107.31) (xy 182.76 107.31)
				(xy 182.46 107.01) (xy 182.46 106) (xy 182.76 105.7) (xy 184.52 105.7) (xy 184.92 105.3) (xy 184.92 103.93)
				(xy 184.51 103.52) (xy 176.23 103.52) (xy 173.15 100.44) (xy 173.15 99.87) (xy 173.45 99.57) (xy 185.14 99.57)
				(xy 186.47 100.9) (xy 188.32 100.9) (xy 188.72 100.5) (xy 188.72 98.09) (xy 185.92 95.29) (xy 185.92 91.26)
				(xy 186.78 90.4) (xy 187.78 90.4) (xy 188.09 90.71) (xy 188.09 91.2) (xy 188.49 91.6) (xy 189.2 91.6)
				(xy 189.6 91.2) (xy 189.6 89.78) (xy 189.21 89.39) (xy 182.75 89.39) (xy 182.45 89.09) (xy 182.45 87.8)
				(xy 182.75 87.5) (xy 184.54 87.5) (xy 184.94 87.1) (xy 184.94 85.81) (xy 184.54 85.41) (xy 174.9 85.41)
				(xy 173.14 83.65) (xy 173.14 81.81) (xy 173.44 81.51) (xy 185.11 81.51) (xy 186.45 82.85) (xy 189.23 82.85)
				(xy 189.62 82.46) (xy 189.62 64.8)
			)
		)
	)
)