(kicad_pcb (version 20171130) (host pcbnew no-vcs-found-7586afd~61~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 53)
    (zones 0)
    (modules 7)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 1)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 +3V3)
  (net 4 NSS)
  (net 5 MOSI)
  (net 6 MISO)
  (net 7 SCK)
  (net 8 RST)
  (net 9 FSKTimeOut)
  (net 10 RxTimeOut)
  (net 11 TxRxDONE)
  (net 12 "Net-(J2-Pad1)")
  (net 13 "Net-(J4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net FSKTimeOut)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net NSS)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net RST)
    (add_net RxTimeOut)
    (add_net SCK)
    (add_net TxRxDONE)
  )
  (module lib:microduino (layer B.Cu) (tedit 5A42B2C9)
    (at 106.299 72.263 180)
    (tags "foont print ruotato mettere i comp su F Cu")
    (fp_text reference U1 (at 0.359999 3.450001 270) (layer B.SilkS))
    (fp_text value Microduino (at 0.232999 -2.137999 180) (layer B.SilkS) hide)
    (fp_text user GND (at 8.255 12.7 90) (layer F.SilkS))
    (fp_text user RST (at 8.255 10.16 90) (layer F.SilkS))
    (fp_text user D6 (at 8.255 7.62 90) (layer F.SilkS))
    (fp_text user D5 (at 8.255 5.08 90) (layer F.SilkS))
    (fp_text user D4 (at 8.255 2.54 90) (layer F.SilkS))
    (fp_text user D3 (at 8.255 0 90) (layer B.SilkS) hide)
    (fp_text user D2 (at 8.255 -2.54 90) (layer F.SilkS))
    (fp_text user D1 (at 8.255 -5.08 90) (layer B.SilkS) hide)
    (fp_text user D0 (at 8.255 -6.985 90) (layer F.SilkS))
    (fp_text user RX (at 12.065 -7.62 90) (layer F.SilkS))
    (fp_text user TX (at 12.065 -5.715 90) (layer F.SilkS))
    (fp_text user A7 (at 5.715 -5.08 90) (layer F.SilkS))
    (fp_text user A6 (at 6.35 -7.62 270) (layer F.SilkS))
    (fp_text user A5 (at 4.445 -7.62 90) (layer F.SilkS))
    (fp_text user A4 (at 2.54 -7.62 90) (layer F.SilkS))
    (fp_text user A3 (at 0 -7.62 90) (layer F.SilkS))
    (fp_text user A2 (at -2.54 -7.62 90) (layer B.SilkS) hide)
    (fp_text user A1 (at -4.445 -7.62 90) (layer B.SilkS) hide)
    (fp_text user A0 (at -6.35 -7.62 90) (layer F.SilkS))
    (fp_text user REF (at -5.715 -5.08 90) (layer F.SilkS))
    (fp_text user D13 (at -8.255 -7.62 90) (layer F.SilkS))
    (fp_text user D12 (at -8.255 -5.08 90) (layer B.SilkS) hide)
    (fp_text user D11 (at -8.255 -2.54 90) (layer F.SilkS))
    (fp_text user D10 (at -8.255 0 90) (layer F.SilkS))
    (fp_text user D9 (at -8.255 2.54 90) (layer F.SilkS))
    (fp_text user D8 (at -8.255 5.08 90) (layer F.SilkS))
    (fp_text user D7 (at -8.255 7.62 90) (layer F.SilkS))
    (fp_text user 3V3 (at -8.255 10.16 90) (layer F.SilkS))
    (fp_text user 5V (at -8.255 12.7 90) (layer F.SilkS))
    (fp_text user SCK (at -12.065 -7.62 90) (layer F.SilkS))
    (fp_text user SO (at -12.065 -5.08 90) (layer F.SilkS))
    (fp_text user SI (at -12.065 -2.54 90) (layer F.SilkS))
    (fp_text user SS (at -12.065 0 90) (layer F.SilkS))
    (fp_text user SDA (at 2.54 -12.065) (layer B.SilkS))
    (fp_text user SCL (at 5.08 -12.065) (layer F.SilkS))
    (fp_text user SDA (at 2.54 -12.065) (layer F.SilkS))
    (fp_text user SCL (at 5.08 -12.065) (layer B.SilkS))
    (fp_text user SS (at -12.065 0 90) (layer B.SilkS))
    (fp_text user SI (at -12.065 -2.54 90) (layer B.SilkS))
    (fp_text user SO (at -12.065 -5.08 90) (layer B.SilkS))
    (fp_text user SCK (at -12.065 -7.62 90) (layer B.SilkS))
    (fp_text user 5V (at -8.255 12.7 90) (layer B.SilkS))
    (fp_text user 3V3 (at -8.255 10.16 90) (layer B.SilkS) hide)
    (fp_text user D7 (at -8.255 7.62 90) (layer B.SilkS) hide)
    (fp_text user D8 (at -8.255 5.08 90) (layer B.SilkS) hide)
    (fp_text user D9 (at -8.255 2.54 90) (layer B.SilkS) hide)
    (fp_text user D10 (at -8.255 0 90) (layer B.SilkS) hide)
    (fp_text user D11 (at -8.255 -2.54 90) (layer B.SilkS) hide)
    (fp_text user D12 (at -8.255 -5.08 90) (layer F.SilkS))
    (fp_text user D13 (at -8.255 -7.62 90) (layer B.SilkS) hide)
    (fp_text user REF (at -5.715 -5.08 90) (layer B.SilkS) hide)
    (fp_text user A0 (at -6.35 -7.62 90) (layer B.SilkS) hide)
    (fp_text user A1 (at -4.445 -7.62 90) (layer F.SilkS))
    (fp_text user A2 (at -2.54 -7.62 90) (layer F.SilkS))
    (fp_text user A3 (at 0 -7.62 90) (layer B.SilkS) hide)
    (fp_text user A4 (at 2.54 -7.62 90) (layer B.SilkS) hide)
    (fp_text user A5 (at 4.445 -7.62 90) (layer B.SilkS) hide)
    (fp_text user A6 (at 6.35 -7.62 270) (layer B.SilkS) hide)
    (fp_text user A7 (at 5.715 -5.08 90) (layer B.SilkS) hide)
    (fp_text user TX (at 12.065 -5.715 90) (layer B.SilkS))
    (fp_text user RX (at 12.065 -7.62 90) (layer B.SilkS))
    (fp_text user D0 (at 8.255 -6.985 90) (layer B.SilkS) hide)
    (fp_text user D1 (at 8.255 -5.08 90) (layer F.SilkS))
    (fp_text user D2 (at 8.255 -2.54 90) (layer B.SilkS) hide)
    (fp_text user D3 (at 8.255 0 90) (layer F.SilkS))
    (fp_text user D4 (at 8.255 2.54 90) (layer B.SilkS) hide)
    (fp_text user D5 (at 8.255 5.08 90) (layer B.SilkS) hide)
    (fp_text user D6 (at 8.255 7.62 90) (layer B.SilkS) hide)
    (fp_text user RST (at 8.255 10.16 90) (layer B.SilkS) hide)
    (fp_text user GND (at 8.255 12.7 90) (layer B.SilkS))
    (pad 9 thru_hole circle (at 10.16 -7.62 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole circle (at 10.16 -5.08 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 7 thru_hole circle (at 10.16 -2.54 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 11 TxRxDONE))
    (pad 6 thru_hole circle (at 10.16 0 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 5 thru_hole circle (at 10.16 2.54 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 4 thru_hole circle (at 10.16 5.08 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 3 thru_hole circle (at 10.16 7.62 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at 10.16 10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 1 thru_hole circle (at 10.16 12.7 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 10.16 12.7 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 10 thru_hole circle (at 10.16 -10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 3 thru_hole circle (at 10.16 7.62 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 4 thru_hole circle (at 10.16 5.08 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 5 thru_hole circle (at 10.16 2.54 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 6 thru_hole circle (at 10.16 0 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 7 thru_hole circle (at 10.16 -2.54 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 11 TxRxDONE))
    (pad 8 thru_hole circle (at 10.16 -5.08 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 9 thru_hole circle (at 10.16 -7.62 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 11 thru_hole circle (at 7.62 -10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(J4-Pad1)"))
    (pad 12 thru_hole circle (at 5.08 -10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 13 thru_hole circle (at 2.54 -10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 14 thru_hole circle (at 0 -10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 8 RST))
    (pad 15 thru_hole circle (at -2.54 -10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 16 thru_hole circle (at -5.08 -10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 17 thru_hole circle (at -7.62 -10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 18 thru_hole circle (at -10.16 -10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 19 thru_hole circle (at -10.16 -7.62 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 7 SCK))
    (pad 20 thru_hole circle (at -10.16 -5.08 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 6 MISO))
    (pad 21 thru_hole circle (at -10.16 -2.54 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 5 MOSI))
    (pad 22 thru_hole circle (at -10.16 0 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 4 NSS))
    (pad 23 thru_hole circle (at -10.16 2.54 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 24 thru_hole circle (at -10.16 5.08 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 25 thru_hole circle (at -10.16 7.62 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
    (pad 26 thru_hole circle (at -10.16 10.16 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS)
      (net 3 +3V3))
    (pad 27 thru_hole circle (at -10.16 12.7 180) (size 1.8 1.8) (drill 1.5) (layers *.Cu *.Mask B.SilkS))
  )
  (module lib:SMA_EDGE (layer F.Cu) (tedit 5A23202E)
    (at 106.68 60.8203)
    (fp_text reference J1 (at 7.62 0.1397) (layer F.SilkS) hide)
    (fp_text value Conn_Coaxial (at -0.635 2.0447 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -4.064 -1.7653) (size 5.08 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.064 -1.7653) (size 5.08 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -1.7653) (size 1.27 3.5) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -4.064 -1.7653) (size 5.08 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.064 -1.7653) (size 5.08 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -1.7653) (size 1.27 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (module lib:RFM95 (layer B.Cu) (tedit 5A42B2A8)
    (at 106.045 71.12 90)
    (fp_text reference U2 (at 3.175 -9.144 90) (layer B.SilkS) hide)
    (fp_text value RFM95 (at 1.905 -3.175) (layer B.Fab))
    (pad 16 smd rect (at 7.5 7 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 9 FSKTimeOut))
    (pad 15 smd rect (at 7.5 5 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 RxTimeOut))
    (pad 14 smd rect (at 7.5 3 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 11 TxRxDONE))
    (pad 13 smd rect (at 7.5 1 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 12 smd rect (at 7.5 -1 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 7.5 -3 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 7.5 -5 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 7.5 -7 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 8 smd rect (at -7.5 -7 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -7.5 -5 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -7.5 -3 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 RST))
    (pad 5 smd rect (at -7.5 -1 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 4 NSS))
    (pad 4 smd rect (at -7.5 1 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 SCK))
    (pad 3 smd rect (at -7.5 3 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 MOSI))
    (pad 2 smd rect (at -7.5 5 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 MISO))
    (pad 1 smd rect (at -7.5 7 90) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 105.41 77.089)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J2 (at -2.413 0) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 12 "Net-(J2-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 105.3465 74.422)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J3 (at -2.413 0) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 10 RxTimeOut))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 108.585 77.089)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J4 (at 2.286 0) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 13 "Net-(J4-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 108.585 74.422)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference J5 (at 2.413 -0.0635) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 9 FSKTimeOut))
  )
  (gr_line (start 93.599 84.963) (end 93.599 57.0865) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.999 84.963) (end 93.599 84.963) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.999 57.0865) (end 118.999 84.963) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.599 57.0865) (end 118.999 57.0865) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.9165 57.4675) (xy 118.364 57.531) (xy 118.4275 83.947) (xy 93.9165 83.947)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.9165 57.404) (xy 118.364 57.5945) (xy 118.364 83.947) (xy 93.9165 83.947)
      )
    )
  )
)
