(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "D:/Documents/KiCAD/NIST Lightboard/Fabrication/")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "unconnected-(J1-Pad3)")
  (net 4 "unconnected-(J1-Pad4)")
  (net 5 "unconnected-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "unconnected-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "unconnected-(J1-Pad11)")
  (net 12 "Net-(J1-Pad12)")
  (net 13 "unconnected-(J1-Pad13)")
  (net 14 "unconnected-(J1-Pad14)")
  (net 15 "unconnected-(J1-Pad15)")
  (net 16 "Net-(J1-Pad16)")
  (net 17 "unconnected-(J1-Pad17)")
  (net 18 "Net-(J1-Pad18)")
  (net 19 "unconnected-(J1-Pad19)")
  (net 20 "unconnected-(J1-Pad20)")
  (net 21 "unconnected-(J1-Pad21)")
  (net 22 "Net-(J1-Pad22)")
  (net 23 "unconnected-(J1-Pad23)")
  (net 24 "Net-(J1-Pad24)")
  (net 25 "unconnected-(J1-Pad25)")
  (net 26 "Net-(J1-Pad26)")
  (net 27 "Net-(J3-Pad1)")
  (net 28 "Net-(J3-Pad2)")
  (net 29 "Net-(J3-Pad3)")
  (net 30 "Net-(J3-Pad4)")
  (net 31 "Net-(J3-Pad5)")
  (net 32 "Net-(J3-Pad6)")
  (net 33 "Net-(J3-Pad7)")
  (net 34 "Net-(J3-Pad8)")
  (net 35 "Net-(J4-Pad1)")
  (net 36 "Net-(J4-Pad3)")
  (net 37 "Net-(Q1-Pad2)")
  (net 38 "Net-(Q2-Pad2)")
  (net 39 "Net-(Q3-Pad2)")
  (net 40 "Net-(Q4-Pad2)")
  (net 41 "Net-(Q5-Pad2)")
  (net 42 "Net-(Q6-Pad2)")
  (net 43 "Net-(Q7-Pad2)")
  (net 44 "Net-(Q8-Pad2)")
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 55 138.75)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers F&B.Cu *.Mask))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420)
    (at 57.95 131.775 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77 90) (layer "F.SilkS"))
    (fp_text value "SEL RTU" (at 0 5.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 148.2 49.5)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers F&B.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 68.82 110.814284)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1000" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad22)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(Q6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 68.82 105.342856)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1000" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad18)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(Q5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 68.82 116.285712)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1000" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad24)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(Q7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 68.82 94.4)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1000" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(Q3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420)
    (at 144.025 51.975)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "Relay Pins" (at 0 20.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ThroughHoleProjects:NPN_Transistor" (layer "F.Cu")
    (tedit 0)
    (at 106.2 63.55)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=LSSGP072.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/2N3904/2N3904CS-ND/4806876")
    (property "Description" "TRANS NPN 40V TO-92")
    (property "Digi-Key_PN" "2N3904CS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "2N3904")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q2" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "E" (at 5.08 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "C" (at 5.08 2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "B" (at 5.08 0 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(Q2-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "E") (pintype "passive"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420)
    (at 128.85 124.025 -90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.77 90) (layer "F.SilkS"))
    (fp_text value "5V Power" (at 0 5.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J4-Pad3)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 56.6 50.8)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_Pad" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429)
    (at 132.3 104.91)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "GND_VCC_JD-VCC" (at 0 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J4-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ThroughHoleProjects:NPN_Transistor" (layer "F.Cu")
    (tedit 0)
    (at 106.2 51.3)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=LSSGP072.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/2N3904/2N3904CS-ND/4806876")
    (property "Description" "TRANS NPN 40V TO-92")
    (property "Digi-Key_PN" "2N3904CS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "2N3904")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q1" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "E" (at 5.08 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "B" (at 5.08 0 unlocked) (layer "F.SilkS"))
    (fp_text user "C" (at 5.08 2.54 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad1)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(Q1-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "E") (pintype "passive"))
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 146.65 138.3)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers F&B.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 68.82 88.928572)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1000" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(Q2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 68.82 121.757144)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R8" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1000" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad26)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(Q8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ThroughHoleProjects:NPN_Transistor" (layer "F.Cu")
    (tedit 0)
    (at 106.2 100.3)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=LSSGP072.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/2N3904/2N3904CS-ND/4806876")
    (property "Description" "TRANS NPN 40V TO-92")
    (property "Digi-Key_PN" "2N3904CS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "2N3904")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q5" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "B" (at 5.08 0 unlocked) (layer "F.SilkS"))
    (fp_text user "E" (at 5.08 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "C" (at 5.08 2.54 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad5)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 "Net-(Q5-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "E") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 68.82 99.871428)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1000" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(Q4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x13_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A430)
    (at 61.04 85.4)
    (descr "Through hole straight socket strip, 2x13, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x13 2.54mm double row")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -1.27 -2.77) (layer "F.SilkS"))
    (fp_text value "RPi Ribbon Connector" (at -5.59 16.85 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -1.27 15.24 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "unconnected-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "unconnected-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "unconnected-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(J1-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J1-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J1-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "unconnected-(J1-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at -2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J1-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at -2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J1-Pad19)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at -2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(J1-Pad20)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J1-Pad21)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at -2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad22)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J1-Pad23)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at -2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad24)") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(J1-Pad25)") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at -2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad26)") (pinfunction "Pin_26") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x13_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ThroughHoleProjects:NPN_Transistor" (layer "F.Cu")
    (tedit 0)
    (at 106.2 75.8)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=LSSGP072.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/2N3904/2N3904CS-ND/4806876")
    (property "Description" "TRANS NPN 40V TO-92")
    (property "Digi-Key_PN" "2N3904CS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "2N3904")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q3" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "B" (at 5.08 0 unlocked) (layer "F.SilkS"))
    (fp_text user "E" (at 5.08 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "C" (at 5.08 2.54 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad3)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(Q3-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "E") (pintype "passive"))
  )
  (footprint "ThroughHoleProjects:NPN_Transistor" (layer "F.Cu")
    (tedit 0)
    (at 106.2 137.05)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=LSSGP072.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/2N3904/2N3904CS-ND/4806876")
    (property "Description" "TRANS NPN 40V TO-92")
    (property "Digi-Key_PN" "2N3904CS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "2N3904")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q8" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "B" (at 5.08 0 unlocked) (layer "F.SilkS"))
    (fp_text user "C" (at 5.08 2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "E" (at 5.08 -2.54 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad8)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(Q8-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "E") (pintype "passive"))
  )
  (footprint "ThroughHoleProjects:NPN_Transistor" (layer "F.Cu")
    (tedit 0)
    (at 106.2 88.05)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=LSSGP072.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/2N3904/2N3904CS-ND/4806876")
    (property "Description" "TRANS NPN 40V TO-92")
    (property "Digi-Key_PN" "2N3904CS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "2N3904")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q4" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "E" (at 5.08 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "B" (at 5.08 0 unlocked) (layer "F.SilkS"))
    (fp_text user "C" (at 5.08 2.54 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad4)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 "Net-(Q4-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "E") (pintype "passive"))
  )
  (footprint "ThroughHoleProjects:NPN_Transistor" (layer "F.Cu")
    (tedit 0)
    (at 106.2 124.8)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=LSSGP072.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/2N3904/2N3904CS-ND/4806876")
    (property "Description" "TRANS NPN 40V TO-92")
    (property "Digi-Key_PN" "2N3904CS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "2N3904")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q7" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "B" (at 5.08 0 unlocked) (layer "F.SilkS"))
    (fp_text user "E" (at 5.08 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "C" (at 5.08 2.54 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad7)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 "Net-(Q7-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "E") (pintype "passive"))
  )
  (footprint "ThroughHoleProjects:NPN_Transistor" (layer "F.Cu")
    (tedit 0)
    (at 106.2 112.55)
    (property "Category" "Discrete Semiconductor Products")
    (property "DK_Datasheet_Link" "https://my.centralsemi.com/get_document.php?cmp=1&mergetype=pd&mergepath=pd&pdf_id=LSSGP072.PDF")
    (property "DK_Detail_Page" "/product-detail/en/central-semiconductor-corp/2N3904/2N3904CS-ND/4806876")
    (property "Description" "TRANS NPN 40V TO-92")
    (property "Digi-Key_PN" "2N3904CS-ND")
    (property "Family" "Transistors - Bipolar (BJT) - Single")
    (property "MPN" "2N3904")
    (property "Manufacturer" "Central Semiconductor Corp")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (attr through_hole)
    (fp_text reference "Q6" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "C" (at 5.08 2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "B" (at 5.08 0 unlocked) (layer "F.SilkS"))
    (fp_text user "E" (at 5.08 -2.54 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad6)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 "Net-(Q6-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "E") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 68.82 83.457144)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "johwiltb-lightboard.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "1000" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(Q1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 151.3 46.25) (end 51.45 142) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "-  +\n5V Power\n" (at 127.65 128.575) (layer "F.SilkS"))
  (gr_text "NCCoE Lightboard\nJWLB Utility" (at 68.7 63.75) (layer "F.SilkS"))
  (gr_text "Relay Pins" (at 147.875 61.605 90) (layer "F.SilkS"))
  (gr_text "RPi \nConnector" (at 59.85 79.3) (layer "F.SilkS"))
  (gr_text "RTU\n" (at 60.65 127.175) (layer "F.SilkS"))
  (gr_text "GND\nVCC\nJD-VCC" (at 135.275 107.735) (layer "F.SilkS"))
)
