<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="16.256" y2="0" width="0" layer="20"/>
<wire x1="16.256" y1="0" x2="16.256" y2="13.462" width="0" layer="20"/>
<wire x1="16.256" y1="13.462" x2="0" y2="13.462" width="0" layer="20"/>
<wire x1="0" y1="13.462" x2="0" y2="0" width="0" layer="20"/>
<text>KVM Controller
(c) K. C. Lee
CC BY 4.0</text>
</plain>
<libraries>
<library name="Misc Processor">
<packages>
<package name="TSSOP20">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ipc-7351-capacitor">
<description>&lt;b&gt;IPC-7351 compliant SMT capacitors&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft rcl.lbr&lt;br&gt;
Packages generated using genpkg_chp.ulp, genpkg_cae.ulp and genpkg_mld.ulp&lt;br&gt;
Devices are Vishay chip types, generic AEC types and Kemet T491 series molded body types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="CAPC1608X92N">
</package>
</packages>
</library>
<library name="ipc-7351-resistor">
<description>&lt;b&gt;IPC-7351 compliant SMT resistors&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Symbols copied from CadSoft rcl.lbr.&lt;br&gt;
Packages generated using genpkg_chp.ulp.&lt;br&gt;
Devices are Panasonic ERJ series types.&lt;br&gt;
&lt;br&gt;
Weartronics 2006&lt;br&gt;
http://www.weartronics.com/</description>
<packages>
<package name="RESC1608X55N">
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Misc Conn">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Misc Processor" package="TSSOP20" value="STM8SX03F3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="ipc-7351-capacitor" package="CAPC1608X92N" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="ipc-7351-capacitor" package="CAPC1608X92N" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="ipc-7351-capacitor" package="CAPC1608X92N" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="ipc-7351-resistor" package="RESC1608X55N" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="ipc-7351-resistor" package="RESC1608X55N" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CLK" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="DAT" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="GND1" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="H_S1" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="H_S2" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="H_SW" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U_IN1" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U_IN2" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="GND2" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="3V3" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="GND4" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J1" library="Misc Conn" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="GND1" pad="1"/>
<contactref element="GND2" pad="1"/>
<contactref element="GND4" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="8"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="!RST">
<contactref element="U1" pad="4"/>
<contactref element="C4" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SWIM">
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="PS/2_CLK">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="12"/>
<contactref element="CLK" pad="1"/>
</signal>
<signal name="PS/2_DATA">
<contactref element="U1" pad="11"/>
<contactref element="R2" pad="1"/>
<contactref element="DAT" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="17"/>
<contactref element="U_IN2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="16"/>
<contactref element="U_IN1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="15"/>
<contactref element="H_SW" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="13"/>
<contactref element="H_S1" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="14"/>
<contactref element="H_S2" pad="1"/>
</signal>
<signal name="+3.3V">
<contactref element="U1" pad="9"/>
<contactref element="C3" pad="2"/>
<contactref element="3V3" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
