(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 4.69)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user "bonding pads (Si)")
		(41 "User.2" user "cathode strips (Si)")
		(43 "User.3" user "active area (Si)")
		(45 "User.4" user "wirebonds (Si)")
		(47 "User.5" user "handle wafer (Si)")
		(49 "User.6" user "active die (Si)")
		(51 "User.7" user "cathode strips (InGaAs)")
		(53 "User.8" user "bonding pads (InGaAs)")
		(55 "User.9" user "wirebonds (InGaAs)")
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 4.6)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0762)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 127 124.5)
		(pcbplotparams
			(layerselection 0x00000000_00000000_5557f5d5_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(gr_circle
		(center 105.787 124.5)
		(end 108.812 124.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 148.213 124.5)
		(end 151.238 124.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 112 92.5)
		(end 113.5 92.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 142 108.5)
		(end 143.5 108.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 117.5 123.5)
		(end 121.5 125.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 112 156.5)
		(end 113.5 156.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 142 92.5)
		(end 143.5 92.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_poly
		(pts
			(xy 155.5 89) (xy 98.5 89) (xy 98.5 114) (xy 103.5 114) (xy 103.5 119) (xy 98.5 119) (xy 98.5 130)
			(xy 103.5 130) (xy 103.5 135) (xy 98.5 135) (xy 98.5 160) (xy 117.5 160) (xy 117.5 155) (xy 136.5 155)
			(xy 136.5 160) (xy 155.5 160) (xy 155.5 135) (xy 150.5 135) (xy 150.5 130) (xy 155.5 130) (xy 155.5 119)
			(xy 150.5 119) (xy 150.5 114) (xy 155.5 114)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 112 108.5)
		(end 113.5 108.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 107.75 97.375)
		(end 146.25 103.625)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 112 140.5)
		(end 113.5 140.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 107.75 113.375)
		(end 146.25 119.625)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 132.5 123.5)
		(end 136.5 125.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 112 124.5)
		(end 113.5 124.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 142 140.5)
		(end 143.5 140.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 142 156.5)
		(end 143.5 156.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 142 124.5)
		(end 143.5 124.5)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 107.75 129.375)
		(end 146.25 135.625)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 107.75 145.375)
		(end 146.25 151.625)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "XRAY->"
		(at 127 84.5 270)
		(layer "Cmts.User")
	)
	(embedded_fonts no)
)
