<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<text>8</text>
<text>GND</text>
<text>648.ken@gmail.com</text>
<text>Lapel Rev. 2
Jan. 2014</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>VCC</text>
<text>9</text>
<text>10</text>
<wire x1="53.9115" y1="36.2585" x2="53.467" y2="33.782" width="0" layer="20" curve="-100"/>
<wire x1="51.6255" y1="31.6865" x2="53.467" y2="33.782" width="0" layer="20" curve="-57.578935"/>
<wire x1="58.293" y1="18.161" x2="60.2615" y2="16.8275" width="0" layer="20" curve="-100"/>
<wire x1="58.293" y1="18.161" x2="55.626" y2="19.05" width="0" layer="20" curve="-64.942385"/>
<wire x1="55.626" y1="19.05" x2="51.6255" y2="31.6865" width="0" layer="20" curve="-50"/>
<wire x1="53.9115" y1="36.2585" x2="53.721" y2="38.862" width="0" layer="20" curve="-56.67205"/>
<wire x1="53.721" y1="38.862" x2="64.643" y2="46.99" width="0" layer="20" curve="-49.059519"/>
<wire x1="64.643" y1="46.99" x2="66.9925" y2="46.2915" width="0" layer="20" curve="-57.038229"/>
<wire x1="69.469" y1="46.355" x2="71.755" y2="47.117" width="0" layer="20" curve="-53.130102"/>
<wire x1="69.469" y1="46.355" x2="66.9925" y2="46.2915" width="0" layer="20" curve="-122.261011"/>
<wire x1="71.755" y1="47.117" x2="83.312" y2="39.1795" width="0" layer="20" curve="-50"/>
<wire x1="83.312" y1="39.1795" x2="82.931" y2="36.576" width="0" layer="20" curve="-54"/>
<wire x1="83.693" y1="34.163" x2="82.931" y2="36.576" width="0" layer="20" curve="-124.695154"/>
<wire x1="83.693" y1="34.163" x2="85.852" y2="32.258" width="0" layer="20" curve="-73.285543"/>
<wire x1="85.852" y1="32.258" x2="81.407" y2="18.796" width="0" layer="20" curve="-48.865581"/>
<wire x1="81.407" y1="18.796" x2="78.613" y2="18.288" width="0" layer="20" curve="-70"/>
<wire x1="76.835" y1="16.891" x2="78.613" y2="18.288" width="0" layer="20" curve="-104.302889"/>
<wire x1="76.835" y1="16.891" x2="75.6285" y2="14.4145" width="0" layer="20" curve="-60"/>
<wire x1="75.6285" y1="14.4145" x2="61.9125" y2="14.2875" width="0" layer="20" curve="-48"/>
<wire x1="61.9125" y1="14.2875" x2="60.2615" y2="16.8275" width="0" layer="20" curve="-76.741983"/>
<text>ON</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>GND</text>
<text>8</text>
<text>9</text>
<text>GND</text>
<text>10</text>
<text>GND</text>
<text>VCC</text>
<text>Attiny84</text>
<text>+ ISP -</text>
<hole x="61.722" y="20.5105" drill="2"/>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
<text>*</text>
</plain>
<libraries>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun_mod">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS_REV">
</package>
<package name="BATTCON_20MM_4LEGS">
</package>
</packages>
</library>
<library name="_my-parts">
<packages>
<package name="SWITCH_BOTTOM">
</package>
</packages>
</library>
<library name="adafruit_mod">
<packages>
<package name="SEWINGTAP_0.5M">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SEWINGTAP_0.5OCT">
</package>
<package name="SEWINGTAP_0.5SQR">
</package>
</packages>
</library>
<library name="_my-parts_level22">
<packages>
<package name="CT_FLOWER_22_16_INCH">
</package>
<package name="CHICHTECH_22_03X08">
</package>
<package name="CHICKTECH_21_04_INCH">
</package>
<package name="CT_FLOWER_21_16_PAR">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="_my-parts" package="SWITCH_BOTTOM" value="SWITCHBOTTOM"/>
<element name="IC1" library="avr-7" package="SOIC14" value="TINY24/44/84-SSU">
<attribute name="VALUE"/>
</element>
<element name="D6" library="adafruit_mod" package="SEWINGTAP_0.5M" value="SEWTAP"/>
<element name="D5" library="adafruit_mod" package="SEWINGTAP_0.5M" value="SEWTAP"/>
<element name="D4" library="adafruit_mod" package="SEWINGTAP_0.5M" value="SEWTAP"/>
<element name="D3" library="adafruit_mod" package="SEWINGTAP_0.5M" value="SEWTAP"/>
<element name="D7" library="adafruit_mod" package="SEWINGTAP_0.5M" value="SEWTAP"/>
<element name="D8" library="adafruit_mod" package="SEWINGTAP_0.5M" value="SEWTAP"/>
<element name="D9" library="adafruit_mod" package="SEWINGTAP_0.5M" value="SEWTAP"/>
<element name="D10" library="adafruit_mod" package="SEWINGTAP_0.5M" value="SEWTAP"/>
<element name="ISP" library="SparkFun_mod" package="2X3-NS_REV" value="AVR_SPI_PRG_6BACKSIDE">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="_my-parts_level22" package="CT_FLOWER_22_16_INCH" value=""/>
<element name="U$3" library="_my-parts_level22" package="CHICHTECH_22_03X08" value=""/>
<element name="U$4" library="_my-parts_level22" package="CHICKTECH_21_04_INCH" value=""/>
<element name="U$5" library="_my-parts_level22" package="CT_FLOWER_21_16_PAR" value=""/>
<element name="BAT1" library="SparkFun_mod" package="BATTCON_20MM_4LEGS" value=""/>
<element name="C1" library="adafruit_mod" package="C1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="adafruit_mod" package="CHIPLED_1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit_mod" package="R1206" value="">
<attribute name="VALUE"/>
</element>
<element name="TP1" library="adafruit_mod" package="SEWINGTAP_0.5OCT" value="SEWTAPSEWINGTAP_0.5OCT"/>
<element name="TP2" library="adafruit_mod" package="SEWINGTAP_0.5OCT" value="SEWTAPSEWINGTAP_0.5OCT"/>
<element name="TP3" library="adafruit_mod" package="SEWINGTAP_0.5OCT" value="SEWTAPSEWINGTAP_0.5OCT"/>
<element name="TP4" library="adafruit_mod" package="SEWINGTAP_0.5OCT" value="SEWTAPSEWINGTAP_0.5OCT"/>
<element name="TP5" library="adafruit_mod" package="SEWINGTAP_0.5SQR" value="SEWTAPSEWINGTAP_0.5SQR"/>
</elements>
<signals>
<signal name="PB4">
<contactref element="IC1" pad="10"/>
<contactref element="D7" pad="TAP"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="U$2" pad="3"/>
<contactref element="ISP" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="TP5" pad="TAP"/>
</signal>
<signal name="N$3">
</signal>
<signal name="GND1">
</signal>
<signal name="SCK">
<contactref element="IC1" pad="9"/>
<contactref element="D6" pad="TAP"/>
<contactref element="ISP" pad="3"/>
</signal>
<signal name="N$1">
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="7"/>
<contactref element="D4" pad="TAP"/>
<contactref element="ISP" pad="4"/>
</signal>
<signal name="N$8">
</signal>
<signal name="MISO">
<contactref element="IC1" pad="8"/>
<contactref element="D5" pad="TAP"/>
<contactref element="ISP" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="11"/>
<contactref element="D8" pad="TAP"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="12"/>
<contactref element="D9" pad="TAP"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="2"/>
<contactref element="BAT1" pad="3"/>
<contactref element="BAT1" pad="P$5"/>
<contactref element="BAT1" pad="P$1"/>
<contactref element="BAT1" pad="P$6"/>
<contactref element="BAT1" pad="1"/>
<contactref element="BAT1" pad="P$3"/>
<contactref element="BAT1" pad="P$2"/>
<contactref element="BAT1" pad="P$4"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="4"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="6"/>
<contactref element="D3" pad="TAP"/>
</signal>
<signal name="GND_1">
<contactref element="IC1" pad="14"/>
<contactref element="ISP" pad="6"/>
<contactref element="BAT1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="TP1" pad="TAP"/>
<contactref element="TP2" pad="TAP"/>
<contactref element="TP3" pad="TAP"/>
<contactref element="TP4" pad="TAP"/>
</signal>
<signal name="N$18">
<contactref element="IC1" pad="13"/>
<contactref element="D10" pad="TAP"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
