(kicad_pcb (version 4) (host pcbnew 4.0.0-rc1-stable)
  (general
    (links 0)
    (no_connects 0)
    (area -6.806001 -15.569001 42.620001 15.569001)
    (thickness 1.6)
    (drawings 43)
    (tracks 184)
    (zones 0)
    (modules 5)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.1524)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P1-Pad4)")
  (net 5 "Net-(P1-Pad6)")
  (net 6 "Net-(P1-Pad7)")
  (net 7 "Net-(P1-Pad8)")
  (net 8 "Net-(P1-Pad9)")
  (net 9 "Net-(P1-Pad10)")
  (net 10 "Net-(P1-Pad11)")
  (net 11 "Net-(P1-Pad12)")
  (net 12 "Net-(P1-Pad13)")
  (net 13 "Net-(P1-Pad14)")
  (net 14 "Net-(P2-Pad1)")
  (net 15 "Net-(P2-Pad2)")
  (net 16 "Net-(P2-Pad3)")
  (net 17 "Net-(P2-Pad4)")
  (net 18 "Net-(P2-Pad5)")
  (net 19 "Net-(P2-Pad6)")
  (net 20 "Net-(P2-Pad7)")
  (net 21 "Net-(P2-Pad8)")
  (net 22 "Net-(P2-Pad9)")
  (net 23 "Net-(P2-Pad10)")
  (net 24 "Net-(P2-Pad11)")
  (net 25 "Net-(P2-Pad12)")
  (net 26 "Net-(P2-Pad13)")
  (net 27 "Net-(P2-Pad14)")
  (net 28 "Net-(P1-Pad15)")
  (net 29 "Net-(P1-Pad16)")
  (net 30 "Net-(P1-Pad17)")
  (net 31 "Net-(P1-Pad18)")
  (net 32 "Net-(P2-Pad15)")
  (net 33 "Net-(P2-Pad16)")
  (net 34 "Net-(P2-Pad17)")
  (net 35 "Net-(P2-Pad18)")
  (net 36 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad17)")
    (add_net "Net-(P1-Pad18)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad11)")
    (add_net "Net-(P2-Pad12)")
    (add_net "Net-(P2-Pad13)")
    (add_net "Net-(P2-Pad14)")
    (add_net "Net-(P2-Pad15)")
    (add_net "Net-(P2-Pad16)")
    (add_net "Net-(P2-Pad17)")
    (add_net "Net-(P2-Pad18)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P2-Pad9)")
  )
  (module .pretty:ESP3212 (layer F.Cu) (tedit 57CF1864)
    (at 0 0 270)
    (fp_text reference U1 (at -11.557 9.017 270) (layer F.SilkS))
    (fp_text value ESP3212 (at 5.715 14.224 270) (layer F.Fab))
    (fp_text user "ESP3212 - adamjvr " (at -6.604 -2.54 360) (layer F.SilkS))
    (pad 1 smd oval (at -9 5.25 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 2 smd oval (at -9 3.98 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(P1-Pad18)"))
    (pad 3 smd oval (at -9 2.71 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(P1-Pad17)"))
    (pad 4 smd oval (at -9 1.44 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P1-Pad16)"))
    (pad 5 smd oval (at -9 0.17 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P1-Pad15)"))
    (pad 6 smd oval (at -9 -1.1 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P1-Pad14)"))
    (pad 7 smd oval (at -9 -2.37 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P1-Pad13)"))
    (pad 8 smd oval (at -9 -3.64 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P1-Pad12)"))
    (pad 9 smd oval (at -9 -4.91 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P1-Pad11)"))
    (pad 10 smd oval (at -9 -6.18 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P1-Pad10)"))
    (pad 11 smd oval (at -9 -7.45 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad9)"))
    (pad 12 smd oval (at -9 -8.72 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad8)"))
    (pad 13 smd oval (at -9 -9.99 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad7)"))
    (pad 14 smd oval (at -9 -11.26 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad6)"))
    (pad 15 smd oval (at -5.715 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 16 smd oval (at -4.445 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (pad 17 smd oval (at -3.175 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 18 smd oval (at -1.905 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 19 smd oval (at -0.635 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 20 smd oval (at 0.635 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P2-Pad1)"))
    (pad 21 smd oval (at 1.905 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P2-Pad2)"))
    (pad 22 smd oval (at 3.175 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P2-Pad3)"))
    (pad 23 smd oval (at 4.445 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P2-Pad4)"))
    (pad 24 smd oval (at 5.715 -12.75 270) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P2-Pad5)"))
    (pad 25 smd oval (at 9 -11.26 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P2-Pad6)"))
    (pad 26 smd oval (at 9 -9.99 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P2-Pad7)"))
    (pad 27 smd oval (at 9 -8.72 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P2-Pad8)"))
    (pad 28 smd oval (at 9 -7.45 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P2-Pad9)"))
    (pad 29 smd oval (at 9 -6.18 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P2-Pad10)"))
    (pad 30 smd oval (at 9 -4.91 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P2-Pad11)"))
    (pad 31 smd oval (at 9 -3.64 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(P2-Pad12)"))
    (pad 32 smd oval (at 9 -2.37 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P2-Pad13)"))
    (pad 33 smd oval (at 9 -1.1 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P2-Pad14)"))
    (pad 34 smd oval (at 9 0.17 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(P2-Pad15)"))
    (pad 35 smd oval (at 9 1.44 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(P2-Pad16)"))
    (pad 36 smd oval (at 9 2.71 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(P2-Pad17)"))
    (pad 37 smd oval (at 9 3.98 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(P2-Pad18)"))
    (pad 38 smd oval (at 9 5.25 270) (size 2.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x19 (layer F.Cu) (tedit 57CF092A)
    (at 40.64 -13.97 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X19 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P1-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P1-Pad16)"))
    (pad 17 thru_hole oval (at 0 40.64 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P1-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(P1-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x19.wrl
      (at (xyz 0 -0.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x19 (layer F.Cu) (tedit 57CF0924)
    (at 40.64 13.97 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X19 (at 0 -3.556 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P2-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P2-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P2-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P2-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P2-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P2-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P2-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(P2-Pad16)"))
    (pad 17 thru_hole oval (at 0 40.64 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P2-Pad17)"))
    (pad 18 thru_hole oval (at 0 43.18 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P2-Pad18)"))
    (pad 19 thru_hole oval (at 0 45.72 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x19.wrl
      (at (xyz 0 -0.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module .pretty:chi_logo (layer B.Cu) (tedit 57150158)
    (at 4.064 -0.508)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
    (fp_text user "Made In Chicago" (at 2.6162 -3.4) (layer B.Mask))
    (fp_text user AndrewSowa.com (at -2.9718 3.4) (layer B.Mask))
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 57CF18A2)
    (at 35.052 0 90)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 90) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 90) (layer F.Fab))
  )
  (gr_text "ESP-32 Breakout\nBETA\n" (at 39.624 0 90) (layer B.SilkS))
  (gr_text 32 (at 10.16 11.684 90) (layer F.SilkS))
  (gr_text 33 (at 7.62 11.684 90) (layer F.SilkS))
  (gr_text 34 (at 5.08 11.684 90) (layer F.SilkS))
  (gr_text 35 (at 2.54 11.684 90) (layer F.SilkS))
  (gr_text 36 (at 0 11.684 90) (layer F.SilkS))
  (gr_text 37 (at -2.54 11.684 90) (layer F.SilkS))
  (gr_text 20 (at 40.64 11.176 90) (layer F.SilkS))
  (gr_text 21 (at 38.1 11.176 90) (layer F.SilkS))
  (gr_text 22 (at 35.56 11.176 90) (layer F.SilkS))
  (gr_text 23 (at 33.02 11.176 90) (layer F.SilkS))
  (gr_text 24 (at 30.48 11.176 90) (layer F.SilkS))
  (gr_text 25 (at 27.94 11.176 90) (layer F.SilkS))
  (gr_text 26 (at 25.4 11.176 90) (layer F.SilkS))
  (gr_text 27 (at 22.86 11.176 90) (layer F.SilkS))
  (gr_text 28 (at 20.32 11.176 90) (layer F.SilkS))
  (gr_text 29 (at 17.78 11.176 90) (layer F.SilkS))
  (gr_text 30 (at 15.24 11.176 90) (layer F.SilkS))
  (gr_text 31 (at 12.7 11.176 90) (layer F.SilkS))
  (gr_text 38 (at -5.08 11.684 90) (layer F.SilkS))
  (gr_text 19 (at 40.64 -11.176 90) (layer F.SilkS))
  (gr_text 18 (at 38.1 -11.176 90) (layer F.SilkS))
  (gr_text 17 (at 35.56 -11.176 90) (layer F.SilkS))
  (gr_text 16 (at 33.02 -11.176 90) (layer F.SilkS))
  (gr_text 15 (at 30.48 -11.176 90) (layer F.SilkS))
  (gr_text 14 (at 27.94 -11.176 90) (layer F.SilkS))
  (gr_text 13 (at 25.4 -11.176 90) (layer F.SilkS))
  (gr_text 12 (at 22.86 -11.176 90) (layer F.SilkS))
  (gr_text 11 (at 20.32 -11.176 90) (layer F.SilkS))
  (gr_text 10 (at 17.78 -11.176 90) (layer F.SilkS))
  (gr_text 9 (at 15.24 -11.684 90) (layer F.SilkS))
  (gr_text 8 (at 12.7 -11.684 90) (layer F.SilkS))
  (gr_text 7 (at 10.16 -11.684 90) (layer F.SilkS))
  (gr_text 6 (at 7.62 -11.684 90) (layer F.SilkS))
  (gr_text 5 (at 5.08 -11.684 90) (layer F.SilkS))
  (gr_text 4 (at 2.54 -11.684 90) (layer F.SilkS))
  (gr_text 3 (at 0 -11.684 90) (layer F.SilkS))
  (gr_text 2 (at -2.54 -11.684 90) (layer F.SilkS))
  (gr_text 1 (at -5.08 -11.684 90) (layer F.SilkS))
  (gr_line (start 42.545 -15.494) (end -6.731 -15.494) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 42.545 15.494) (end 42.545 -15.494) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -6.731 15.494) (end 42.545 15.494) (layer Edge.Cuts) (width 0.15))
  (gr_line (start -6.731 -15.494) (end -6.731 15.494) (layer Edge.Cuts) (width 0.15))
  (zone (net 36) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -7.112 -15.748) (xy 42.672 -15.748) (xy 42.672 15.748) (xy -7.112 15.748)
      )
    )
  )
)
