(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 44)
    (no_connects 0)
    (area 148.0511 48.9744 217.471601 109.67)
    (thickness 1.6)
    (drawings 16)
    (tracks 96)
    (zones 0)
    (modules 20)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.381)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(LED1-Pad2)")
  (net 2 "Net-(LED2-Pad2)")
  (net 3 "Net-(LED3-Pad2)")
  (net 4 "Net-(OptoLEDShield1-PadAD5)")
  (net 5 "Net-(OptoLEDShield1-PadAD4)")
  (net 6 "Net-(OptoLEDShield1-PadAD3)")
  (net 7 "Net-(OptoLEDShield1-PadAD0)")
  (net 8 "Net-(OptoLEDShield1-PadAD1)")
  (net 9 "Net-(OptoLEDShield1-PadAD2)")
  (net 10 GND)
  (net 11 "Net-(OptoLEDShield1-Pad3V3)")
  (net 12 "Net-(OptoLEDShield1-PadRST)")
  (net 13 "Net-(OptoLEDShield1-Pad0)")
  (net 14 "Net-(OptoLEDShield1-Pad1)")
  (net 15 "Net-(OptoLEDShield1-Pad2)")
  (net 16 "Net-(OptoLEDShield1-Pad3)")
  (net 17 "Net-(OptoLEDShield1-Pad4)")
  (net 18 "Net-(OptoLEDShield1-Pad5)")
  (net 19 "Net-(OptoLEDShield1-Pad6)")
  (net 20 "Net-(OptoLEDShield1-Pad7)")
  (net 21 "Net-(OptoLEDShield1-Pad8)")
  (net 22 "Net-(OptoLEDShield1-Pad9)")
  (net 23 "Net-(OptoLEDShield1-Pad10)")
  (net 24 "Net-(OptoLEDShield1-Pad11)")
  (net 25 "Net-(OptoLEDShield1-Pad12)")
  (net 26 "Net-(OptoLEDShield1-Pad13)")
  (net 27 "Net-(OptoLEDShield1-PadGND3)")
  (net 28 "Net-(OptoLEDShield1-PadAREF)")
  (net 29 +5V)
  (net 30 "Net-(OptoLEDShield1-PadSDA)")
  (net 31 "Net-(OptoLEDShield1-PadSCL)")
  (net 32 "Net-(OptoLEDShield1-PadIO_R)")
  (net 33 "Net-(OptoLEDShield1-PadNC)")
  (net 34 "Net-(OptoLEDShield1-PadSP1)")
  (net 35 "Net-(OptoLEDShield1-PadSP2)")
  (net 36 "Net-(OptoLEDShield1-PadSP3)")
  (net 37 "Net-(OptoLEDShield1-PadSP4)")
  (net 38 "Net-(OptoLEDShield1-PadSP5)")
  (net 39 "Net-(OptoLEDShield1-PadSP6)")
  (net 40 +24V)
  (net 41 "Net-(LED5-Pad2)")
  (net 42 "Net-(LED6-Pad2)")
  (net 43 "Net-(LED7-Pad2)")
  (net 44 "Net-(OptoLEDShield1-PadV_IN)")
  (net 45 "/LED(+)1")
  (net 46 "/LED(-)1")
  (net 47 "/LED(+)2")
  (net 48 "/LED(-)2")
  (net 49 /CTRL1)
  (net 50 /CTRL2)
  (net 51 "Net-(P1-Pad6)")
  (net 52 "Net-(P2-Pad6)")
  (net 53 /REF1)
  (net 54 /REF2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +5V)
    (add_net /CTRL1)
    (add_net /CTRL2)
    (add_net "/LED(+)1")
    (add_net "/LED(+)2")
    (add_net "/LED(-)1")
    (add_net "/LED(-)2")
    (add_net /REF1)
    (add_net /REF2)
    (add_net GND)
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED2-Pad2)")
    (add_net "Net-(LED3-Pad2)")
    (add_net "Net-(LED5-Pad2)")
    (add_net "Net-(LED6-Pad2)")
    (add_net "Net-(LED7-Pad2)")
    (add_net "Net-(OptoLEDShield1-Pad0)")
    (add_net "Net-(OptoLEDShield1-Pad1)")
    (add_net "Net-(OptoLEDShield1-Pad10)")
    (add_net "Net-(OptoLEDShield1-Pad11)")
    (add_net "Net-(OptoLEDShield1-Pad12)")
    (add_net "Net-(OptoLEDShield1-Pad13)")
    (add_net "Net-(OptoLEDShield1-Pad2)")
    (add_net "Net-(OptoLEDShield1-Pad3)")
    (add_net "Net-(OptoLEDShield1-Pad3V3)")
    (add_net "Net-(OptoLEDShield1-Pad4)")
    (add_net "Net-(OptoLEDShield1-Pad5)")
    (add_net "Net-(OptoLEDShield1-Pad6)")
    (add_net "Net-(OptoLEDShield1-Pad7)")
    (add_net "Net-(OptoLEDShield1-Pad8)")
    (add_net "Net-(OptoLEDShield1-Pad9)")
    (add_net "Net-(OptoLEDShield1-PadAD0)")
    (add_net "Net-(OptoLEDShield1-PadAD1)")
    (add_net "Net-(OptoLEDShield1-PadAD2)")
    (add_net "Net-(OptoLEDShield1-PadAD3)")
    (add_net "Net-(OptoLEDShield1-PadAD4)")
    (add_net "Net-(OptoLEDShield1-PadAD5)")
    (add_net "Net-(OptoLEDShield1-PadAREF)")
    (add_net "Net-(OptoLEDShield1-PadGND3)")
    (add_net "Net-(OptoLEDShield1-PadIO_R)")
    (add_net "Net-(OptoLEDShield1-PadNC)")
    (add_net "Net-(OptoLEDShield1-PadRST)")
    (add_net "Net-(OptoLEDShield1-PadSCL)")
    (add_net "Net-(OptoLEDShield1-PadSDA)")
    (add_net "Net-(OptoLEDShield1-PadSP1)")
    (add_net "Net-(OptoLEDShield1-PadSP2)")
    (add_net "Net-(OptoLEDShield1-PadSP3)")
    (add_net "Net-(OptoLEDShield1-PadSP4)")
    (add_net "Net-(OptoLEDShield1-PadSP5)")
    (add_net "Net-(OptoLEDShield1-PadSP6)")
    (add_net "Net-(OptoLEDShield1-PadV_IN)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P2-Pad6)")
  )
  (module freetronics_footprints:ARDUINO_SHIELD locked (layer F.Cu) (tedit 5A6A4616)
    (at 148.5011 105.0036)
    (descr http://www.thingiverse.com/thing:9630)
    (fp_text reference OptoLEDShield1 (at 59.3989 -19.5036 90) (layer F.SilkS))
    (fp_text value ARDUINO_SHIELD (at 10.16 -54.61) (layer F.SilkS) hide)
    (pad AD5 thru_hole oval (at 63.5 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(OptoLEDShield1-PadAD5)"))
    (pad AD4 thru_hole oval (at 60.96 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(OptoLEDShield1-PadAD4)"))
    (pad AD3 thru_hole oval (at 58.42 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(OptoLEDShield1-PadAD3)"))
    (pad AD0 thru_hole oval (at 50.8 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(OptoLEDShield1-PadAD0)"))
    (pad AD1 thru_hole oval (at 53.34 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(OptoLEDShield1-PadAD1)"))
    (pad AD2 thru_hole oval (at 55.88 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(OptoLEDShield1-PadAD2)"))
    (pad V_IN thru_hole oval (at 45.72 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(OptoLEDShield1-PadV_IN)"))
    (pad GND2 thru_hole oval (at 43.18 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad GND1 thru_hole oval (at 40.64 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(OptoLEDShield1-Pad3V3)"))
    (pad RST thru_hole oval (at 33.02 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(OptoLEDShield1-PadRST)"))
    (pad 0 thru_hole oval (at 63.5 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(OptoLEDShield1-Pad0)"))
    (pad 1 thru_hole oval (at 60.96 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(OptoLEDShield1-Pad1)"))
    (pad 2 thru_hole oval (at 58.42 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(OptoLEDShield1-Pad2)"))
    (pad 3 thru_hole oval (at 55.88 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(OptoLEDShield1-Pad3)"))
    (pad 4 thru_hole oval (at 53.34 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(OptoLEDShield1-Pad4)"))
    (pad 5 thru_hole oval (at 50.8 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(OptoLEDShield1-Pad5)"))
    (pad 6 thru_hole oval (at 48.26 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(OptoLEDShield1-Pad6)"))
    (pad 7 thru_hole oval (at 45.72 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(OptoLEDShield1-Pad7)"))
    (pad 8 thru_hole oval (at 41.656 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(OptoLEDShield1-Pad8)"))
    (pad 9 thru_hole oval (at 39.116 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(OptoLEDShield1-Pad9)"))
    (pad 10 thru_hole oval (at 36.576 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(OptoLEDShield1-Pad10)"))
    (pad 11 thru_hole oval (at 34.036 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(OptoLEDShield1-Pad11)"))
    (pad 12 thru_hole oval (at 31.496 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(OptoLEDShield1-Pad12)"))
    (pad 13 thru_hole oval (at 28.956 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(OptoLEDShield1-Pad13)"))
    (pad GND3 thru_hole oval (at 26.416 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(OptoLEDShield1-PadGND3)"))
    (pad AREF thru_hole oval (at 23.876 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(OptoLEDShield1-PadAREF)"))
    (pad 5V thru_hole oval (at 38.1 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 +5V))
    (pad "" np_thru_hole circle (at 66.04 -7.62 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 66.04 -35.56 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 15.24 -50.8 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 13.97 -2.54 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad SDA thru_hole oval (at 21.336 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(OptoLEDShield1-PadSDA)"))
    (pad SCL thru_hole oval (at 18.796 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(OptoLEDShield1-PadSCL)"))
    (pad IO_R thru_hole oval (at 30.48 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(OptoLEDShield1-PadIO_R)"))
    (pad NC thru_hole oval (at 27.94 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(OptoLEDShield1-PadNC)"))
    (pad SP1 thru_hole circle (at 63.5 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(OptoLEDShield1-PadSP1)"))
    (pad SP2 thru_hole circle (at 66.04 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(OptoLEDShield1-PadSP2)"))
    (pad SP3 thru_hole circle (at 63.5 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(OptoLEDShield1-PadSP3)"))
    (pad SP4 thru_hole circle (at 66.04 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(OptoLEDShield1-PadSP4)"))
    (pad SP5 thru_hole circle (at 63.5 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(OptoLEDShield1-PadSP5)"))
    (pad SP6 thru_hole circle (at 66.04 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(OptoLEDShield1-PadSP6)"))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59E161E8)
    (at 172.72 60.96)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference LED1 (at 1 -4.5) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "/LED(+)1"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(LED1-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59E161EC)
    (at 180.34 60.96)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference LED2 (at 1 -4.5) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(LED1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(LED2-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59E161F0)
    (at 187.96 60.96)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference LED3 (at 1 -4.5) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(LED2-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(LED3-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59E161F5)
    (at 195.58 60.96)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference LED4 (at 1 -4.5) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(LED3-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 46 "/LED(-)1"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A6A46BE)
    (at 203.708 69.088)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 0) (layer F.SilkS) hide)
    (fp_text value 3.3k (at 3.792 0.012) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(OptoLEDShield1-Pad0)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A58122E)
    (at 210.566 63.754 180)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.048 2.032 180) (layer F.SilkS))
    (fp_text value SW_SPST (at 3.75 6.7 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(OptoLEDShield1-Pad0)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 +5V))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(OptoLEDShield1-Pad0)"))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 +5V))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A581602)
    (at 167.132 57.404 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 1.27 -2.54 270) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +24V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A6A46EA)
    (at 167.132 75.438 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.54 0 270) (layer F.SilkS) hide)
    (fp_text value 4.7uF (at 2.662 -2.068 270) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 +24V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A6A470D)
    (at 191.008 86.106)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.54 0) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 2.692 2.094) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 +5V))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 5A580BD7)
    (at 179.07 96.266)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference LED5 (at 1 -4.5) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 47 "/LED(+)2"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 "Net-(LED5-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 5A580BD2)
    (at 186.69 96.266)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference LED6 (at 1 -4.5) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 "Net-(LED5-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 42 "Net-(LED6-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 5A580BCD)
    (at 194.31 96.266)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference LED7 (at 1 -4.5) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 42 "Net-(LED6-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 "Net-(LED7-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 5A580BC8)
    (at 201.93 96.266)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference LED8 (at 1 -4.5) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1.27 4.5) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 "Net-(LED7-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 48 "/LED(-)2"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A6A46CB)
    (at 177.038 70.104 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 0 180) (layer F.SilkS) hide)
    (fp_text value 3.3k (at 3.938 0.004 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(OptoLEDShield1-Pad8)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5A6A46A3)
    (at 188.468 84.836 180)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33 180) (layer F.SilkS) hide)
    (fp_text value MCP4922-E/P (at 3.868 8.236 270) (layer F.SilkS))
    (fp_text user %R (at 3.81 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 +5V))
    (pad 8 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(OptoLEDShield1-Pad8)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(OptoLEDShield1-Pad10)"))
    (pad 10 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /CTRL1))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(OptoLEDShield1-Pad13)"))
    (pad 11 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 +5V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(OptoLEDShield1-Pad11)"))
    (pad 12 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 +5V))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /CTRL2))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 5A5815F1)
    (at 163.576 72.898 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value CONN_01X07 (at 0 17.57 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/LED(+)1"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/LED(-)1"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /CTRL1))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /REF1))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 +24V))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 5A5815F7)
    (at 163.576 92.71 180)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value CONN_01X07 (at 0 17.57 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/LED(+)2"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/LED(-)2"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /CTRL2))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /REF2))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 +24V))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_Tantal_D5.0mm_P5.00mm (layer F.Cu) (tedit 5A6A46F9)
    (at 192.278 81.534)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=5.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 5.0mm Tantal Electrolytic Capacitor")
    (fp_text reference C4 (at 2.54 -1.524) (layer F.SilkS) hide)
    (fp_text value 10uF (at 2.422 -1.434) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 +5V))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D5.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module freetronics_footprints:POWER_JACK_PTH (layer F.Cu) (tedit 5AFDC4DA)
    (at 169.164 109.22)
    (fp_text reference CON1 (at -1.016 -4.318) (layer Eco1.User))
    (fp_text value BARREL_JACK (at -2.5908 -3.6068) (layer Eco1.User))
    (pad 1 thru_hole oval (at 0 -13.69822) (size 4.4958 4.4958) (drill 2.9972) (layers *.Cu *.Mask)
      (net 40 +24V))
    (pad 3 thru_hole oval (at 0 -7.69874) (size 4.4958 4.4958) (drill 2.9972) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2 thru_hole oval (at 4.699 -10.69848 90) (size 4.4958 4.4958) (drill 2.9972) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (gr_text "Use SR-05 series LEDS from Luxeon\n2 LEDs per connectors" (at 185.3 65.8) (layer B.SilkS))
  (gr_text github.com/anekimken/KiCad/tree/master/OptoLEDboard (at 190.7 89.4) (layer B.SilkS))
  (gr_text "Stanford Microsystems Lab\nAdam Nekimken" (at 210.8 94.5 90) (layer F.SilkS))
  (gr_text "Buckpuck 3021-D-E" (at 160.9 84.3 270) (layer F.SilkS))
  (gr_text "Buckpuck 3021-D-E" (at 160.9 64.4 270) (layer F.SilkS))
  (gr_text "+24 V min\n+32 V max" (at 170.5 90.4) (layer F.SilkS))
  (gr_line (start 159.512 51.562) (end 160.782 51.562) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.512 105.156) (end 159.512 51.562) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.63 105.156) (end 159.512 105.156) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.36 51.562) (end 160.782 51.562) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.63 102.362) (end 214.63 105.156) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.17 99.822) (end 214.63 102.362) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.17 66.802) (end 217.17 99.822) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.63 64.262) (end 217.17 66.802) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 214.63 52.832) (end 214.63 64.262) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.36 51.562) (end 214.63 52.832) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 10) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 213.36 64.135) (xy 215.9 67.31) (xy 215.9 99.06) (xy 213.36 101.6) (xy 213.36 103.505)
        (xy 160.782 104.14) (xy 160.528 52.578) (xy 213.36 52.705)
      )
    )
  )
)
