(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 41)
    (no_connects 0)
    (area 119.199999 98.149999 151.750001 117.600001)
    (thickness 1.6)
    (drawings 19)
    (tracks 191)
    (zones 0)
    (modules 20)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.1525)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.1525)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.39)
    (via_min_drill 0.255)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 0.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(U1-Pad20)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D3-Pad1)")
  (net 7 MISO)
  (net 8 SCK)
  (net 9 MOSI)
  (net 10 RESET)
  (net 11 MD_PAD_UP)
  (net 12 MD_PAD_DOWN)
  (net 13 MD_PAD_TL)
  (net 14 MD_PAD_LEFT)
  (net 15 MD_PAD_RIGHT)
  (net 16 MD_PAD_TR)
  (net 17 MD_PAD_TH)
  (net 18 JAP)
  (net 19 NTSC)
  (net 20 MD_RESET_OUT)
  (net 21 MD_RESET_IN)
  (net 22 PAD_DBG_LED)
  (net 23 NTSC_LED)
  (net 24 JAP_LED)
  (net_class Default "This is the default net class."
    (clearance 0.1525)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net JAP)
    (add_net JAP_LED)
    (add_net MD_PAD_DOWN)
    (add_net MD_PAD_LEFT)
    (add_net MD_PAD_RIGHT)
    (add_net MD_PAD_TH)
    (add_net MD_PAD_TL)
    (add_net MD_PAD_TR)
    (add_net MD_PAD_UP)
    (add_net MD_RESET_IN)
    (add_net MD_RESET_OUT)
    (add_net MISO)
    (add_net MOSI)
    (add_net NTSC)
    (add_net NTSC_LED)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(U1-Pad20)")
    (add_net PAD_DBG_LED)
    (add_net RESET)
    (add_net SCK)
  )
  (net_class Power ""
    (clearance 0.1525)
    (trace_width 0.35)
    (via_dia 0.7)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 5BC7A1F0)
    (at 132.2 106.98 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 -6.05 90) (layer F.SilkS) hide)
    (fp_text value "ATMEGA??8P(A)" (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 MD_PAD_RIGHT))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 MD_PAD_TL))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 MD_RESET_IN))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 MD_RESET_OUT))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 MD_PAD_TR))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 MD_PAD_TH))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 NTSC_LED))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 JAP_LED))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 PAD_DBG_LED))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 MOSI))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 MISO))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 NTSC))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 JAP))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 RESET))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 MD_PAD_UP))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 MD_PAD_DOWN))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 MD_PAD_LEFT))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5BC77BF6)
    (at 133.4 114.29 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference С2 (at 0 -1.25 270) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5BC77C04)
    (at 132.63 100.82)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference С3 (at 0 -1.25) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad20)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:KP-2012SGD (layer F.Cu) (tedit 5BC78840)
    (at 148.895 99.75)
    (fp_text reference D1 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value KP-2012SGD (at 6.9 0) (layer F.Fab))
    (pad 2 smd rect (at 1.175 0) (size 1.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.175 0) (size 1.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
  )
  (module Custom:KP-2012SGD (layer F.Cu) (tedit 5BC7884B)
    (at 148.895 103.75)
    (fp_text reference D2 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value KP-2012SGD (at 6.9 0) (layer F.Fab))
    (pad 2 smd rect (at 1.175 0) (size 1.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.175 0) (size 1.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
  )
  (module Custom:KP-2012SGD (layer F.Cu) (tedit 5BC78859)
    (at 148.895 101.75)
    (fp_text reference D3 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value KP-2012EC (at 6.375 0) (layer F.Fab))
    (pad 2 smd rect (at 1.175 0) (size 1.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.175 0) (size 1.25 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
  )
  (module Custom:Soldering_Point_1.5x3mm (layer F.Cu) (tedit 5BC77DD0)
    (at 147.99 115.1 90)
    (fp_text reference J1 (at 4 0 90) (layer F.SilkS) hide)
    (fp_text value +5V (at 0 2.4 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.1 180) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Custom:Soldering_Point_1.5x3mm (layer F.Cu) (tedit 5BC77DFD)
    (at 149.99 115.1 90)
    (fp_text reference J2 (at 4 0 90) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2.4 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.1 180) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Custom:MD_PAD_CONN (layer F.Cu) (tedit 5BC77B36)
    (at 121.73 109.88 270)
    (fp_text reference J3 (at 9.2 0 270) (layer F.SilkS) hide)
    (fp_text value MD_PAD_CONN (at 0 2.35 270) (layer F.Fab))
    (fp_text user "Mega Drive Pad" (at 0 -4 270) (layer F.SilkS))
    (fp_text user 9 (at 4 -2.25 360) (layer F.SilkS))
    (fp_text user 7 (at 6 -2.25 360) (layer F.SilkS))
    (fp_text user 6 (at -2 -2.25 360) (layer F.SilkS))
    (fp_text user 4 (at 2 -2.25 360) (layer F.SilkS))
    (fp_text user 3 (at 0 -2.25 360) (layer F.SilkS))
    (fp_text user 2 (at -4 -2.25 540) (layer F.SilkS))
    (fp_text user 1 (at -6 -2.25 360) (layer F.SilkS))
    (pad 1 smd rect (at -6 0 270) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 11 MD_PAD_UP))
    (pad 2 smd rect (at -4 0 270) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 12 MD_PAD_DOWN))
    (pad 6 smd rect (at -2 0 270) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 13 MD_PAD_TL))
    (pad 3 smd rect (at 0 0 270) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 14 MD_PAD_LEFT))
    (pad 4 smd rect (at 2 0 270) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 15 MD_PAD_RIGHT))
    (pad 9 smd rect (at 4 0 270) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 16 MD_PAD_TR))
    (pad 7 smd rect (at 6 0 270) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 17 MD_PAD_TH))
    (pad 5 smd circle (at 0.05 0 270) (size 0.1 0.1) (layers Dwgs.User))
    (pad 8 smd circle (at -0.05 0 270) (size 0.1 0.1) (layers Dwgs.User))
  )
  (module Custom:Soldering_Point_1.5x3mm (layer F.Cu) (tedit 5BC77E4F)
    (at 121.73 99.98)
    (fp_text reference J4 (at 4 0) (layer F.SilkS) hide)
    (fp_text value Language (at -5.43 0.04) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.1 90) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 18 JAP))
  )
  (module Custom:Soldering_Point_1.5x3mm (layer F.Cu) (tedit 5BC77EA6)
    (at 138.437344 100.7 270)
    (fp_text reference J5 (at 4 0 270) (layer F.SilkS) hide)
    (fp_text value Video_Mode_DFO (at -9.36 -0.32 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.1) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 19 NTSC))
  )
  (module Custom:Soldering_Point_1.5x3mm (layer F.Cu) (tedit 5BC77EE1)
    (at 121.73 101.98)
    (fp_text reference J6 (at 4 0) (layer F.SilkS) hide)
    (fp_text value Video_Mode (at -6.54 -0.08) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.1 90) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 19 NTSC))
  )
  (module Custom:Soldering_Point_1.5x3mm (layer F.Cu) (tedit 5BC77F32)
    (at 140.437344 115.105846 90)
    (fp_text reference J7 (at 4 0 90) (layer F.SilkS) hide)
    (fp_text value MD_Reset_Out (at 0 2.4 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.1 180) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 20 MD_RESET_OUT))
  )
  (module Custom:Soldering_Point_1.5x3mm (layer F.Cu) (tedit 5BC77F34)
    (at 138.437344 115.105846 90)
    (fp_text reference J8 (at 4 0 90) (layer F.SilkS) hide)
    (fp_text value MD_Reset_In (at 0 2.4 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -0.1 180) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 21 MD_RESET_IN))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5BC77C22)
    (at 144.06 109.55)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BC77C16)
    (at 146.07 106.34 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 PAD_DBG_LED))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BC77C11)
    (at 150.07 106.34 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 NTSC_LED))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5BC77C1A)
    (at 148.07 106.34 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 JAP_LED))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5BC7A111)
    (at 131.8 114.29 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference С1 (at 0 -1.25 270) (layer F.SilkS) hide)
    (fp_text value "0.1 uF" (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:AVR-ISP-6-SMD (layer B.Cu) (tedit 5BC7C716)
    (at 144.06 106.98)
    (descr "Double rangee de contacts 2 x 4 pins")
    (tags CONN)
    (fp_text reference ISP1 (at 0 3.81) (layer B.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 0 -3.81) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.54 -1.27) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 7 MISO))
    (pad 2 smd rect (at -2.54 1.27) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 0 -1.27) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 8 SCK))
    (pad 4 smd rect (at 0 1.27) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 9 MOSI))
    (pad 5 smd rect (at 2.54 -1.27) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 10 RESET))
    (pad 6 smd rect (at 2.54 1.27) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model pin_array/pins_array_3x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text ISP (at 144.04 110.79) (layer B.SilkS))
  (gr_text "Rev. 5BC7C4FE" (at 145.38 116.26) (layer B.SilkS))
  (gr_text "Mega Drive++ R" (at 141.71 99.87) (layer B.SilkS))
  (gr_line (start 119.25 98.2) (end 119.25 117.55) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.7 98.2) (end 151.7 117.55) (layer Edge.Cuts) (width 0.1))
  (dimension 17.5 (width 0.3) (layer Dwgs.User)
    (gr_text "17,500 mm" (at 173.2 107.8 270) (layer Dwgs.User))
    (feature1 (pts (xy 150 116.55) (xy 174.55 116.55)))
    (feature2 (pts (xy 150 99.05) (xy 174.55 99.05)))
    (crossbar (pts (xy 171.85 99.05) (xy 171.85 116.55)))
    (arrow1a (pts (xy 171.85 116.55) (xy 171.263579 115.423496)))
    (arrow1b (pts (xy 171.85 116.55) (xy 172.436421 115.423496)))
    (arrow2a (pts (xy 171.85 99.05) (xy 171.263579 100.176504)))
    (arrow2b (pts (xy 171.85 99.05) (xy 172.436421 100.176504)))
  )
  (dimension 30.55 (width 0.3) (layer Dwgs.User)
    (gr_text "30,550 mm" (at 135.475 79.8) (layer Dwgs.User))
    (feature1 (pts (xy 150.75 99.5) (xy 150.75 78.45)))
    (feature2 (pts (xy 120.2 99.5) (xy 120.2 78.45)))
    (crossbar (pts (xy 120.2 81.15) (xy 150.75 81.15)))
    (arrow1a (pts (xy 150.75 81.15) (xy 149.623496 81.736421)))
    (arrow1b (pts (xy 150.75 81.15) (xy 149.623496 80.563579)))
    (arrow2a (pts (xy 120.2 81.15) (xy 121.326504 81.736421)))
    (arrow2b (pts (xy 120.2 81.15) (xy 121.326504 80.563579)))
  )
  (gr_line (start 119.25 98.2) (end 151.7 98.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.25 117.55) (end 151.7 117.55) (layer Edge.Cuts) (width 0.1))
  (gr_text Region (at 144.06 103.75) (layer F.SilkS))
  (gr_text Language (at 142.99 101.75) (layer F.SilkS))
  (gr_text Pad (at 145.18 99.75) (layer F.SilkS))
  (gr_text "Reset in" (at 138.437344 110.395846 90) (layer F.SilkS))
  (gr_text "Reset out" (at 140.327344 109.895846 90) (layer F.SilkS))
  (gr_text VMode (at 125.8 101.94) (layer F.SilkS))
  (gr_text DFO (at 138.47 103.65 90) (layer F.SilkS))
  (gr_text Language (at 126.88 99.91) (layer F.SilkS))
  (gr_text GND (at 149.99 111.92 90) (layer F.SilkS))
  (gr_text +5V (at 147.99 111.97 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 117.5 97.5) (xy 117.5 117.5) (xy 153 117.5) (xy 153 97.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.55 103.35) (xy 128.55 110.6) (xy 135.85 110.6) (xy 135.85 103.35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 132.25 110.6) (xy 132.95 110.6) (xy 132.95 116.05) (xy 132.25 116.05)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 149.35 100.45) (xy 150.95 100.45) (xy 150.95 101.05) (xy 149.35 101.05) (xy 149.35 104.2)
        (xy 148.4 104.2) (xy 148.4 98.95) (xy 149.35 98.95)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 117.5 97.5) (xy 153 97.5) (xy 153 117.5) (xy 117.5 117.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 150.95 102.45) (xy 150.95 103.05) (xy 149.35 103.05) (xy 149.35 102.45)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 147.6 106.75) (xy 147.6 107.45) (xy 145.75 107.45) (xy 145.75 106.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.35))
    (polygon
      (pts
        (xy 142.45 104.7) (xy 143.15 104.7) (xy 143.15 106.75) (xy 142.45 106.75)
      )
    )
  )
)
