(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 50)
    (no_connects 0)
    (area 50.724999 50.064999 100.405001 94.603001)
    (thickness 1.6)
    (drawings 26)
    (tracks 278)
    (zones 0)
    (modules 24)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.635)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585CC138)
    (at 63.5 57.15 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value C_Small (at 0.635 -14.605 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585CC13F)
    (at 74.93 57.15 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value C_Small (at -1.27 27.305 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585CC2C9)
    (at 71.12 77.47)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 4.445 -0.635) (layer F.SilkS))
    (fp_text value C_Small (at 1.905 5.08) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585CC116)
    (at 87.63 73.66 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -4.445 0 360) (layer F.SilkS))
    (fp_text value C_Small (at -0.635 -15.24 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 585CBF92)
    (at 83.82 53.34)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 4.445 0) (layer F.SilkS))
    (fp_text value C_Small (at 6.985 27.94) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585CBF20)
    (at 63.5 58.42 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at -0.635 -14.605 90) (layer F.SilkS))
    (fp_text value C_Small (at 0.635 -14.605 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585CBF9A)
    (at 74.93 58.42 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at -5.08 -26.035 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 27.305 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585CBF5D)
    (at 69.85 77.47)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 8.255 5.08) (layer F.SilkS))
    (fp_text value C_Small (at 1.905 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585CBF6B)
    (at 87.63 72.39 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C9 (at 1.27 -15.24 270) (layer F.SilkS))
    (fp_text value C_Small (at 1.27 -15.24 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 585CBF95)
    (at 82.55 53.34)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C10 (at 20.32 1.27) (layer F.SilkS))
    (fp_text value C_Small (at 3.81 28.575) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585CC13C)
    (at 66.675 53.975 270)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L1 (at 11.43 -0.635 360) (layer F.SilkS))
    (fp_text value L_Small (at 3.175 17.78 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585CBF50)
    (at 74.295 69.215 180)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L2 (at 11.43 -4.445 180) (layer F.SilkS))
    (fp_text value L_Small (at 3.175 -12.7 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585CC113)
    (at 79.375 66.675 270)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L3 (at -1.27 -0.635 360) (layer F.SilkS))
    (fp_text value L_Small (at 5.715 -22.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
  )
  (module Choke_Toroid_ThroughHole:Choke_Toroid_5x10mm_Vertical (layer F.Cu) (tedit 585CBFC2)
    (at 76.835 61.595)
    (descr "Toroid, Coil, Choke,  5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (tags "Toroid, Coil, Choke, 5mm x 10mm, Vertical, Inductor, Drossel, Thruhole,")
    (fp_text reference L4 (at 11.43 -4.445) (layer F.SilkS))
    (fp_text value L_Small (at 10.16 20.32) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 -5.08) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(C10-Pad1)"))
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585CBF44)
    (at 69.215 59.055)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L5 (at -20.955 3.175) (layer F.SilkS))
    (fp_text value L_Small (at -1.27 22.86) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.6 0) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585CBFAD)
    (at 69.215 71.755 270)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L6 (at 1.905 20.32 270) (layer F.SilkS))
    (fp_text value L_Small (at 0 19.685 270) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 270) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.6 0 270) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585CBFB7)
    (at 81.915 71.755)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L7 (at 20.955 3.175) (layer F.SilkS))
    (fp_text value L_Small (at 1.905 9.525) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.6 0) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Taiyo-Yuden_NR-30xx_HandSoldering (layer F.Cu) (tedit 585CBFA2)
    (at 81.915 59.055 90)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-30xx, 3.0mmx3.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L8 (at 0.635 20.32 90) (layer F.SilkS))
    (fp_text value L_Small (at 0.635 20.32 90) (layer F.Fab))
    (pad 1 smd rect (at -1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.6 0 90) (size 1.8 2.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (model Inductors.3dshapes/Inductor_Taiyo-Yuden_NR-30xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:SMA_Vertical_Or_Edge (layer F.Cu) (tedit 585CBF53)
    (at 57.785 65.405 270)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference P1 (at -2.54 8.255 270) (layer F.SilkS))
    (fp_text value BNC (at 0.635 8.89 270) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 smd rect (at 2.54 1.778 270) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 270) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at 0 1.524 270) (size 1.524 5.588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.54 1.778 270) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.54 1.778 270) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.54 1.778 270) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Connect.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:SMA_Vertical_Or_Edge (layer F.Cu) (tedit 585CBF7C)
    (at 93.345 65.405 90)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference P2 (at -0.635 8.89 90) (layer F.SilkS))
    (fp_text value BNC (at 0.635 10.795 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 smd rect (at 2.54 1.778 90) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at 0 1.524 90) (size 1.524 5.588) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -2.54 1.778 90) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.54 1.778 90) (size 1.6002 4.9022) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.54 1.778 90) (size 1.6002 4.9022) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Connect.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585CC0CB)
    (at 54.61 54.61)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -5.715) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 6.35 -5.715) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585CC0D2)
    (at 54.61 76.2)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 1.27 6.35) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 5.715 5.715) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585CC0D8)
    (at 96.52 76.2)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at -0.635 6.35) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at -4.445 5.715) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 585CC0C6)
    (at 96.52 54.61)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at -0.635 -5.715) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at -3.81 -5.715) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text O (at 64.77 68.58) (layer B.Mask))
  (gr_text O (at 62.23 71.12) (layer B.Mask))
  (gr_text o (at 64.135 73.025) (layer B.Mask))
  (gr_text <>< (at 60.96 74.295) (layer B.Mask))
  (gr_text ><> (at 64.135 76.835) (layer B.Mask))
  (gr_text "mark@halibut.com  @SmittyHalibut" (at 52.07 52.07) (layer F.SilkS))
  (gr_text "BY-NC-SA 2016 Mark Smith" (at 74.93 78.74) (layer F.SilkS))
  (gr_text "LPF v1.0a" (at 57.785 78.74) (layer F.SilkS))
  (gr_arc (start 53.34 77.47) (end 53.34 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97.79 77.47) (end 100.33 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97.79 53.34) (end 97.79 50.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 53.34 53.34) (end 50.8 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.8 61.595) (end 50.8 53.34) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.34 61.595) (end 50.8 61.595) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.34 69.215) (end 53.34 61.595) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.8 69.215) (end 53.34 69.215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.8 77.47) (end 50.8 69.215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 80.01) (end 53.34 80.01) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 69.215) (end 100.33 77.47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 69.215) (end 100.33 69.215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 61.595) (end 97.79 69.215) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 61.595) (end 97.79 61.595) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.33 53.34) (end 100.33 61.595) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 53.34 50.8) (end 97.79 50.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 50.8) (xy 100.33 50.8) (xy 100.33 80.01) (xy 50.8 80.01)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.8 50.8) (xy 100.33 50.8) (xy 100.33 80.01) (xy 50.8 80.01)
      )
    )
  )
)
