(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "PICO ADC TEST")
    (date "2024-01-31")
    (rev "R0.1")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "core") (thickness 1.24) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "prepreg") (thickness 0.1) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 120.25 123.5)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(IC2-LMD)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "TO_ADC_H")
  (net 5 "Net-(IC1-IRS)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(IC2-INH)")
  (net 8 "Net-(C6-Pad2)")
  (net 9 "+3.3V")
  (net 10 "Net-(C9-Pad1)")
  (net 11 "TO_ADC_L")
  (net 12 "Net-(IC2-LON)")
  (net 13 "Net-(IC2-VIN)")
  (net 14 "Net-(IC2-LOP)")
  (net 15 "Net-(IC2-VIP)")
  (net 16 "Net-(IC1-VCOM)")
  (net 17 "Net-(IC1-VREF)")
  (net 18 "Net-(IC1-VREFT)")
  (net 19 "Net-(IC1-VREFB)")
  (net 20 "Net-(IC2-RCLMP)")
  (net 21 "DAC_G")
  (net 22 "Net-(IC2-VCM)")
  (net 23 "Net-(IC1-VIN-)")
  (net 24 "Net-(IC1-VIN+)")
  (net 25 "5VVGA")
  (net 26 "5VLNA")
  (net 27 "Net-(U1-B)")
  (net 28 "VOH")
  (net 29 "VOL")
  (net 30 "+5V")
  (net 31 "ADC_CLK")
  (net 32 "D9")
  (net 33 "D8")
  (net 34 "D7")
  (net 35 "D6")
  (net 36 "D5")
  (net 37 "D4")
  (net 38 "D3")
  (net 39 "D2")
  (net 40 "D1")
  (net 41 "D0")
  (net 42 "Net-(IC2-HILO)")
  (net 43 "Net-(IC2-VPOS)")
  (net 44 "Net-(IC2-ENBV)")
  (net 45 "Net-(IC2-ENBL)")
  (net 46 "Net-(U1-A)")
  (net 47 "GPIO21")
  (net 48 "GPIO17")
  (net 49 "GPIO18")
  (net 50 "GPIO19")
  (net 51 "GPIO11")
  (net 52 "GPIO22")
  (net 53 "GPIO12")
  (net 54 "GPIO26")
  (net 55 "GPIO16")
  (net 56 "GPIO27")
  (net 57 "GPIO20")
  (net 58 "GPIO28")
  (net 59 "CS")
  (net 60 "SCLK")
  (net 61 "MOSI")
  (net 62 "unconnected-(U2-RUN-Pad30)")
  (net 63 "unconnected-(U2-ADC_VREF-Pad35)")
  (net 64 "unconnected-(U2-3V3_EN-Pad37)")
  (net 65 "unconnected-(U2-VSYS-Pad39)")
  (net 66 "SWCLK")
  (net 67 "SWDIO")
  (net 68 "unconnected-(IC3-VOUTB-Pad6)")
  (net 69 "unconnected-(U1-COM-Pad2)")
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 183.25 121)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C13" (at 5.5 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 16 "Net-(IC1-VCOM)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 191.25 106.25 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C9" (at 11.5 -5.5 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 10 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 11 "TO_ADC_L") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 198.25 101.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C21" (at -10 2.25 90) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 25 "5VVGA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 172.8875 83.4875 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C26" (at 0.6375 3.7375) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 9 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 172.8625 85.8375 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C25" (at 0.6125 4.5875) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 9 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PICO_ADC_Test:SOP64P600X175-20N" (layer "F.Cu")
    (at 187.5 93.25 -90)
    (descr "RQ-20 (QSOP)")
    (tags "Integrated Circuit")
    (property "ARROW PART NUMBER" "AD8331ARQZ")
    (property "ARROW PRICE/STOCK" "https://www.arrow.com/en/products/ad8331arqz/analog-devices")
    (property "DATASHEET LINK" "http://www.analog.com/static/imported-files/data_sheets/AD8331_8332_8334.pdf")
    (property "HEIGHT" "1.75mm")
    (property "MANUFACTURER_NAME" "Analog Devices")
    (property "MANUFACTURER_PART_NUMBER" "AD8331ARQZ")
    (property "MOUSER PART NUMBER" "584-AD8331ARQZ")
    (property "MOUSER PRICE/STOCK" "https://www.mouser.co.uk/ProductDetail/Analog-Devices/AD8331ARQZ?qs=%2FtpEQrCGXCwx0%2F22gf7ohQ%3D%3D")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Integrated Circuit")
    (attr smd)
    (fp_text reference "IC2" (at -3.25 -5 -180) (layer "F.SilkS"))
    (fp_text value "AD8331ARQZ" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.715 -2.88) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(IC2-LMD)") (pinfunction "LMD") (pintype "passive"))
    (pad "2" smd roundrect (at -2.715 -2.24) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(IC2-INH)") (pinfunction "INH") (pintype "passive"))
    (pad "3" smd roundrect (at -2.715 -1.6) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "5VLNA") (pinfunction "VPSL") (pintype "passive"))
    (pad "4" smd roundrect (at -2.715 -0.96) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(IC2-LON)") (pinfunction "LON") (pintype "passive"))
    (pad "5" smd roundrect (at -2.715 -0.32) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(IC2-LOP)") (pinfunction "LOP") (pintype "passive"))
    (pad "6" smd roundrect (at -2.715 0.32) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "COML") (pintype "passive"))
    (pad "7" smd roundrect (at -2.715 0.96) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(IC2-VIP)") (pinfunction "VIP") (pintype "passive"))
    (pad "8" smd roundrect (at -2.715 1.6) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(IC2-VIN)") (pinfunction "VIN") (pintype "passive"))
    (pad "9" smd roundrect (at -2.715 2.24) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "MODE") (pintype "passive"))
    (pad "10" smd roundrect (at -2.715 2.88) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "DAC_G") (pinfunction "GAIN") (pintype "passive"))
    (pad "11" smd roundrect (at 2.715 2.88) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(IC2-VCM)") (pinfunction "VCM") (pintype "passive"))
    (pad "12" smd roundrect (at 2.715 2.24) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(IC2-RCLMP)") (pinfunction "RCLMP") (pintype "passive"))
    (pad "13" smd roundrect (at 2.715 1.6) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(IC2-HILO)") (pinfunction "HILO") (pintype "passive"))
    (pad "14" smd roundrect (at 2.715 0.96) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(IC2-VPOS)") (pinfunction "VPOS") (pintype "passive"))
    (pad "15" smd roundrect (at 2.715 0.32) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "VOH") (pinfunction "VOH") (pintype "passive"))
    (pad "16" smd roundrect (at 2.715 -0.32) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "VOL") (pinfunction "VOL") (pintype "passive"))
    (pad "17" smd roundrect (at 2.715 -0.96) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "COMM_1") (pintype "passive"))
    (pad "18" smd roundrect (at 2.715 -1.6) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(IC2-ENBV)") (pinfunction "ENBV") (pintype "passive"))
    (pad "19" smd roundrect (at 2.715 -2.24) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(IC2-ENBL)") (pinfunction "ENBL") (pintype "passive"))
    (pad "20" smd roundrect (at 2.715 -2.88) (size 0.44 1.52) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "COMM_2") (pintype "passive"))
    (model "E:\\kicad_my_library\\SamacSys_Parts.3dshapes\\AD8331ARQZ.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 174.75 101.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.mouser.vn/datasheet/2/40/cx5r_KGM-3223198.pdf")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT NEW GLOBAL PN KGM31HR51A475KL 10V 4.7uF X5R 1206 10% Tol")
    (property "MPN" "1206ZD475KAT4A")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C3" (at -3.75 -1.75 90) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 5 "Net-(IC1-IRS)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 185 84.5 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R7" (at -3.25 -13.92 90) (layer "F.SilkS"))
    (fp_text value "280R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 8 "Net-(C6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 12 "Net-(IC2-LON)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 167.75 101.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.mouser.vn/datasheet/2/40/cx5r_KGM-3223198.pdf")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT NEW GLOBAL PN KGM31HR51A475KL 10V 4.7uF X5R 1206 10% Tol")
    (property "MPN" "1206ZD475KAT4A")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C7" (at -3.75 0.75 90) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 9 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 183.25 116.5)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C15" (at 5.525 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at -5.05 1.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 18 "Net-(IC1-VREFT)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 172.5 101.5 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R1" (at 3.75 1 90) (layer "F.SilkS"))
    (fp_text value "18R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 9 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 5 "Net-(IC1-IRS)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 193.5 101.5 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R3" (at -10.5 4 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 25 "5VVGA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 44 "Net-(IC2-ENBV)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric" (layer "F.Cu")
    (at 203.25 101.5 90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?34102")
    (property "Description" "Ferrite Beads 75ohms 25%")
    (property "Height" "1.05")
    (property "Manufacturer_Name" "Murata Electronics")
    (property "Manufacturer_Part_Number" "BLM21BB750SN1D")
    (property "Mouser Part Number" "81-BLM21B750S")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Murata-Electronics/BLM21BB750SN1D/?qs=Ncw4LTdqe05b2FdOdGUHhQ%3D%3D")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "25%")
    (property "ki_description" "BLM21_N1D Series EMI Suppression Filter 75+/-25% at 100MHz 700mA @85")
    (attr smd)
    (fp_text reference "FB4" (at -10 0.25 90) (layer "F.SilkS"))
    (fp_text value "ILHB1206ER750V" (at 0 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.575 0 90) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 25 "5VVGA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.575 0 90) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 30 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PICO_ADC_Test:SOT95P240X120-3N" (layer "F.Cu")
    (at 186.75 78.25)
    (descr "SOT-23")
    (tags "Diode")
    (property "Description" "Diode Small Signal Switching 75V 0.3A 3-Pin SOT-23 T/R")
    (property "Height" "1.2")
    (property "Manufacturer_Name" "Diodes Incorporated")
    (property "Manufacturer_Part_Number" "BAV99-7-F")
    (property "Mouser Part Number" "621-BAV99-F")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/BAV99-7-F?qs=E9Ihi8A05%252BSTVRjo74hQDA%3D%3D")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode Small Signal Switching 75V 0.3A 3-Pin SOT-23 T/R")
    (attr smd)
    (fp_text reference "D1" (at -4.25 -2) (layer "F.SilkS"))
    (fp_text value "BAV99-7-F" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.2 -0.95 90) (size 0.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at -1.2 0.95 90) (size 0.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "3" smd rect (at 1.2 0 90) (size 0.6 0.85) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(U1-B)") (pintype "passive"))
    (model "E:\\kicad_my_library\\SamacSys_Parts.3dshapes\\BAV99-7-F.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 184 108.75 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "5%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C20" (at -10 8 90) (layer "F.SilkS"))
    (fp_text value "50pF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 23 "Net-(IC1-VIN-)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 24 "Net-(IC1-VIN+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 166.95 72 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0.975 12.762 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "SWCLK") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "SWDIO") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric" (layer "F.Cu")
    (at 198.25 93.225 90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?34102")
    (property "Description" "Ferrite Beads 75ohms 25%")
    (property "Height" "1.05")
    (property "Manufacturer_Name" "Murata Electronics")
    (property "Manufacturer_Part_Number" "BLM21BB750SN1D")
    (property "Mouser Part Number" "81-BLM21B750S")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Murata-Electronics/BLM21BB750SN1D/?qs=Ncw4LTdqe05b2FdOdGUHhQ%3D%3D")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "25%")
    (property "ki_description" "BLM21_N1D Series EMI Suppression Filter 75+/-25% at 100MHz 700mA @85")
    (attr smd)
    (fp_text reference "FB5" (at 4.225 3.75 90) (layer "F.SilkS"))
    (fp_text value "ILHB1206ER750V" (at 0 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.575 0 90) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 30 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.575 0 90) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 26 "5VLNA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 170 101.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C8" (at -3.75 0 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 9 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (at 130.46 96.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 180) (layer "F.SilkS"))
    (fp_text value "22-23-2021" (at -2 9.275 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 177.5 97.75 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R9" (at 6.75 1.5) (layer "F.SilkS"))
    (fp_text value "12K" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 20 "Net-(IC2-RCLMP)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 180) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric" (layer "F.Cu")
    (at 188.75 101.5 -90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?34102")
    (property "Description" "Ferrite Beads 75ohms 25%")
    (property "Height" "1.05")
    (property "Manufacturer_Name" "Murata Electronics")
    (property "Manufacturer_Part_Number" "BLM21BB750SN1D")
    (property "Mouser Part Number" "81-BLM21B750S")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Murata-Electronics/BLM21BB750SN1D/?qs=Ncw4LTdqe05b2FdOdGUHhQ%3D%3D")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "25%")
    (property "ki_description" "BLM21_N1D Series EMI Suppression Filter 75+/-25% at 100MHz 700mA @85")
    (attr smd)
    (fp_text reference "FB3" (at 10 -5.75 -90) (layer "F.SilkS"))
    (fp_text value "ILHB1206ER750V" (at 0 1.9 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.575 0 270) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 29 "VOL") (pintype "passive"))
    (pad "2" smd roundrect (at 1.575 0 270) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 10 "Net-(C9-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 177 101.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C4" (at -3.75 -2.5 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 5 "Net-(IC1-IRS)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric" (layer "F.Cu")
    (at 186.25 101.5 -90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?34102")
    (property "Description" "Ferrite Beads 75ohms 25%")
    (property "Height" "1.05")
    (property "Manufacturer_Name" "Murata Electronics")
    (property "Manufacturer_Part_Number" "BLM21BB750SN1D")
    (property "Mouser Part Number" "81-BLM21B750S")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Murata-Electronics/BLM21BB750SN1D/?qs=Ncw4LTdqe05b2FdOdGUHhQ%3D%3D")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "25%")
    (property "ki_description" "BLM21_N1D Series EMI Suppression Filter 75+/-25% at 100MHz 700mA @85")
    (attr smd)
    (fp_text reference "FB1" (at 10 -6.75 -90) (layer "F.SilkS"))
    (fp_text value "ILHB1206ER750V" (at 0 1.9 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.575 0 270) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 28 "VOH") (pintype "passive"))
    (pad "2" smd roundrect (at 1.575 0 270) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 196 93.25 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C23" (at -4.25 -4.5 90) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 26 "5VLNA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" locked (layer "F.Cu")
    (at 201.75 120)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Horizontal" locked (layer "F.Cu")
    (at 130.46 78.47)
    (descr "Through hole angled socket strip, 1x06, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x06 2.54mm single row")
    (property "Digi-Key_PN" "732-5319-ND")
    (property "MPN" "61300611121")
    (property "Manufacturer" "Würth Elektronik")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "CONN HEADER VERT 6POS 2.54MM")
    (property "ki_keywords" "61300611121")
    (attr through_hole)
    (fp_text reference "J3" (at -2.21 15.28) (layer "F.SilkS"))
    (fp_text value "61300611121" (at -4.38 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.775 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "GPIO17") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "GPIO16") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "GPIO12") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "GPIO11") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 177.5 95.5 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C17" (at 6.25 0.75) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 20 "Net-(IC2-RCLMP)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PICO_ADC_Test:MCP4812-EMS" (layer "F.Cu")
    (at 176.7 89.125)
    (descr "8 Lead MS MSOP")
    (tags "Integrated Circuit")
    (property "ARROW PART NUMBER" "MCP4812-E/MS")
    (property "ARROW PRICE/STOCK" "https://www.arrow.com/en/products/mcp4812-ems/microchip-technology")
    (property "DATASHEET LINK" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002249B.pdf")
    (property "HEIGHT" "1.1mm")
    (property "MANUFACTURER_NAME" "Microchip")
    (property "MANUFACTURER_PART_NUMBER" "MCP4812-E/MS")
    (property "MOUSER PART NUMBER" "579-MCP4812-E/MS")
    (property "MOUSER PRICE/STOCK" "https://www.mouser.co.uk/ProductDetail/Microchip-Technology/MCP4812-E-MS?qs=bxUt0k7cytJEpyWPtzKy6A%3D%3D")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Integrated Circuit")
    (attr smd)
    (fp_text reference "IC3" (at -6.45 2.625) (layer "F.SilkS"))
    (fp_text value "MCP4812-E_MS" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.2 -0.975 90) (size 0.45 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+3.3V") (pinfunction "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at -2.2 -0.325 90) (size 0.45 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "CS") (pinfunction "~{CS}") (pintype "passive"))
    (pad "3" smd roundrect (at -2.2 0.325 90) (size 0.45 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "SCLK") (pinfunction "SCK") (pintype "passive"))
    (pad "4" smd roundrect (at -2.2 0.975 90) (size 0.45 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "MOSI") (pinfunction "SDI") (pintype "passive"))
    (pad "5" smd roundrect (at 2.2 0.975 90) (size 0.45 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "~{LDAC}") (pintype "passive"))
    (pad "6" smd roundrect (at 2.2 0.325 90) (size 0.45 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "unconnected-(IC3-VOUTB-Pad6)") (pinfunction "VOUTB") (pintype "passive+no_connect"))
    (pad "7" smd roundrect (at 2.2 -0.325 90) (size 0.45 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "8" smd roundrect (at 2.2 -0.975 90) (size 0.45 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "DAC_G") (pinfunction "VOUTA") (pintype "passive"))
    (model "E:\\kicad_my_library\\SamacSys_Parts.3dshapes\\MCP4812-E_MS.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 179.05 84.525 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C10" (at -3.775 -15.45 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 12 "Net-(IC2-LON)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 13 "Net-(IC2-VIN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" locked (layer "F.Cu")
    (at 123.75 120)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 189.75 84.5 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C5" (at -3.25 -10.5 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 6 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 7 "Net-(IC2-INH)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PICO_ADC_Test:SOP65P640X120-28N" (layer "F.Cu")
    (at 172.75 112.2125 180)
    (descr "PW(R-PDSO-G28)")
    (tags "Integrated Circuit")
    (property "Description" "10-Bit, 65-MSPS Analog-to-Digital Converter (ADC)")
    (property "Height" "1.2")
    (property "Manufacturer_Name" "Texas Instruments")
    (property "Manufacturer_Part_Number" "ADC10065CIMT/NOPB")
    (property "Mouser Part Number" "926-ADC10065CIMTNOPB")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=926-ADC10065CIMTNOPB")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "10-Bit, 65-MSPS Analog-to-Digital Converter (ADC)")
    (attr smd)
    (fp_text reference "IC1" (at 5 4.7125) (layer "F.SilkS"))
    (fp_text value "ADC10065CIMT_NOPB" (at 11.25 6.5) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 11.25 6.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.938 -4.225 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "ADC_CLK") (pinfunction "CLK") (pintype "passive"))
    (pad "2" smd roundrect (at -2.938 -3.575 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(IC1-IRS)") (pinfunction "VDDA_1") (pintype "passive"))
    (pad "3" smd roundrect (at -2.938 -2.925 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSSA_1") (pintype "passive"))
    (pad "4" smd roundrect (at -2.938 -2.275 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(IC1-VCOM)") (pinfunction "VCOM") (pintype "passive"))
    (pad "5" smd roundrect (at -2.938 -1.625 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(IC1-IRS)") (pinfunction "IRS") (pintype "passive"))
    (pad "6" smd roundrect (at -2.938 -0.975 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(IC1-VREF)") (pinfunction "VREF") (pintype "passive"))
    (pad "7" smd roundrect (at -2.938 -0.325 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(IC1-VREFT)") (pinfunction "VREFT") (pintype "passive"))
    (pad "8" smd roundrect (at -2.938 0.325 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(IC1-VREFB)") (pinfunction "VREFB") (pintype "passive"))
    (pad "9" smd roundrect (at -2.938 0.975 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(IC1-IRS)") (pinfunction "VDDA_2") (pintype "passive"))
    (pad "10" smd roundrect (at -2.938 1.625 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(IC1-IRS)") (pinfunction "VDDA_3") (pintype "passive"))
    (pad "11" smd roundrect (at -2.938 2.275 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSSA_2") (pintype "passive"))
    (pad "12" smd roundrect (at -2.938 2.925 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(IC1-VIN-)") (pinfunction "VIN-") (pintype "passive"))
    (pad "13" smd roundrect (at -2.938 3.575 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(IC1-VIN+)") (pinfunction "VIN+") (pintype "passive"))
    (pad "14" smd roundrect (at -2.938 4.225 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSSA_3") (pintype "passive"))
    (pad "15" smd roundrect (at 2.938 4.225 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "DF") (pintype "passive"))
    (pad "16" smd roundrect (at 2.938 3.575 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "D9") (pinfunction "D9") (pintype "passive"))
    (pad "17" smd roundrect (at 2.938 2.925 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "D8") (pinfunction "D8") (pintype "passive"))
    (pad "18" smd roundrect (at 2.938 2.275 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "D7") (pinfunction "D7") (pintype "passive"))
    (pad "19" smd roundrect (at 2.938 1.625 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "D6") (pinfunction "D6") (pintype "passive"))
    (pad "20" smd roundrect (at 2.938 0.975 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "D5") (pinfunction "D5") (pintype "passive"))
    (pad "21" smd roundrect (at 2.938 0.325 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSSIO") (pintype "passive"))
    (pad "22" smd roundrect (at 2.938 -0.325 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+3.3V") (pinfunction "VDDIO") (pintype "passive"))
    (pad "23" smd roundrect (at 2.938 -0.975 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "D4") (pinfunction "D4") (pintype "passive"))
    (pad "24" smd roundrect (at 2.938 -1.625 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "D3") (pinfunction "D3") (pintype "passive"))
    (pad "25" smd roundrect (at 2.938 -2.275 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "D2") (pinfunction "D2") (pintype "passive"))
    (pad "26" smd roundrect (at 2.938 -2.925 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "D1") (pinfunction "D1") (pintype "passive"))
    (pad "27" smd roundrect (at 2.938 -3.575 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "D0") (pinfunction "D0") (pintype "passive"))
    (pad "28" smd roundrect (at 2.938 -4.225 270) (size 0.45 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "STBY") (pintype "passive"))
    (model "E:\\kicad_my_library\\SamacSys_Parts.3dshapes\\ADC10065CIMT_NOPB.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 181.45 84.525 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C11" (at -3.775 -14.55 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 14 "Net-(IC2-LOP)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 15 "Net-(IC2-VIP)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PICO_ADC_Test:AMPHENOL_132357-11" locked (layer "F.Cu")
    (at 191.25 70.75 -90)
    (property "Description" "JOHNSON - 142-0701-801 - \\u5C04\\u9891/\\u540C\\u8F74\\u63D2\\u5B54, SMA, PCB\\u5B89\\u88C5")
    (property "Height" "")
    (property "Manufacturer_Name" "Cinch Connectivity Solutions")
    (property "Manufacturer_Part_Number" "142-0701-801")
    (property "Mouser Part Number" "530-142-0701-801")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Johnson-Cinch-Connectivity-Solutions/142-0701-801?qs=PcPxjN2Z58KbDaDuDxyLHA%3D%3D")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "JOHNSON - 142-0701-801 - \\u5C04\\u9891/\\u540C\\u8F74\\u63D2\\u5B54, SMA, PCB\\u5B89\\u88C5")
    (fp_text reference "J1" (at 1.25 9.5 unlocked) (layer "F.SilkS"))
    (fp_text value "AMPHENOL_132357-11" (at 5.0927 -13.3985 -270 unlocked) (layer "F.SilkS") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 2.35 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(U1-A)") (pinfunction "1") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd rect locked (at 1.575 -4.25 270) (size 4.9 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd rect locked (at 1.575 -4.25 270) (size 4.9 1.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd rect locked (at 1.575 4.25 270) (size 4.9 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd rect locked (at 1.575 4.25 270) (size 4.9 1.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive") (thermal_bridge_angle 45))
    (model "${KIPRJMOD}/Library/3d/142-0701-801.stp"
      (offset (xyz -1 0 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 180))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 187.25 84.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?45199")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT .018uF 50volts 10%")
    (property "MPN" "VJ1206Y183KXAAC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C6" (at 3.25 10.25 90) (layer "F.SilkS"))
    (fp_text value "18nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 7 "Net-(IC2-INH)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 8 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" locked (layer "F.Cu")
    (at 123.75 73)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-89-3" (layer "F.Cu")
    (at 191.6125 75)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags "SOT-89-3")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "MD0100N8-G")
    (attr smd)
    (fp_text reference "U1" (at 3.6375 1.5) (layer "F.SilkS"))
    (fp_text value "MD0100N8-G" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.2 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.95 -1.5) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(U1-A)") (pinfunction "A") (pintype "unspecified"))
    (pad "2" smd custom (at -1.8625 0) (size 1.475 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "unconnected-(U1-COM-Pad2)") (pinfunction "COM") (pintype "unspecified+no_connect") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly
          (pts
            (xy 3.8625 0.8665)
            (xy 0.7375 0.8665)
            (xy 0.7375 -0.8665)
            (xy 3.8625 -0.8665)
          )
          (width 0) (fill yes))
      ))
    (pad "3" smd rect (at -1.95 1.5) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(U1-B)") (pinfunction "B") (pintype "unspecified"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 200.75 101.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C22" (at -10 1.25 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 25 "5VVGA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 193.75 93.25 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C24" (at -4.25 -5.25 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 26 "5VLNA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric" (layer "F.Cu")
    (at 189.75 79.75 -90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?34102")
    (property "Description" "Ferrite Beads 75ohms 25%")
    (property "Height" "1.05")
    (property "Manufacturer_Name" "Murata Electronics")
    (property "Manufacturer_Part_Number" "BLM21BB750SN1D")
    (property "Mouser Part Number" "81-BLM21B750S")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Murata-Electronics/BLM21BB750SN1D/?qs=Ncw4LTdqe05b2FdOdGUHhQ%3D%3D")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "25%")
    (property "ki_description" "BLM21_N1D Series EMI Suppression Filter 75+/-25% at 100MHz 700mA @85")
    (attr smd)
    (fp_text reference "FB2" (at 0 -2 -90) (layer "F.SilkS"))
    (fp_text value "ILHB1206ER750V" (at 0 1.9 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.575 0 270) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 27 "Net-(U1-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.575 0 270) (size 1.05 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2380952381)
      (net 6 "Net-(C5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 192.25 84.5 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 22pF 10volts C0G 5%")
    (property "MPN" "VJ1206A220JXQPW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C12" (at 3.75 9.5 90) (layer "F.SilkS"))
    (fp_text value "22pF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 7 "Net-(IC2-INH)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 90) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (at 130.46 73.38 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at -1.87 -2.33 180) (layer "F.SilkS"))
    (fp_text value "22-23-2021" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 181.5 101.5 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R5" (at -3.75 -4 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 25 "5VVGA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 43 "Net-(IC2-VPOS)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 187.5 109.75)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R10" (at 6.75 9.75) (layer "F.SilkS"))
    (fp_text value "18R" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 23 "Net-(IC1-VIN-)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 11 "TO_ADC_L") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 181.75 91.75 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C18" (at 2 7.75 90) (layer "F.SilkS"))
    (fp_text value "1nF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 21 "DAC_G") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 183.25 114.25)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C16" (at 5.5 0.25) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 19 "Net-(IC1-VREFB)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" locked (layer "F.Cu")
    (at 130.46 119.11 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J7" (at 1.36 -2.33 180) (layer "F.SilkS"))
    (fp_text value "22-23-2021" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 179.25 101.5 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R6" (at -3.7625 -3.25 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 25 "5VVGA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 42 "Net-(IC2-HILO)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 184 101.5 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R4" (at 10.5 -7.5 90) (layer "F.SilkS"))
    (fp_text value "100R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 28 "VOH") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 191.25 101.5 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R8" (at 10.5 -4.75 90) (layer "F.SilkS"))
    (fp_text value "100R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 29 "VOL") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 270) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 10 "Net-(C9-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "PICO_ADC_Test:RPi_Pico_SMD" locked (layer "F.Cu")
    (at 148.75 97 180)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 0) (layer "F.SilkS"))
    (fp_text value "Pico" (at 0 2.159) (layer "F.Fab"))
    (fp_text user "GP20" (at 13.054 11.43 45) (layer "F.SilkS"))
    (fp_text user "GP0" (at -12.8 -24.13 45) (layer "F.SilkS"))
    (fp_text user "GP6" (at -12.8 -3.81 45) (layer "F.SilkS"))
    (fp_text user "AGND" (at 13.054 -6.35 45) (layer "F.SilkS"))
    (fp_text user "SWDIO" (at 5.6 26.2) (layer "F.SilkS"))
    (fp_text user "GP11" (at -13.2 11.43 45) (layer "F.SilkS"))
    (fp_text user "GP21" (at 13.054 8.9 45) (layer "F.SilkS"))
    (fp_text user "GP1" (at -12.9 -21.6 45) (layer "F.SilkS"))
    (fp_text user "GP9" (at -12.8 3.81 45) (layer "F.SilkS"))
    (fp_text user "GP16" (at 13.054 24.13 45) (layer "F.SilkS"))
    (fp_text user "3V3" (at 12.9 -13.9 45) (layer "F.SilkS"))
    (fp_text user "SWCLK" (at -5.7 26.2) (layer "F.SilkS"))
    (fp_text user "GP3" (at -12.8 -13.97 45) (layer "F.SilkS"))
    (fp_text user "GP27" (at 13.054 -3.8 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 12.8 19.05 45) (layer "F.SilkS"))
    (fp_text user "GP2" (at -12.9 -16.51 45) (layer "F.SilkS"))
    (fp_text user "GP8" (at -12.8 1.27 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 12.8 6.35 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -12.8 -19.05 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 12.8 -19.05 45) (layer "F.SilkS"))
    (fp_text user "VBUS" (at 13.3 -24.2 45) (layer "F.SilkS"))
    (fp_text user "GP28" (at 13.054 -9.144 45) (layer "F.SilkS"))
    (fp_text user "GP13" (at -13.054 16.51 45) (layer "F.SilkS"))
    (fp_text user "GP5" (at -12.8 -8.89 45) (layer "F.SilkS"))
    (fp_text user "GP10" (at -13.054 8.89 45) (layer "F.SilkS"))
    (fp_text user "GP12" (at -13.2 13.97 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -12.8 -6.35 45) (layer "F.SilkS"))
    (fp_text user "ADC_VR" (at 13.5 -12 45) (layer "F.SilkS"))
    (fp_text user "VSYS" (at 13 -21.25 45) (layer "F.SilkS"))
    (fp_text user "GP19" (at 13.054 13.97 45) (layer "F.SilkS"))
    (fp_text user "GP26" (at 13.054 -1.27 45) (layer "F.SilkS"))
    (fp_text user "GP14" (at -13.1 21.59 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -12.8 19.05 45) (layer "F.SilkS"))
    (fp_text user "GP17" (at 13.054 21.59 45) (layer "F.SilkS"))
    (fp_text user "RUN" (at 13 1.27 45) (layer "F.SilkS"))
    (fp_text user "GP4" (at -12.8 -11.43 45) (layer "F.SilkS"))
    (fp_text user "GP18" (at 13.054 16.51 45) (layer "F.SilkS"))
    (fp_text user "GP7" (at -12.7 -1.3 45) (layer "F.SilkS"))
    (fp_text user "3V3_EN" (at 13.5 -17.25 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -12.8 6.35 45) (layer "F.SilkS"))
    (fp_text user "GP22" (at 13.054 3.81 45) (layer "F.SilkS"))
    (fp_text user "GP15" (at -13.054 24.13 45) (layer "F.SilkS"))
    (fp_text user "Copper Keepouts shown on Dwgs layer" (at 0.1 -30.2) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole oval locked (at -2.725 -24 180) (size 1.8 1.8) (drill 1.8) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole oval locked (at -2.425 -20.97 180) (size 1.5 1.5) (drill 1.5) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole oval locked (at 2.425 -20.97 180) (size 1.5 1.5) (drill 1.5) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole oval locked (at 2.725 -24 180) (size 1.8 1.8) (drill 1.8) (layers "*.Cu" "*.Mask"))
    (pad "1" smd roundrect locked (at -8.89 -24.13 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "ADC_CLK") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "2" smd roundrect locked (at -8.89 -21.59 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "D0") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -8.89 -19.05 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect locked (at -8.89 -16.51 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "D1") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at -8.89 -13.97 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "D2") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd roundrect locked (at -8.89 -11.43 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "D3") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd roundrect locked (at -8.89 -8.89 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "D4") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at -8.89 -6.35 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd roundrect locked (at -8.89 -3.81 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "D5") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "10" smd roundrect locked (at -8.89 -1.27 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "D6") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "11" smd roundrect locked (at -8.89 1.27 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "D7") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd roundrect locked (at -8.89 3.81 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "D8") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at -8.89 6.35 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect locked (at -8.89 8.89 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "D9") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "15" smd roundrect locked (at -8.89 11.43 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "GPIO11") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at -8.89 13.97 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "GPIO12") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "17" smd roundrect locked (at -8.89 16.51 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "CS") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "18" smd roundrect locked (at -8.89 19.05 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "19" smd roundrect locked (at -8.89 21.59 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "SCLK") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "20" smd roundrect locked (at -8.89 24.13 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "MOSI") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "21" smd roundrect locked (at 8.89 24.13 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "GPIO16") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "22" smd roundrect locked (at 8.89 21.59 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "GPIO17") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "23" smd roundrect locked (at 8.89 19.05 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "24" smd roundrect locked (at 8.89 16.51 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "GPIO18") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "25" smd roundrect locked (at 8.89 13.97 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "GPIO19") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "26" smd roundrect locked (at 8.89 11.43 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "GPIO20") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "27" smd roundrect locked (at 8.89 8.89 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "GPIO21") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "28" smd roundrect locked (at 8.89 6.35 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "29" smd roundrect locked (at 8.89 3.81 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "GPIO22") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "30" smd roundrect locked (at 8.89 1.27 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "unconnected-(U2-RUN-Pad30)") (pinfunction "RUN") (pintype "input+no_connect"))
    (pad "31" smd roundrect locked (at 8.89 -1.27 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "GPIO26") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "32" smd roundrect locked (at 8.89 -3.81 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "GPIO27") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "33" smd roundrect locked (at 8.89 -6.35 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "AGND") (pintype "power_in"))
    (pad "34" smd roundrect locked (at 8.89 -8.89 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "GPIO28") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "35" smd roundrect locked (at 8.89 -11.43 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "unconnected-(U2-ADC_VREF-Pad35)") (pinfunction "ADC_VREF") (pintype "power_in+no_connect"))
    (pad "36" smd roundrect locked (at 8.89 -13.97 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+3.3V") (pinfunction "3V3") (pintype "power_in"))
    (pad "37" smd roundrect locked (at 8.89 -16.51 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "unconnected-(U2-3V3_EN-Pad37)") (pinfunction "3V3_EN") (pintype "input+no_connect"))
    (pad "38" smd roundrect locked (at 8.89 -19.05 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "bidirectional"))
    (pad "39" smd roundrect locked (at 8.89 -21.59 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "unconnected-(U2-VSYS-Pad39)") (pinfunction "VSYS") (pintype "power_in+no_connect"))
    (pad "40" smd roundrect locked (at 8.89 -24.13 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "+5V") (pinfunction "VBUS") (pintype "power_in"))
    (pad "41" smd roundrect locked (at -2.54 23.9 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "SWCLK") (pinfunction "SWCLK") (pintype "input"))
    (pad "42" smd roundrect locked (at 0 23.9 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "43" smd roundrect locked (at 2.54 23.9 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "SWDIO") (pinfunction "SWDIO") (pintype "bidirectional"))
    (model "${KIPRJMOD}/Library/3d/Pico.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via" locked (layer "F.Cu")
    (at 201.75 73)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_3.2mm_M3_Pad_Via" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6.4 6.4) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle locked (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 177.5 93 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C19" (at 6.25 -0.25) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 22 "Net-(IC2-VCM)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 183.25 118.75)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C14" (at 5.5 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 17 "Net-(IC1-VREF)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 187.5 107.5)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R11" (at 6.75 10.25) (layer "F.SilkS"))
    (fp_text value "18R" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 24 "Net-(IC1-VIN+)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 4 "TO_ADC_H") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 187.5 105.25)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at 6.25 11) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 4 "TO_ADC_H") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (at 195.75 101.5 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "1%")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R2" (at -10.5 3.25 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 25 "5VVGA") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4625 0 90) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2222222222)
      (net 45 "Net-(IC2-ENBL)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Horizontal" locked (layer "F.Cu")
    (at 133 101.33)
    (descr "Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 2x06 2.54mm double row")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J6" (at -5.65 -2.77) (layer "F.SilkS") hide)
    (fp_text value "90122-0126" (at -5.65 15.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -8.315 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at -2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "+3.3V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "GPIO21") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "GPIO28") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "GPIO20") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "GPIO27") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "GPIO19") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "GPIO26") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "GPIO18") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "GPIO22") (pinfunction "Pin_12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 193.75 88 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "DATASHEET LINK" "https://www.vishay.com/doc?28548")
    (property "Description" "Multilayer Ceramic Capacitors MLCC - SMD/SMT 1206 0.1uF 10volts X7R 10%")
    (property "MPN" "VJ1206Y104KXQCW1BC")
    (property "Sheetfile" "PICO_ADC_Test.kicad_sch")
    (property "Sheetname" "")
    (property "Size" "1206")
    (property "Tolerance" "10%")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at -3.25 2) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "Net-(IC2-LMD)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 120.25 73) (mid 121.275126 70.525126) (end 123.75 69.5)
    (layer "Edge.Cuts"))
  (gr_line (start 120.25 120) (end 120.25 73)
    (layer "Edge.Cuts"))
  (gr_line (start 205.25 73) (end 205.25 120)
    (layer "Edge.Cuts"))
  (gr_line (start 123.75 69.5) (end 201.75 69.5)
    (layer "Edge.Cuts"))
  (gr_arc (start 201.75 69.5) (mid 204.224874 70.525126) (end 205.25 73)
    (layer "Edge.Cuts"))
  (gr_arc (start 123.75 123.5) (mid 121.275126 122.474874) (end 120.25 120)
    (layer "Edge.Cuts"))
  (gr_line (start 201.75 123.5) (end 123.75 123.5)
    (layer "Edge.Cuts"))
  (gr_arc (start 205.25 120) (mid 204.224874 122.474874) (end 201.75 123.5)
    (layer "Edge.Cuts"))
  (gr_text "SWDIO" (at 172.5 78.5 90) (layer "F.SilkS" knockout))
  (gr_text "+5V" (at 167.75 78.5 90) (layer "F.SilkS" knockout))
  (gr_text "SWCLK" (at 170.25 78.5 90) (layer "F.SilkS" knockout))
  (gr_text "GND\n" (at 175.25 78.5 90) (layer "F.SilkS" knockout))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 205.25 123.5) (xy 120.25 123.5))
    (height -4)
    (gr_text "85.0000 mm" (at 162.75 126.35) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 120.25 123.5) (xy 120.25 69.5))
    (height -5.25)
    (gr_text "54.0000 mm" (at 113.85 96.5 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type leader) (layer "Dwgs.User")
    (pts (xy 120.25 123.5) (xy 113 131.25))
    (gr_text "(0;0)" (at 100.3 131.25) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 0) (units_format 0) (precision 4) (override_value "(0;0)"))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (text_frame 0) (extension_offset 0.5))
  )
  (dimension (type radial) (layer "Dwgs.User")
    (pts (xy 201.75 120) (xy 204.5 122))
    (leader_length 3.81)
    (gr_text "R 3.5 mm" (at 215.25 124.240934) (layer "Dwgs.User"))
    (format (prefix "R ") (suffix "") (units 3) (units_format 1) (precision 4) (override_value "3.5"))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 127.45 73)
        (xy 127.45 70.5)
        (xy 187.639744 70.5)
        (xy 187.25 71.45)
        (xy 187.55 72.9)
        (xy 188.4 72.9)
        (xy 188.152941 70.5)
        (xy 193.746154 70.5)
        (xy 193.1 71.7)
        (xy 194.4 73.25)
        (xy 195.35 73.2)
        (xy 194.790244 70.5)
        (xy 198.05 70.5)
        (xy 198.05 73)
        (xy 198.853571 70.5)
        (xy 204.25 70.5)
        (xy 204.25 76.521428)
        (xy 201.75 76.7)
        (xy 204.25 76.7)
        (xy 204.25 104.96962)
        (xy 200.8 105.45)
        (xy 204.25 105.45)
        (xy 204.25 116.3)
        (xy 201.75 116.3)
        (xy 204.25 116.657142)
        (xy 204.25 122.5)
        (xy 198.600847 122.5)
        (xy 198.05 120)
        (xy 198.05 122.5)
        (xy 185.8 122.5)
        (xy 185.8 121.45)
        (xy 185.526087 122.5)
        (xy 180.739796 122.5)
        (xy 180.4 120.65)
        (xy 180.4 122.5)
        (xy 178.672989 122.5)
        (xy 177.75 122.5)
        (xy 173.75 122.5)
        (xy 172.75 122.5)
        (xy 169.35 122.5)
        (xy 169.35 121.4)
        (xy 169.13 122.5)
        (xy 156.6872 122.5)
        (xy 156.3 116.45)
        (xy 156.3 122.5)
        (xy 152.85 122.5)
        (xy 152.85 121)
        (xy 152.622727 122.5)
        (xy 144.922727 122.5)
        (xy 144.65 121)
        (xy 144.65 122.5)
        (xy 141.2 122.5)
        (xy 141.2 116.35)
        (xy 140.212409 122.5)
        (xy 131.2875 122.5)
        (xy 130.75 120.35)
        (xy 130.75 122.5)
        (xy 127.45 122.5)
        (xy 127.45 120)
        (xy 126.992254 122.5)
        (xy 121.25 122.5)
        (xy 121.25 116.732203)
        (xy 123.8 116.3)
        (xy 121.25 116.3)
        (xy 121.25 76.7)
        (xy 123.8 76.7)
        (xy 121.25 76.311016)
        (xy 121.25 70.5)
        (xy 126.815079 70.5)
      )
    )
    (polygon
      (pts
        (xy 182.75 114.25)
        (xy 181.85 121.9)
        (xy 183.65 121.9)
        (xy 183.65 113.35)
      )
    )
    (polygon
      (pts
        (xy 145.1 120.15)
        (xy 145.35 119.95)
        (xy 145.1 118)
      )
    )
    (polygon
      (pts
        (xy 152.2 120.1)
        (xy 152.4 120.1)
        (xy 152.4 117.95)
      )
    )
    (polygon
      (pts
        (xy 170 118.9)
        (xy 170.8 118.55)
        (xy 169.75 118.55)
      )
    )
    (polygon
      (pts
        (xy 136.7 117.75)
        (xy 133 117.75)
        (xy 136.7 117.98125)
        (xy 136.7 118)
        (xy 136.8 117.9875)
        (xy 137 118)
        (xy 137 117.9625)
        (xy 137.1 117.95)
        (xy 136.7 116.35)
      )
    )
    (polygon
      (pts
        (xy 131.15 117.85)
        (xy 133 117.75)
        (xy 131.15 117.75)
      )
    )
    (polygon
      (pts
        (xy 160 117)
        (xy 160.5 117)
        (xy 160.5 115.25)
        (xy 159.75 115)
      )
    )
    (polygon
      (pts
        (xy 151.15 116.9)
        (xy 151.15 116.75)
        (xy 146.35 116.75)
      )
    )
    (polygon
      (pts
        (xy 141.2 115.8)
        (xy 141.2 103.75)
        (xy 141.05 103.75)
      )
    )
    (polygon
      (pts
        (xy 136.7 114.7875)
        (xy 133 115.25)
        (xy 136.7 115.25)
        (xy 136.7 115.75)
        (xy 136.744118 115.25)
        (xy 137 115.25)
        (xy 137 114.75)
        (xy 136.785873 114.776765)
        (xy 137.15 110.65)
        (xy 136.7 106.7)
      )
    )
    (polygon
      (pts
        (xy 156.3 115.65)
        (xy 156.45 115.65)
        (xy 156.3 103.8)
      )
    )
    (polygon
      (pts
        (xy 130.45 115.35)
        (xy 132.25 115.35)
        (xy 132.35 115.2)
      )
    )
    (polygon
      (pts
        (xy 134.35 114)
        (xy 134.35 104.15)
        (xy 134.1 104.15)
      )
    )
    (polygon
      (pts
        (xy 181.7 113.1)
        (xy 183.65 113.35)
        (xy 183.85 112.85)
        (xy 181.7 112.85)
      )
    )
    (polygon
      (pts
        (xy 171.05 113.25)
        (xy 173.55 113.25)
        (xy 173.6 113.1)
      )
    )
    (polygon
      (pts
        (xy 179.45 113.1)
        (xy 180.95 112.85)
        (xy 179.35 112.85)
      )
    )
    (polygon
      (pts
        (xy 129.1 111.2)
        (xy 129.25 111.2)
        (xy 129.1 101.35)
      )
    )
    (polygon
      (pts
        (xy 186.1 111.1)
        (xy 189.05 111.1)
        (xy 186 110.95)
      )
    )
    (polygon
      (pts
        (xy 192.65 107.5)
        (xy 192.65 104.7)
        (xy 192.5 104.65)
      )
    )
    (polygon
      (pts
        (xy 174.35 105.3)
        (xy 183.65 105.3)
        (xy 183.65 106.45)
        (xy 184.5 106.35)
        (xy 183.838889 105.3)
        (xy 184 105.3)
        (xy 184.15 104.75)
      )
    )
    (polygon
      (pts
        (xy 166.5 104.75)
        (xy 168 104.75)
        (xy 166.5 104.5)
      )
    )
    (polygon
      (pts
        (xy 135.9 102.6)
        (xy 136.25 104.25)
        (xy 137.5 104.55)
        (xy 138.55 103.95)
        (xy 138.05 102.35)
      )
    )
    (polygon
      (pts
        (xy 159.75 103)
        (xy 159.75 103.75)
        (xy 160.5 104)
        (xy 160.5 102.75)
      )
    )
    (polygon
      (pts
        (xy 134.2 103.6)
        (xy 135.2 103.6)
        (xy 135.25 103.5)
      )
    )
    (polygon
      (pts
        (xy 141.2 103.05)
        (xy 141.2 91.15)
        (xy 141 91.15)
      )
    )
    (polygon
      (pts
        (xy 156.3 103)
        (xy 156.55 102.9)
        (xy 156.3 90.95)
      )
    )
    (polygon
      (pts
        (xy 166.4 100.45)
        (xy 166.85 101.25)
        (xy 170.95 101.4)
        (xy 171.1 100.35)
      )
    )
    (polygon
      (pts
        (xy 174.5 101)
        (xy 175.4375 100.875)
        (xy 176.75 101.25)
        (xy 178.25 100.5)
        (xy 174.4 100.5)
      )
    )
    (polygon
      (pts
        (xy 197.25 101.15)
        (xy 201.45 101.05)
        (xy 201.3 100.3)
        (xy 197.2 100.3)
      )
    )
    (polygon
      (pts
        (xy 135.6 100)
        (xy 130.45 100)
        (xy 135.6 100.551785)
        (xy 135.6 100.85)
        (xy 135.608679 100.552715)
        (xy 136.05 100.6)
        (xy 135.85 100)
        (xy 135.624818 100)
        (xy 135.8 94)
      )
    )
    (polygon
      (pts
        (xy 172.15 100.45)
        (xy 173.15 100.2)
        (xy 172.15 100.2)
      )
    )
    (polygon
      (pts
        (xy 168.35 99.1)
        (xy 169.4 98.95)
        (xy 168.35 98.95)
      )
    )
    (polygon
      (pts
        (xy 171.6 99.1)
        (xy 171.65 98.95)
        (xy 170.65 98.95)
      )
    )
    (polygon
      (pts
        (xy 176.45 99.1)
        (xy 176.75 99.1)
        (xy 177.636364 99.1)
        (xy 178.1 99.1)
        (xy 178.4 98.625)
        (xy 176.45 91.9)
      )
    )
    (polygon
      (pts
        (xy 131.2 97.6)
        (xy 133 97.6)
        (xy 131.2 97.35)
      )
    )
    (polygon
      (pts
        (xy 131.15 95.1)
        (xy 135 94.9)
        (xy 131.15 94.9)
      )
    )
    (polygon
      (pts
        (xy 192.35 94.4)
        (xy 192.55 94.35)
        (xy 193 92.9)
        (xy 192.35 92.85)
      )
    )
    (polygon
      (pts
        (xy 193.1 94.05)
        (xy 193.55 94.4)
        (xy 196.95 94.4)
        (xy 196.8 93.85)
      )
    )
    (polygon
      (pts
        (xy 199.35 91.8)
        (xy 199 93.2)
        (xy 199.3 93.75)
        (xy 200.8 93)
        (xy 199.7 93)
        (xy 199.7 91.7)
      )
    )
    (polygon
      (pts
        (xy 136.7 93.2)
        (xy 137 92.85)
        (xy 137.25 91.85)
        (xy 136.7 91.05)
      )
    )
    (polygon
      (pts
        (xy 181.1 92.5)
        (xy 181.2 92.85)
        (xy 182.3 92.8)
        (xy 182.3 92.45)
      )
    )
    (polygon
      (pts
        (xy 183.15 92.85)
        (xy 183.15 91.8)
        (xy 184.6 91.8)
        (xy 184.6 91.6)
        (xy 182.75 91.45)
      )
    )
    (polygon
      (pts
        (xy 160.55 92.55)
        (xy 160.8 92.55)
        (xy 160.8 91.05)
      )
    )
    (polygon
      (pts
        (xy 177.65 91.6)
        (xy 176.4 91.6)
        (xy 177.65 91.713636)
        (xy 177.65 92.15)
        (xy 178.062983 91.844751)
        (xy 178.6 91.8)
        (xy 178.65 91.6)
        (xy 178.490909 91.6)
        (xy 178.463098 91.549014)
        (xy 178.8 91.3)
        (xy 177.65 86.1)
      )
    )
    (polygon
      (pts
        (xy 159.25 91.5)
        (xy 160.5 91.5)
        (xy 160.5 89.5)
        (xy 159.25 89.5)
      )
    )
    (polygon
      (pts
        (xy 194.25 90.95)
        (xy 194.95 90.85)
        (xy 194.95 89.15)
      )
    )
    (polygon
      (pts
        (xy 194.25 90.95)
        (xy 193.9 90)
        (xy 193.3 90)
      )
    )
    (polygon
      (pts
        (xy 171.1 90.65)
        (xy 171.4 90.4)
        (xy 171.1 88.75)
      )
    )
    (polygon
      (pts
        (xy 129.1 90.4)
        (xy 129.2 90.4)
        (xy 129.1 88.9)
      )
    )
    (polygon
      (pts
        (xy 141.2 90.4)
        (xy 141.2 78.35)
        (xy 141 78.35)
      )
    )
    (polygon
      (pts
        (xy 131.6 90.2)
        (xy 131.8 90.25)
        (xy 131.8 88.9)
      )
    )
    (polygon
      (pts
        (xy 156.3 90.25)
        (xy 156.5 78.35)
        (xy 156.3 78.3)
      )
    )
    (polygon
      (pts
        (xy 160.8 90.25)
        (xy 160.8 88.45)
        (xy 160.7 88.45)
      )
    )
    (polygon
      (pts
        (xy 135.6 89)
        (xy 135.75 89)
        (xy 135.6 81.25)
      )
    )
    (polygon
      (pts
        (xy 162.121483 75.010123)
        (xy 162 75)
        (xy 162 75.25)
        (xy 162.108075 75.25)
        (xy 161.7 82.55)
        (xy 162.15 88.75)
        (xy 162.15 75.25)
        (xy 165 75.25)
        (xy 162.15 75.0125)
        (xy 162.15 74.5)
      )
    )
    (polygon
      (pts
        (xy 194.3 87.6)
        (xy 194.5 88.6)
        (xy 194.75 88.6)
        (xy 194.7 87.45)
      )
    )
    (polygon
      (pts
        (xy 171.75 88.45)
        (xy 173.5 88.15)
        (xy 173.55 82.1)
        (xy 171.75 82.1)
      )
    )
    (polygon
      (pts
        (xy 129.1 88.35)
        (xy 129.35 80.45)
        (xy 129.1 80.3)
      )
    )
    (polygon
      (pts
        (xy 131.65 88.35)
        (xy 131.8 88.35)
        (xy 131.8 78.95)
      )
    )
    (polygon
      (pts
        (xy 193.25 87)
        (xy 194.45 87.1)
        (xy 194.85 86.6)
        (xy 193.5 86.6)
      )
    )
    (polygon
      (pts
        (xy 177.65 85.7)
        (xy 178 85.6)
        (xy 177.65 83.2)
      )
    )
    (polygon
      (pts
        (xy 191.8 85.1)
        (xy 192 85.15)
        (xy 192 83.9)
      )
    )
    (polygon
      (pts
        (xy 187.05 81.65)
        (xy 183.15 81.65)
        (xy 183.15 82)
        (xy 187.05 81.662962)
        (xy 187.05 82.15)
        (xy 187.35 82.15)
        (xy 187.05 78.2)
      )
    )
    (polygon
      (pts
        (xy 188.3 82)
        (xy 188.5 82)
        (xy 188.3 79)
      )
    )
    (polygon
      (pts
        (xy 190.65 76.2)
        (xy 191.2 81.1)
        (xy 191.2 76.15)
      )
    )
    (polygon
      (pts
        (xy 136.75 80.25)
        (xy 137 80.25)
        (xy 136.75 78.3)
      )
    )
    (polygon
      (pts
        (xy 187.05 78.2)
        (xy 187.3 78.05)
        (xy 187.05 75.15)
      )
    )
    (polygon
      (pts
        (xy 141.2 77.65)
        (xy 141.2 72.95)
        (xy 141.05 72.95)
      )
    )
    (polygon
      (pts
        (xy 156.3 76.290872)
        (xy 150.6 76.65)
        (xy 156.3 76.65)
        (xy 156.3 77.6)
        (xy 156.329082 76.65)
        (xy 156.55 76.65)
        (xy 156.79 76.26)
        (xy 156.340152 76.288342)
        (xy 156.45 72.7)
        (xy 156.3 72.7)
      )
    )
    (polygon
      (pts
        (xy 135.3 77.15)
        (xy 136.95 77.15)
        (xy 137 77)
      )
    )
    (polygon
      (pts
        (xy 147.75 75.5)
        (xy 148.25 75.5)
        (xy 148.25 74.25)
      )
    )
    (polygon
      (pts
        (xy 149.25 74.445)
        (xy 149.15 74.45)
        (xy 149.25 74.45)
        (xy 149.25 75.5)
        (xy 149.75 75.5)
        (xy 149.33 74.45)
        (xy 152.2 74.45)
        (xy 152.15 74.3)
        (xy 149.32647 74.441176)
        (xy 149.25 74.25)
      )
    )
    (polygon
      (pts
        (xy 131.2 74.7)
        (xy 133 74.7)
        (xy 133 74.55)
      )
    )
    (polygon
      (pts
        (xy 131.4 72.25)
        (xy 133 72.05)
        (xy 131.3 72.05)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "In1.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 127.45 73.05)
        (xy 127.45 70.5)
        (xy 165.6 70.5)
        (xy 165.6 71.45)
        (xy 165.8 71.45)
        (xy 165.641667 70.5)
        (xy 175.761111 70.5)
        (xy 175.9 71.75)
        (xy 175.9 70.5)
        (xy 198.05 70.5)
        (xy 198.05 73)
        (xy 198.841667 70.5)
        (xy 204.25 70.5)
        (xy 204.25 76.360869)
        (xy 201.65 76.7)
        (xy 204.25 76.7)
        (xy 204.25 97.35)
        (xy 203.3 97.35)
        (xy 204.25 97.556521)
        (xy 204.25 98.91)
        (xy 203.25 99.15)
        (xy 204.25 99.15)
        (xy 204.25 116.3)
        (xy 201.75 116.3)
        (xy 204.25 116.607017)
        (xy 204.25 122.5)
        (xy 198.558475 122.5)
        (xy 198.05 120)
        (xy 198.05 122.5)
        (xy 152.85 122.5)
        (xy 152.85 120.95)
        (xy 152.677778 122.5)
        (xy 144.914706 122.5)
        (xy 144.65 121)
        (xy 144.65 122.5)
        (xy 127.45 122.5)
        (xy 127.45 120)
        (xy 126.99918 122.5)
        (xy 121.25 122.5)
        (xy 121.25 116.645762)
        (xy 123.8 116.3)
        (xy 121.25 116.3)
        (xy 121.25 76.7)
        (xy 123.8 76.7)
        (xy 121.25 76.440677)
        (xy 121.25 70.5)
        (xy 126.92381 70.5)
      )
    )
    (polygon
      (pts
        (xy 131.1 120.45)
        (xy 133 120.45)
        (xy 131.15 120.3)
      )
    )
    (polygon
      (pts
        (xy 152.05 120.1)
        (xy 152.4 120.1)
        (xy 152.4 117.95)
      )
    )
    (polygon
      (pts
        (xy 145.1 120)
        (xy 145.45 119.95)
        (xy 145.1 118)
      )
    )
    (polygon
      (pts
        (xy 151.45 119.75)
        (xy 151.45 119.6)
        (xy 146.15 119.6)
      )
    )
    (polygon
      (pts
        (xy 131.3 117.9)
        (xy 133 117.75)
        (xy 131.35 117.75)
      )
    )
    (polygon
      (pts
        (xy 146.35 116.95)
        (xy 151.2 116.75)
        (xy 146.35 116.75)
      )
    )
    (polygon
      (pts
        (xy 130.5 115.35)
        (xy 132.15 115.35)
        (xy 132.2 115.2)
      )
    )
    (polygon
      (pts
        (xy 132.15 115.35)
        (xy 133 115.35)
        (xy 133 115.25)
      )
    )
    (polygon
      (pts
        (xy 129.1 114.05)
        (xy 129.2 114.05)
        (xy 129.1 111.75)
      )
    )
    (polygon
      (pts
        (xy 134.328703 111.941666)
        (xy 134.2 113.1)
        (xy 134.340404 113.1)
        (xy 134.35 114.05)
        (xy 134.35 104.15)
        (xy 134.25 104.15)
      )
    )
    (polygon
      (pts
        (xy 129.1 111.75)
        (xy 129.3 104.15)
        (xy 129.1 104.15)
      )
    )
    (polygon
      (pts
        (xy 129.1 103.6)
        (xy 129.2 103.6)
        (xy 129.1 101.3)
      )
    )
    (polygon
      (pts
        (xy 134.2 103.55)
        (xy 134.35 103.6)
        (xy 134.35 102.1)
      )
    )
    (polygon
      (pts
        (xy 133 100.15)
        (xy 133 100)
        (xy 130.45 100)
      )
    )
    (polygon
      (pts
        (xy 131.3 97.6)
        (xy 132.95 97.6)
        (xy 132.95 97.45)
      )
    )
    (polygon
      (pts
        (xy 132.95 95.05)
        (xy 132.9 94.9)
        (xy 131.3 94.9)
      )
    )
    (polygon
      (pts
        (xy 131.777157 88.9)
        (xy 131.7 88.9)
        (xy 131.791566 90.319277)
        (xy 131.8 91.15)
        (xy 131.8 81.3)
        (xy 131.7 81.3)
      )
    )
    (polygon
      (pts
        (xy 129.1 91.1)
        (xy 129.103571 90.75)
        (xy 129.3 90.75)
        (xy 129.120512 89.089743)
        (xy 129.2 81.3)
        (xy 129.1 81.3)
      )
    )
    (polygon
      (pts
        (xy 171.1 90.6)
        (xy 171.35 88.8)
        (xy 171.1 88.8)
      )
    )
    (polygon
      (pts
        (xy 129.1 80.75)
        (xy 129.2 80.75)
        (xy 129.1 79.15)
      )
    )
    (polygon
      (pts
        (xy 131.6 80.65)
        (xy 131.7 80.75)
        (xy 131.8 80.75)
        (xy 131.8 79.1)
      )
    )
    (polygon
      (pts
        (xy 131.15 74.7)
        (xy 133 74.7)
        (xy 131.2 74.6)
      )
    )
    (polygon
      (pts
        (xy 167.7 73.35)
        (xy 169.5 73.35)
        (xy 167.6 73.2)
      )
    )
    (polygon
      (pts
        (xy 169.5 73.35)
        (xy 174.3 73.35)
        (xy 174.25 73.2)
      )
    )
    (polygon
      (pts
        (xy 133 72.15)
        (xy 133 72.05)
        (xy 131.3 72.05)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "In2.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 127.3 72.95)
        (xy 127.45 73)
        (xy 127.45 70.5)
        (xy 130.7 70.5)
        (xy 130.7 72.25)
        (xy 130.95 72.25)
        (xy 130.713514 70.5)
        (xy 175.828261 70.5)
        (xy 175.6 71.55)
        (xy 175.85 71.7)
        (xy 175.85 70.5)
        (xy 198.05 70.5)
        (xy 198.05 73.1)
        (xy 198.2 73.05)
        (xy 198.068103 70.5)
        (xy 204.25 70.5)
        (xy 204.25 76.517857)
        (xy 201.7 76.7)
        (xy 204.25 76.7)
        (xy 204.25 95.45)
        (xy 203.35 95.45)
        (xy 204.25 95.684782)
        (xy 204.25 98.821428)
        (xy 203.25 99.25)
        (xy 204.25 99.25)
        (xy 204.25 116.3)
        (xy 201.75 116.3)
        (xy 204.25 116.572727)
        (xy 204.25 122.5)
        (xy 198.284375 122.5)
        (xy 198.05 120)
        (xy 198.05 122.5)
        (xy 152.85 122.5)
        (xy 152.85 120.95)
        (xy 152.452564 122.5)
        (xy 144.737879 122.5)
        (xy 144.65 121.05)
        (xy 144.65 122.5)
        (xy 127.45 122.5)
        (xy 127.45 120)
        (xy 127.125926 122.5)
        (xy 121.25 122.5)
        (xy 121.25 116.607017)
        (xy 123.75 116.3)
        (xy 121.25 116.3)
        (xy 121.25 76.7)
        (xy 123.7 76.7)
        (xy 121.25 76.382407)
        (xy 121.25 70.5)
        (xy 127.426724 70.5)
      )
    )
    (polygon
      (pts
        (xy 145.1 120.15)
        (xy 145.35 120.05)
        (xy 145.1 117.95)
      )
    )
    (polygon
      (pts
        (xy 152.1 119.95)
        (xy 152.4 120)
        (xy 152.4 118)
      )
    )
    (polygon
      (pts
        (xy 134.35 119.1)
        (xy 134.35 115.05)
        (xy 134.2 115)
      )
    )
    (polygon
      (pts
        (xy 130.75 118)
        (xy 131.05 118.05)
        (xy 130.75 117)
      )
    )
    (polygon
      (pts
        (xy 151.15 116.95)
        (xy 151.15 116.75)
        (xy 146.35 116.75)
      )
    )
    (polygon
      (pts
        (xy 133.9 112.65)
        (xy 134.35 114.9)
        (xy 134.35 111.8)
      )
    )
    (polygon
      (pts
        (xy 128.05 112)
        (xy 129.3 111.75)
        (xy 128.1 111.75)
      )
    )
    (polygon
      (pts
        (xy 129.15 103.358064)
        (xy 128.3 103.55)
        (xy 129.15 104.274074)
        (xy 129.15 111.2)
        (xy 129.25 111.2)
        (xy 129.180301 104.299886)
        (xy 129.65 104.7)
        (xy 130.2 104.25)
        (xy 129.85 103.2)
        (xy 129.170741 103.353381)
        (xy 129.15 101.3)
      )
    )
    (polygon
      (pts
        (xy 134.2 111.2)
        (xy 134.35 111.2)
        (xy 134.35 104.15)
      )
    )
    (polygon
      (pts
        (xy 134.15 102.3)
        (xy 134.35 103.6)
        (xy 134.35 102.25)
      )
    )
    (polygon
      (pts
        (xy 133 100.1)
        (xy 133 100)
        (xy 130.45 100)
      )
    )
    (polygon
      (pts
        (xy 131.25 97.6)
        (xy 133.05 97.6)
        (xy 131.2 97.4)
      )
    )
    (polygon
      (pts
        (xy 127.85 92.55)
        (xy 132.1 92.55)
        (xy 127.85 92.1)
      )
    )
    (polygon
      (pts
        (xy 129.4 89.55)
        (xy 130.75 89.45)
        (xy 130.7 88.35)
        (xy 129.7 87.7)
      )
    )
    (polygon
      (pts
        (xy 162.15 84.75)
        (xy 162.15 82.45)
        (xy 162 82.45)
      )
    )
    (polygon
      (pts
        (xy 160.35 84.7)
        (xy 160.65 82)
        (xy 160.35 82)
      )
    )
    (polygon
      (pts
        (xy 174.05 75.9)
        (xy 174.3 75.9)
        (xy 174.3 73.2)
      )
    )
    (polygon
      (pts
        (xy 129.1 75.2)
        (xy 129.35 75.2)
        (xy 129.1 74.15)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 127.45 72.9)
        (xy 127.45 70.5)
        (xy 146.6 70.5)
        (xy 146.602326 70.5)
        (xy 175.722222 70.5)
        (xy 175.9 71.7)
        (xy 175.9 70.5)
        (xy 198.05 70.5)
        (xy 198.05 72.9)
        (xy 198.573636 70.5)
        (xy 204.25 70.5)
        (xy 204.25 76.51132)
        (xy 201.75 76.7)
        (xy 204.25 76.7)
        (xy 204.25 116.3)
        (xy 201.75 116.3)
        (xy 204.25 116.511864)
        (xy 204.25 122.5)
        (xy 198.388983 122.5)
        (xy 198.05 120)
        (xy 198.05 122.5)
        (xy 152.85 122.5)
        (xy 152.85 121.05)
        (xy 152.569355 122.5)
        (xy 144.958824 122.5)
        (xy 144.65 121)
        (xy 144.65 122.5)
        (xy 127.45 122.5)
        (xy 127.45 120)
        (xy 127.062069 122.5)
        (xy 121.25 122.5)
        (xy 121.25 116.563157)
        (xy 123.75 116.3)
        (xy 121.25 116.3)
        (xy 121.25 76.7)
        (xy 123.8 76.7)
        (xy 121.25 76.431578)
        (xy 121.25 70.5)
        (xy 127.100909 70.5)
      )
    )
    (polygon
      (pts
        (xy 145.1 120.2)
        (xy 145.45 119.95)
        (xy 145.1 118)
      )
    )
    (polygon
      (pts
        (xy 151.9 119.8)
        (xy 152.4 120.1)
        (xy 152.4 117.95)
      )
    )
    (polygon
      (pts
        (xy 151.2 116.9)
        (xy 151.2 116.7)
        (xy 146.35 116.7)
      )
    )
    (polygon
      (pts
        (xy 130.45 115.35)
        (xy 132.2 115.35)
        (xy 132.45 115.15)
      )
    )
    (polygon
      (pts
        (xy 129.1 114.05)
        (xy 129.25 114.05)
        (xy 129.1 111.75)
      )
    )
    (polygon
      (pts
        (xy 134.2 113.2)
        (xy 134.35 113.35)
        (xy 134.35 111.75)
      )
    )
    (polygon
      (pts
        (xy 129.1 111.25)
        (xy 129.4 111.25)
        (xy 129.1 101.3)
      )
    )
    (polygon
      (pts
        (xy 133.95 111.2)
        (xy 134.35 111.2)
        (xy 134.35 108.45)
      )
    )
    (polygon
      (pts
        (xy 179.3 105.15)
        (xy 181.5 105.15)
        (xy 181.5 105)
      )
    )
    (polygon
      (pts
        (xy 181.5 103.5)
        (xy 181.45 103.35)
        (xy 179.25 103.35)
      )
    )
    (polygon
      (pts
        (xy 130.5 100)
        (xy 136 100.5)
        (xy 136 100)
      )
    )
    (polygon
      (pts
        (xy 131.3 97.6)
        (xy 133 97.6)
        (xy 133 97.5)
      )
    )
    (polygon
      (pts
        (xy 131.3 95)
        (xy 132.95 94.9)
        (xy 131.3 94.9)
      )
    )
    (polygon
      (pts
        (xy 171.1 90.55)
        (xy 171.3 90.5)
        (xy 171.1 88.85)
      )
    )
    (polygon
      (pts
        (xy 129.1 90.45)
        (xy 129.2 88.9)
        (xy 129.1 88.9)
      )
    )
    (polygon
      (pts
        (xy 131.8 90.35)
        (xy 131.8 88.9)
        (xy 131.7 88.9)
      )
    )
    (polygon
      (pts
        (xy 135.6 88.95)
        (xy 135.65 88.95)
        (xy 135.6 81.2)
      )
    )
    (polygon
      (pts
        (xy 129.1 88.35)
        (xy 129.35 88.3)
        (xy 129.1 78.45)
      )
    )
    (polygon
      (pts
        (xy 131.75 88.35)
        (xy 131.75 85.65)
        (xy 131.4 85.65)
      )
    )
    (polygon
      (pts
        (xy 162.05 84.75)
        (xy 162.15 84.75)
        (xy 162.15 82.5)
      )
    )
    (polygon
      (pts
        (xy 160.4 79.7)
        (xy 160.55 79.7)
        (xy 160.35 74.45)
      )
    )
    (polygon
      (pts
        (xy 135.5 77.35)
        (xy 135.55 77.15)
        (xy 131.1 77.15)
      )
    )
    (polygon
      (pts
        (xy 167.75 73.35)
        (xy 174.3 73.35)
        (xy 174.3 73.2)
      )
    )
  )
)
