(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.05)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C5-Pad2)")
  (net 2 "GND")
  (net 3 "24V")
  (net 4 "DF_5V")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(D7-Pad1)")
  (net 7 "Net-(J4-Pad2)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(D3-Pad1)")
  (net 11 "Net-(D4-Pad1)")
  (net 12 "Net-(J4-Pad3)")
  (net 13 "RESET")
  (net 14 "5V")
  (net 15 "Net-(D3-Pad2)")
  (net 16 "Net-(D5-Pad1)")
  (net 17 "Net-(D8-Pad1)")
  (net 18 "Net-(D9-Pad1)")
  (net 19 "O_INFO")
  (net 20 "MOSI")
  (net 21 "I_FORK1")
  (net 22 "Player_RX")
  (net 23 "Player_TX")
  (net 24 "Net-(R3-Pad1)")
  (net 25 "Net-(Q1-Pad2)")
  (net 26 "Net-(Q1-Pad1)")
  (net 27 "Net-(F1-Pad1)")
  (net 28 "Net-(R7-Pad1)")
  (net 29 "Net-(R9-Pad2)")
  (net 30 "unconnected-(RV1-Pad3)")
  (net 31 "unconnected-(U5-Pad4)")
  (net 32 "unconnected-(U5-Pad5)")
  (net 33 "unconnected-(U5-Pad7)")
  (net 34 "unconnected-(U5-Pad8)")
  (net 35 "unconnected-(U5-Pad16)")
  (net 36 "unconnected-(U5-Pad13)")
  (net 37 "unconnected-(U5-Pad12)")
  (net 38 "unconnected-(U5-Pad11)")
  (net 39 "unconnected-(U5-Pad9)")
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 51.2 65.7)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 5.8 10.3) (layer "F.SilkS"))
    (fp_text value "ATtiny85-20P" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "RESET") (pinfunction "~{RESET}/PB5") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Player_RX") (pinfunction "XTAL1/PB3") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Player_TX") (pinfunction "XTAL2/PB4") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "MOSI") (pinfunction "AREF/PB0") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "O_INFO") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "I_FORK1") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-89-3_Handsoldering" (layer "F.Cu")
    (tedit 5C33D6DD)
    (at 72 76.4 180)
    (descr "SOT-89-3 Handsoldering")
    (tags "SOT-89-3 Handsoldering")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at -0.5 3.5) (layer "F.SilkS"))
    (fp_text value "BCX 55 SMD" (at 0.3 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.5 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.15 -1.5 180) (size 2.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(Q1-Pad1)") (pinfunction "C") (pintype "passive"))
    (pad "2" smd custom (at -2.0625 0 180) (size 2.475 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(Q1-Pad2)") (pinfunction "B") (pintype "input") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 5.3625 0.8665)
            (xy 1.2375 0.8665)
            (xy 1.2375 -0.8665)
            (xy 5.3625 -0.8665)
          ) (width 0) (fill yes))
      ))
    (pad "3" smd rect (at -2.15 1.5 180) (size 2.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF_Handsoldering" (layer "F.Cu")
    (tedit 5905D919)
    (at 110.55 78.5)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.75) (layer "F.SilkS"))
    (fp_text value "LL4148" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.75) (layer "F.Fab"))
    (pad "1" smd rect (at -2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420)
    (at 76.5 89.4 -90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.77 90) (layer "F.SilkS"))
    (fp_text value "Phone AB" (at 0 5.31 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MELF_MMB-0207" (layer "F.Cu")
    (tedit 58FE61C0)
    (at 78 81.4 90)
    (descr "Resistor, MELF, MMB-0207, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MELF Resistor")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at -3 2.5 180) (layer "F.SilkS"))
    (fp_text value "VIT ZC207 15K" (at 0 2.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.45 0 90) (size 2.1 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 2.45 0 90) (size 2.1 2.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MELF_MMB-0207.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 104.5 63 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D7" (at -1 -2 90) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 6 "Net-(D7-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "DF_5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.5 62 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 3 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 14 "5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 13 "RESET") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.5 68)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -3 -0.5) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 22 "Player_RX") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 29 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 79.5 67.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "560R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 28 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 5 "Net-(C5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.25 90.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 3 0.5) (layer "F.SilkS"))
    (fp_text value "180R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 8 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF_Handsoldering" (layer "F.Cu")
    (tedit 5905D919)
    (at 110.53 85.5)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0 -1.75) (layer "F.SilkS"))
    (fp_text value "LL4148" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.75) (layer "F.Fab"))
    (pad "1" smd rect (at -2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D4-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-4_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 66.8 83.675 180)
    (descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 5.8 -2.33) (layer "F.SilkS"))
    (fp_text value "KB817" (at 3.81 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "3" thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "I_FORK1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 71.5 81)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 3 0.5) (layer "F.SilkS"))
    (fp_text value "100R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 8 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 24 "Net-(R3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_ACP_CA6-H2,5_Horizontal" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 89 64.575 -90)
    (descr "Potentiometer, horizontal, ACP CA6-H2,5, http://www.acptechnologies.com/wp-content/uploads/2017/06/01-ACP-CA6.pdf")
    (tags "Potentiometer horizontal ACP CA6-H2,5")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV1" (at 0 -2.06 90) (layer "F.SilkS"))
    (fp_text value "4k7" (at 0 7.06 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 2.5 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D3-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 2.5 270) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(R7-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5 270) (size 1.62 1.62) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "unconnected-(RV1-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_ACP_CA6-H2,5_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.5 67 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0.5 2 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 6 "Net-(D7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT" (layer "F.Cu")
    (tedit 5B741BB0)
    (at 126.553 70.5)
    (descr "DCDC-Converter, RECOM, RECOM_R-78E-0.5, SIP-3, pitch 2.54mm, package size 11.6x8.5x10.4mm^3, https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf")
    (tags "dc-dc recom buck sip-3 pitch 2.54mm")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -2.553 3.5) (layer "F.SilkS"))
    (fp_text value "R-78E5.0-0.5" (at 2.54 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.25) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 3 "24V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 14 "5V") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_RECOM_R-78E-0.5_THT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 64 63 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at -1 2 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 17 "Net-(D8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420)
    (at 132.5 82.96)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "24VDC" (at 0 5.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(F1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A425)
    (at 54.29 78.475)
    (descr "Through hole straight socket strip, 2x03, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x03 2.54mm double row")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -1.27 -2.77) (layer "F.SilkS"))
    (fp_text value "AVR-ISP-6" (at -1.27 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "O_INFO") (pinfunction "MISO") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "5V") (pinfunction "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "I_FORK1") (pinfunction "SCK") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "MOSI") (pinfunction "MOSI") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "RESET") (pinfunction "~{RST}") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.5 67 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0.5 2 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 18 "Net-(D9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 55 87.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 21 "I_FORK1") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 14 "5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF_Handsoldering" (layer "F.Cu")
    (tedit 5905D919)
    (at 110.5 89)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0 -1.75) (layer "F.SilkS"))
    (fp_text value "LL4148" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.75) (layer "F.Fab"))
    (pad "1" smd rect (at -2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(D5-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L4.6mm_W5.5mm_P2.50mm_MKS02_FKP02" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 73 67.4 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*5.5mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 5.5mm Capacitor")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at -2.5 2 180) (layer "F.SilkS"))
    (fp_text value "1u" (at 1.25 4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W5.5mm_P2.50mm_MKS02_FKP02.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 119 104.9)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 119 74.9)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.5 62 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 3.5 -0.5) (layer "F.SilkS"))
    (fp_text value "KEM X7R1206 10U" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 14 "5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 126.5 66 180)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "JP1" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "Jumper_2_Open" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 14 "5V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "DF_5V") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 64 67.5 -90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D8" (at 1 -2 90) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 17 "Net-(D8-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 19 "O_INFO") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF_Handsoldering" (layer "F.Cu")
    (tedit 5905D89D)
    (at 127.5 78)
    (descr "Diode MELF Handsoldering")
    (tags "Diode MELF Handsoldering")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -6.5 1) (layer "F.SilkS"))
    (fp_text value "SMS 2100 DIO" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.25) (layer "F.Fab"))
    (pad "1" smd rect (at -3.4 0) (size 3.5 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "24V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 3.4 0) (size 3.5 2.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 78.5 75.4)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "100k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 25 "Net-(Q1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 20 "MOSI") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "simonwidmer:DFPlayer_V2" (layer "F.Cu")
    (tedit 58F47D10)
    (at 101.89 79.63 -90)
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at 0 10.16 90) (layer "F.SilkS"))
    (fp_text value "DFPlayerMini" (at 0 -0.5 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -7.62 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "DF_5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" thru_hole circle locked (at -7.62 2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(R9-Pad2)") (pinfunction "RX") (pintype "input"))
    (pad "3" thru_hole circle locked (at -7.62 5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Player_TX") (pinfunction "TX") (pintype "output"))
    (pad "4" thru_hole circle locked (at -7.62 7.62 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "unconnected-(U5-Pad4)") (pinfunction "DAC_R") (pintype "output"))
    (pad "5" thru_hole circle locked (at -7.62 10.16 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "unconnected-(U5-Pad5)") (pinfunction "DAC_L") (pintype "output"))
    (pad "6" thru_hole circle locked (at -7.62 12.7 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(D3-Pad2)") (pinfunction "SPK_1") (pintype "output"))
    (pad "7" thru_hole circle locked (at -7.62 15.24 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "unconnected-(U5-Pad7)") (pinfunction "GND") (pintype "bidirectional"))
    (pad "8" thru_hole circle locked (at -7.62 17.78 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "unconnected-(U5-Pad8)") (pinfunction "SPK_2") (pintype "output"))
    (pad "9" thru_hole circle locked (at 10.16 17.78 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "unconnected-(U5-Pad9)") (pinfunction "IO_1") (pintype "bidirectional"))
    (pad "10" thru_hole circle locked (at 10.16 15.24 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "bidirectional"))
    (pad "11" thru_hole circle locked (at 10.16 12.7 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "unconnected-(U5-Pad11)") (pinfunction "IO_2") (pintype "bidirectional"))
    (pad "12" thru_hole circle locked (at 10.16 10.16 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "unconnected-(U5-Pad12)") (pinfunction "ADKEY_1") (pintype "bidirectional"))
    (pad "13" thru_hole circle locked (at 10.16 7.62 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "unconnected-(U5-Pad13)") (pinfunction "ADKEY_2") (pintype "bidirectional"))
    (pad "14" thru_hole circle locked (at 10.16 5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad3)") (pinfunction "USB+") (pintype "bidirectional"))
    (pad "15" thru_hole circle locked (at 10.16 2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)") (pinfunction "USB-") (pintype "bidirectional"))
    (pad "16" thru_hole circle locked (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "unconnected-(U5-Pad16)") (pinfunction "BUSY") (pintype "bidirectional"))
  )
  (footprint "Connector_USB:USB_A_Molex_67643_Horizontal" (layer "F.Cu")
    (tedit 5EA03975)
    (at 113 98 -90)
    (descr "USB type A, Horizontal, https://www.molex.com/pdm_docs/sd/676433910_sd.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 3.5 -3.19 90) (layer "F.SilkS"))
    (fp_text value "USB_A" (at 3.5 14.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.5 3.7 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.5) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 "DF_5V") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 4.5 0 270) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad3)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 7 0 270) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle (at 10.07 2.71 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "5" thru_hole circle (at -3.07 2.71 270) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Molex_67643_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 58.5 62)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -3.5 0) (layer "F.SilkS"))
    (fp_text value "X7R-G1206 100N" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 14 "5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 64 74.9)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "Diode_SMD:D_MiniMELF_Handsoldering" (layer "F.Cu")
    (tedit 5905D919)
    (at 62.75 87.9)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 6 1) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.75) (layer "F.Fab"))
    (pad "1" smd rect (at -2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C5-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 121.5 62.025 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D9" (at -0.975 -2 90) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 18 "Net-(D9-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 14 "5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF_Handsoldering" (layer "F.Cu")
    (tedit 5905D919)
    (at 110.55 82)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -1.75) (layer "F.SilkS"))
    (fp_text value "LL4148" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.75) (layer "F.Fab"))
    (pad "1" smd rect (at -2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2.75 0) (size 3.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D3-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT" (layer "F.Cu")
    (tedit 5B741BB0)
    (at 109.553 68.2075)
    (descr "DCDC-Converter, RECOM, RECOM_R-78E-0.5, SIP-3, pitch 2.54mm, package size 11.6x8.5x10.4mm^3, https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf")
    (tags "dc-dc recom buck sip-3 pitch 2.54mm")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 2.54 -7.56) (layer "F.SilkS"))
    (fp_text value "R-78E5.0-0.5" (at 2.54 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.25) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 3 "24V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.5 2.3) (drill 1) (layers *.Cu *.Mask)
      (net 4 "DF_5V") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_RECOM_R-78E-0.5_THT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "simonwidmer:wing_logo_l" (layer "F.Cu")
    (tedit 0)
    (at 121.5 89)
    (attr through_hole)
    (fp_text reference "wing_logo_l" (at 0 5) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
  )
  (footprint "Capacitor_SMD:C_1210_3225Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108 73)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -1.5 2.5) (layer "F.SilkS"))
    (fp_text value "KEM X5R1210 10U" (at 0 2.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "24V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0) (size 1.15 2.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.5 72.5 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -1.5 -2) (layer "F.SilkS"))
    (fp_text value "KEM X7R1206 10U" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "DF_5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 180) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 71.5 84)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 3 0.5) (layer "F.SilkS"))
    (fp_text value "330R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "24V") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 24 "Net-(R3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_2512_6332Metric_Pad1.52x3.35mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 126 82.5)
    (descr "Fuse SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "Märchentelefon.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at -5 1.5) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 0 2.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.9875 0) (size 1.525 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.163934)
      (net 27 "Net-(F1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.9875 0) (size 1.525 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.163934)
      (net 9 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 136 111) (end 136 58.75) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 47 93) (end 47 58.75) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 101 111) (end 101 93) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 47 58.75) (end 136 58.75) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 101 111) (end 136 111) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 101 93) (end 47 93) (layer "Edge.Cuts") (width 0.05))
  (gr_text "PB1" (at 64 70.5) (layer "F.SilkS"))
  (gr_text "A  B" (at 75.5 87) (layer "F.SilkS"))
  (gr_text "24VDC" (at 128.5 85.5) (layer "F.SilkS"))
  (gr_text "storyphone\nv1/2022\n" (at 133 101) (layer "F.SilkS"))
  (gr_text "Gehäuse: CB EAC-02-WH" (at 56.5 124) (layer "Cmts.User"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136 111)
        (xy 101 111)
        (xy 101 93.5)
        (xy 47 93)
        (xy 47 58.5)
        (xy 136.5 58.5)
      )
    )
  )
)
