(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010ec_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Boost_Gerbers/")
    )
  )
  (net 0 "")
  (net 1 "Net-(9v1-Pin_1)")
  (net 2 "Net-(In1-Pin_1)")
  (net 3 "Net-(Q2-B)")
  (net 4 "Net-(Q2-C)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 "Net-(D1-K)")
  (net 7 "GND")
  (net 8 "Net-(LED1-A)")
  (net 9 "Net-(Out1-Pin_1)")
  (net 10 "Net-(Q2-E)")
  (net 11 "Net-(swGnd1-Pin_1)")
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 168.148 92.202 180)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "Gnd" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 166.37 113.284 180)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "SwG" (at 0 2.032) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(swGnd1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 166.116 104.394)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -2.37) (layer "F.SilkS") hide)
    (fp_text value "43k" (at 3.81 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(Q2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 173.228 113.284 180)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "OG" (at 0 2.032) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 163.068 96.774 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 -2.37) (layer "F.SilkS") hide)
    (fp_text value "390" (at 3.81 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Q2-E)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 155.448 93.472)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -2.37) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 3.81 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q2-C)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 160.02 113.284 180)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "In" (at 0 2.032) (layer "F.SilkS"))
    (fp_text value "~" (at -3.81 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.07 2.032) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(In1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 151.13 94.742 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q2" (at 1.27 -1.778 90) (layer "F.SilkS"))
    (fp_text value "2N5088" (at 1.27 2.79 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 -1.778 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -0.508 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(Q2-E)") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(Q2-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 3.048 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q2-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 156.21 113.284 180)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "InG" (at 0 2.032) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.032) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 172.212 92.202 180)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "9v" (at 0 -1.998) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(9v1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "F.Cu")
    (at 151.13 104.1 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 -2.5 90) (layer "F.SilkS") hide)
    (fp_text value "0.1UF" (at 2.754 -2.159 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(In1-Pin_1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(Q2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 173.736 101.092 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -2.37) (layer "F.SilkS") hide)
    (fp_text value "430k" (at 3.81 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(Q2-B)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (at 166.116 96.52)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D1" (at 3.81 -2.12) (layer "F.SilkS") hide)
    (fp_text value "1N5817" (at 3.81 2.12) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(9v1-Pin_1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "F.Cu")
    (at 160.488 104.14 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*2.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 2.5mm Capacitor")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 -2.5) (layer "F.SilkS") hide)
    (fp_text value "0.1UF" (at 2.5 0 270) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q2-C)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W2.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 155.448 100.33)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 5.01 -2.37) (layer "F.SilkS") hide)
    (fp_text value "4.7K" (at 3.81 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(LED1-A)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(swGnd1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 163.195 113.284 180)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "SW" (at 0 2.032) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.05) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-K)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm" (layer "F.Cu")
    (at 169.545 113.284 180)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "O" (at 0 2.032) (layer "F.SilkS"))
    (fp_text value "~" (at 0 2.05) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.032) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(Out1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Potentiometer_THT:Potentiometer_Omeg_PC16BU_Vertical" (layer "F.Cu")
    (at 166.5948 107.95 90)
    (descr "Potentiometer, vertical, Omeg PC16BU, http://www.omeg.co.uk/pc6bubrc.htm")
    (tags "Potentiometer vertical Omeg PC16BU")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer, US symbol")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "POT1" (at 0.254 -7.342 90) (layer "B.SilkS"))
    (fp_text value "100K" (at 0.254 -2.46 90) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.254 -7.286 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.34 2.34) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -5 90) (size 2.34 2.34) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(Out1-Pin_1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 -10 90) (size 2.34 2.34) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(C2-Pad2)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Omeg_PC16BU_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 152.4 113.284 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "LPB1_Boost.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "LED" (at -2.032 1.275 180) (layer "F.SilkS"))
    (fp_text value "~" (at 0 4.87 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(LED1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 175.26 113.665) (end 175.26 91.44)
    (layer "Edge.Cuts"))
  (gr_arc (start 149.225 114.935) (mid 148.326974 114.563026) (end 147.955 113.665)
    (layer "Edge.Cuts"))
  (gr_line (start 147.955 91.44) (end 147.955 113.665)
    (layer "Edge.Cuts"))
  (gr_line (start 173.99 90.17) (end 149.225 90.17)
    (layer "Edge.Cuts"))
  (gr_arc (start 147.955 91.44) (mid 148.326974 90.541974) (end 149.225 90.17)
    (layer "Edge.Cuts"))
  (gr_arc (start 175.26 113.665) (mid 174.888026 114.563026) (end 173.99 114.935)
    (layer "Edge.Cuts"))
  (gr_arc (start 173.99 90.17) (mid 174.888026 90.541974) (end 175.26 91.44)
    (layer "Edge.Cuts"))
  (gr_line (start 149.225 114.935) (end 173.99 114.935)
    (layer "Edge.Cuts"))
  (gr_text "GuitarML" (at 148.336 108.077) (layer "F.SilkS"))
  (gr_text "Boost v2" (at 148.1836 109.728) (layer "F.SilkS"))
  (zone (net 7) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 175.26 113.665)
        (xy 175.26 91.44)
        (xy 173.99 90.17)
        (xy 149.225 90.17)
        (xy 147.955 91.44)
        (xy 147.955 113.665)
        (xy 149.225 114.935)
        (xy 173.355 114.935)
      )
    )
  )
  (zone (net 7) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 175.26 113.665)
        (xy 175.26 91.44)
        (xy 173.99 90.17)
        (xy 149.225 90.17)
        (xy 147.955 91.44)
        (xy 147.955 113.665)
        (xy 149.225 114.935)
        (xy 173.355 114.935)
      )
    )
  )
)
