(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "C")
  (title_block
    (title "Differential Buffer Board")
    (date "10/21/2022")
    (rev "v01")
    (company "NHMFL")
    (comment 1 "Sujana Uppalapati")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 "GND")
  (net 4 "+15V")
  (net 5 "-15V")
  (net 6 "Net-(C4-Pad2)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C7-Pad2)")
  (net 9 "Net-(C7-Pad1)")
  (net 10 "Net-(C10-Pad2)")
  (net 11 "Net-(C10-Pad1)")
  (net 12 "Net-(J1-Pad1)")
  (net 13 "Net-(J1-Pad2)")
  (net 14 "Net-(J1-Pad3)")
  (net 15 "Net-(J1-Pad4)")
  (net 16 "Net-(J1-Pad6)")
  (net 17 "Net-(J1-Pad7)")
  (net 18 "Net-(J1-Pad8)")
  (net 19 "Net-(J1-Pad9)")
  (net 20 "Net-(J2-Pad1)")
  (net 21 "Net-(J2-Pad3)")
  (net 22 "Net-(J2-Pad6)")
  (net 23 "Net-(J2-Pad8)")
  (net 24 "Net-(J3-Pad1)")
  (net 25 "Net-(J3-Pad3)")
  (net 26 "Net-(R5-Pad1)")
  (net 27 "Net-(R5-Pad2)")
  (net 28 "Net-(R6-Pad2)")
  (net 29 "Net-(R11-Pad1)")
  (net 30 "Net-(R11-Pad2)")
  (net 31 "Net-(R12-Pad2)")
  (net 32 "Net-(R17-Pad1)")
  (net 33 "Net-(R17-Pad2)")
  (net 34 "Net-(R18-Pad2)")
  (net 35 "Net-(R23-Pad1)")
  (net 36 "Net-(R23-Pad2)")
  (net 37 "Net-(R24-Pad2)")
  (net 38 "Net-(R25-Pad1)")
  (net 39 "Net-(R26-Pad2)")
  (net 40 "/Offset1")
  (net 41 "/Offset2")
  (net 42 "/Offset3")
  (net 43 "/Offset4")
  (net 44 "/Ref1")
  (net 45 "/Ref2")
  (net 46 "/Ref3")
  (net 47 "/Ref4")
  (net 48 "unconnected-(U5-Pad6)")
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 95.14 200.18)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at 0.384 -1.75) (layer "F.SilkS"))
    (fp_text value "470k" (at 1.778 3.746502) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(R23-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(R24-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 105.05 120.63)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP7" (at 0.0856 -1.74) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0.000003 2.540006) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(J2-Pad3)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 45.16 243.97)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP15" (at -0.127 -2.032) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at -0.000007 2.539995) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(J3-Pad3)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 90.14 205.28 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D16" (at 2.51 -2 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809991 2.28601 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(C10-Pad1)") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 77.089 104.6226 90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at -1.8674 0.131 180) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.777996 3.746489 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 80.52 162.446 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at -1.708 0.0498 180) (layer "F.SilkS"))
    (fp_text value "2000pF" (at 1.778004 3.746501 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 66.2178 105.537)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP3" (at 0.0022 -1.767) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at -0.000012 2.539997) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(J1-Pad2)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 77.54 187.546 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at -1.7026 -0.201) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.778011 3.74649 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(C10-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 105.746 135.99 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 4.847643 -0.059934) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.778011 3.746498 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 89.535 129.1336 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D7" (at 2.0036 -1.985 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809991 2.286 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(C4-Pad1)") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "A") (pintype "input"))
  )
  (footprint "KiCAD Library_SU:Bourns_3296W" (layer "F.Cu")
    (tedit 615EFFF3)
    (at 154.36 219.24)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R30" (at -1.35 -3.32) (layer "F.SilkS"))
    (fp_text value "10K" (at 192.809508 42.727488) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 "/Offset4") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5.08 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(R26-Pad2)") (pintype "passive"))
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 90.17 193.24 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D15" (at 2.5122 -2.035 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.81 2.286 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(C10-Pad1)") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "A") (pintype "input"))
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 66.881356 201.500377)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP12" (at -0.0278 -1.791) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J1-Pad9)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 84.45 161.07 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D10" (at 2.4582 -2.105 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.810011 2.286 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad2)") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 77.09 155.306 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at -1.6642 -0.101 180) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.778003 3.746511 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C7-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:Bourns_3296W" (layer "F.Cu")
    (tedit 615EFFF3)
    (at 141.03 219.16)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R29" (at -1.4 -3.35) (layer "F.SilkS"))
    (fp_text value "10K" (at 2.54001 3.809995) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 "/Offset3") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5.08 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(R26-Pad2)") (pintype "passive"))
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 157.988 255.27)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad4" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_DIP_Thru:DIP08_Thru" (layer "F.Cu")
    (tedit 5EBB17A1)
    (at 98.36 164.78)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost90 10)
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "U3" (at -1.5096 -2.1898 90 unlocked) (layer "F.SilkS"))
    (fp_text value "INA114(8-Pin)" (at 3.81 2.54) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(R18-Pad2)") (pinfunction "Rg") (pintype "input"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad2)") (pinfunction "Vin-") (pintype "input"))
    (pad "3" thru_hole circle locked (at 5.08 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 "Net-(C7-Pad1)") (pinfunction "Vin+") (pintype "input"))
    (pad "4" thru_hole circle locked (at 7.62 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 7.62 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 46 "/Ref3") (pinfunction "Ref") (pintype "input"))
    (pad "6" thru_hole circle locked (at 5.08 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad6)") (pinfunction "Vo") (pintype "output"))
    (pad "7" thru_hole circle locked (at 2.54 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" thru_hole circle locked (at 0 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "Net-(R17-Pad2)") (pinfunction "Rg") (pintype "input"))
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 84.965 205.2802 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D13" (at 2.5302 -2.055 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809989 2.286002 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(C10-Pad2)") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_SOIC:SOIC-8" (layer "F.Cu")
    (tedit 615F0EF6)
    (at 128.055 235.9575)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at -1.505 -2.1315 90) (layer "F.SilkS"))
    (fp_text value "Ref200AU" (at 2.222501 2.22249) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.27 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
    (pad "3" smd rect locked (at 2.54 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "4" smd rect locked (at 3.81 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" smd rect locked (at 3.81 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "6" smd rect locked (at 2.54 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "unconnected-(U5-Pad6)") (pinfunction "S") (pintype "passive+no_connect"))
    (pad "7" smd rect locked (at 1.27 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(R26-Pad2)") (pintype "passive"))
    (pad "8" smd rect locked (at 0 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
      (offset (xyz 1.905 2.794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 66.2178 118.9482)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP5" (at 0.1122 -1.7482) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0 2.540006) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J1-Pad3)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 89.535 141.2494 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D8" (at 1.9594 -1.985 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809994 2.286005 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(C4-Pad1)") (pinfunction "A") (pintype "input"))
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 105.83 152.39)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP10" (at -0.0144 -1.77) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0 2.539996) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(J2-Pad6)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 108.136315 243.017901)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP17" (at 0 -1.77) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at -0.000012 2.539993) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 94.7166 99.06 90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.2 -1.7566 90) (layer "F.SilkS"))
    (fp_text value "30k" (at 1.778009 3.746493 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(R5-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(R5-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 80.9498 130.5306 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at -1.7106 0.0498 180) (layer "F.SilkS"))
    (fp_text value "2000pF" (at 1.777999 3.746508 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 105.12 184.92)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP13" (at -0.03 -1.81) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0.000012 2.540004) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(J2-Pad8)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 66.896 197.72)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 0.3322 -1.7336) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.778 3.7465) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(J1-Pad9)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C10-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 150.748511 230.307948 90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 4.792947 -0.101132 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.777995 3.746505 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 84.455 129.1844 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D6" (at 1.9944 -1.985 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809997 2.285997 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad2)") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 100.91 154.354 90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 4.7372 -0.0796 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.777999 3.746506 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 157.988 90.932)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad3" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_DIP_Thru:DIP08_Thru" (layer "F.Cu")
    (tedit 5EBB17A1)
    (at 98.3996 100.7364)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost90 10)
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "U1" (at -1.58 -2.21 90 unlocked) (layer "F.SilkS"))
    (fp_text value "INA114(8-Pin)" (at 3.80999 2.540011) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R6-Pad2)") (pinfunction "Rg") (pintype "input"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)") (pinfunction "Vin-") (pintype "input"))
    (pad "3" thru_hole circle locked (at 5.08 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)") (pinfunction "Vin+") (pintype "input"))
    (pad "4" thru_hole circle locked (at 7.62 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 7.62 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 44 "/Ref1") (pinfunction "Ref") (pintype "input"))
    (pad "6" thru_hole circle locked (at 5.08 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad1)") (pinfunction "Vo") (pintype "output"))
    (pad "7" thru_hole circle locked (at 2.54 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" thru_hole circle locked (at 0 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(R5-Pad2)") (pinfunction "Rg") (pintype "input"))
  )
  (footprint "KiCAD Library_SU:D_400" (layer "F.Cu")
    (tedit 615EFF7D)
    (at 73.1012 91.4146 -90)
    (descr "Diode, Thru Hole, 400mil Spacing")
    (tags "400")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TVS1" (at 5.3154 2.6812 90) (layer "F.SilkS"))
    (fp_text value "P6KE39CA(33V)" (at 5.079992 3.047988 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 10.16 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)") (pintype "passive"))
  )
  (footprint "KiCAD Library_SU:D_400" (layer "F.Cu")
    (tedit 615EFF7D)
    (at 73.1012 123.4186 -90)
    (descr "Diode, Thru Hole, 400mil Spacing")
    (tags "400")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TVS2" (at 5.0114 2.6412 90) (layer "F.SilkS"))
    (fp_text value "P6KE39CA(33V)" (at 5.080002 3.048003 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 10.16 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad2)") (pintype "passive"))
  )
  (footprint "KiCAD Library_SU:Bourns_3296W" (layer "F.Cu")
    (tedit 615EFFF3)
    (at 115.08 219.23)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R27" (at -1.32 -3.31) (layer "F.SilkS"))
    (fp_text value "10K" (at 2.540002 3.809998) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 "/Offset1") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5.08 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(R26-Pad2)") (pintype "passive"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 77.089 91.4146 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at -1.7046 -0.021) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 66.48 169.3)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP9" (at -0.0478 -1.7854) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at -0.000004 2.539988) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(J1-Pad7)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 43.434 90.932)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad1" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 77.299222 200.765928 90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at -1.8266 0.061) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.777999 3.746502 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C10-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Connector_Phoenix:MCV_3Pin_1803439" (layer "F.Cu")
    (tedit 5F3AFEB9)
    (at 45.175 228.16 -90)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -3.85 3.985 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "MCV_3Pin_1803439" (at 3.810006 6.350009 90) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(J3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at 3.81 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole roundrect (at 7.62 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(J3-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_3Pin_1803439.stp"
      (offset (xyz 7.62 3.048 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "ap_SOIC:SOIC-8" (layer "F.Cu")
    (tedit 615F0EF6)
    (at 152.975 236.0375)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U7" (at -1.465 -2.1375 90) (layer "F.SilkS"))
    (fp_text value "ADA4077-2" (at 2.222511 2.222495) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/Ref3") (pinfunction "OUT_A") (pintype "output"))
    (pad "2" smd rect locked (at 1.27 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/Ref3") (pinfunction "-IN_A") (pintype "input"))
    (pad "3" smd rect locked (at 2.54 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/Offset3") (pinfunction "+IN_A") (pintype "input"))
    (pad "4" smd rect locked (at 3.81 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect locked (at 3.81 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/Offset4") (pinfunction "+IN_B") (pintype "input"))
    (pad "6" smd rect locked (at 2.54 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/Ref4") (pinfunction "-IN_B") (pintype "input"))
    (pad "7" smd rect locked (at 1.27 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/Ref4") (pinfunction "OUT_B") (pintype "output"))
    (pad "8" smd rect locked (at 0 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
      (offset (xyz 1.905 2.794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "KiCAD Library_SU:C_Tant_3024" (layer "F.Cu")
    (tedit 615EFF39)
    (at 78.10375 235.76 -90)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C18" (at -4.26 5.99375 180) (layer "F.SilkS"))
    (fp_text value "47uF" (at 0.127012 8.191495 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 6.604 2.286) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 0 5.842 270) (size 6.604 2.286) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
  )
  (footprint "ap_SOIC:SOIC-8" (layer "F.Cu")
    (tedit 615F0EF6)
    (at 142.745 236.0175)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U6" (at -1.435 -2.1375 90) (layer "F.SilkS"))
    (fp_text value "ADA4077-2" (at 2.222489 2.222512) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/Ref1") (pinfunction "OUT_A") (pintype "output"))
    (pad "2" smd rect locked (at 1.27 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/Ref1") (pinfunction "-IN_A") (pintype "input"))
    (pad "3" smd rect locked (at 2.54 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "/Offset1") (pinfunction "+IN_A") (pintype "input"))
    (pad "4" smd rect locked (at 3.81 0) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd rect locked (at 3.81 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/Offset2") (pinfunction "+IN_B") (pintype "input"))
    (pad "6" smd rect locked (at 2.54 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/Ref2") (pinfunction "-IN_B") (pintype "input"))
    (pad "7" smd rect locked (at 1.27 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/Ref2") (pinfunction "OUT_B") (pintype "output"))
    (pad "8" smd rect locked (at 0 -5.715) (size 0.762 1.5748) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
      (offset (xyz 1.905 2.794 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 66.476 165.48)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0.3022 -1.7164) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.778012 3.746498) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(J1-Pad7)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C7-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:C_Tant_3024" (layer "F.Cu")
    (tedit 615EFF39)
    (at 71.83625 219.38 90)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C17" (at 4.18 -0.13625 180) (layer "F.SilkS"))
    (fp_text value "47uF" (at 0.127002 8.191488 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 6.604 2.286) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 0 5.842 90) (size 6.604 2.286) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 84.455 141.2494 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D5" (at 1.9994 -1.985 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809994 2.286 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad2)") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 105.986442 167.945533 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 4.82167 -0.026748) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 66.2178 101.5746)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -0.0578 -1.7646) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.778005 3.746502) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(J1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 80.9498 98.5266 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 1.6634 1.7198 90) (layer "F.SilkS"))
    (fp_text value "2000pF" (at 1.777999 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:220uH_HDS124-221MTR" (layer "F.Cu")
    (tedit 6164819F)
    (at 55.62 219.35 90)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L1" (at 7.97 -1.32 180) (layer "F.SilkS"))
    (fp_text value "220uH" (at 0.253938 13.970005 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 5.5118 3.0226) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(J3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 0 10.16 90) (size 5.5118 3.0226) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 94.3484 130.6412 90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 1.0706 -1.7666 90) (layer "F.SilkS"))
    (fp_text value "30k" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(R11-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(R11-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 77.089 136.6266 90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -1.8334 0.121) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C4-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 84.48 173.12 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D9" (at 2.0032 -2.035 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809994 2.285991 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad2)") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 66.846 187.57)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 0.3022 -1.7866) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.77799 3.746509) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(J1-Pad8)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(C10-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 105.07 216.81)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP16" (at -0.06 -1.71) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0.000004 2.540005) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "KiCAD Library_SU:220uH_HDS124-221MTR" (layer "F.Cu")
    (tedit 6164819F)
    (at 55.51 235.74 90)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L2" (at 7.97 -1.16 180) (layer "F.SilkS"))
    (fp_text value "220uH" (at 0.25409 13.969874 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 5.5118 3.0226) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(J3-Pad3)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 0 10.16 90) (size 5.5118 3.0226) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pinfunction "2") (pintype "passive"))
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 100.69 122.154 90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 4.7378 -0.0096) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 84.965 193.266 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D14" (at 2.496 -2.035 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.810003 2.285991 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(C10-Pad2)") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 94.71 162.724 90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 1.0908 -1.7966 90) (layer "F.SilkS"))
    (fp_text value "30k" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(R17-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(R17-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 89.535 109.22 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at 1.99 -1.985 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809994 2.286 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_DIP_Thru:DIP08_Thru" (layer "F.Cu")
    (tedit 5EBB17A1)
    (at 98.21 196.88)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost90 10)
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "U4" (at -1.5196 -2.2126 -270 unlocked) (layer "F.SilkS"))
    (fp_text value "INA114(8-Pin)" (at 3.81001 2.53999) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R24-Pad2)") (pinfunction "Rg") (pintype "input"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(C10-Pad2)") (pinfunction "Vin-") (pintype "input"))
    (pad "3" thru_hole circle locked (at 5.08 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "Net-(C10-Pad1)") (pinfunction "Vin+") (pintype "input"))
    (pad "4" thru_hole circle locked (at 7.62 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 7.62 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 47 "/Ref4") (pinfunction "Ref") (pintype "input"))
    (pad "6" thru_hole circle locked (at 5.08 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad8)") (pinfunction "Vo") (pintype "output"))
    (pad "7" thru_hole circle locked (at 2.54 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" thru_hole circle locked (at 0 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 "Net-(R23-Pad2)") (pinfunction "Rg") (pintype "input"))
  )
  (footprint "KiCAD Library_SU:D_400" (layer "F.Cu")
    (tedit 615EFF7D)
    (at 73.76 187.56 -90)
    (descr "Diode, Thru Hole, 400mil Spacing")
    (tags "400")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TVS4" (at 5.1918 2.6812 90) (layer "F.SilkS"))
    (fp_text value "P6KE39CA(33V)" (at 5.080003 3.048 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 10.16 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(C10-Pad2)") (pintype "passive"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 94.68 194.694 90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at 1.0718 -1.7666 90) (layer "F.SilkS"))
    (fp_text value "30k" (at 1.778012 3.746502 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(R23-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(R23-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 45.201742 219.349999)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP14" (at -0.127 -2.032) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0.000003 2.54001) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(J3-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 66.216 123.37)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0.0022 -1.7048) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.778 3.746498) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(J1-Pad3)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C4-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 77.089 123.3932 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at -1.6632 -0.061) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.778005 3.746491 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C4-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:C_Electrolytic_SMD_EMVY101ARA101MKE0S" (layer "F.Cu")
    (tedit 61647E1C)
    (at 90.46 233.89)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C20" (at -6.2 -2.82) (layer "F.SilkS"))
    (fp_text value "100uF" (at 0.380992 13.589) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.2954 4.7752) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 0 9.144) (size 1.2954 4.7752) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 66.31 151.54)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP8" (at -0.0978 -1.7598) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at -0.000001 2.540012) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J1-Pad6)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 66.176 133.59)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -0.0678 -1.7382) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.777936 3.7465) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(J1-Pad4)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C4-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 89.53 161.07 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D11" (at 2.422 -2.025 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.810001 2.286005 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(C7-Pad1)") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "A") (pintype "input"))
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 89.535 96.4438 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at 1.9638 -2.015 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809997 2.286012 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad1)") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 66.2178 91.4146)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.0578 -1.7246) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.778 3.7465) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 61.19 142.33)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP1" (at -0.127 -2.032) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "KiCAD Library_SU:MCV_9Pin_1803497" (layer "F.Cu")
    (tedit 615EFF57)
    (at 153 159.36 90)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -3.66 3.97 90) (layer "F.SilkS"))
    (fp_text value "MCV_9Pin_1803497" (at 14.692 27.833 90) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(J2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at 3.81 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole roundrect (at 7.62 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(J2-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole roundrect (at 11.43 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole roundrect (at 15.24 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole roundrect (at 19.05 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(J2-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole roundrect (at 22.86 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole roundrect (at 26.67 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(J2-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole roundrect (at 30.48 0 90) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "9") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_6-Pin_1803468.stp"
      (offset (xyz -2.5908 -3.4798 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 158.93873 236.022736 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 4.870585 -0.054244) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 95.106 136.27)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0.314 -1.74) (layer "F.SilkS"))
    (fp_text value "470k" (at 1.778 3.7465) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(R11-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(R12-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 84.455 109.22 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 1.99 -2.025 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809997 2.286002 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)") (pinfunction "A") (pintype "input"))
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 66.846 183.6284)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP11" (at -0.0678 -1.835) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(J1-Pad8)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 125.8 235.966 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 4.844 0.01 unlocked) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(R25-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 105.9942 103.6574 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 4.901126 0.000176) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.778003 3.746507 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 66.18 137.49)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP6" (at 0.0622 -1.7462) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at 0.000009 2.539992) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(J1-Pad4)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 140.5 230.294 90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 4.792947 -0.162259 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.777992 3.746498 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 95.3516 103.505)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -0.127 -1.778) (layer "F.SilkS"))
    (fp_text value "470k" (at 1.777996 3.74651) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(R5-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(R6-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 66.296 155.31)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0.3522 -1.7372) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.778003 3.746489) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J1-Pad6)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(C7-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 148.45 236.036 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 4.90679 -0.015528) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.778003 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:MCV_9Pin_1803497" (layer "F.Cu")
    (tedit 615EFF57)
    (at 44.395 127.14 -90)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -3.7 3.905 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "MCV_9Pin_1803497" (at 7.874 5.588 90) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect (at 0 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at 3.81 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(J1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole roundrect (at 7.62 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(J1-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole roundrect (at 11.43 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(J1-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole roundrect (at 15.24 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole roundrect (at 19.05 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(J1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole roundrect (at 22.86 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(J1-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole roundrect (at 26.67 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J1-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole roundrect (at 30.48 0 270) (size 2.54 5.08) (drill 1.4224) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 19 "Net-(J1-Pad9)") (pinfunction "9") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Phoenix_MC.3dshapes/MCV_6-Pin_1803468.stp"
      (offset (xyz -2.5908 -3.4798 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_400" (layer "F.Cu")
    (tedit 615EFF7D)
    (at 73.1012 155.321 -90)
    (descr "Diode, Thru Hole, 400mil Spacing")
    (tags "400")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TVS3" (at 5.319 2.7312 90) (layer "F.SilkS"))
    (fp_text value "P6KE39CA(33V)" (at 5.080003 3.048007 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 10.16 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad2)") (pintype "passive"))
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 84.455 96.4438 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 2.0038 -2.045 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.809994 2.286007 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "A") (pintype "input"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 129.31 224.826 -90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at 2.68 1.75 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(R26-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Pad_Hole:125_Hole_Iso" (layer "F.Cu")
    (tedit 5F1621FD)
    (at 43.434 255.27)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Pad2" (at 0.635 3.81) (layer "F.SilkS") hide)
    (fp_text value "125_hole_iso" (at 0.635 5.715) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 4.445) (clearance 4.445))
  )
  (footprint "ap_PCB_Misc:Maglab_Logo" (layer "F.Cu")
    (tedit 5F3FD4DC)
    (at 75.175 258.105)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "M1" (at 2.0574 3.13436) (layer "F.SilkS") hide)
    (fp_text value "MAGLAB_LOGO_1_2" (at 2.62382 1.36652) (layer "F.Fab") hide)
    (fp_text user "NATIONAL" (at 9.144 -4.2545) (layer "F.SilkS"))
    (fp_text user "AGLAB" (at 11.176 -1.5875) (layer "F.SilkS"))
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 103.68 239.986 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C22" (at -1.726 0.09 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.77799 3.746491 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:C_Electrolytic_SMD_EMVY101ARA101MKE0S" (layer "F.Cu")
    (tedit 61647E1C)
    (at 90.61 216.8222)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C19" (at -6.25 -2.8622) (layer "F.SilkS"))
    (fp_text value "100uF" (at 0.38099 13.589005) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.2954 4.7752) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 0 9.144) (size 1.2954 4.7752) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 95.313793 168.311949)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0.2984 -1.7794) (layer "F.SilkS"))
    (fp_text value "470k" (at 1.778 3.7465) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(R17-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(R18-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:Bourns_3296W" (layer "F.Cu")
    (tedit 615EFFF3)
    (at 128.12 219.26)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R28" (at -1.34 -3.27) (layer "F.SilkS"))
    (fp_text value "10K" (at 2.539992 3.809998) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 "/Offset2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5.08 0) (size 2.032 2.032) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(R26-Pad2)") (pintype "passive"))
  )
  (footprint "ap_Resistor_SMD:R_1206" (layer "F.Cu")
    (tedit 5F3AF27A)
    (at 77.089 168.529 90)
    (descr "Resistor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at -1.841 -0.009) (layer "F.SilkS"))
    (fp_text value "10k" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C7-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0508 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_DIP_Thru:DIP08_Thru" (layer "F.Cu")
    (tedit 5EBB17A1)
    (at 98.15 132.87)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost90 10)
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "U2" (at -1.5096 -2.3112 -270 unlocked) (layer "F.SilkS"))
    (fp_text value "INA114(8-Pin)" (at 3.810034 2.540009) (layer "F.Fab") hide)
    (pad "1" thru_hole roundrect locked (at 0 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(R12-Pad2)") (pinfunction "Rg") (pintype "input"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad2)") (pinfunction "Vin-") (pintype "input"))
    (pad "3" thru_hole circle locked (at 5.08 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(C4-Pad1)") (pinfunction "Vin+") (pintype "input"))
    (pad "4" thru_hole circle locked (at 7.62 0) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 7.62 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 45 "/Ref2") (pinfunction "Ref") (pintype "input"))
    (pad "6" thru_hole circle locked (at 5.08 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad3)") (pinfunction "Vo") (pintype "output"))
    (pad "7" thru_hole circle locked (at 2.54 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" thru_hole circle locked (at 0 -7.62) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "Net-(R11-Pad2)") (pinfunction "Rg") (pintype "input"))
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 100.95 216.786 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C21" (at -1.76 0.016 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.777992 3.746502 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 105.856 200.07 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 4.837032 -0.035289) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.77799 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "-15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 66.2178 87.3506)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP2" (at -0.1078 -1.7806) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at -0.000007 2.539995) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 100.72 186.424 90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 4.8006 -0.0652 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 81.332096 194.61859 -90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -1.6886 0.0598) (layer "F.SilkS"))
    (fp_text value "2000pF" (at 1.777995 3.746509 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 270) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "KiCAD Library_SU:D_300" (layer "F.Cu")
    (tedit 615EFF71)
    (at 89.52 173.12 90)
    (descr "Diode, Thru Hole, 300mil Spacing")
    (tags "300")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D12" (at 2.42 -2.02 90) (layer "F.SilkS"))
    (fp_text value "FDH333" (at 3.810034 2.285998 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle locked (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "-15V") (pinfunction "K") (pintype "input"))
    (pad "2" thru_hole circle locked (at 7.62 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(C7-Pad1)") (pinfunction "A") (pintype "input"))
  )
  (footprint "KiCAD Library_SU:TestPoint_RCW-0C_SMD" (layer "F.Cu")
    (tedit 615DE2F7)
    (at 105.0544 88.9762)
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TP4" (at 0.1256 -1.7462) (layer "F.SilkS"))
    (fp_text value "TestPoint_S2761-46R" (at -0.000007 2.539992) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0) (size 3.048 1.524) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(J2-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KISYS3DMOD}/TestPoint.3dshapes/s2761-46r.stp"
      (offset (xyz 0.0254 0 0.254))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "ap_Cap_SMD:C_1206" (layer "F.Cu")
    (tedit 5F3ADD4B)
    (at 100.9396 89.8144 90)
    (descr "Capacitor SMD 1206 Package")
    (tags "1206")
    (property "Sheetfile" "Differential buffer Board.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.778 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.778 3.7465 90) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at 0 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 3.048 0 90) (size 1.7272 1.8288) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
      (offset (xyz 1.524 -0.0127 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 33.655 82.55) (end 167.64 264.16) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "-15V" (at 50.386838 235.65256) (layer "F.SilkS"))
  (gr_text "PS C+" (at 147.32 140.335) (layer "F.SilkS"))
  (gr_text "PS D-" (at 50.5206 157.734) (layer "F.SilkS"))
  (gr_text "PS A-" (at 50.5206 131.064) (layer "F.SilkS"))
  (gr_text "+15V" (at 50.291429 228.229793) (layer "F.SilkS"))
  (gr_text "PS B-" (at 147.32 147.955) (layer "F.SilkS"))
  (gr_text "PS B" (at 134.038635 215.948447) (layer "F.SilkS"))
  (gr_text "PS D+" (at 147.32 132.715) (layer "F.SilkS"))
  (gr_text "PS D" (at 160.347885 215.891783) (layer "F.SilkS"))
  (gr_text "1" (at 39.991497 225.679183 270) (layer "F.SilkS"))
  (gr_text "Differential Buffered Holec Current \n" (at 159.137808 143.922337 90) (layer "F.SilkS"))
  (gr_text "PS A+" (at 147.32 159.385) (layer "F.SilkS"))
  (gr_text "COM" (at 50.164412 231.803593) (layer "F.SilkS"))
  (gr_text "PS C-" (at 50.5206 150.114) (layer "F.SilkS"))
  (gr_text "PS B-" (at 50.5206 138.684) (layer "F.SilkS"))
  (gr_text "PS D-" (at 147.32 128.905) (layer "F.SilkS"))
  (gr_text "PS C-" (at 147.32 136.525) (layer "F.SilkS"))
  (gr_text "PS C+" (at 50.5206 146.304) (layer "F.SilkS"))
  (gr_text "PS B+" (at 147.32 151.765) (layer "F.SilkS"))
  (gr_text "DC Power Input" (at 39.769947 232.287855 -90) (layer "F.SilkS"))
  (gr_text "1" (at 39.168573 124.841633 -90) (layer "F.SilkS"))
  (gr_text "PS A" (at 120.966056 215.956521) (layer "F.SilkS"))
  (gr_text "Differential Buffer Board(v01)\nS Uppalapati 2022 " (at 109.4 255.41) (layer "F.SilkS"))
  (gr_text "PS C" (at 147.004226 215.893944) (layer "F.SilkS"))
  (gr_text "Buffered Holec Current\n" (at 38.1 143.51 270) (layer "F.SilkS"))
  (gr_text "COM" (at 147.32 144.145) (layer "F.SilkS"))
  (gr_text "PS A+" (at 50.5206 127.254) (layer "F.SilkS"))
  (gr_text "PS D+" (at 50.5206 153.924) (layer "F.SilkS"))
  (gr_text "PS B+" (at 50.5206 134.874) (layer "F.SilkS"))
  (gr_text "COM" (at 50.419 142.748) (layer "F.SilkS"))
  (gr_text "PS A-" (at 147.32 155.575) (layer "F.SilkS"))
  (gr_text "1" (at 158.275071 161.794109 90) (layer "F.SilkS"))
  (zone (net 3) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.135 266.7)
        (xy 25.4 264.795)
        (xy 25.4 76.2)
        (xy 191.135 76.2)
      )
    )
  )
  (zone (net 3) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 191.135 266.7)
        (xy 24.765 266.7)
        (xy 25.4 76.2)
        (xy 191.135 76.2)
      )
    )
  )
)
